/*
 *	This is an example configuration file.
 */

# Yet another comment

router id 62.168.0.1;

define xyzzy = (120+10);

protocol device {
#	disabled;
#	interface "eth*", "ppp*";
}

protocol direct {
}

protocol kernel {
	disabled;
	ipv4;			# Must be specified at least one channel
#	learn;			# Learn all routes from the kernel
#	scan time 10;		# Scan kernel tables every 10 seconds
}

protocol static {
#	disabled;

	ipv4 {
		export all;

		import filter {
			print "ahoj";
			print source;
			if source = RTS_STATIC then {
				print "It is from static";
			}
			print from;
			from = 1.2.3.4;
			print from;

			preference = 15;
			print preference;
			preference = 29;
			print preference;
			rip_metric = 1;
			print rip_metric;
			rip_metric = rip_metric + 5;
			print rip_metric;

			bgp_community = -empty-;
			print "hi";
			bgp_community = add(bgp_community, (1,2));
			print "hello";
			bgp_community = add(bgp_community, (2,3));
			bgp_community.add((4,5));
			print "community = ", bgp_community;
			bgp_community.delete((2,3));
			print "community = ", bgp_community;
			bgp_community.empty;
			print "community = ", bgp_community;
			print "done";

			accept;
		};
	};
	route 0.0.0.0/0 via 195.113.31.113;
	route 62.168.0.0/25 reject;
	route 1.2.3.4/32 via 195.113.31.124;
	route 10.0.0.0/8 reject;
	route 10.1.1.0/24 via 62.168.0.3;
	route 10.1.2.0/24 via 62.168.0.3;
	route 10.1.3.0/24 via 62.168.0.4;
	route 10.2.0.0/24 via "arc0";
}
