
--  ===========================================================
-- Copyright (C)  2009 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description:    HUAWEI POE MIB Definition 
-- Reference:      This mib was extracted from IEEE 802.3af
-- Version:        V1.0
-- History:        Liuhui ,2009-08-24, Create
-- ===========================================================

	HUAWEI-POE-MIB DEFINITIONS ::= BEGIN
 
		IMPORTS
			hwDatacomm			
				FROM HUAWEI-MIB			
			InterfaceIndex			
				FROM IF-MIB			
			EnabledStatus			
				FROM P-BRIDGE-MIB			
			OBJECT-GROUP, NOTIFICATION-GROUP			
				FROM SNMPv2-CONF			
			Integer32, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE			
				FROM SNMPv2-SMI;
	
	
		hwPoeMIB MODULE-IDENTITY 
			LAST-UPDATED "200908241133Z"		-- August 24, 2009 at 11:33 GMT
			ORGANIZATION 
				"Huawei Technologies co.,Ltd."
			CONTACT-INFO 
				"R&D BeiJing, Huawei Technologies co.,Ltd.
				Huawei Bld.,NO.3 Xinxi Rd., 
				Shang-Di Information Industry Base,
				Hai-Dian District Beijing P.R. China
				Zip:100085 
				Http://www.huawei.com                       
				E-mail:support@huawei.com"
			DESCRIPTION 
				"The HUAWEI-POE-MIB contains objects to manage POE."
			::= { hwDatacomm 195 }
		
	
--
-- Node definitions
--
	
		hwPoeGlobalObjects OBJECT IDENTIFIER ::= { hwPoeMIB 1 }
		
		
		hwPoePower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object identifies the maximum POE power of the system."
			::= { hwPoeGlobalObjects 1 }
			
		hwPoePowerRsvPercent OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object identifies the reserved percent of total POE power."
			::= { hwPoeGlobalObjects 4 }
		
		hwPoePowerUtilizationThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object identifies the utilization threshold of total POE power."
			::= { hwPoeGlobalObjects 5 }		
		
		hwPoeSlotTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwPoeSlotEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This object indicates the slot configuration table of POE."
			::= { hwPoeMIB 2 }
		
		
		hwPoeSlotEntry OBJECT-TYPE
			SYNTAX HwPoeSlotEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This object indicates the entry of the slot configuration table of POE."
			INDEX { hwPoeSlotId }
			::= { hwPoeSlotTable 1 }
		
		HwPoeSlotEntry ::=
			SEQUENCE { 
				hwPoeSlotId
					Integer32,
				hwPoeSlotMaximumPower
					Integer32,
				hwPoeSlotAvailablePower
					Integer32,
				hwPoeSlotReferencePower
					Integer32,
				hwPoeSlotConsumingPower
					Integer32,
				hwPoeSlotPeakPower
					Integer32,
				hwPoeSlotLegacyDetect
					EnabledStatus,
				hwPoeSlotPowerManagementManner
					INTEGER,
				hwPoeSlotIsPoeDevice
					OCTET STRING,
				hwPoeDimmId
				  Integer32,
				hwPoeSlotPowerRsvPercent
				  Integer32,
				hwPoeSlotPowerUtilizationThreshold
				  Integer32
			 }

		
		hwPoeSlotId OBJECT-TYPE
			SYNTAX Integer32 (0..8)
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This object identifies the slot ID."
			::= { hwPoeSlotEntry 1 }
		
		
		hwPoeSlotMaximumPower OBJECT-TYPE
			SYNTAX Integer32 (0..1600000)
			UNITS "mW"
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object identifies the maximum power set by users. The value is expressed in mW."
			DEFVAL { '1B1980'h }
			::= { hwPoeSlotEntry 2 }
		
		
		hwPoeSlotAvailablePower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object idenfies the available Power. The value is expressed in mW."
			::= { hwPoeSlotEntry 3 }
		
		
		hwPoeSlotReferencePower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object identifies the total reference power of a slot. The value is expressed in mW."
			::= { hwPoeSlotEntry 4 }
		
		
		hwPoeSlotConsumingPower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object identifies the total consuming power of a slot. The value is expressed in mW."
			::= { hwPoeSlotEntry 5 }
		
		
		hwPoeSlotPeakPower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object identifies the total peak power of a slot. The value is expressed in mW."
			::= { hwPoeSlotEntry 6 }
		
		
		hwPoeSlotLegacyDetect OBJECT-TYPE
			SYNTAX EnabledStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the compatibility detection of a non-standard device. (1:enable;  2:disable(default))"
			DEFVAL { disabled }
			::= { hwPoeSlotEntry 7 }
		
		
		hwPoeSlotPowerManagementManner OBJECT-TYPE
			SYNTAX INTEGER
				{
				manual(1),
				auto(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object identifies the power management manner. (1:manual, 2:auto(default))."
			DEFVAL { auto }
			::= { hwPoeSlotEntry 8 }
		
		
		hwPoeSlotIsPoeDevice OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates whether the device supports PoE."
			::= { hwPoeSlotEntry 9 }
		

		hwPoeDimmId OBJECT-TYPE
			SYNTAX Integer32 (0..1)
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"This object identifies the DIMM ID."
			::= { hwPoeSlotEntry 10 }

		hwPoeSlotPowerRsvPercent OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object identifies the reserved percent of POE power in slot."
			::= { hwPoeSlotEntry 11 }

		hwPoeSlotPowerUtilizationThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object identifies the utilization threshold of total POE power in slot."
			::= { hwPoeSlotEntry 12 }
		
		hwPoePortTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwPoePortEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This object indicates the table that contains the configuration parameters of a POE interface. One entry corresponds to a POE interface."
			::= { hwPoeMIB 3 }
		
		
		hwPoePortEntry OBJECT-TYPE
			SYNTAX HwPoePortEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This object indicates the entry of POE Port Table."
			INDEX { hwPoePortIfIndex }
			::= { hwPoePortTable 1 }
		
		HwPoePortEntry ::=
			SEQUENCE { 
				hwPoePortIfIndex
					InterfaceIndex,
				hwPoePortName
					OCTET STRING,
				hwPoePortEnable
					EnabledStatus,
				hwPoePortPriority
					INTEGER,
				hwPoePortMaximumPower
					Integer32,
				hwPoePortPowerOnStatus
					OCTET STRING,
				hwPoePortPowerStatus
					OCTET STRING,
				hwPoePortPdClass
					Integer32,
				hwPoePortReferencePower
					Integer32,
				hwPoePortConsumingPower
					Integer32,
				hwPoePortPeakPower
					Integer32,
				hwPoePortAveragePower
					Integer32,
				hwPoePortCurrent
					OCTET STRING,
				hwPoePortVoltage
					OCTET STRING,
				hwPoePortManualOperation
					INTEGER
			 }

		
		hwPoePortIfIndex OBJECT-TYPE
			SYNTAX InterfaceIndex
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This object indicates the interface index."
			::= { hwPoePortEntry 1 }
		
		
		hwPoePortName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the interface name."
			::= { hwPoePortEntry 2 }
		
		
		hwPoePortEnable OBJECT-TYPE
			SYNTAX EnabledStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the enabling status of an interface. (1:enable(default);  2:disable)"
			DEFVAL { enable }
			::= { hwPoePortEntry 3 }
		
		
		hwPoePortPriority OBJECT-TYPE
			SYNTAX INTEGER
				{
				critical(1),
				high(2),
				low(3)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object identifies the priority of an interface. (1:critical, 2:high, 3:low(default))"
			DEFVAL { low }
			::= { hwPoePortEntry 4 }
		
		
		hwPoePortMaximumPower OBJECT-TYPE
			SYNTAX Integer32 (0..30000)
			UNITS "mW"
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object identifies the maximum power of an interface.The value is expressed in mW."
			DEFVAL { '9088'h }
			::= { hwPoePortEntry 5 }
		
		
		hwPoePortPowerOnStatus OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the powering status of an interface."
			::= { hwPoePortEntry 6 }
		
		
		hwPoePortPowerStatus OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the status of an interface."
			::= { hwPoePortEntry 7 }
		
		
		hwPoePortPdClass OBJECT-TYPE
			SYNTAX Integer32 (0..7)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object identifies the class of a PD."
			::= { hwPoePortEntry 8 }
		
		
		hwPoePortReferencePower OBJECT-TYPE
			SYNTAX Integer32 (0..30000)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object identifies the guaranteed power of an interface. The value is expressed in mW."
			::= { hwPoePortEntry 9 }
		
		
		hwPoePortConsumingPower OBJECT-TYPE
			SYNTAX Integer32 (0..30000)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object identifies the consuming power of an interface. The value is expressed in mW."
			::= { hwPoePortEntry 10 }
		
		
		hwPoePortPeakPower OBJECT-TYPE
			SYNTAX Integer32 (0..30000)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object identifies the peak power of an interface. The value is expressed in mW."
			::= { hwPoePortEntry 11 }
		
		
		hwPoePortAveragePower OBJECT-TYPE
			SYNTAX Integer32 (0..30000)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object identifies the average power of an interface. The value is expressed in mW."
			::= { hwPoePortEntry 12 }
		
		
		hwPoePortCurrent OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the current of an interface. The value is expressed in mA."
			::= { hwPoePortEntry 13 }
		
		
		hwPoePortVoltage OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the voltage of an interface. The value is expressed in V."
			::= { hwPoePortEntry 14 }
		
		
		hwPoePortManualOperation OBJECT-TYPE
			SYNTAX INTEGER
				{
				powerOff(1),
				powerOn(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates that a PD connected to an interface is powered on or powered off manually."
			::= { hwPoePortEntry 15 }
		

		
		hwPoeTrapObjects OBJECT IDENTIFIER ::= { hwPoeMIB 39 }
		
		hwPoePdPriority OBJECT-TYPE
			SYNTAX INTEGER
				{
				critical(1),
				high(2),
				low(3)
				}
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"This object identifies the PD priority.(1:critical, 2:high, 3:low(default))"
			::= { hwPoeTrapObjects 1 }
		
		hwPoeSlotNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"This object identifies the slot ID."
			::= { hwPoeTrapObjects 2 }

		hwPoeCurConsumPower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"This object identifies the current consuming power."
			::= { hwPoeTrapObjects 3 }

		hwPoeConsumPowerThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"This object identifies the threshold of consuming power."
			::= { hwPoeTrapObjects 4 }
			
		hwPoeDeviceID OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"This object identifies the device ID."
			::= { hwPoeTrapObjects 5 }
		
		hwFrameID OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"This object identifies the CSS Frame ID."
			::= { hwPoeTrapObjects 6 }
			
		hwPoeNotification OBJECT IDENTIFIER ::= { hwPoeMIB 40 }
		
		
		hwPoeDimmError NOTIFICATION-TYPE
			OBJECTS { hwPoeSlotNum, hwPoeDimmId }
			STATUS current
			DESCRIPTION 
				"This object indicates the Dimm chip error."
			::= { hwPoeNotification 1 }
		
		
		hwPoePowerOff NOTIFICATION-TYPE
			OBJECTS { hwPoePortName }
			STATUS current
			DESCRIPTION 
				"This object indicates a PD connected to an interface is powered off."
			::= { hwPoeNotification 2 }
		
		
		hwPoePowerOn NOTIFICATION-TYPE
			OBJECTS { hwPoePortName }
			STATUS current
			DESCRIPTION 
				"This object indicates that a PD connected to an interface is powered on."
			::= { hwPoeNotification 3 }
		
		
		hwPoeSlotPowerOverload NOTIFICATION-TYPE
			OBJECTS { hwPoeSlotNum, hwPoeSlotConsumingPower }
			STATUS current
			DESCRIPTION 
				"This object indicates that the power consumed by a slot exceeds the threshold."
			::= { hwPoeNotification 4 }
		
		
		hwPoeSlotPowerOverloadResume NOTIFICATION-TYPE
			OBJECTS { hwPoeSlotNum, hwPoeSlotConsumingPower }
			STATUS current
			DESCRIPTION 
				"This object indicates that the power consumed by a slot does not exceed the threshold."
			::= { hwPoeNotification 5 }
		
		
		hwPoePdPowerOverload NOTIFICATION-TYPE
			OBJECTS { hwPoePortName, hwPoePortConsumingPower, hwPoePortMaximumPower }
			STATUS current
			DESCRIPTION 
				"This object indicates the power consumed by a PD connected to an interface exceeds the threshold."
			::= { hwPoeNotification 6 }
		
		
		hwPoePdPowerOverloadResume NOTIFICATION-TYPE
			OBJECTS { hwPoePortName, hwPoePortConsumingPower, hwPoePortMaximumPower }
			STATUS current
			DESCRIPTION 
				"This object indicates that the power consumed by a PD connected to an interface does not exceed the threshold."
			::= { hwPoeNotification 7 }
		
		hwPoePdConnected NOTIFICATION-TYPE
			OBJECTS { hwPoePortName }
			STATUS current
			DESCRIPTION 
				"This object indicates that a PD is connected to an interface."
			::= { hwPoeNotification 8 }
		
		
		hwPoePdDisconnected NOTIFICATION-TYPE
			OBJECTS { hwPoePortName }
			STATUS current
			DESCRIPTION 
				"This object indicates that a PD is disconnected from an interface."
			::= { hwPoeNotification 9 }
		
		hwPoePdClassInvalid NOTIFICATION-TYPE
			OBJECTS { hwPoePortName }
			STATUS current
			DESCRIPTION 
				"This object indicates that a PD of an invalid class is detected."
			::= { hwPoeNotification 10 }
		
		hwPoePdClassOvercurrent NOTIFICATION-TYPE
			OBJECTS { hwPoePortName }
			STATUS current
			DESCRIPTION 
				"This object indicates that overcurrent occurs during the classification of a PD."
			::= { hwPoeNotification 11 }
		
		hwPoePdPowerOvercurrent NOTIFICATION-TYPE
			OBJECTS { hwPoePortName }
			STATUS current
			DESCRIPTION 
				"This object indicates that overcurrent occurs during the powering of a PD."
			::= { hwPoeNotification 12 }
		
		hwPoePdPowerOvercurrentResume NOTIFICATION-TYPE
			OBJECTS { hwPoePortName }
			STATUS current
			DESCRIPTION 
				"This object indicates that overcurrent is rectified."
			::= { hwPoeNotification 13 }
		
		hwPoePowerOnFail NOTIFICATION-TYPE
			OBJECTS { hwPoePortName }
			STATUS current
			DESCRIPTION 
				"This object indicates that a PD fails to be powered on."
			::= { hwPoeNotification 14 }
		
		hwPoePowerOffCurrentLimits NOTIFICATION-TYPE
			OBJECTS { hwPoePortName }
			STATUS current
			DESCRIPTION 
				"This object indicates that a PD is powered off because its current meets or exceeds the limit of current."
			::= { hwPoeNotification 15 }
		
		hwPoePdPriorityDifferent NOTIFICATION-TYPE
			OBJECTS { hwPoePortName, hwPoePortPriority, hwPoePdPriority }
			STATUS current
			DESCRIPTION 
				"This object indicates that the priority of PD is different from the port."
			::= { hwPoeNotification 16 }
		
		hwPoePowerOverUtilizationThreshold  NOTIFICATION-TYPE
		  OBJECTS { hwPoeDeviceID, hwPoeCurConsumPower, hwPoeConsumPowerThreshold}
			STATUS current
			DESCRIPTION 
				"This object indicates that the PSE is overdrawing power."
			::= { hwPoeNotification 17 }
		
		hwPoePowerOverUtilizationThresholdResume  NOTIFICATION-TYPE
		  OBJECTS { hwPoeDeviceID, hwPoeCurConsumPower, hwPoeConsumPowerThreshold}
			STATUS current
			DESCRIPTION 
				"This object indicates that the PSE is not overdrawing power."
			::= { hwPoeNotification 18 }
			
		hwPoeBoardInsertedWrongFrame  NOTIFICATION-TYPE
		  OBJECTS {hwFrameID, hwPoeSlotNum }
			STATUS current
			DESCRIPTION 
				"This object indicates that the poe board is inserted in the frame does not support poe."
			::= { hwPoeNotification 19 }			
						
		hwPoePowerAbsent  NOTIFICATION-TYPE
		  OBJECTS {hwFrameID, hwPoeSlotNum }
			STATUS current
			DESCRIPTION 
				"This object indicates that the poe power is absent."
			::= { hwPoeNotification 20 }

		hwPoePowerAbsentResume  NOTIFICATION-TYPE
		  OBJECTS {hwFrameID, hwPoeSlotNum }
			STATUS current
			DESCRIPTION 
				"This object indicates that the poe power is present."
			::= { hwPoeNotification 21 }

		hwPoeRpsPowerOutputAlarm  NOTIFICATION-TYPE
		  OBJECTS {hwPoeSlotNum }
			STATUS current
			DESCRIPTION 
				"This object indicates that the RPS power can not provide POE power for this device."
			::= { hwPoeNotification 22 }

		hwPoeRpsPowerOutputAlarmResume  NOTIFICATION-TYPE
		  OBJECTS {hwPoeSlotNum }
			STATUS current
			DESCRIPTION 
				"This object indicates that the RPS power can provide POE power for this device."
			::= { hwPoeNotification 23 }

		
		hwPoeConformance OBJECT IDENTIFIER ::= { hwPoeMIB 100 }
		
		
		hwPoeGroups OBJECT IDENTIFIER ::= { hwPoeConformance 1 }
		
		
		hwPoeSlotGroup OBJECT-GROUP
			OBJECTS { hwPoeSlotMaximumPower, hwPoeSlotReferencePower, hwPoeSlotConsumingPower, hwPoeSlotPeakPower, hwPoeSlotPowerManagementManner, 
				hwPoeSlotIsPoeDevice, hwPoeSlotLegacyDetect, hwPoeSlotPowerRsvPercent, hwPoeSlotPowerUtilizationThreshold, hwPoeDimmId,
				hwPoeSlotAvailablePower }
			STATUS current
			DESCRIPTION 
				"This object indicates the POE's slot table group."
			::= { hwPoeGroups 1 }
		
		
		hwPoePortGroup OBJECT-GROUP
			OBJECTS { hwPoePortEnable, hwPoePortPriority, hwPoePortMaximumPower, hwPoePortPowerOnStatus, hwPoePortPowerStatus, 
				hwPoePortReferencePower, hwPoePortName, hwPoePortConsumingPower, hwPoePortPeakPower, hwPoePortAveragePower, 
				hwPoePortCurrent, hwPoePortVoltage, hwPoePortManualOperation, hwPoePortPdClass }
			STATUS current
			DESCRIPTION 
				"This object indicates the POE's port table group."
			::= { hwPoeGroups 2 }
		
		
		hwPoeGlobalGroup OBJECT-GROUP
			OBJECTS { hwPoePowerUtilizationThreshold, hwPoePowerRsvPercent, hwPoePower }
			STATUS current
			DESCRIPTION 
				"This object indicates the POE's global table group."
			::= { hwPoeGroups 3 }
		
		
		hwPoeNotificationGroup NOTIFICATION-GROUP
			NOTIFICATIONS { hwPoeDimmError, hwPoePowerOff, hwPoePowerOn, hwPoePdPowerOverload, hwPoePdPowerOverloadResume, 
				hwPoePdConnected, hwPoePdDisconnected, hwPoePdClassInvalid, hwPoePdClassOvercurrent, hwPoePdPowerOvercurrent, 
				hwPoePdPowerOvercurrentResume, hwPoePowerOnFail, hwPoePowerOffCurrentLimits, hwPoePowerOverUtilizationThresholdResume , hwPoePowerOverUtilizationThreshold , 
				hwPoePdPriorityDifferent, hwPoeSlotPowerOverload, hwPoeSlotPowerOverloadResume , hwPoeBoardInsertedWrongFrame ,hwPoePowerAbsent,hwPoePowerAbsentResume,
				hwPoeRpsPowerOutputAlarm, hwPoeRpsPowerOutputAlarmResume }
			STATUS current
			DESCRIPTION 
				"This object indicates the POE's notification table group."
			::= { hwPoeGroups 4 }
		
		hwPoeTrapObjectsGroup OBJECT-GROUP
			OBJECTS { hwPoePdPriority, hwPoeSlotNum, hwPoeCurConsumPower,hwPoeConsumPowerThreshold,hwPoeDeviceID,hwFrameID }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwPoeGroups 5 }
		
	
	END

--
-- HUAWEI-POE-MIB.mib
--
