-- ==================================================================
-- Copyright (C) 2017 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description: HUAWEI VPLS Management Extended MIB
-- Reference:
-- Version:     V2.46
-- History:
--              V1.0 PanJun, 2006-05-08, publish
-- ==================================================================

    HUAWEI-VPLS-EXT-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            hwDatacomm            
                FROM HUAWEI-MIB            
            InterfaceIndex,InterfaceIndexOrZero,ifName
                FROM IF-MIB            
            OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP            
                FROM SNMPv2-CONF            
            sysUpTime            
                FROM SNMPv2-MIB            
            IpAddress,TimeTicks,Unsigned32, Counter64, OBJECT-TYPE, MODULE-IDENTITY, 
            NOTIFICATION-TYPE            
                FROM SNMPv2-SMI            
            DisplayString, RowStatus, TruthValue, TEXTUAL-CONVENTION,DateAndTime            
                FROM SNMPv2-TC            
            VrId            
                FROM VRRP-MIB
            EnabledStatus
                FROM P-BRIDGE-MIB
            hwL2VpnVcLimitClass, hwL2VpnVsiVcNumber, hwVplsVcNumberUpperThreshold,
            hwVplsVcNumberMaxNum    
                FROM HUAWEI-L2VPN-MIB;


        hwL2VpnVplsExt MODULE-IDENTITY 
            LAST-UPDATED "201708171644Z"           --Aug 17, 2017 at 16:44 GMT"
            ORGANIZATION 
                "Huawei Technologies Co.,Ltd."
            CONTACT-INFO 
                "Huawei Industrial Base
                  Bantian, Longgang
                   Shenzhen 518129
                   People's Republic of China
                   Website: http://www.huawei.com
                   Email: support@huawei.com
                 "
            DESCRIPTION 
                "The HUAWEI-VPLS-EXT-MIB contains objects to
                manage VPLS."
             REVISION "201708171644Z"           --Aug 17, 2017 at 16:44 GMT 
             DESCRIPTION "add change reason
                Add Leaf Node to HWVplsPwSuppStatisticsEntry, HWVplsAcSuppStatisticsEntry"

             REVISION "201708081000Z"           --Aug 08, 2017 at 10:00 GMT 
             DESCRIPTION "add change reason
                Modify description of  hwVplsAcIfIndex"

             REVISION "201707171000Z"           --Jul 17, 2017 at 10:00 GMT 
             DESCRIPTION "add change reason
                Add Leaf Node to hwVplsHardPipeStatisticsEntry"

             REVISION "201611281000Z"           --Nov 28, 2016 at 10:00 GMT 
             DESCRIPTION               
             "Add OBJECTS(hwVplsBLabelNotEnough, hwVplsBLabelNotEnoughClear)." 

             REVISION "201611181000Z"           --Nov 18, 2016 at 10:00 GMT 
             DESCRIPTION               
             "Add hwVplsNotificationGroup(hwVplsBLabelNotEnough, hwVplsBLabelNotEnoughClear)." 

              REVISION "201610311000Z"           --Oct 31, 2016 at 10:00 GMT 
             DESCRIPTION               
             "Add VPLS MIB Trap(hwVplsBLabelNotEnough)." 

              REVISION "201610311000Z"           --Oct 31, 2016 at 10:00 GMT 
             DESCRIPTION               
             "Add VPLS MIB Trap(hwVplsBLabelNotEnoughClear)."

             REVISION "201609271000Z"           --Sep 27, 2016 at 10:00 GMT 
             DESCRIPTION "modify hwVplsDiffServMode range"  

             REVISION "201607111000Z"           --July 11, 2016 at 10:00 GMT 
             DESCRIPTION "add change reason
                Add Leaf Node to hwVplsLdpStatisticsEntry"  

             REVISION "201511171000Z"           --Nov 17, 2015 at 10:00 GMT 
             DESCRIPTION "add change reason
                TDM Bit Rate Matched(93),
                TDM Bit Rate Unmatched(94)"  

              REVISION "201501071000Z"           --Jan 7, 2015 at 10:00 GMT 
             DESCRIPTION "add change reason
                Aging(91)
                Verification(92)"  

              REVISION "201412081000Z"           --Dec 8, 2014 at 10:00 GMT 
             DESCRIPTION               
             "Add OBJECT(hwVplsVsiProtectGroupMode) to VPLS MIB Trap(hwVplsPwRedundancyDegraded)." 

              REVISION "201412081000Z"           --Dec 8, 2014 at 10:00 GMT 
             DESCRIPTION               
             "Add OBJECT(hwVplsVsiProtectGroupMode) to VPLS MIB Trap(hwVplsPwRedundancyDegradedClear)." 

              REVISION "201412081000Z"           --Dec 8, 2014 at 10:00 GMT 
             DESCRIPTION               
             "Add Leaf Node(hwVplsVsiProtectGroupMode) to hwVplsVsiProtectGroupEntry" 

             REVISION "201410271600Z"           --Oct 27, 2014 at 16:00 GMT 
             DESCRIPTION               
             "Add VPLS protect group table(hwVplsVsiProtectGroupTable)." 
			 
             REVISION "201410271600Z"           --Oct 27, 2014 at 16:00 GMT 
             DESCRIPTION               
             "Add VPLS MIB Trap(hwVplsPwRedundancyDegraded)." 
			 
             REVISION "201410271600Z"           --Oct 27, 2014 at 16:00 GMT 
             DESCRIPTION               
             "Add VPLS MIB Trap(hwVplsPwRedundancyDegradedClear)." 

             REVISION "201402111600Z"           -- Feb 11, 2014 at 16:00 GMT 
             DESCRIPTION  
             "The max length of hwVplsLdpPeerQosProfileName,hwVplsVsiQosProfileName changed
              from 31 to 63." 


             REVISION "201307131100Z"           -- July 13, 2013 at 11:00 GMT 
             DESCRIPTION  
             "Add Leaf Nodes(hwL2vpnTnlType, hwL2vpnTunnelIndex) to hwVplsMIBObjects;  
              Add OBJECT(hwL2vpnTnlType, hwL2vpnTunnelIndex) to VPLS MIB Trap(hwVplsVcDown)." 

           REVISION  "201306250950Z"             --Jun 25,2013 at 09:51 GMT
           DESCRIPTION "add change reason
                Route Unreachable(89)
                Route Reachable(90)"  

           REVISION  "200704122100Z"
           DESCRIPTION "20130126 "  
           
           REVISION "201406181000Z"              -- June 18, 2014 at 10:00 GMT
           DESCRIPTION
                "Add trap nodes about VPLS VC limit alarm."
                                
            ::= { hwL2Vpn 1 }

        
    
--
-- Textual conventions
--

        HWL2VpnVcEncapsType ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                "An indication of the L2Vpn's VC encapsulation type:
                Frame Relay DLCI ( Martini Mode ) (1)
                ATM AAL5 SDU VCC transport (2)
                ATM transparent cell transport (3)
                Vlan (4)
                Ethernet (5)
                HDLC (6)
                PPP (7)
                SONET/SDH Circuit Emulation Service Over MPLS (CEM) (8)
                ATM n-to-one VCC cell transport (9)
                ATM n-to-one VPC cell transport (10)
                IP Layer2 Transport (11)
                ATM one-to-one VCC Cell Mode (12)
                ATM one-to-one VPC Cell Mode (13)
                ATM AAL5 PDU VCC transport (14)
                Frame-Relay Port mode (15)
                SONET/SDH Circuit Emulation over Packet (CEP) (16)
                Structure-agnostic E1 over Packet (SAE1oP)  (17)
                Structure-agnostic T1 (DS1) over Packet (SAT1oP)  (18)
                Structure-agnostic E3 over Packet (SAE3oP) (19)
                Structure-agnostic T3 (DS3) over Packet (SAT3oP) (20)
                CESoPSN basic mode (21)
                TDMoIP basic mode (22)
                CESoPSN TDM with CAS (23)
                TDMoIP TDM with CAS (24)
                Frame Relay DLCI (25)
                IP-interworking (64)
                unknown (255)
                "
            SYNTAX INTEGER
                {
                frameRelayDlciMartini(1),
                atmAal5SduVccTransport(2),
                atmTransparentCellTransport(3),
                vlan(4),
                ethernet(5),
                hdlc(6),
                ppp(7),
                cem(8),
                atmN2OneVccCellTransport(9),
                atmN2OneVpcCellTransport(10),
                ipLayer2Transport(11),
                atmOne2OneVccCellMode(12),
                atmOne2OneVpcCellMode(13),
                atmAal5PduVccTransport(14),
                frameRelayPortMode(15),
                cep(16),
                saE1oP(17),
                saT1oP(18),
                saE3oP(19),
                saT3oP(20),
                cESoPsnBasicMode(21),
                tDMoIPbasicMode(22),
                l2VpnCESoPSNTDMwithCAS(23),
                l2VpnTDMoIPTDMwithCAS(24),
                frameRelayDlci(25),
                ipInterworking(64),
                unknown(255)
                }

        HWEnableValue ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                "Represents a boolean value."
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }

        HWL2VpnStateChangeReason ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                "The type indicates the reason of VC's or VSI's status change:
                Invalid reason type (1) 
                VC Created (2) 
                VC Deleted (3) 
                LDP Session Down (4)
                LDP Session Up (5)
                LDP Same Mapping Received with different label or MTU (6)
                LDP Same Mapping Received Interface Parameter matching (7)
                LDP Mapping Received Inteface Parameter UnMatched(8)
                LDP Mapping Received UnPass CBit Check(9)
                LDP Mapping Received UnPass PW Loop Check(10)
                LDP New Mapping Received (11)  
                LDP New Mapping Received but Remote VC Down(12)
                LDP Withdrawn Received (13)
                LDP Release Received (14)
                LDP Request Received (15)
                LDP GR End processing (16)
                RSVP message received (17)
                Interface Up (18)
                Interface Down (19)
                Interface encapsulation changed (20)
                Refresh (21)
                Download Again (22)
                Tunnel Up (23)
                Tunnel Down (24)
                VC state change when New RLB Received (25)
                RLB Deleted (26)
                VC created or turned to another remote CE (27)
                Out Interface in Invalid state (28)
                Out Interface in Valid now (29)
                LDP Notification Forwarding (30)
                LDP Notification Not-Forwarding (31)
                PW Restart (32)   
                Download FTN&ILM for EthernetTrunk(33)
                   AC OAM Fault Detect Disable(34)
                   Remote AC Fault(35)
                   Remote AC Fault Resume(36)
                   Local AC Fault(37)
                   Local AC Fault Resume(38)
                   Remote PSN Fault(39)
                   Remote PSN Fault Resume(40)
                   Local PSN Fault(41)
                   Local PSN Fault Resume(42)
                   BFD for PW State Change to:Down(43)
                   BFD for PW State Change to:Up(44)
                   BFD for PW State Change to:Admin Down(45)
                   BFD for PW Disable(46)
                   Manual Set Enable(47)
                   Manual Set Disable(48)
                   Delay Time Out(49)
                   Resume Time Out(50)
                VRRP Master(51)
                VRRP Backup(52)
                VRRP Init(53)
                VRRP Delete(54)
                Track VRRP(55)
                Undo track VRRP(56)
                Lsp Ping Time Out(57)
                VC State Down when New RLB was Received(58)
                MTU Matched(59)
                MTU Unmatched(60)
                VSI was shuted(61)
                VSI was resumed(62)
                Set Admin VSI(63)
                Undo set Admin VSI(64)
                BVSI Bind AC(65)
                BVSI Unbind AC(66)
                IVSI Bind BVSI(67)
                IVSI Unbind BVSI(68)
                Deleted VSI(69)
                Reconstruct FWD Table(70)
                MCLAG Master(71)
                MCLAG Backup(72)
                Admin PW Up(73)
                Admin PW Down(74)
                VCCV OK(75)
                VCCV Failed(76)
                Localifnet OK(77)
                Invclabel OK(78)
                Localifnet Release(79)
                Invclabel Release(80)
                Switchover Enable(81)
                Switchover Disable(82)
                Set BVSI(83)
                undo Set BVSI(84)
                Shutdown BVSI(85)
                Undo Shutdown BVSI(86)
                Notification Received(87)
                PW APS Switch(88) 
                Route Unreachable(89)
                Route Reachable(90)
                Aging(91)
                Verification(92)
                TDM Bit Rate Matched(93)
                TDM Bit Rate Unmatched(94)
                "
            SYNTAX INTEGER
                {
                invalidReason(1),
                vcCreated(2),
                vcDeleted(3),
                ldpSessionDown(4),
                ldpSessionUp(5),
                receivedDifLabelOrMtu(6),
                receivedIntfParaMatching(7),
                receivedIntfParaUnMatched(8),
                receivedUnPassCbitCheck(9),
                receivedUnPassPwLoopCheck(10),
                receivedNewMapping(11),
                receivedNewMappingButRemoteVcDown(12),
                receivedWithdrawn(13),
                receivedLdpRelease(14),
                receivedLdpRequest(15),
                ldpGrEndProcessing(16),
                receivedRsvpMessage(17),
                interfaceUp(18),
                interfaceDown(19),
                interfaceEncapChanged(20),
                refresh(21),
                downloadAgain(22),
                tunnelUp(23),
                tunnelDown(24),
                receivedNewRlb(25),
                deletedRlb(26),
                vcCreatedOrTurnedToAnother(27),
                outInterInInvalidState(28),
                outInterInValidNow(29),
                ldpNotifiForward(30),
                ldpNotifiNotForward(31),
                pwRestart(32),
                downloadFtnAndIlmForEthTrunk(33),
                acOamFaultDetectDisable(34),
                remoteAcFault(35),
                remoteAcFaultResume(36),
                localAcFault(37),
                localAcFaultResume(38),
                remotePsnFault(39),
                remotePsnFaultResume(40),
                localPsnFault(41),
                localPsnFaultResume(42),
                bfdForPwStateChangeToDown(43),
                bfdForPwStateChangeToUp(44),
                bfdForPwStateChangeToAdminDown(45),
                bfdForPwDisable(46),
                manualSetEnable(47),
                manualSetDisable(48),
                delayTimeOut(49),
                resumeTimeOut(50),
                vrrpMaster(51),
                vrrpBackup(52),
                vrrpInit(53),
                vrrpDelete(54),
                vrrpTrack(55),
                undoVrrpTrack(56),
                lspPingTimeOut(57),
                vcDownWhenReceivedNewRLB(58),
                mtuMatched(59),
                mtuUnmatched(60),
                vsiShut(61),
                vsiResume(62),
                setAdminVSI(63),
                undosetAdminVSI(64),  
                bvsiBindAc(65),
                bvsiUnbindAc(66),
                ivsiBindBVSI(67),
                ivsiUnbindBVSI(68),
                deletedVSI(69),
                reconstructFwdTable(70),
                mclagMaster(71),
                mclagBackup(72),
                adminPwUp(73),
                adminPwDown(74),
                vccvOk(75),
                vccvFailed(76),
                localIfnetOk(77),
                inVcLabelOk(78),
                localIfnetRelease(79),
                inVcLabelRelease(80),
                switchOverEnable(81),
                switchOverDisable(82),
                setBVSI(83),
                undoSetBVSI(84),
                shutdownBVSI(85),
                undoShutdownBVSI(86),
                notificationReceived(87),
                pwApsSwitch(88),                   
                routeUnreachable(89),
                routeReachable(90),
                aging(91),
                verification(92),
                tdmBitRateMatched(93),
                tdmBitRateUnmatched(94)
                }

    
--
-- Node definitions
--

        hwL2Vpn OBJECT IDENTIFIER ::= { hwDatacomm 119 }

        
--           
-- The VPLS Attribute Group
-- 
        hwVplsMIBObjects OBJECT IDENTIFIER ::= { hwL2VpnVplsExt 1 }

        
--           
-- The VPLS Table
-- 
        hwVplsTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is the VPLS's configuration table. Users can 
                create or delete the VSI by it."
            ::= { hwVplsMIBObjects 1 }

        
        hwVplsEntry OBJECT-TYPE
            SYNTAX HWVplsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of a VPLS entry."
            INDEX { hwVplsVsiName }
            ::= { hwVplsTable 1 }

        
        HWVplsEntry ::=
            SEQUENCE { 
                hwVplsVsiName
                    DisplayString,
                hwVplsSignal
                    INTEGER,
                hwVplsRD
                    DisplayString,
                hwVplsVsiID
                    Unsigned32,
                hwVplsVcType
                    HWL2VpnVcEncapsType,
                hwVplsStatus
                    INTEGER,
                hwVplsMtu
                    Unsigned32,
                hwVplsTunnelPolicy
                    DisplayString,
                hwVplsDescription
                    DisplayString,
                hwVplsLearnStyle
                    INTEGER,
                hwVplsMacLearnEnable
                    HWEnableValue,
                hwVplsMacLimitEnable
                    HWEnableValue,
                hwVplsStatisticsEnable
                    HWEnableValue,
                hwVplsUnknowMulticast
                    INTEGER,
                hwVplsUnknowUnicast
                    INTEGER,
                hwVplsPreference
                    Unsigned32,
                hwVplsVsiType
                    INTEGER,
                hwVplsAdminVsiName
                    DisplayString,
                hwVplsAcIsolateFlag
                    HWEnableValue,
                hwVplsDiffServMode
                    INTEGER,
                hwVplsDiffServServiceClass
                    INTEGER,
                hwVplsDiffServColor
                    INTEGER,
                hwVplsDiffServDSName
                    OCTET STRING,
                hwVplsInterfaceWithdraw    
                    HWEnableValue,
                hwVplsUpe2NpeWithdraw    
                    HWEnableValue,                    
                hwVplsUpe2UpeWithdraw    
                    HWEnableValue,       
                hwVplsNpe2UpeWithdraw    
                    HWEnableValue,                           
                hwVplsDiscovery
                    INTEGER,
                hwVplsMacWithdrawEnable
                    EnabledStatus,
                hwVplsVsiCir
                    Unsigned32,
                hwVplsVsiPir
                    Unsigned32,
                hwVplsVsiQosProfileName
                    DisplayString,
                hwVplsAdminStatus
                    INTEGER,
                hwVplsIgnoreAcState
                    EnabledStatus,
                hwVplsEnableStatistic
                    EnabledStatus,
                hwVplsResetStatistic
                    INTEGER,
                hwVplsResetStatisticTime
                    DateAndTime,
                hwVplsAgingTime
                    Unsigned32,  
                hwVplsUnknowUnicastMacLearning
                    EnabledStatus,  
                hwVplsFlowLabel
                    EnabledStatus,     
                hwVplsServiceName
                    OCTET STRING,                                          
                hwVplsRowStatus
                    RowStatus
             }

        hwVplsVsiName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..31))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "This object indicates the VSI's name."
            ::= { hwVplsEntry 1 }

        
        hwVplsSignal OBJECT-TYPE
            SYNTAX INTEGER
                {
                ldp(1),
                bgp(2),
                unknown(255)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the signal type.
                If the signal type is LDP, VSI-ID must be designated.
                If the signal type is BGP, RD must be designated.
                The default value is unknown(255)."
            ::= { hwVplsEntry 2 }

        
        hwVplsRD OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0 | 3..21))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the Route Distinguisher."
            ::= { hwVplsEntry 3 }

        
        hwVplsVsiID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the VSI id.
                The default value is 0."
            ::= { hwVplsEntry 4 }

        
        hwVplsVcType OBJECT-TYPE
            SYNTAX HWL2VpnVcEncapsType
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the VC's encapsulation type."
            ::= { hwVplsEntry 5 }

        
        hwVplsStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                up(1),
                down(2),
                admindown(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the VPLS's status."
            ::= { hwVplsEntry 6 }

        
        hwVplsMtu OBJECT-TYPE
            SYNTAX Unsigned32 (328..65535)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the VPLS's MTU.The default value is 1500."
            ::= { hwVplsEntry 7 }

        
        hwVplsTunnelPolicy OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..39))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the tunnel policy."
            ::= { hwVplsEntry 8 }

        
        hwVplsDescription OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..64))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the description information."
            ::= { hwVplsEntry 9 }

        
        hwVplsLearnStyle OBJECT-TYPE
            SYNTAX INTEGER
                {
                qualify(1),
                unqualify(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the style of learning the MAC
                address."
            ::= { hwVplsEntry 10 }

        
        hwVplsMacLearnEnable OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the enable sign of learning the MAC
                address."
            ::= { hwVplsEntry 11 }

        
        hwVplsMacLimitEnable OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the enable sign of the MAC addresses
                number limit."
            ::= { hwVplsEntry 12 }

        
        hwVplsStatisticsEnable OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the enable sign of statistics."
            ::= { hwVplsEntry 13 }

        
        hwVplsUnknowMulticast OBJECT-TYPE
            SYNTAX INTEGER
                {
                broadcast(1),
                drop(2),
                localHandle(3)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the processing mode when the
                multicast MAC entry not found in FDB."
            ::= { hwVplsEntry 14 }

        
        hwVplsUnknowUnicast OBJECT-TYPE
            SYNTAX INTEGER
                {
                broadcast(1),
                drop(2),
                localHandle(3)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the processing mode when the
                unicast MAC entry not found in FDB."
            ::= { hwVplsEntry 15 }

        
        hwVplsPreference OBJECT-TYPE
            SYNTAX Unsigned32 (0..65535)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the preference.The default value is 0."
            ::= { hwVplsEntry 16 }

        
        hwVplsVsiType OBJECT-TYPE
            SYNTAX INTEGER
                {
                operationVsi(1),
                adminVsi(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the VSI's type."
            ::= { hwVplsEntry 17 }

        
        hwVplsAdminVsiName OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the AdminVsi's name this VSI binding to"
            ::= { hwVplsEntry 18 }

        
        hwVplsAcIsolateFlag OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates whether the AC in the VSI is isolated"
            ::= { hwVplsEntry 19 }

        
        hwVplsDiffServMode OBJECT-TYPE
            SYNTAX INTEGER
                {
                pipe(1),
                shortpipe(2),
                uniform(3),
                egressPipe(4),
                egressShortpipe(5),
                egressShortpipeTrustInnerVlan8021p(6),
                egressShortpipeTrustIpDscp(7) 
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Different service mode of the interface binding of vsi , 
                default is uniform."
            ::= { hwVplsEntry 20 }

        
        hwVplsDiffServServiceClass OBJECT-TYPE
            SYNTAX INTEGER
                {
                be(1),
                af1(2),
                af2(3),
                af3(4),
                af4(5),
                ef(6),
                cs6(7),
                cs7(8),
                invalidClass(255)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "PHB in the ingress PE, the value must be 
                be,f1,af2,af3,af4,ef,cs6,cs7.The default value is invalidClass(255)."
            ::= { hwVplsEntry 21 }

        
        hwVplsDiffServColor OBJECT-TYPE
            SYNTAX INTEGER
                {
                green(1),
                yellow(2),
                red(3),  
                invalidColor(255)  
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Remarked color of packet in the ingress 
                PE, the value must be green,yellow,red.The default value is invalidColor(255)."
            ::= { hwVplsEntry 22 }

        
        hwVplsDiffServDSName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..8))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Name of different service domain"
            ::= { hwVplsEntry 23 }

        hwVplsInterfaceWithdraw OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Enable VSI send LDP mac-withdraw when VSI receive interface status changes event."
            ::= { hwVplsEntry 24 }
        
        hwVplsUpe2NpeWithdraw OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "VSI forward message to all the NPE when VSI receive message from UPE."
            ::= { hwVplsEntry 25 }           
            
        hwVplsUpe2UpeWithdraw OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "VSI forward message to all the other UPE when VSI receive message from UPE."
            ::= { hwVplsEntry 26 }    
            
        hwVplsNpe2UpeWithdraw OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "VSI forward message to all the UPE when VSI receive message from NPE."
            ::= { hwVplsEntry 27 }   

        hwVplsDiscovery OBJECT-TYPE
            SYNTAX INTEGER
                {
                static(1),
                auto(2),
                none(3)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the discovery type.
                If the discovery type is static, the signal must be LDP.
                If the discovery type is auto, the signal must be BGP."
            ::= { hwVplsEntry 28 }

        hwVplsMacWithdrawEnable OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the enable sign of the MAC address withdraw."
            ::= { hwVplsEntry 29 }

        hwVplsVsiCir OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the committed information rate, based on VSI."
            ::= { hwVplsEntry 30 }

        hwVplsVsiPir OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the peak information rate, based on VSI."
            ::= { hwVplsEntry 31 }

        hwVplsVsiQosProfileName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..63))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the QoS profile's name, based on VSI."
            ::= { hwVplsEntry 32 }

        hwVplsAdminStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                up(1),
                down(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the VSI's admin status."
            ::= { hwVplsEntry 33 }


        hwVplsIgnoreAcState OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the enable sign of the ignorer of AC state."
            ::= { hwVplsEntry 34 }


        hwVplsEnableStatistic OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The enable sign of VSI's traffic statistics."
            ::= { hwVplsEntry 35 }


        hwVplsResetStatistic OBJECT-TYPE
            SYNTAX INTEGER
                {
                resetStatistic(1),
                unknownStatus(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Reset traffic statistics of VSI."
            ::= { hwVplsEntry 36 }


        hwVplsResetStatisticTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Last time of clean out."
            ::= { hwVplsEntry 37 }

        hwVplsAgingTime OBJECT-TYPE
            SYNTAX Unsigned32 (0..4294967295)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The aging time of the VSI MAC address."
            ::= { hwVplsEntry 38 }

        hwVplsUnknowUnicastMacLearning OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies 
                whether the MAC address learning function for the discarded unknown unicast packets is enabled."
            ::= { hwVplsEntry 39 }

        hwVplsFlowLabel OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The value of this object identifies whether the PW FlowLabel is enabled."
            ::= { hwVplsEntry 40 }
               
        hwVplsServiceName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..100))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The service name of the VSI"
            ::= { hwVplsEntry 41 }
               
        hwVplsRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "RowStatus for this Table.
                Restriction:
                  After the signal type, VSI ID and RD are configured, 
                  the configuration can not be modify or delete."
            ::= { hwVplsEntry 51 }

        
--           
-- The VPLS's RT Table
-- 
        hwVplsRtTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsRtEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is the configuration table of VPN Target.
                Users can create or delete the VPN Target of a VSI."
            ::= { hwVplsMIBObjects 2 }

        
        hwVplsRtEntry OBJECT-TYPE
            SYNTAX HWVplsRtEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of a RT entry."
            INDEX { hwVplsVsiName, hwVplsRtType, hwVplsRtName }
            ::= { hwVplsRtTable 1 }

        
        HWVplsRtEntry ::=
            SEQUENCE { 
                hwVplsRtType
                    INTEGER,
                hwVplsRtName
                    DisplayString,
                hwVplsRtRowStatus
                    RowStatus
             }

        hwVplsRtType OBJECT-TYPE
            SYNTAX INTEGER
                {
                import(1),
                export(2)
                }
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the VC's encapsulation type."
            ::= { hwVplsRtEntry 1 }

        
        hwVplsRtName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (3..21))
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the RT."
            ::= { hwVplsRtEntry 2 }

        
        hwVplsRtRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "RowStatus for this Table.
                The max number of entries supported is 16.
                Not support modifying configuration."
            ::= { hwVplsRtEntry 51 }

        
--           
-- The VPLS's AC Table
-- 
        hwVplsAcTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsAcEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is the configuration table of AC.
                Users can create or delete the AC of a VSI."
            ::= { hwVplsMIBObjects 3 }

        
        hwVplsAcEntry OBJECT-TYPE
            SYNTAX HWVplsAcEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of a AC entry."
            INDEX { hwVplsVsiName, hwVplsAcIfIndex }
            ::= { hwVplsAcTable 1 }

        
        HWVplsAcEntry ::=
            SEQUENCE { 
                hwVplsAcIfIndex
                    InterfaceIndex,
                hwVplsAcStatus
                    INTEGER,
                hwVplsAcUpStartTime
                    DisplayString,
                hwVplsAcUpSumTime 
                    Unsigned32,
                hwVplsAcRowStatus
                    RowStatus
             }

        hwVplsAcIfIndex OBJECT-TYPE
            SYNTAX InterfaceIndex
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the interface index. There is only one VSI that can be created in one interface."
            ::= { hwVplsAcEntry 1 }

        
        hwVplsAcStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                up(1),
                down(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the AC's status."
            ::= { hwVplsAcEntry 2 }
 
        hwVplsAcUpStartTime OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..63))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Specifies the time this AC status has been Up(1)."
            ::= { hwVplsAcEntry 3 }
                        
        hwVplsAcUpSumTime OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Specifies the cumulate time this AC status has been Up(1)."
            ::= { hwVplsAcEntry 4 }
        
        hwVplsAcRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "RowStatus for this Table.
                Not support modifying configuration."
            ::= { hwVplsAcEntry 51 }

        
--           
-- The VPLS's BgpInfo Table
-- 
        hwVplsBgpInfoTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsBgpInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is the configuration table of BGP information.
                Users can create or delete the BgpInfo entry."
            ::= { hwVplsMIBObjects 4 }

        
        hwVplsBgpInfoEntry OBJECT-TYPE
            SYNTAX HWVplsBgpInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of a BgpInfo entry."
            INDEX { hwVplsVsiName, hwVplsBgpInfoSiteID }
            ::= { hwVplsBgpInfoTable 1 }

        
        HWVplsBgpInfoEntry ::=
            SEQUENCE { 
                hwVplsBgpInfoSiteID
                    Unsigned32,
                hwVplsBgpInfoRange
                    Unsigned32,
                hwVplsBgpInfoOffset
                    Unsigned32,
                hwVplsBgpInfoRowStatus
                    RowStatus
             }

        hwVplsBgpInfoSiteID OBJECT-TYPE
            SYNTAX Unsigned32 (0..65534)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the site ID."
            ::= { hwVplsBgpInfoEntry 1 }

        
        hwVplsBgpInfoRange OBJECT-TYPE
            SYNTAX Unsigned32 (1..65534)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the range."
            ::= { hwVplsBgpInfoEntry 2 }

        
        hwVplsBgpInfoOffset OBJECT-TYPE
            SYNTAX Unsigned32 (0..1)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Default original CE offset, default value is 0, calculate the VC in/out label."
            ::= { hwVplsBgpInfoEntry 3 }

        
        hwVplsBgpInfoRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "RowStatus for this Table.
                Restriction:
                  Support creating only one entry currently.
                  Before creating, the corresponding VSI's RD and signal
                  type must be designated.
                  The signal type must be BGP.
                  Site can not be modified.
                  Range can increase, but can't decrease."
            ::= { hwVplsBgpInfoEntry 51 }

        
--           
-- The VPLS's PW Table
-- 
        hwVplsPwTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsPwEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is the configuration table of PW.
                Users can create or delete the PW entry."
            ::= { hwVplsMIBObjects 5 }

        
        hwVplsPwEntry OBJECT-TYPE
            SYNTAX HWVplsPwEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of a PW entry."
            INDEX { hwVplsVsiName, hwVplsPwID, hwVplsPwRemoteIp }
            ::= { hwVplsPwTable 1 }

        
        HWVplsPwEntry ::=
            SEQUENCE { 
                hwVplsPwID
                    Unsigned32,
                hwVplsPwRemoteIp
                    IpAddress,
                hwVplsPwTnlPolicy
                    DisplayString,
                hwVplsPwType
                    INTEGER,
                hwVplsPwIsUpe
                    TruthValue,
                hwVplsPwInboundLabel
                    Unsigned32,
                hwVplsPwOutboundLabel
                    Unsigned32,
                hwVplsPwStatus
                    INTEGER,
                hwVplsPwVrIfIndex
                    InterfaceIndexOrZero,
                hwVplsPwVrID
                    Unsigned32,
                hwVplsPwUpStartTime 
                    DisplayString,
                hwVplsPwUpSumTime
                    Unsigned32,
                hwVplsPwRowStatus
                    RowStatus,
                hwVplsPwState
                    INTEGER,
                hwVplsPwWorkingState
                    INTEGER
             }

        hwVplsPwID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the PW ID."
            ::= { hwVplsPwEntry 1 }

        
        hwVplsPwRemoteIp OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the IP address of the remote end."
            ::= { hwVplsPwEntry 2 }

        
        hwVplsPwTnlPolicy OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..19))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the tunnel policy."
            ::= { hwVplsPwEntry 3 }

        
        hwVplsPwType OBJECT-TYPE
            SYNTAX INTEGER
                {
                normal(1),
                other(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the PW type."
            ::= { hwVplsPwEntry 4 }

        
        hwVplsPwIsUpe OBJECT-TYPE
            SYNTAX TruthValue
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the VPLS is UPE or not."
            ::= { hwVplsPwEntry 5 }

        
        hwVplsPwInboundLabel OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the inbound label."
            ::= { hwVplsPwEntry 6 }

        
        hwVplsPwOutboundLabel OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the outbound label."
            ::= { hwVplsPwEntry 7 }

        
        hwVplsPwStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                down(1),
                up(2),
                plugout(3),
                backup(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the PW's status."
            ::= { hwVplsPwEntry 8 }

        
        hwVplsPwVrIfIndex OBJECT-TYPE
            SYNTAX InterfaceIndexOrZero
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the VRRP interface this PW binding to."
            ::= { hwVplsPwEntry 9 }

        
        hwVplsPwVrID OBJECT-TYPE
            SYNTAX Unsigned32 (0..255)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the VrID this PW binding to."
            ::= { hwVplsPwEntry 10 }

        hwVplsPwUpStartTime OBJECT-TYPE                                             
            SYNTAX DisplayString (SIZE (0..63))                                                  
            MAX-ACCESS read-only                                               
            STATUS current                                                     
            DESCRIPTION                                                        
                "Specifies the time this PW status was Up(1)."                 
            ::= { hwVplsPwEntry 11 }                                       
                                                                           
        hwVplsPwUpSumTime OBJECT-TYPE                                          
            SYNTAX Unsigned32                                                  
            MAX-ACCESS read-only                                               
            STATUS current                                                     
            DESCRIPTION                                                        
                "Specifies the cumulate time this PW status has been Up(1)."   
            ::= { hwVplsPwEntry 12 }                                       
 
         hwVplsPwState OBJECT-TYPE                                          
            SYNTAX INTEGER
                {
                down(1),
                up(2)
                }                                                  
            MAX-ACCESS read-only                                               
            STATUS current                                                     
            DESCRIPTION                                                        
                "This object indicates the PW's state."   
            ::= { hwVplsPwEntry 13 }
        hwVplsPwWorkingState OBJECT-TYPE                                          
            SYNTAX INTEGER
                {
                master(1),
                backup(2)
                }                                                  
            MAX-ACCESS read-only                                               
            STATUS current                                                     
            DESCRIPTION                                                        
                "This object indicates the PW's working state."   
            ::= { hwVplsPwEntry 14 }
                        
        hwVplsPwRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "RowStatus for this Table.
                Restriction:
                  Not support creating or modifying entry currently.
                  If the signal type is LDP, we can delete PW by deleting Peer.
                  If the signal type is BGP, we can delete PW by configuring RD.
                  If the signal type is LDP, we need import PW ID value.
                  If the signal type is BGP, we can import 0 as PW ID value."
            ::= { hwVplsPwEntry 51 }
        
        
--           
-- The VPLS's Statistic Table
-- 
        hwVplsStatisticsTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains the VPLS's packets Statistic."
            ::= { hwVplsMIBObjects 6 }

        
        hwVplsStatisticsEntry OBJECT-TYPE
            SYNTAX HWVplsStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of the VPLS's packets statistic."
            INDEX { hwVplsVsiName }
            ::= { hwVplsStatisticsTable 1 }

        
        HWVplsStatisticsEntry ::=
            SEQUENCE { 
                hwVplsOutFrames
                    Counter64,
                hwVplsInFrames
                    Counter64,
                hwVplsOutBytes
                    Counter64,
                hwVplsInBytes
                    Counter64,
                hwVplsInDiscardFrames
                    Counter64
             }

        hwVplsOutFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames transmitted out of the VSI."
            ::= { hwVplsStatisticsEntry 1 }

        
        hwVplsInFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames received on the VSI."
            ::= { hwVplsStatisticsEntry 2 }

        
        hwVplsOutBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of bytes transmitted out of the VSI."
            ::= { hwVplsStatisticsEntry 3 }

        
        hwVplsInBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of bytes received on the VSI."
            ::= { hwVplsStatisticsEntry 4 }

        
        hwVplsInDiscardFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames received and then discarded on the VSI."
            ::= { hwVplsStatisticsEntry 5 }

        
--           
-- The Leaf Nodes of hwVplsMIBObjects
-- 
        hwVplsUpDownNotifEnable OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-write
            STATUS obsolete
            DESCRIPTION
                "This object indicates the enable sign of VPLS notification.
                The default value is disable (2)."
            ::= { hwVplsMIBObjects 7 }
        
        hwVplsStateChangeReason OBJECT-TYPE
            SYNTAX HWL2VpnStateChangeReason
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "This object indicates the reason of VC state change."
            ::= { hwVplsMIBObjects 8 }
        

--          
-- The VPLS LDP's Statistic Table
-- 
        hwVplsLdpStatisticsTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsLdpStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains the VPLS-PW's Traffic Statistic."
            ::= { hwVplsMIBObjects 9 }

        
        hwVplsLdpStatisticsEntry OBJECT-TYPE
            SYNTAX HWVplsLdpStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of the VPLS-PW's Traffic Statistic."
            INDEX { hwVplsVsiName, hwVplsLdpStatPwID, hwVplsLdpStatRemoteIpAddr }
            ::= { hwVplsLdpStatisticsTable 1 }

        
        HWVplsLdpStatisticsEntry ::=
            SEQUENCE { 
                hwVplsLdpStatPwID
                    Unsigned32,
                hwVplsLdpStatRemoteIpAddr
                    IpAddress,     
                hwVplsLdpStatEnable
                    HWEnableValue,
                hwVplsLdpStatInTrafficRate
                    Counter64,
                hwVplsLdpStatOutTrafficRate
                    Counter64,
                hwVplsLdpStatInFrameRate
                    Counter64,
                hwVplsLdpStatOutFrameRate
                    Counter64,
                hwVplsLdpStatInBytes
                    Counter64,
                hwVplsLdpStatOutBytes
                    Counter64,
                hwVplsLdpStatInFrames
                    Counter64,
                hwVplsLdpStatOutFrames
                    Counter64,
                hwVplsLdpStatInUnicastFrames
                    Counter64,
                hwVplsLdpStatOutUnicastFrames
                    Counter64,
                hwVplsLdpStatInMulticastFrames
                    Counter64,
                hwVplsLdpStatOutMulticastFrames
                    Counter64,
                hwVplsLdpStatInBroadcastFrames
                    Counter64,
                hwVplsLdpStatOutBroadcastFrames
                    Counter64,
                hwVplsLdpStatInDiscardFrames
                    Counter64,
                hwVplsLdpStatOutDiscardFrames
                    Counter64,
                hwVplsLdpStatInErrorFrames
                    Counter64,
                hwVplsLdpStatOutErrorFrames
                    Counter64,
                hwVplsLdpStatInUnknowFrames
                    Counter64,
                hwVplsLdpStatResetTime
                    DateAndTime,
                hwVplsLdpStatResetStatistic
                    INTEGER,
                hwVplsLdpStatInUnicastBytes
                    Counter64,
                hwVplsLdpStatOutUnicastBytes
                    Counter64,
                hwVplsLdpStatInMulticastBytes
                    Counter64,
                hwVplsLdpStatOutMulticastBytes
                    Counter64,
                hwVplsLdpStatInBroadcastBytes
                    Counter64,
                hwVplsLdpStatOutBroadcastBytes
                    Counter64	
             }

        hwVplsLdpStatPwID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the PW ID."
            ::= { hwVplsLdpStatisticsEntry 1 }

        
        hwVplsLdpStatRemoteIpAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the IP address of the remote end."
            ::= { hwVplsLdpStatisticsEntry 2 }   
            
        hwVplsLdpStatEnable OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the enable sign of LDP VPLS-PW's traffic statistics."
            ::= { hwVplsLdpStatisticsEntry 3 }
        
        
        hwVplsLdpStatInTrafficRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The traffic rate received on the PW."
            ::= { hwVplsLdpStatisticsEntry 4 }

        
        hwVplsLdpStatOutTrafficRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The traffic rate transmitted out of the PW."
            ::= { hwVplsLdpStatisticsEntry 5 }

        
        hwVplsLdpStatInFrameRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of Frames received on the PW."
            ::= { hwVplsLdpStatisticsEntry 6 }

        
        hwVplsLdpStatOutFrameRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of Frames transmitted out of the PW."
            ::= { hwVplsLdpStatisticsEntry 7 }

        
        hwVplsLdpStatInBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of bytes received on the PW."
            ::= { hwVplsLdpStatisticsEntry 8 }

        
        hwVplsLdpStatOutBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of bytes transmitted out of the PW."
            ::= { hwVplsLdpStatisticsEntry 9 }

        
        hwVplsLdpStatInFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames received on the PW."
            ::= { hwVplsLdpStatisticsEntry 10 }

        
        hwVplsLdpStatOutFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames transmitted out of the PW."
            ::= { hwVplsLdpStatisticsEntry 11 }

        
        hwVplsLdpStatInUnicastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of unicast frames received on the PW."
            ::= { hwVplsLdpStatisticsEntry 12 }

        
        hwVplsLdpStatOutUnicastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of unicast frames transmitted out of the PW."
            ::= { hwVplsLdpStatisticsEntry 13 }

        
        hwVplsLdpStatInMulticastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of multicast frames received on the PW."
            ::= { hwVplsLdpStatisticsEntry 14 }

        
        hwVplsLdpStatOutMulticastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of multicast frames transmitted out of the PW."
            ::= { hwVplsLdpStatisticsEntry 15 }

        
        hwVplsLdpStatInBroadcastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of broadcast frames received on the PW."
            ::= { hwVplsLdpStatisticsEntry 16 }

        
        hwVplsLdpStatOutBroadcastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of broadcast frames transmitted out of the PW."
            ::= { hwVplsLdpStatisticsEntry 17 }

        
        hwVplsLdpStatInDiscardFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames received and then discarded on the PW."
            ::= { hwVplsLdpStatisticsEntry 18 }

        
        hwVplsLdpStatOutDiscardFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames transmitted out and then discarded on the PW."
            ::= { hwVplsLdpStatisticsEntry 19 }

        
        hwVplsLdpStatInErrorFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of error frames received on the PW."
            ::= { hwVplsLdpStatisticsEntry 20 }

        
        hwVplsLdpStatOutErrorFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of error frames transmitted out of the PW."
            ::= { hwVplsLdpStatisticsEntry 21 }

        
        hwVplsLdpStatInUnknowFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of unknown frames received on the PW."
            ::= { hwVplsLdpStatisticsEntry 22 }

        
        hwVplsLdpStatResetTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Last time of clean out."
            ::= { hwVplsLdpStatisticsEntry 23 }


        hwVplsLdpStatResetStatistic OBJECT-TYPE
            SYNTAX INTEGER
                {
                resetStatistic(1)                           
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Reset traffic statistics of VSI's LDP peer."
            ::= { hwVplsLdpStatisticsEntry 24 }


        hwVplsLdpStatInUnicastBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of unicast bytes received on the PW."
            ::= { hwVplsLdpStatisticsEntry 25 }

        
        hwVplsLdpStatOutUnicastBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of unicast bytes transmitted out of the PW."
            ::= { hwVplsLdpStatisticsEntry 26 }

        
        hwVplsLdpStatInMulticastBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of multicast bytes received on the PW."
            ::= { hwVplsLdpStatisticsEntry 27 }

        
        hwVplsLdpStatOutMulticastBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of multicast bytes transmitted out of the PW."
            ::= { hwVplsLdpStatisticsEntry 28 }

        
        hwVplsLdpStatInBroadcastBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of broadcast bytes received on the PW."
            ::= { hwVplsLdpStatisticsEntry 29 }

        
        hwVplsLdpStatOutBroadcastBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of broadcast bytes transmitted out of the PW."
            ::= { hwVplsLdpStatisticsEntry 30 }

--          
-- The VPLS BGP's Statistic Table
-- 
        hwVplsBgpStatisticsTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsBgpStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains the VPLS-PW's Traffic Statistic."
            ::= { hwVplsMIBObjects 10 }

        
        hwVplsBgpStatisticsEntry OBJECT-TYPE
            SYNTAX HWVplsBgpStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of the VPLS-PW's Traffic Statistic."
            INDEX { hwVplsVsiName, hwVplsBgpStatSiteID, hwVplsBgpStatRemoteIpAddr }
            ::= { hwVplsBgpStatisticsTable 1 }

        
        HWVplsBgpStatisticsEntry ::=
            SEQUENCE { 
                hwVplsBgpStatSiteID
                    Unsigned32,
                hwVplsBgpStatRemoteIpAddr
                    IpAddress,     
                hwVplsBgpStatEnable
                    HWEnableValue,
                hwVplsBgpStatInTrafficRate
                    Counter64,
                hwVplsBgpStatOutTrafficRate
                    Counter64,
                hwVplsBgpStatInFrameRate
                    Counter64,
                hwVplsBgpStatOutFrameRate
                    Counter64,
                hwVplsBgpStatInBytes
                    Counter64,
                hwVplsBgpStatOutBytes
                    Counter64,
                hwVplsBgpStatInFrames
                    Counter64,
                hwVplsBgpStatOutFrames
                    Counter64,
                hwVplsBgpStatInUnicastFrames
                    Counter64,
                hwVplsBgpStatOutUnicastFrames
                    Counter64,
                hwVplsBgpStatInMulticastFrames
                    Counter64,
                hwVplsBgpStatOutMulticastFrames
                    Counter64,
                hwVplsBgpStatInBroadcastFrames
                    Counter64,
                hwVplsBgpStatOutBroadcastFrames
                    Counter64,
                hwVplsBgpStatInDiscardFrames
                    Counter64,
                hwVplsBgpStatOutDiscardFrames
                    Counter64,
                hwVplsBgpStatInErrorFrames
                    Counter64,
                hwVplsBgpStatOutErrorFrames
                    Counter64,
                hwVplsBgpStatInUnknowFrames
                    Counter64,
                hwVplsBgpStatResetTime
                    DateAndTime
             }

        hwVplsBgpStatSiteID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the Site ID."
            ::= { hwVplsBgpStatisticsEntry 1 }

        
        hwVplsBgpStatRemoteIpAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the IP address of the remote end."
            ::= { hwVplsBgpStatisticsEntry 2 } 
            
          hwVplsBgpStatEnable OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the enable sign of BGP VPLS-PW's traffic statistics."
            ::= { hwVplsBgpStatisticsEntry 3 }
            

        
        hwVplsBgpStatInTrafficRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The traffic rate received on the PW."
            ::= { hwVplsBgpStatisticsEntry 4 }

        
        hwVplsBgpStatOutTrafficRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The traffic rate transmitted out of the PW."
            ::= { hwVplsBgpStatisticsEntry 5 }

        
        hwVplsBgpStatInFrameRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of Frames received on the PW."
            ::= { hwVplsBgpStatisticsEntry 6 }

        
        hwVplsBgpStatOutFrameRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of Frames transmitted out of the PW."
            ::= { hwVplsBgpStatisticsEntry 7 }

        
        hwVplsBgpStatInBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of bytes received on the PW."
            ::= { hwVplsBgpStatisticsEntry 8 }

        
        hwVplsBgpStatOutBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of bytes transmitted out of the PW."
            ::= { hwVplsBgpStatisticsEntry 9 }

        
        hwVplsBgpStatInFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames received on the PW."
            ::= { hwVplsBgpStatisticsEntry 10 }

        
        hwVplsBgpStatOutFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames transmitted out of the PW."
            ::= { hwVplsBgpStatisticsEntry 11 }

        
        hwVplsBgpStatInUnicastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of unicast frames received on the PW."
            ::= { hwVplsBgpStatisticsEntry 12 }

        
        hwVplsBgpStatOutUnicastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of unicast frames transmitted out of the PW."
            ::= { hwVplsBgpStatisticsEntry 13 }

        
        hwVplsBgpStatInMulticastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of multicast frames received on the PW."
            ::= { hwVplsBgpStatisticsEntry 14 }

        
        hwVplsBgpStatOutMulticastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of multicast frames transmitted out of the PW."
            ::= { hwVplsBgpStatisticsEntry 15 }

        
        hwVplsBgpStatInBroadcastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of broadcast frames received on the PW."
            ::= { hwVplsBgpStatisticsEntry 16 }

        
        hwVplsBgpStatOutBroadcastFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of broadcast frames transmitted out of the PW."
            ::= { hwVplsBgpStatisticsEntry 17 }

        
        hwVplsBgpStatInDiscardFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames received and then discarded on the PW."
            ::= { hwVplsBgpStatisticsEntry 18 }

        
        hwVplsBgpStatOutDiscardFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames transmitted out and then discarded on the PW."
            ::= { hwVplsBgpStatisticsEntry 19 }

        
        hwVplsBgpStatInErrorFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of error frames received on the PW."
            ::= { hwVplsBgpStatisticsEntry 20 }

        
        hwVplsBgpStatOutErrorFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of error frames transmitted out of the PW."
            ::= { hwVplsBgpStatisticsEntry 21 }

        
        hwVplsBgpStatInUnknowFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of unknown frames received on the PW."
            ::= { hwVplsBgpStatisticsEntry 22 }

        
        hwVplsBgpStatResetTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Last time of clean out."
            ::= { hwVplsBgpStatisticsEntry 23 }


--          
-- The VPLS's LDP peer Table
-- 
        hwVplsLdpPeerTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwVplsLdpPeerEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is the configuration table of VPLS's LDP peer.
                Users can create or delete the LDP peer entry."
            ::= { hwVplsMIBObjects 11 }


        hwVplsLdpPeerEntry OBJECT-TYPE
            SYNTAX HwVplsLdpPeerEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of a LDP peer entry."
            INDEX { hwVplsVsiName, hwVplsLdpPeerRouterID, hwVplsLdpPeerPwId }
            ::= { hwVplsLdpPeerTable 1 }


        HwVplsLdpPeerEntry ::=
            SEQUENCE { 
                hwVplsLdpPeerRouterID
                    IpAddress,
                hwVplsLdpPeerPwId
                    Unsigned32,
                hwVplsLdpPeerTnlPolicyName
                    DisplayString,
                hwVplsLdpPeerUpeType
                    INTEGER,
                hwVplsLdpPeerTransLable
                    Unsigned32,
                hwVplsLdpPeerRecvLable
                    Unsigned32,
                hwVplsLdpPeerVrrpIfIndex
                    InterfaceIndexOrZero,
                hwVplsLdpPeerVirtualRouterId
                    Unsigned32,
                hwVplsLdpPeerCir
                    Unsigned32,
                hwVplsLdpPeerPir
                    Unsigned32,
                hwVplsLdpPeerQosProfileName
                    DisplayString,
                hwVplsLdpPeerStatus
                    INTEGER,
                hwVplsLdpPeerPwName
                    DisplayString,
                hwVplsLdpPeerIgnoreStpLoopCheck
                    EnabledStatus,
                hwVplsLdpPeerRowStatus
                    RowStatus
            }


        hwVplsLdpPeerRouterID OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the IP address of the LDP peer."
            ::= { hwVplsLdpPeerEntry 1 }


        hwVplsLdpPeerPwId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the PW ID."
            ::= { hwVplsLdpPeerEntry 2 }


        hwVplsLdpPeerTnlPolicyName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..19))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the name of tunnel policy."
            ::= { hwVplsLdpPeerEntry 3 }


        hwVplsLdpPeerUpeType OBJECT-TYPE
            SYNTAX INTEGER
                {
                upe(1),
                staticupe(2),
                unknown(3)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the VPLS is UPE , static UPE or not."
            ::= { hwVplsLdpPeerEntry 4 }


        hwVplsLdpPeerTransLable OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the transmitted label."
            ::= { hwVplsLdpPeerEntry 5 }


        hwVplsLdpPeerRecvLable OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the received label."
            ::= { hwVplsLdpPeerEntry 6 }


        hwVplsLdpPeerVrrpIfIndex OBJECT-TYPE
            SYNTAX InterfaceIndexOrZero
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the VRRP interface this PW binding to."
            ::= { hwVplsLdpPeerEntry 7 }


        hwVplsLdpPeerVirtualRouterId OBJECT-TYPE
            SYNTAX Unsigned32 (0..255)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the virtual router ID this PW binding to."
            ::= { hwVplsLdpPeerEntry 8 }


        hwVplsLdpPeerCir OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the committed information rate, based on the LDP peer."
            ::= { hwVplsLdpPeerEntry 9 }


        hwVplsLdpPeerPir OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the peak information rate, based on the LDP peer."
            ::= { hwVplsLdpPeerEntry 10 }


        hwVplsLdpPeerQosProfileName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..63))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the QoS profile's name, based on the LDP peer."
            ::= { hwVplsLdpPeerEntry 11 }

        
        hwVplsLdpPeerStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                down(1),
                up(2),
                plugout(3),
                backup(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the LDP peer's status."
            ::= { hwVplsLdpPeerEntry 12 }


        hwVplsLdpPeerPwName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..15))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the name of PW."
            ::= { hwVplsLdpPeerEntry 13 }


        hwVplsLdpPeerIgnoreStpLoopCheck OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the enable sign of the ignorer of 
                STP loop check."
            ::= { hwVplsLdpPeerEntry 14 }


        hwVplsLdpPeerRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Row status for this Table."
            ::= { hwVplsLdpPeerEntry 51 }


--
-- The VPLS LDP's QoS Statistic Table
--
        hwVplsLdpQosStatisticTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsLdpQosStatisticEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains the VPLS LDP's traffic statistic, 
                based on VSI LDP's peer and QoS."
            ::= { hwVplsMIBObjects 12 }


        hwVplsLdpQosStatisticEntry OBJECT-TYPE
            SYNTAX HWVplsLdpQosStatisticEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of the VPLS LDP's traffic statistic."
            INDEX { hwVplsVsiName, hwVplsLdpQosStatPwId, hwVplsLdpQosStatRemoteIpAddr, hwVplsLdpQosStatQueueId }
            ::= { hwVplsLdpQosStatisticTable 1 }


        HWVplsLdpQosStatisticEntry ::=
            SEQUENCE { 
                hwVplsLdpQosStatPwId
                    Unsigned32,
                hwVplsLdpQosStatRemoteIpAddr
                    IpAddress,
                hwVplsLdpQosStatQueueId
                    INTEGER,
                hwVplsLdpQosStatTotalPassPacket
                    Counter64,
                hwVplsLdpQosStatTotalPassByte
                    Counter64,
                hwVplsLdpQosStatTotalDiscardPacket
                    Counter64,
                hwVplsLdpQosStatTotalDiscardByte
                    Counter64,
                hwVplsLdpQosStatPassPacketRate
                    Counter64,
                hwVplsLdpQosStatPassByteRate
                    Counter64,
                hwVplsLdpQosStatDiscardPacketRate
                    Counter64,
                hwVplsLdpQosStatDiscardByteRate
                    Counter64
            }


        hwVplsLdpQosStatPwId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The PW ID."
            ::= { hwVplsLdpQosStatisticEntry 1 }

        
        hwVplsLdpQosStatRemoteIpAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The IP address of the remote end."
            ::= { hwVplsLdpQosStatisticEntry 2 }   


        hwVplsLdpQosStatQueueId OBJECT-TYPE
            SYNTAX INTEGER
                {
                be(1),
                af1(2),
                af2(3),
                af3(4),
                af4(5),
                ef(6),
                cs6(7),
                cs7(8)
                }
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The queue's ID. The value must be 
                be,af1,af2,af3,af4,ef,cs6,cs7."
            ::= { hwVplsLdpQosStatisticEntry 3 }


        hwVplsLdpQosStatTotalPassPacket OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Number of total passed packets, based on LDP peer and QoS."
            ::= { hwVplsLdpQosStatisticEntry 4 }


        hwVplsLdpQosStatTotalPassByte OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Number of total passed bytes, based on LDP peer and QoS."
            ::= { hwVplsLdpQosStatisticEntry 5 }


        hwVplsLdpQosStatTotalDiscardPacket OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Number of total discarded packets, based on LDP peer and QoS."
            ::= { hwVplsLdpQosStatisticEntry 6 }


        hwVplsLdpQosStatTotalDiscardByte OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Number of total discarded bytes, based on LDP peer and QoS."
            ::= { hwVplsLdpQosStatisticEntry 7 }


        hwVplsLdpQosStatPassPacketRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Rate of passed packets for the last 30 seconds, 
                based on LDP peer and QoS. Unit: pps"
            ::= { hwVplsLdpQosStatisticEntry 8 }


        hwVplsLdpQosStatPassByteRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Rate of passed bytes for the last 30 seconds, 
                based on LDP peer and QoS. Unit: bps"
            ::= { hwVplsLdpQosStatisticEntry 9 }


        hwVplsLdpQosStatDiscardPacketRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Rate of discarded packets for the last 30 seconds, 
                based on LDP peer and QoS. Unit: pps"
            ::= { hwVplsLdpQosStatisticEntry 10 }


        hwVplsLdpQosStatDiscardByteRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Rate of discarded bytes for the last 30 seconds, 
                based on LDP peer and QoS. Unit: bps"
            ::= { hwVplsLdpQosStatisticEntry 11 }


--
-- The VPLS's Statistic Table
--
        hwVplsStatisticTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsStatisticEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains the VPLS's traffic statistic, based on VSI."
            ::= { hwVplsMIBObjects 13 }


        hwVplsStatisticEntry OBJECT-TYPE
            SYNTAX HWVplsStatisticEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of the VPLS's traffic statistic."
            INDEX { hwVplsVsiName }
            ::= { hwVplsStatisticTable 1 }


        HWVplsStatisticEntry ::=
            SEQUENCE { 
                hwVplsStatEnable
                    EnabledStatus,
                hwVplsStatResetStatistic
                    INTEGER,
                hwVplsStatResetTime
                    DateAndTime,
                hwVplsStatQosPacketRate
                    Counter64,
                hwVplsStatQosByteRate
                    Counter64,
                hwVplsStatQosPacket
                    Counter64,
                hwVplsStatQosByte
                    Counter64
            }


        hwVplsStatEnable OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the enable sign of VSI's traffic statistics."
            ::= { hwVplsStatisticEntry 1 }


        hwVplsStatResetStatistic OBJECT-TYPE
            SYNTAX INTEGER
                {
                resetStatistic(1)                           
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Reset traffic statistics of VSI."
            ::= { hwVplsStatisticEntry 2 }


        hwVplsStatResetTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Last time of clean out."
            ::= { hwVplsStatisticEntry 3 }


        hwVplsStatQosPacketRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of packets received on the VSI."
            ::= { hwVplsStatisticEntry 4 }

        
        hwVplsStatQosByteRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of bytes received on the VSI."
            ::= { hwVplsStatisticEntry 5 }


        hwVplsStatQosPacket OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of packets received on the VSI."
            ::= { hwVplsStatisticEntry 6 }

        
        hwVplsStatQosByte OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of bytes received on the VSI."
            ::= { hwVplsStatisticEntry 7 }


--
-- The VPLS's QoS Statistic Table
--
        hwVplsQosStatisticTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsQosStatisticEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains the VPLS's traffic statistic, based on VSI and QoS."
            ::= { hwVplsMIBObjects 14 }


        hwVplsQosStatisticEntry OBJECT-TYPE
            SYNTAX HWVplsQosStatisticEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of the VPLS's traffic statistics."
            INDEX { hwVplsVsiName, hwVplsQosStatQueueId }
            ::= { hwVplsQosStatisticTable 1 }


        HWVplsQosStatisticEntry ::=
            SEQUENCE { 
                hwVplsQosStatQueueId
                    INTEGER,
                hwVplsQosStatTotalPassPacket
                    Counter64,
                hwVplsQosStatTotalPassByte
                    Counter64,
                hwVplsQosStatTotalDiscardPacket
                    Counter64,
                hwVplsQosStatTotalDiscardByte
                    Counter64,
                hwVplsQosStatPassPacketRate
                    Counter64,
                hwVplsQosStatPassByteRate
                    Counter64,
                hwVplsQosStatDiscardPacketRate
                    Counter64,
                hwVplsQosStatDiscardByteRate
                    Counter64
            }


        hwVplsQosStatQueueId OBJECT-TYPE
            SYNTAX INTEGER
                {
                be(1),
                af1(2),
                af2(3),
                af3(4),
                af4(5),
                ef(6),
                cs6(7),
                cs7(8)
                }
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The queue's ID. The value must be 
                be,af1,af2,af3,af4,ef,cs6,cs7."
            ::= { hwVplsQosStatisticEntry 1 }


        hwVplsQosStatTotalPassPacket OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Number of total passed packets, based on VSI and QoS."
            ::= { hwVplsQosStatisticEntry 2 }


        hwVplsQosStatTotalPassByte OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Number of total passed bytes, based on VSI and QoS."
            ::= { hwVplsQosStatisticEntry 3 }


        hwVplsQosStatTotalDiscardPacket OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Number of total discarded packets, based on VSI and QoS."
            ::= { hwVplsQosStatisticEntry 4 }


        hwVplsQosStatTotalDiscardByte OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Number of total discarded bytes, based on VSI and QoS."
            ::= { hwVplsQosStatisticEntry 5 }


        hwVplsQosStatPassPacketRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Rate of passed packets for the last 30 seconds, 
                based on VSI and QoS. Unit: pps"
            ::= { hwVplsQosStatisticEntry 6 }


        hwVplsQosStatPassByteRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Rate of passed bytes for the last 30 seconds, 
                based on VSI and QoS. Unit: bps"
            ::= { hwVplsQosStatisticEntry 7 }


        hwVplsQosStatDiscardPacketRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Rate of discarded packets for the last 30 seconds, 
                based on VSI and QoS. Unit: pps"
            ::= { hwVplsQosStatisticEntry 8 }


        hwVplsQosStatDiscardByteRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Rate of discarded bytes for the last 30 seconds, 
                based on VSI and QoS. Unit: bps"
            ::= { hwVplsQosStatisticEntry 9 }

--           
-- The Leaf Nodes of hwVplsMIBObjects
-- 
        hwL2vpnTnlType OBJECT-TYPE
           SYNTAX INTEGER
           {
                lsp(1),
                crlsp(2),
                other(3)
           }
           MAX-ACCESS accessible-for-notify
           STATUS current
           DESCRIPTION
                "This object indicates the tunnel type."
           ::= { hwVplsMIBObjects 15 }

        hwL2vpnTunnelIndex OBJECT-TYPE
           SYNTAX Unsigned32 (0..65535)
           MAX-ACCESS accessible-for-notify
           STATUS current
           DESCRIPTION
                "This object indicates the mplsTunnelIndex.
                It contains an unused value for
                mplsTunnelIndex, or a zero to indicate
                that none exist. Negative values are not allowed,
                as they do not correspond to valid values of
                mplsTunnelIndex.

                Note that this object offers an unused value
                for an mplsTunnelIndex value at the ingress
                side of a tunnel. At other LSRs the value
                of mplsTunnelIndex SHOULD be taken from the
                value signaled by the MPLS signaling protocol.
            "
           ::= { hwVplsMIBObjects 16 }      

--
-- The VPLS's protect group Table
--
        hwVplsVsiProtectGroupTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsVsiProtectGroupEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is the VPLS protect group's configuration table. Users can create or delete the VPLS protect group by it."
            ::= { hwVplsMIBObjects 17 }


        hwVplsVsiProtectGroupEntry OBJECT-TYPE
            SYNTAX HWVplsVsiProtectGroupEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of a VPLS protect group entry."
            INDEX { hwVplsVsiName, hwVplsVsiProtectGroupName }
            ::= { hwVplsVsiProtectGroupTable 1 }


        HWVplsVsiProtectGroupEntry ::=
            SEQUENCE { 
                hwVplsVsiProtectGroupName
                    DisplayString,
                hwVplsVsiProtectGroupMode
                    INTEGER
            }

        hwVplsVsiProtectGroupName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..15))
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the VPLS protect group's name."
            ::= { hwVplsVsiProtectGroupEntry 1 }

        hwVplsVsiProtectGroupMode OBJECT-TYPE
            SYNTAX INTEGER
                {
                none(0),
                frr(1),
                master(2),
                independent(3)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the VPLS protect group's mode."
            ::= { hwVplsVsiProtectGroupEntry 2 }

--
-- The VPLS HARD-PIPE's Statistic Table
--
        hwVplsHardPipeStatisticsTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsHardPipeStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains the VPLS-PW's hard-pipe Traffic Statistic."
            ::= { hwVplsMIBObjects 18 }

        
        hwVplsHardPipeStatisticsEntry OBJECT-TYPE
            SYNTAX HWVplsHardPipeStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of the VPLS-PW's hard-pipe Traffic Statistic."
            INDEX { hwVplsVsiName, hwVplsHardPipeStatPwID, hwVplsHardPipeStatRemoteIpAddr }
            ::= { hwVplsHardPipeStatisticsTable 1 }

        
        HWVplsHardPipeStatisticsEntry ::=
            SEQUENCE { 
                hwVplsHardPipeStatPwID
                    Unsigned32,
                hwVplsHardPipeStatRemoteIpAddr
                    IpAddress,     
                hwVplsHardPipeStatEnable
                    HWEnableValue,
                hwVplsHardPipeStatPassFrameRate
                    Counter64,
                hwVplsHardPipeStatPassBytesRate
                    Counter64,
                hwVplsHardPipeStatDropFrameRate
                    Counter64,
                hwVplsHardPipeStatDropBytesRate
                    Counter64,  
                hwVplsHardPipeStatPassFrames
                    Counter64,
                hwVplsHardPipeStatPassBytes
                    Counter64,
                hwVplsHardPipeStatDropFrame
                    Counter64,
                hwVplsHardPipeStatDropBytes
                    Counter64, 					
                hwVplsHardPipeStatResetTime
                    DateAndTime,
                hwVplsHardPipeStatResetStatistic
                    INTEGER				
             }

        hwVplsHardPipeStatPwID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the PW ID."
            ::= { hwVplsHardPipeStatisticsEntry 1 }

        
        hwVplsHardPipeStatRemoteIpAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the IP address of the remote end."
            ::= { hwVplsHardPipeStatisticsEntry 2 }   
            
        hwVplsHardPipeStatEnable OBJECT-TYPE
            SYNTAX HWEnableValue
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the enable sign of LDP VPLS-PW's hard-pipe traffic statistics."
            ::= { hwVplsHardPipeStatisticsEntry 3 }
        
        
        hwVplsHardPipeStatPassFrameRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of Frames received on the PW."
            ::= { hwVplsHardPipeStatisticsEntry 4 }

        
        hwVplsHardPipeStatPassBytesRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "TThe rate of bytes received on the PW."
            ::= { hwVplsHardPipeStatisticsEntry 5 }

        
        hwVplsHardPipeStatDropFrameRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "he rate of Frames transmitted out of the PW."
            ::= { hwVplsHardPipeStatisticsEntry 6 }

        
        hwVplsHardPipeStatDropBytesRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of bytes transmitted out of the PW."
            ::= { hwVplsHardPipeStatisticsEntry 7 }

        
        hwVplsHardPipeStatPassFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames received on the PW."
            ::= { hwVplsHardPipeStatisticsEntry 8 }

        
        hwVplsHardPipeStatPassBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of bytes received on the PW."
            ::= { hwVplsHardPipeStatisticsEntry 9 }

        
        hwVplsHardPipeStatDropFrame OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames dropped on the PW."
            ::= { hwVplsHardPipeStatisticsEntry 10 }

        
        hwVplsHardPipeStatDropBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of bytes dropped on the PW."
            ::= { hwVplsHardPipeStatisticsEntry 11 }
			
        
        hwVplsHardPipeStatResetTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Last time of clean out."
            ::= { hwVplsHardPipeStatisticsEntry 12 }

			
        hwVplsHardPipeStatResetStatistic OBJECT-TYPE
            SYNTAX INTEGER
                {
                resetStatistic(1)                           
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Reset traffic statistics of VSI's LDP peer."
            ::= { hwVplsHardPipeStatisticsEntry 13 }

--          
-- The VPLS PW Suppression's Statistic Table
-- 
        hwVplsPwSuppStatisticsTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsPwSuppStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains the VPLS-PW's suppresssion Traffic Statistic."
            ::= { hwVplsMIBObjects 19 }

        
        hwVplsPwSuppStatisticsEntry OBJECT-TYPE
            SYNTAX HWVplsPwSuppStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of the VPLS-PW's suppresssion Traffic Statistic."
            INDEX { hwVplsVsiName}
            ::= { hwVplsPwSuppStatisticsTable 1 }

        
        HWVplsPwSuppStatisticsEntry::=
            SEQUENCE { 
                hwVplsPwSuppStatCir
                    Counter64,
                hwVplsPwSuppStatPir
                    Counter64,
                hwVplsPwSuppStatCbs
                    Counter64,
                hwVplsPwSuppStatPbs
                    Counter64,  
                hwVplsPwSuppStatPassFrames
                    Counter64,
                hwVplsPwSuppStatPassBytes
                    Counter64,
                hwVplsPwSuppStatDropFrames
                    Counter64,
                hwVplsPwSuppStatDropBytes
                    Counter64, 	
                hwVplsPwSuppStatPassBbsRate
                    Counter64,
                hwVplsPwSuppStatPassPbsRate
                    Counter64,
                hwVplsPwSuppStatDropBbsRate
                    Counter64,
                hwVplsPwSuppStatDropPbsRate
                    Counter64, 				
                hwVplsPwSuppStatResetTime
                    DateAndTime,
                hwVplsPwSuppStatResetStatistic
                    INTEGER				
             }
	     
        hwVplsPwSuppStatCir OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the committed information rate, based on VSI."
            ::= { hwVplsPwSuppStatisticsEntry 1 }

        
        hwVplsPwSuppStatPir OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the peak information rate, based on VSI."
            ::= { hwVplsPwSuppStatisticsEntry 2 }

        
        hwVplsPwSuppStatCbs OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the CBS limitation, based on VSI."
            ::= { hwVplsPwSuppStatisticsEntry 3 }

        hwVplsPwSuppStatPbs OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the PBS limitation, based on VSI."
            ::= { hwVplsPwSuppStatisticsEntry 4 } 
        
        hwVplsPwSuppStatPassFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames passed from PW."
            ::= { hwVplsPwSuppStatisticsEntry 5 }
        
        hwVplsPwSuppStatPassBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bytes passed from PW."
            ::= { hwVplsPwSuppStatisticsEntry 6 }

        
        hwVplsPwSuppStatDropFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames dropped from PW."
            ::= { hwVplsPwSuppStatisticsEntry 7 }

        
        hwVplsPwSuppStatDropBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bytes dropped from PW."
            ::= { hwVplsPwSuppStatisticsEntry 8 }

        
        hwVplsPwSuppStatPassBbsRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of bps passed from PW."
            ::= { hwVplsPwSuppStatisticsEntry 9 }

        
        hwVplsPwSuppStatPassPbsRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of pbs passed from PW."
            ::= { hwVplsPwSuppStatisticsEntry 10 }

        
        hwVplsPwSuppStatDropBbsRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of bps dropped from PW."
            ::= { hwVplsPwSuppStatisticsEntry 11 }

        
        hwVplsPwSuppStatDropPbsRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of pbs dropped from PW."
            ::= { hwVplsPwSuppStatisticsEntry 12 }						
        
        hwVplsPwSuppStatResetTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Last time of clean out."
            ::= { hwVplsPwSuppStatisticsEntry 13 }
			
        hwVplsPwSuppStatResetStatistic OBJECT-TYPE
            SYNTAX INTEGER
                {
                resetStatistic(1)                           
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Reset suppression traffic statistics of VSI."
            ::= { hwVplsPwSuppStatisticsEntry 14 }

--          
-- The VPLS AC Suppression's Statistic Table
-- 
        hwVplsAcSuppStatisticsTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWVplsAcSuppStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains the VPLS-AC's suppresssion Traffic Statistic."
            ::= { hwVplsMIBObjects 20 }

        
        hwVplsAcSuppStatisticsEntry OBJECT-TYPE
            SYNTAX HWVplsAcSuppStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of the VPLS-AC's suppresssion Traffic Statistic."
            INDEX { hwVplsVsiName}
            ::= { hwVplsAcSuppStatisticsTable 1 }

        
        HWVplsAcSuppStatisticsEntry::=
            SEQUENCE { 
                hwVplsAcSuppStatCir
                    Counter64,
                hwVplsAcSuppStatPir
                    Counter64,
                hwVplsAcSuppStatCbs
                    Counter64,
                hwVplsAcSuppStatPbs
                    Counter64,  
                hwVplsAcSuppStatPassFrames
                    Counter64,
                hwVplsAcSuppStatPassBytes
                    Counter64,
                hwVplsAcSuppStatDropFrame
                    Counter64,
                hwVplsAcSuppStatDropBytes
                    Counter64, 	
                hwVplsAcSuppStatPassBbsRate
                    Counter64,
                hwVplsAcSuppStatPassPbsRate
                    Counter64,
                hwVplsAcSuppStatDropBbsRate
                    Counter64,
                hwVplsAcSuppStatDropPbsRate
                    Counter64, 				
                hwVplsAcSuppStatResetTime 
                    DateAndTime,
                hwVplsAcSuppStatResetStatistic
                    INTEGER				
             }
	     
        hwVplsAcSuppStatCir OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the committed information rate, based on VSI."
            ::= { hwVplsAcSuppStatisticsEntry 1 }

        
        hwVplsAcSuppStatPir OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the peak information rate, based on VSI."
            ::= { hwVplsAcSuppStatisticsEntry 2 }

        
        hwVplsAcSuppStatCbs OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the CBS limitation, based on VSI."
            ::= { hwVplsAcSuppStatisticsEntry 3 }

        hwVplsAcSuppStatPbs OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the PBS limitation, based on VSI."
            ::= { hwVplsAcSuppStatisticsEntry 4 } 
        
        hwVplsAcSuppStatPassFrames OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames passed from AC."
            ::= { hwVplsAcSuppStatisticsEntry 5 }
        
        hwVplsAcSuppStatPassBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bytes passed from PW."
            ::= { hwVplsAcSuppStatisticsEntry 6 }

        
        hwVplsAcSuppStatDropFrame OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of frames dropped from AC."
            ::= { hwVplsAcSuppStatisticsEntry 7 }

        
        hwVplsAcSuppStatDropBytes OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bytes dropped from AC."
            ::= { hwVplsAcSuppStatisticsEntry 8 }

        
        hwVplsAcSuppStatPassBbsRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of bps passed from AC."
            ::= { hwVplsAcSuppStatisticsEntry 9 }

        
        hwVplsAcSuppStatPassPbsRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of pbs passed from AC."
            ::= { hwVplsAcSuppStatisticsEntry 10 }

        
        hwVplsAcSuppStatDropBbsRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of bps dropped from AC."
            ::= { hwVplsAcSuppStatisticsEntry 11 }

        
        hwVplsAcSuppStatDropPbsRate OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The rate of pbs dropped from AC."
            ::= { hwVplsAcSuppStatisticsEntry 12 }						
        
        hwVplsAcSuppStatResetTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Last time of clean out."
            ::= { hwVplsAcSuppStatisticsEntry 13 }
			
        hwVplsAcSuppStatResetStatistic OBJECT-TYPE
            SYNTAX INTEGER
                {
                resetStatistic(1)                           
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Reset suppression traffic statistics of VSI."
            ::= { hwVplsAcSuppStatisticsEntry 14 }

--           
-- VPLS MIB Trap Definitions
-- 
        hwVplsMIBTraps OBJECT IDENTIFIER ::= { hwL2VpnVplsExt 2 }

        
        hwVplsVcDown NOTIFICATION-TYPE
            OBJECTS { hwVplsPwType, hwVplsStateChangeReason, sysUpTime, hwVplsPwTnlPolicy, hwL2vpnTnlType, hwL2vpnTunnelIndex }
            STATUS current
            DESCRIPTION 
                "This notification indicates the VC's state changes to down."
            ::= { hwVplsMIBTraps 1 }

        
        hwVplsVcUp NOTIFICATION-TYPE
            OBJECTS { hwVplsPwType, hwVplsStateChangeReason, sysUpTime, hwVplsPwTnlPolicy }
            STATUS current
            DESCRIPTION 
                "This notification indicates the VC's state changes to up."
            ::= { hwVplsMIBTraps 2 }

        
        hwVplsVsiDown NOTIFICATION-TYPE
            OBJECTS { hwVplsVsiID, hwVplsStateChangeReason, hwVplsStatus, ifName }
            STATUS current
            DESCRIPTION 
                "This notification indicates the VSI's state changes to down."
            ::= { hwVplsMIBTraps 3 }

        
        hwVplsVsiUp NOTIFICATION-TYPE
            OBJECTS { hwVplsVsiID, hwVplsStateChangeReason, hwVplsStatus, ifName }
            STATUS current
            DESCRIPTION 
                "This notification indicates the VSI's state changes to up."
            ::= { hwVplsMIBTraps 4 }

        
        hwVplsVcBackup NOTIFICATION-TYPE
            OBJECTS { hwVplsPwType, hwVplsStateChangeReason, sysUpTime }
            STATUS current
            DESCRIPTION 
                "This notification indicates the VC's state changes to backup."
            ::= { hwVplsMIBTraps 5 }
        
        
        hwVplsVsiDeleted NOTIFICATION-TYPE
            OBJECTS { hwVplsVsiID }
            STATUS current
            DESCRIPTION 
                "This notification indicates the VSI is deleted."
            ::= { hwVplsMIBTraps 6 }


        hwVplsVcDeleted NOTIFICATION-TYPE
            OBJECTS { hwVplsPwType }
            STATUS current
            DESCRIPTION 
                "This notification indicates the VC is deleted."
            ::= { hwVplsMIBTraps 7 }
            
            
        hwVplsVcStatusChange NOTIFICATION-TYPE
            OBJECTS { hwVplsStateChangeReason, hwVplsPwState, hwVplsPwWorkingState, sysUpTime }
            STATUS current
            DESCRIPTION 
                "This notification indicates the VC is deleted."
            ::= { hwVplsMIBTraps 8 }
            
            
        hwVplsVcNumberThresholdExceed NOTIFICATION-TYPE
            OBJECTS { hwL2VpnVcLimitClass, hwL2VpnVsiVcNumber, hwVplsVcNumberUpperThreshold, hwVplsVcNumberMaxNum }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the number of VPLS VCs reaches the upper threshold."
            ::= { hwVplsMIBTraps 9 }


        hwVplsVcNumberThresholdClear NOTIFICATION-TYPE
            OBJECTS { hwL2VpnVcLimitClass, hwL2VpnVsiVcNumber }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the number of VPLS VCs falls below the lower threshold."
            ::= { hwVplsMIBTraps 10 }


        hwVplsVcNumberMaxExceed NOTIFICATION-TYPE
            OBJECTS { hwL2VpnVcLimitClass, hwVplsVcNumberMaxNum }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the number of VPLS VCs reaches the maximum limit."
            ::= { hwVplsMIBTraps 11 }


        hwVplsVcNumberMaxClear NOTIFICATION-TYPE
            OBJECTS { hwL2VpnVcLimitClass, hwVplsVcNumberMaxNum }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the number of VPLS VCs is less than 95% of the maximum limit."
            ::= { hwVplsMIBTraps 12 }

        hwVplsPwRedundancyDegraded NOTIFICATION-TYPE
            OBJECTS { hwVplsVsiProtectGroupMode }
            STATUS current
            DESCRIPTION 
                "VPLS PW redundancy reported a protect degraded alarm."
            ::= { hwVplsMIBTraps 13 }
			
        hwVplsPwRedundancyDegradedClear NOTIFICATION-TYPE
            OBJECTS { hwVplsVsiProtectGroupMode }
            STATUS current
            DESCRIPTION 
                "VPLS PW redundancy reported the clearing of the protect degraded alarm."
            ::= { hwVplsMIBTraps 14 }

        hwVplsBLabelNotEnough NOTIFICATION-TYPE
            OBJECTS { hwVplsVsiName }
            STATUS current
            DESCRIPTION 
                "The block labels of VPLS are not enough."
            ::= { hwVplsMIBTraps 15 }
            
        hwVplsBLabelNotEnoughClear NOTIFICATION-TYPE
            OBJECTS { hwVplsVsiName }
            STATUS current
            DESCRIPTION 
                "The block labels of VPLS are enough."
            ::= { hwVplsMIBTraps 16 }            
                                            
--    Conformance information
-- 
        hwVplsMIBConformance OBJECT IDENTIFIER ::= { hwL2VpnVplsExt 3 }

        
        hwVplsMIBCompliances OBJECT IDENTIFIER ::= { hwVplsMIBConformance 1 }

        
--  this module
        hwVplsMIBCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION 
                "The compliance statement for systems supporting 
                the HUAWEI-VPLS-EXT-MIB."
            MODULE -- this module
                MANDATORY-GROUPS { hwVplsGroup, hwVplsRtGroup, hwVplsAcGroup, hwVplsBgpInfoGroup, hwVplsPwGroup, 
                    hwVplsStatisticsGroup, hwVplsNotificationControlGroup, hwVplsStateReasonGroup, hwVplsNotificationGroup, 
                    hwVplsLdpStatisticsGroup, hwVplsBgpStatisticsGroup, hwVplsLdpPeerGroup, hwVplsLdpQosStatisticGroup,
                    hwVplsStatisticGroup, hwVplsQosStatisticGroup,hwVplsTunnelInfoGroup
                     }
            ::= { hwVplsMIBCompliances 1 }

        
        hwVplsMIBGroups OBJECT IDENTIFIER ::= { hwVplsMIBConformance 2 }

        
        hwVplsGroup OBJECT-GROUP
            OBJECTS { hwVplsSignal, hwVplsRD, hwVplsVsiID, hwVplsVcType, hwVplsStatus, 
                hwVplsMtu, hwVplsTunnelPolicy, hwVplsDescription, hwVplsLearnStyle, hwVplsMacLearnEnable, 
                hwVplsMacLimitEnable, hwVplsStatisticsEnable, hwVplsUnknowMulticast, hwVplsUnknowUnicast, hwVplsPreference, 
                hwVplsVsiType, hwVplsAdminVsiName, hwVplsAcIsolateFlag, hwVplsDiffServMode, hwVplsDiffServServiceClass, 
                hwVplsDiffServColor, hwVplsDiffServDSName,hwVplsInterfaceWithdraw,hwVplsUpe2NpeWithdraw,hwVplsUpe2UpeWithdraw,
                hwVplsNpe2UpeWithdraw, hwVplsDiscovery, hwVplsMacWithdrawEnable, hwVplsVsiCir, hwVplsVsiPir, hwVplsVsiQosProfileName, 
                hwVplsAdminStatus, hwVplsIgnoreAcState, hwVplsEnableStatistic, hwVplsResetStatistic, hwVplsResetStatisticTime,hwVplsAgingTime, hwVplsUnknowUnicastMacLearning, hwVplsFlowLabel, 
                hwVplsServiceName, hwVplsRowStatus
                 }
            STATUS current
            DESCRIPTION 
                "The VPLS group."
            ::= { hwVplsMIBGroups 1 }

        
        hwVplsRtGroup OBJECT-GROUP
            OBJECTS { hwVplsRtRowStatus }
            STATUS current
            DESCRIPTION 
                "The VPLS's RT group."
            ::= { hwVplsMIBGroups 2 }

        
        hwVplsAcGroup OBJECT-GROUP
            OBJECTS { hwVplsAcStatus, hwVplsAcUpStartTime, hwVplsAcUpSumTime, hwVplsAcRowStatus }
            STATUS current
            DESCRIPTION 
                "The VPLS's AC group."
            ::= { hwVplsMIBGroups 3 }

        
        hwVplsBgpInfoGroup OBJECT-GROUP
            OBJECTS { hwVplsBgpInfoRange, hwVplsBgpInfoOffset, hwVplsBgpInfoRowStatus }
            STATUS current
            DESCRIPTION 
                "The VPLS's BGP information group."
            ::= { hwVplsMIBGroups 4 }

        
        hwVplsPwGroup OBJECT-GROUP
            OBJECTS { hwVplsPwTnlPolicy, hwVplsPwType, hwVplsPwIsUpe, hwVplsPwInboundLabel, hwVplsPwOutboundLabel, 
                hwVplsPwStatus, hwVplsPwVrIfIndex, hwVplsPwVrID, hwVplsPwUpStartTime, hwVplsPwUpSumTime, 
                hwVplsPwState, hwVplsPwWorkingState, hwVplsPwRowStatus }
            STATUS current
            DESCRIPTION 
                "The VPLS's PW group."
            ::= { hwVplsMIBGroups 5 }

        
        hwVplsStatisticsGroup OBJECT-GROUP
            OBJECTS { hwVplsOutFrames, hwVplsInFrames, hwVplsOutBytes, hwVplsInBytes, hwVplsInDiscardFrames
                 }
            STATUS current
            DESCRIPTION 
                "The VPLS's Statistic group."
            ::= { hwVplsMIBGroups 6 }

        
        hwVplsNotificationControlGroup OBJECT-GROUP
            OBJECTS { hwVplsUpDownNotifEnable }
            STATUS current
            DESCRIPTION 
                "The VPLS's Notification Control group."
            ::= { hwVplsMIBGroups 7 }

        
        hwVplsStateReasonGroup OBJECT-GROUP
            OBJECTS { hwVplsStateChangeReason }
            STATUS current
            DESCRIPTION 
                "The VPLS's VC and VSI State Change Reason group."
            ::= { hwVplsMIBGroups 8 }

        
        hwVplsNotificationGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwVplsVcDown, hwVplsVcUp, hwVplsVsiDown, hwVplsVsiUp, hwVplsVcBackup, hwVplsVsiDeleted, hwVplsVcDeleted, hwVplsVcStatusChange,
                 hwVplsVcNumberThresholdExceed, hwVplsVcNumberThresholdClear, hwVplsVcNumberMaxExceed, hwVplsVcNumberMaxClear, hwVplsPwRedundancyDegraded,
                 hwVplsPwRedundancyDegradedClear, hwVplsBLabelNotEnough, hwVplsBLabelNotEnoughClear }
            STATUS current
            DESCRIPTION 
                "The VPLS Notification group."
            ::= { hwVplsMIBGroups 9 }

        

        
        hwVplsLdpStatisticsGroup OBJECT-GROUP
            OBJECTS {hwVplsLdpStatEnable,hwVplsLdpStatInTrafficRate, hwVplsLdpStatOutTrafficRate, hwVplsLdpStatInFrameRate, hwVplsLdpStatOutFrameRate, hwVplsLdpStatInBytes, 
                hwVplsLdpStatOutBytes, hwVplsLdpStatInFrames, hwVplsLdpStatOutFrames, hwVplsLdpStatInUnicastFrames, hwVplsLdpStatOutUnicastFrames, 
                hwVplsLdpStatInMulticastFrames, hwVplsLdpStatOutMulticastFrames, hwVplsLdpStatInBroadcastFrames, hwVplsLdpStatOutBroadcastFrames, hwVplsLdpStatInDiscardFrames, 
                hwVplsLdpStatOutDiscardFrames, hwVplsLdpStatInErrorFrames, hwVplsLdpStatOutErrorFrames, hwVplsLdpStatInUnknowFrames, hwVplsLdpStatResetTime, hwVplsLdpStatResetStatistic
                 }
            STATUS current
            DESCRIPTION 
                "The VPLS Ldp's Statistic group."
            ::= { hwVplsMIBGroups 10 }

        
        hwVplsBgpStatisticsGroup OBJECT-GROUP
            OBJECTS {hwVplsBgpStatEnable,hwVplsBgpStatInTrafficRate, hwVplsBgpStatOutTrafficRate, hwVplsBgpStatInFrameRate, hwVplsBgpStatOutFrameRate, hwVplsBgpStatInBytes, 
                hwVplsBgpStatOutBytes, hwVplsBgpStatInFrames, hwVplsBgpStatOutFrames, hwVplsBgpStatInUnicastFrames, hwVplsBgpStatOutUnicastFrames, 
                hwVplsBgpStatInMulticastFrames, hwVplsBgpStatOutMulticastFrames, hwVplsBgpStatInBroadcastFrames, hwVplsBgpStatOutBroadcastFrames, hwVplsBgpStatInDiscardFrames, 
                hwVplsBgpStatOutDiscardFrames, hwVplsBgpStatInErrorFrames, hwVplsBgpStatOutErrorFrames, hwVplsBgpStatInUnknowFrames, hwVplsBgpStatResetTime
                 }
            STATUS current
            DESCRIPTION 
                "The VPLS Bgp's Statistic group."
            ::= { hwVplsMIBGroups 11 }


        hwVplsLdpPeerGroup OBJECT-GROUP
            OBJECTS { hwVplsLdpPeerTnlPolicyName, hwVplsLdpPeerUpeType, hwVplsLdpPeerTransLable, hwVplsLdpPeerRecvLable, hwVplsLdpPeerVrrpIfIndex, 
                hwVplsLdpPeerVirtualRouterId, hwVplsLdpPeerCir, hwVplsLdpPeerPir, hwVplsLdpPeerQosProfileName, hwVplsLdpPeerStatus, hwVplsLdpPeerPwName, 
                hwVplsLdpPeerIgnoreStpLoopCheck, hwVplsLdpPeerRowStatus
                }
            STATUS current
            DESCRIPTION 
                "The VPLS LDP's peer group."
            ::= { hwVplsMIBGroups 12 }


        hwVplsLdpQosStatisticGroup OBJECT-GROUP
            OBJECTS { hwVplsLdpQosStatTotalPassPacket, hwVplsLdpQosStatTotalPassByte, hwVplsLdpQosStatTotalDiscardPacket, hwVplsLdpQosStatTotalDiscardByte, 
                hwVplsLdpQosStatPassPacketRate, hwVplsLdpQosStatPassByteRate, hwVplsLdpQosStatDiscardPacketRate, hwVplsLdpQosStatDiscardByteRate
                 }
            STATUS current
            DESCRIPTION 
                "The VPLS's QoS statistic group."
            ::= { hwVplsMIBGroups 13 }


        hwVplsStatisticGroup OBJECT-GROUP
            OBJECTS { hwVplsStatEnable, hwVplsStatResetStatistic, hwVplsStatResetTime, hwVplsStatQosPacketRate, hwVplsStatQosByteRate, 
                hwVplsStatQosPacket, hwVplsStatQosByte
                 }
            STATUS current
            DESCRIPTION 
                "The VPLS's QoS statistic group."
            ::= { hwVplsMIBGroups 14 }


        hwVplsQosStatisticGroup OBJECT-GROUP
            OBJECTS { hwVplsQosStatTotalPassPacket, hwVplsQosStatTotalPassByte, hwVplsQosStatTotalDiscardPacket, hwVplsQosStatTotalDiscardByte, 
                hwVplsQosStatPassPacketRate, hwVplsQosStatPassByteRate, hwVplsQosStatDiscardPacketRate, hwVplsQosStatDiscardByteRate
                 }
            STATUS current
            DESCRIPTION 
                "The VPLS's QoS statistic group."
            ::= { hwVplsMIBGroups 15 }
        hwVplsTunnelInfoGroup OBJECT-GROUP
            OBJECTS { hwL2vpnTnlType, hwL2vpnTunnelIndex
                 }
            STATUS current
            DESCRIPTION 
                "The VPLS's tunnel information group."
            ::= { hwVplsMIBGroups 16 }

    END

--
-- HUAWEI-VPLS-EXT-MIB.mib
--