-- =====================================================================
-- Copyright (C) 2017 by  HUAWEI TECHNOLOGIES. All rights reserved.
--
-- Description: Huawei Configuration management MIB
-- Reference:   HUAWEI Enterprise MIB
-- Version:     V2.20
-- History:
--  2017-0405   V2.19  zhangquanquan modify HWPatchErrorType
--  2017-01-25  V2.18  xuxiangdong modify TrustStartup
--  2017-01-05  V2.17  Hanxian modify hwCodeSign for software code signature
--  2016-12-20  V2.16  Hanxian add hwCodeSign for software code signature
--  2016-09-08  V2.15  Zhangquanquan add hwTpmStaticMeasureAlarm for TrustStartup
--  2015-03-10  V2.14  Lin Bing Modified hwPatchFailReason for patch
--  2015-01-12  V2.13  chenruirui Add hwSysEvmTraps for evm
--  2014-09-15  V2.12  xuetao Modified hwSysRebootReason for cfm
--  2014-09-12  V2.11  xuetao Modified hwSysCfgFileName for cfm
--  2014-09-03  V2.10  Song Chuanheng Modified hwIssuState for issu
--  2014-07-28  V2.09  Zhang Bin Modified hwPatchErrorType for patch
--  2014-07-23  V2.08  Xu Yuming Modified hwPatchFailReason for patch
--  2014-07-08  V2.07  Wang Feng    Add hwSysWlanApUpgradeAssistantPackageNotMatchNotify for wlan ap upgrade  
--  2014-06-03  V2.06  Li Shanghong  Modified hwSystemBoardExlude/hwSystemBoardExludeClear to hwSystemBoardExclude/hwSystemBoardExcludeClear 
--  2014-05-22  V2.05  Zhang Xiudong  Add nodes for android upgrade
--                                    Add hwSysReloadAndroidFile to hwSysReloadScheduleEntry (1 OBJECT IDENTIFIER)
--                                    Add hwSysAndroidFile,hwSysAndroidFileNum,hwSysAndroidFileTable,hwSysAndroidFileEntry,hwSysAndroidFileIndex,hwSysAndroidFileName,hwSysAndroidFileSize,hwSysAndroidFileLocation,hwSysAndroidFileReason
--  2014-03-27  V2.04  Wang Feng    Add nodes for wlan ap upgrade
--                                  Add hwSysWlanApUpgrade to huaweiSystemManMIBObjects (1 OBJECT IDENTIFIER)
--                                  Add hwSysWlanApUpgradeCmd, hwSysWlanApUpgradeStatus, hwSysWlanApUpgradeNotifications to hwSysWlanApUpgrade (3 OBJECT IDENTIFIER)
--  2014-03-18  V2.03  Cheng Hailiang Add hwIssuPatchFile leaf into HwSysUpgradeEntry.
--  2014-03-17  V2.02  Liu WenJuan  Add two trap nodes hwSystemBoardExlude and hwSystemBoardExludeClear to huaweiSystemManMIBNotifications table.
--  2013-10-21  V2.01  Luo Dengwei  Add two trap nodes hwSysPafChangeNotification and hwSysLicenseChangeNotification to huaweiSystemManMIBNotifications table.
--  2011-09-23  v1.13   hujian           Added hwSysVoiceFileTable,hwSysVoiceFileNum,hwSysVoiceLicenseFile,hwSysCurVoiceFileIndex
--  2011-08-23  v1.12   niwei           Added hwSysSwitchoverStateMultiTable 
--  2011-04-26  V1.11   Zhang Yong      Modified syntax of hwSysReloadReason, changed from size (1..255) to size (0..255).
--  2005-04-21  V1.10   Zhang Xianping  Added traps for disk fault.
--  2003-05-28  V1.00   Yu Bo           Initial version for first baseline.
-- =====================================================================
HUAWEI-SYS-MAN-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        PhysicalIndex, entPhysicalIndex, entPhysicalName
            FROM ENTITY-MIB            
            EnabledStatus            
                FROM P-BRIDGE-MIB            
        OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP            
            FROM SNMPv2-CONF            
        Integer32, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE, IpAddress, Unsigned32            
            FROM SNMPv2-SMI            
        RowPointer, DateAndTime, DisplayString, RowStatus, TEXTUAL-CONVENTION            
            FROM SNMPv2-TC
        hwDatacomm            
            FROM HUAWEI-MIB
        SnmpAdminString
            FROM SNMP-FRAMEWORK-MIB;

    huaweiSystemManMIB MODULE-IDENTITY 
        LAST-UPDATED "201708170000Z"        -- August 17, 2017  GMT
        ORGANIZATION 
            "Huawei Technologies Co.,Ltd."
        CONTACT-INFO 
            "Huawei Industrial Base
              Bantian, Longgang
               Shenzhen 518129
               People's Republic of China
               Website: http://www.huawei.com
               Email: support@huawei.com
             "
        DESCRIPTION 
            "The HUAWEI-SYS-MAN-MIB contains objects to manage the system.
            The module defines the information about system, such as system
            time, the current configuration file and system image file, system
            reload actions, and notifications. By querying the system time,
            configuration files and system image files, NMS can reboot the device
            in the specified time and the specified configuration and system image."
	   REVISION
           "201708170000Z"
       DESCRIPTION 
           "modify description of hwSysDelayReboot,hwPatchErrorTrap,hwPatchUpdateTrap."
       REVISION
           "201704050000Z"
       DESCRIPTION 
           "modify HWPatchErrorType."
       REVISION
           "201701250000Z"
       DESCRIPTION 
           "modify TrustStartup."	    
       REVISION
           "201701250000Z"	   
       DESCRIPTION 
           "modify hwCodeSign for software code signature."	    
       REVISION
           "201612200000Z"
       DESCRIPTION 
           "add hwCodeSign for software code signature."			
       REVISION
           "201609080000Z"
       DESCRIPTION 
           "Add hwTpmStaticMeasureAlarm for TrustStartup."
       REVISION
           "201503100000Z"
       DESCRIPTION 
           "Modified hwPatchFailReason for patch." 
       REVISION
           "201501120000Z"
       DESCRIPTION 
           "Add hwSysEvmTraps for evm."      
       REVISION
           "201409150000Z"
       DESCRIPTION 
           "Modified hwSysRebootReason. Add new reboot reason."
       REVISION
           "201409120000Z"
       DESCRIPTION 
           "Modified hwSysCfgFileName description. hwSysCfgFileName is a string of 5 to 64 characters."
       REVISION
           "201409030000Z"
       DESCRIPTION 
           "Add two hwIssuState: issuRollBackByUserCancel, issuRollBackByExceptional to hwIssuState."
       REVISION
           "201407280000Z"
       DESCRIPTION 
           "Add one hwPatchErrorCode : patchMisoperation to hwPatchErrorType ."
       REVISION
           "201407230000Z"
       DESCRIPTION 
           "Modified hwPatchFailReason for patch." 
       REVISION
           "201407080000Z"
       DESCRIPTION 
           " Add hwSysWlanApUpgradeAssistantPackageNotMatchNotify for wlan ap upgrade." 
       REVISION
           "201406030000Z"
       DESCRIPTION 
           "Modified hwSystemBoardExlude/hwSystemBoardExludeClear to hwSystemBoardExclude/hwSystemBoardExcludeClear." 
      REVISION
           "201405220000Z"
       DESCRIPTION 
           "Add nodes for android upgrade."
       REVISION
           "201403270000Z"
       DESCRIPTION 
           "Add nodes for wlan ap upgrade."
       REVISION
           "201403180000Z"
       DESCRIPTION 
           "Add hwIssuPatchFile leaf into HwSysUpgradeEntry."
       REVISION
           "201403170000Z"
       DESCRIPTION 
           "Add two trap nodes hwSystemBoardExlude and hwSystemBoardExludeClear to huaweiSystemManMIBNotifications Table."
       REVISION
           "201310210000Z"
       DESCRIPTION 
           "Add two trap nodes hwSysPafChangeNotification and hwSysLicenseChangeNotification to huaweiSystemManMIBNotifications Table."

        ::= { hwDatacomm 19 }        

    --
    -- Node definitions
    --
        HWPatchErrorType ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                "           
                description.
                "
            SYNTAX INTEGER
                {
                initNoMemory(1),
                initMemProtectFail(2),
                fetchInputIsNull(5),
                fetchFlagNotSame(6),
                fetchProgVerInvalid(7),
                fetchProgCrcInvalid(8),
                fetchPatNoInvalid(9),
                fetchTotalNumInvalid(10),
                fetchUnitCrcInvalid(11),
                fetchFuncNumTooMany(12),
                fetchTypeInvalid(13),
                fetchCommonAfterTemp(14),
                fetchLengthNotSuited(15),
                fetchCodeAddrNotSuited(16),
                fetchDataAddrNotSuited(17),
                fetchBaseAddrNotSuited(18),
                fetchCodeLenOverflow(19),
                fetchDataLenOverflow(20),
                fetchOldAfterIndependent(103),
                fetchUpdateDependency(104),
                chgproChangeModeFailed(30),
                activeNumInvalid(40),
                activeHasBeenActived(41),
                activeNotExist(42),
                activeStateInvalid(43),
                activeCodeAddrNotSuited(44),
                activeDataAddrNotSuited(45),
                activeBaseAddrNotSuited(46),
                activeFormatUnknown(47),
                runNumInvalid(55),
                runHasInRunning(56),
                runNotActive(57),
                runIdleState(58),
                runBadState(59),
                deactNumInvalid(70),
                deactRunOrActive(71),
                deactRunningState(72),
                deactBadState(73),
                removeNumInvalid(80),
                removeHasInIdle(81),
                removeBadStatus(82),
                caclcrcFileCrcInvalid(90),
                caclcrcUnitCrcInvalid(91),
                caclcrcOutputIsNull(92),
                caclcrcNumInvalid(93),
                caclcrcBadUnitCrc(95),
                showNumInvalid(100),
                showCodeLenIsZero(101),
                showDataLenIsZero(102),
                addlistBadParam(105),
                addlistMemAllocFail(106),
                depToListBadParamDep(107),
                depToListBadParamList(108),
                depToListMemFreeFail(109),
                depToListAddItemFail(110),
                listToDepBadParamDep(111),
                listToDepBadParamList(112),
                listToDepBadParamDepCount(113),
                updateDepBadParam(114),
                updateDepMemAllocFail(115),
                updateDepDepToListFail(116),
                updateDepToInterFail(117),
                updateDepFromInterFail(118),
                updateDepListToDepFail(119),
                depToInterBadParam(120),
                depToInterInvalidNo(121),
                depToInterAddFail(122),
                interToDepBadParam(123),
                interToDepAppendFail(124),
                appendListBadParam(125),
                appendListAddFail(126),
                indActiveBadParam(127),
                indActiveAlreadyActive(128),
                indActiveListFail(129),
                indActiveListGenFail(130),
                indActiveListAppendFail(131),
                indActiveMemFreeFail(132),
                indActiveDepIdle(133),
                indActiveDepInvalid(134),
                indActiveCodeAddrNotSuited(135),
                indActiveDataAddrNotSuited(136),
                indActiveBaseAddrNotSuited(137),
                indActiveNotLoaded(138),
                indActiveFuncFail(139),
                indPatchFileNoInd(140),
                indRunFail(141),
                indDeactiveFail(142),
                indRemoveFail(143),
                indGetDepOfPara(144),
                indGetDepOnPara(145),
                indGetDepOnFail(146),
                fetchBufferPara(147),
                fetchBufferFail(148),
                getStatePara(149),
                indActiveAlreadyRunning(150),
                indFreeListInputNull(151),
                indFreeListMemFreeErr(152),
                indBitTblToArrayInputNull(153),
                indBitTblToArrayFreeFail(154),
                indBitTblToArrayAllocFail(155),
                indBitTblToArrayBitsetMore(156),
                indBitTblToArrayBitsetLess(157),
                listToDepBadParamAllocFail(158),
                listToDepBadParamFreeFail(159),
                indDeactiveFreeNull(160),
                indRemoveFreeFail(161),
                getInfoBufNull(162),
                getInfoOutputNull(163),
                getInfoFlagNotSame(164),
                getInfoProgCrcInvalid(165),
                getInfoFileCrcInvalid(166),
                getInfoUnitCrcInvalid(167),
                indPatchOpNotconfig(169),
                normalOpNotconfig(170),
                indDeactiveDeative(173),
                indDeactiveRunning(174),
                indDeactiveInvalid(176),
                indRunDeactive(177),
                indRunRunning(178),
                indRunIdle(179),
                indRunInvalid(180),
                indActiveIdle(171),
                indActiveInvalid(172),
                indFetchActive(183),
                indFetchRunning(185),
                indFetchDeactive(184),
                indFetchInvalid(186),
                indRemoveIdle(181),
                indRemoveInvalid(182),
                patchFileNotExist(187),
                patchRestoreFailed(188),
                patchPackageError(189),
                patchMisoperation(190),
                patchSystemUnstable(191),
                unknown(65535)
                }

    huaweiSystemManMIBObjects OBJECT IDENTIFIER ::= { huaweiSystemManMIB 1 }

    hwSysClock OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 1 }

    hwSysLocalClock OBJECT-TYPE
        SYNTAX DateAndTime
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the local time of the device."
        ::= { hwSysClock 1 }

    hwSysCurrent OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 2 }

    hwSysCurTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysCurEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The current status of system. A configuration file and an image 
            file are used to describe the current status."
        ::= { hwSysCurrent 1 }

    hwSysCurEntry OBJECT-TYPE
        SYNTAX HwSysCurEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry of hwSysCurTable. It is indexed by hwSysCurEntPhysicalIndex."
        INDEX { hwSysCurEntPhysicalIndex }
        ::= { hwSysCurTable 1 }

    HwSysCurEntry ::=
        SEQUENCE { 
            hwSysCurEntPhysicalIndex
                Integer32,
            hwSysCurCFGFileIndex
                Integer32,
            hwSysCurImageIndex
                Integer32,
            hwSysCurPafFileIndex
                Integer32,
            hwSysCurLicenseIndex
                Integer32,
            hwSysCurPatchFileIndex
                Integer32,
            hwSysCurVoiceFileIndex
                Integer32
         }

    hwSysCurEntPhysicalIndex OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object identifies the system index."
        ::= { hwSysCurEntry 1 }

    hwSysCurCFGFileIndex OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of the 
            configuration file in the configuration file list.
            The value is referenced from hwSysCFGFileTable.
            The value ranges from 1 to 2147483647.
            "
        ::= { hwSysCurEntry 2 }

    hwSysCurImageIndex OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies 
            the index of the image file in the image file list.
            The value is referenced from hwSysImageTable.
            The value ranges from 1 to 2147483647.
            "
        ::= { hwSysCurEntry 3 }
    
    hwSysCurPafFileIndex OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies 
            the index of the PAF file in the PAF file list.
            "
        ::= { hwSysCurEntry 4 }

    hwSysCurLicenseIndex OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies 
            the index of the license file in the license file list.
            "
        ::= { hwSysCurEntry 5 }

    hwSysCurPatchFileIndex OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies 
            the index of the patch file in the patch file list.
            "
        ::= { hwSysCurEntry 6 }

    hwSysCurVoiceFileIndex OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of the 
            configuration file in the configuration file list.
            The value is referenced from hwSysCFGFileTable.
            The value ranges from 1 to 2147483647.
            "
        ::= { hwSysCurEntry 7 }
        
    hwSysReload OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 3 }

    hwSysReloadSchedule OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "The value of this object identifies 
            the record number used when the device restarts.
            The value ranges from 0 to 2147483647.
            After the system restarts, the value returns to 0.
            0: initial value.
            65536: main board schedule method.
            "
        ::= { hwSysReload 1 }

    hwSysReloadAction OBJECT-TYPE
        SYNTAX INTEGER
            {
            reloadUnavailable(1),
            reloadOnSchedule(2),
            reloadAtOnce(3),
            reloadCancel(4)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The value of this object identifies restart types.
             1: reloadUnavailable
             2: reloadOnSchedule, indicating periodical restart
             3: reloadAtOnce, indicating immediate restart without considering hwSysReloadScheduleTime
             4: reloadCancel, indicating that all the planned restart activities are cancelled. If hwSysReloadSchedule 
                is invalid or the rows that hwSysReloadScheduleEntry and hwSysReloadSchedule point to are not activated, 
                all the restart activities are ignored and an inconsistent value is returned.
            When the restart of the system is complete or no restart activities exist, the value of this object is reloadUnavailable(1).
            "
        ::= { hwSysReload 2 }
    
    hwSysReloadScheduleTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysReloadScheduleEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A reload parameters table."
        ::= { hwSysReload 3 }

    hwSysReloadScheduleEntry OBJECT-TYPE
        SYNTAX HwSysReloadScheduleEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Entry of hwSysReloadScheduleTable."
        INDEX { hwSysReloadScheduleIndex }
        ::= { hwSysReloadScheduleTable 1 }

    HwSysReloadScheduleEntry ::=
        SEQUENCE { 
            hwSysReloadScheduleIndex
                Integer32,
            hwSysReloadEntity
                PhysicalIndex,
            hwSysReloadCfgFile
                Integer32,
            hwSysReloadImage
                Integer32,
            hwSysReloadReason
                DisplayString,
            hwSysReloadScheduleTime
                DateAndTime,
            hwSysReloadRowStatus
                RowStatus,
            hwSysReloadPafFile
                Integer32,
            hwSysReloadLicenseFile
                Integer32,
            hwSysReloadPatchFile
                Integer32,
            hwSysReloadPatchState
                INTEGER,
            hwSysReloadOperateDestType
                INTEGER,
            hwSysReloadOperateDestIndex
                DisplayString,
            hwSysReloadVoiceFile
                Integer32,
	    hwSysReloadAndroidFile
                Integer32
         }

    hwSysReloadScheduleIndex OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of the instance. 
            The value ranges from 0 to 2147483647."
        ::= { hwSysReloadScheduleEntry 1 }

    hwSysReloadEntity OBJECT-TYPE
        SYNTAX PhysicalIndex
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object indicates the index of the restarting entity.
            The value is referred to from entPhysicalTable.
            1. When get/get-next, 1 means active main board, 2 means slave main board,
               65535 means other board.
            2. When set, 2 means slave main board, other values mean active main board.
            "
        ::= { hwSysReloadScheduleEntry 2 }

    hwSysReloadCfgFile OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The value of this object identifies the configuration file used after the restart.
            The value is limited by hwSysCFGFileTable. 
            The value ranges from 0 to 2147483647.
            The default value is 0, which means the configuration file remains unchanged.
            "
        ::= { hwSysReloadScheduleEntry 3 }

    hwSysReloadImage OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The value of this object identifies the image file used after the restart.
            The value is limited by hwSysImageTable.
            The value ranges from 1 to 2147483647.
            "
        ::= { hwSysReloadScheduleEntry 4 }

    hwSysReloadReason OBJECT-TYPE
        SYNTAX DisplayString (SIZE (0..255))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object indicates the cause of the restart.
            The value is a string of 0 to 255 characters.
            After the system restarts, the character string is deleted.
            "
        ::= { hwSysReloadScheduleEntry 5 }

    hwSysReloadScheduleTime OBJECT-TYPE
        SYNTAX DateAndTime (SIZE(8))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object indicates the time of the restart.
            The only valid value of this object is an 8-byte string which indicates the local time of the switch.
            The maximum scheduled time is 30 days from the current system clock time. If the value set is earlier 
            than the value of hwSysLocalClock or beyond the maximum scheduled time limit, a bad value error occurred.
            The value of all-zero octet strings indicates system restart at once if the reload action is reloadOnSchedule(1).
            "
        ::= { hwSysReloadScheduleEntry 6 }

    hwSysReloadRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "If one of values of hwSysReloadEntity, hwSysReloadCfgFile and hwSysReloadImage is invalid, 
            the value of hwSysReloadRowStatus cannot be set to 'active'.
            A valid entry means the specified element is available in the current system. Reload an entity 
            indexed by hwSysReloadEntity with the startup configuration file and the image may be not allowed. Herein the entry is invalid.
            "
        ::= { hwSysReloadScheduleEntry 7 }

    hwSysReloadPafFile OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The value of this object identifies the PAF file used after the restart."
        ::= { hwSysReloadScheduleEntry 8 }

    hwSysReloadLicenseFile OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The value of this object identifies the license file used after the restart."
        ::= { hwSysReloadScheduleEntry 9 }

    hwSysReloadPatchFile OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The value of this object identifies the patch file used after the restart."
        ::= { hwSysReloadScheduleEntry 10 }

    hwSysReloadPatchState OBJECT-TYPE
        SYNTAX INTEGER
            {
            run(1),
            unused(255)
            }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The value of this object identifies the running status of the patch at the next startup. 
            That is, whether the loaded patch is in the Run state at the next startup.
            run(1): indicates that the loaded patch is in the Run state at the next startup.
            unused(255): indicates that the loaded patch is in the original state at the next startup.
            "
        ::= { hwSysReloadScheduleEntry 11 }

    hwSysReloadOperateDestType OBJECT-TYPE
        SYNTAX INTEGER
        {
        all(1),
        slave(2),
        chassis(3),
        unused(4)
        }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object indicates the object to be restarted."
        ::= { hwSysReloadScheduleEntry 12 }

    hwSysReloadOperateDestIndex OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object indicates the index of the board needs to be restarted.
             The get/get-next result is 'unused'. but, you can't use 'unused' 
             to set.
            "
        ::= { hwSysReloadScheduleEntry 13 }

    hwSysReloadVoiceFile OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The value of this object identifies the license file used after the restart."
        ::= { hwSysReloadScheduleEntry 14 }    

    hwSysReloadAndroidFile OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The value of this object identifies the android file used after the restart.
            The value is limited by hwSysAndroidFileTable. 
            The value ranges from 0 to 2147483647.
            The default value is 0, which means the android file remains unchanged.
            "
        ::= { hwSysReloadScheduleEntry 15 }

    hwSysReboot OBJECT-TYPE
        SYNTAX INTEGER
            {
            unused(1),
            rebootWholeRoute(2),
            rebootSlave(3),
            slaveSwitch(4)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The value of this object identifies the restart of the master and slave boards.
            Values are as follows
            unused(1): indicates that this value is not used. Generally, this value is read.
            rebootAllRoute(2): indicates that the integrated device is restarted.
            rebootSlave(3): indicates that the slave board is restarted.
            slaveSwitch(4): indicates that the switchover between the main and slave boards is performed.
            "
        ::= { hwSysReload 4 }

    hwSysSlaveSwitchEnable OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The value of this object identifies whether the switchover between the main and the slave boards is enabled.
            enable(1): indicates that the switchover between the main and slave boards is enabled.
            disable(2): indicates that the switchover between the main and slave boards is not enabled.
            "
        ::= { hwSysReload 5 }

    hwSysLatestRebootErrorInfo OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the cause of the last restart."
        ::= { hwSysReload 6 }
        
    hwSysSlaveSwitchTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysSlaveSwitchEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A slave switchover enable parameters table."
        ::= { hwSysReload 7 }
        
    hwSysSlaveSwitchEntry OBJECT-TYPE
        SYNTAX HwSysSlaveSwitchEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Entry of hwSysSlaveSwitchTable."
        INDEX { hwSysSlaveSwitchIndex }
        ::= { hwSysSlaveSwitchTable 1 }
        
    HwSysSlaveSwitchEntry ::=
        SEQUENCE {
            hwSysSlaveSwitchIndex
                Integer32,
            hwSysSlaveSwitchChassisNum
                DisplayString,
            hwSysSlaveSwitchOperType
                INTEGER,
            hwSysSlaveSwitchEnableStatus
                EnabledStatus,
            hwSysSlaveSwitchSrc
                DisplayString,
            hwSysSlaveSwitchDst
                DisplayString
         }
    
    hwSysSlaveSwitchIndex OBJECT-TYPE
        SYNTAX Integer32 (1..80)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of the object identifies the index of the table."
        ::= { hwSysSlaveSwitchEntry 1 }
        
    hwSysSlaveSwitchChassisNum OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The value of the object identifies the chassis number."
        ::= { hwSysSlaveSwitchEntry 2 }
    
    hwSysSlaveSwitchOperType OBJECT-TYPE
        SYNTAX INTEGER
        {
        unused(1),
        slaveSwitch(2),
        slaveSwitchLock(3)
        }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Operation type. The object has the following values:
            unused(1): means the default value.
            slaveswitch(2): perform force switchover.
            slaveswitchlock(3): enable the force switchover, 
            this value should be used with the object of hwSysSlaveSwitchEnableStatus.
            "
        ::= { hwSysSlaveSwitchEntry 3 }

    hwSysSlaveSwitchEnableStatus OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The enable status of switchover for AMB 
            (Active Main Board) and SMB (Standby Main Board).
            enable(1): enable the force switchover.
            disable(2): disable the force switchover.
            "
        ::= { hwSysSlaveSwitchEntry 4 }
    
    hwSysSlaveSwitchSrc OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The source slot for slave switchover."
        ::= { hwSysSlaveSwitchEntry 5 }
        
    hwSysSlaveSwitchDst OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The destination slot for slave switchover."
        ::= { hwSysSlaveSwitchEntry 6 }
    
    hwSysDelayReboot OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A delay after which the device is restarted. 
			Similar to the effect achieved when you set hwSysReboot to rebootAllRoute(2), this function delays device restart. 
			The value ranges from 0 to 43200, in minutes. If the value is 65535, delayed restart is cancelled. 
			loadCancel indicates that all the planned restart activities are cancelled.  
			If hwSysReloadSchedule is invalid, or the row where hwSysReloadScheduleEntry and hwSysReloadSchedule are directed are not activated, all the restart activities are ignored, and inconsistent values are returned. If the system restart is completed or no restart activity exists, the value of the object is reloadUnavailable (1). "
        ::= { hwSysReload 8 }

    hwSysImage OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 4 }

    hwSysImageNum OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of image files.
            The object calculates the number of image files given by hwSysImageTable.
            The value ranges from 0 to 2147483647.
            "
        ::= { hwSysImage 1 }

    hwSysImageTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysImageEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The system image management table."
        ::= { hwSysImage 2 }

    hwSysImageEntry OBJECT-TYPE
        SYNTAX HwSysImageEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A system image entry. Each entry consists of information of
            a system image.
            hwSysImageIndex exclusively decides an image file."
        INDEX { hwSysImageIndex }
        ::= { hwSysImageTable 1 }

    HwSysImageEntry ::=
        SEQUENCE { 
            hwSysImageIndex
                Integer32,
            hwSysImageName
                DisplayString,
            hwSysImageSize
                Integer32,
            hwSysImageLocation
                    DisplayString,
                hwSysImageVersion
                DisplayString,
            hwSysImageReason   
            DisplayString
        }

    hwSysImageIndex OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of the image file."
        ::= { hwSysImageEntry 1 }

    hwSysImageName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the name of the image file.
            A file name containing path and suffix is a string of 4 to 64 characters.
            "
        ::= { hwSysImageEntry 2 }

    hwSysImageSize OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the size of the image file.
            The value ranges from 0 to 2147483647, in bytes. The size depends 
            on the actual file and is limited by the physical storage device.
            "
        ::= { hwSysImageEntry 3 }

    hwSysImageLocation OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the location of the image file, namely the path.           
            "
        ::= { hwSysImageEntry 4 }
    
        hwSysImageVersion OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the version of the image file."
            ::= { hwSysImageEntry 5 }
    hwSysImageReason OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..255))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the error cause of the image file."            
            ::= { hwSysImageEntry 6 }
    hwSysCFGFile OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 5 }

    hwSysCFGFileNum OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of configuration files.
            The object calculates the number of configuration files given by hwSysCFGFileTable.
            The value ranges from 0 to 2147483647.
            "
        ::= { hwSysCFGFile 1 }

    hwSysCFGFileTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysCFGFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table of configuration files in this system."
        ::= { hwSysCFGFile 2 }

    hwSysCFGFileEntry OBJECT-TYPE
        SYNTAX HwSysCFGFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A configuration file entry. Each entry consists of information of
            a configuration file.
            hwSysCFGFileIndex exclusively decides a configuration file."
        INDEX { hwSysCFGFileIndex }
        ::= { hwSysCFGFileTable 1 }

    HwSysCFGFileEntry ::=
        SEQUENCE { 
            hwSysCFGFileIndex
                Integer32,
            hwSysCFGFileName
                DisplayString,
            hwSysCFGFileSize
                Integer32,
            hwSysCFGFileLocation
                DisplayString,
        hwSysCFGFileReason 
          DisplayString
         }

    hwSysCFGFileIndex OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of the configuration file."
        ::= { hwSysCFGFileEntry 1 }

    hwSysCFGFileName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the name of the configuration file.
            Currently, Huawei products support two formats of configuration files, namely, .CFG and .ZIP.
            A file name containing path and suffix is a string of 5 to 64 characters.
            "
        ::= { hwSysCFGFileEntry 2 }

    hwSysCFGFileSize OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the size of the configuration file.
            The value ranges from 0 to 2147483647.
            "
        ::= { hwSysCFGFileEntry 3 }

    hwSysCFGFileLocation OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the location of the configuration file, namely, the path."
        ::= { hwSysCFGFileEntry 4 }

    hwSysCFGFileReason OBJECT-TYPE
        SYNTAX DisplayString (SIZE (0..255))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the error cause of the configuration file." 
        ::= { hwSysCFGFileEntry 5 }
    hwSysPafFile OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 6 }

    hwSysPafFileNum OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of PAF files in the system."
        ::= { hwSysPafFile 1 }

    hwSysPafFileTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysPafFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table of paf files in this system."
        ::= { hwSysPafFile 2 }

    hwSysPafFileEntry OBJECT-TYPE
        SYNTAX HwSysPafFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A paf file entry. Each entry consists of information of
            a paf file.
            hwSysPafFileIndex  exclusively decides a configuration file."
        INDEX { hwSysPafFileIndex }
        ::= { hwSysPafFileTable 1 }

    HwSysPafFileEntry ::=
        SEQUENCE { 
            hwSysPafFileIndex
                Integer32,
            hwSysPafFileName
                DisplayString,
            hwSysPafFileSize
                Integer32,
            hwSysPafFileLocation
                DisplayString,
            hwSysPafFileVersion
                DisplayString
         }

    hwSysPafFileIndex OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of this table."
        ::= { hwSysPafFileEntry 1 }

    hwSysPafFileName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the name of the PAF file."
        ::= { hwSysPafFileEntry 2 }

    hwSysPafFileSize OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the size of the PAF file."
        ::= { hwSysPafFileEntry 3 }

    hwSysPafFileLocation OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the position of the PAF file."
        ::= { hwSysPafFileEntry 4 }

    hwSysPafFileVersion OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the version of the PAF file."
        ::= { hwSysPafFileEntry 5 }

    hwSysLicenseFile OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 7 }

    hwSysLicenseFileNum OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of license files in the system."
        ::= { hwSysLicenseFile 1 }

    hwSysLicenseFileTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysLicenseFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table of license files in this system."
        ::= { hwSysLicenseFile 2 }

    hwSysLicenseFileEntry OBJECT-TYPE
        SYNTAX HwSysLicenseFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A license file entry. Each entry consists of information of
            a license  file.
            hwSysLicenseFileIndex exclusively decides a configuration file."
        INDEX { hwSysLicenseFileIndex }
        ::= { hwSysLicenseFileTable 1 }

    HwSysLicenseFileEntry ::=
        SEQUENCE { 
            hwSysLicenseFileIndex
                Integer32,
            hwSysLicenseFileName
                DisplayString,
            hwSysLicenseFileSize
                Integer32,
            hwSysLicenseFileLocation
                DisplayString
         }

    hwSysLicenseFileIndex OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of this table."
        ::= { hwSysLicenseFileEntry 1 }

    hwSysLicenseFileName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the name of the license file."
        ::= { hwSysLicenseFileEntry 2 }

    hwSysLicenseFileSize OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the size of the license file."
        ::= { hwSysLicenseFileEntry 3 }

    hwSysLicenseFileLocation OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the position of the license file."
        ::= { hwSysLicenseFileEntry 4 }

    hwPatch OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 8 }

    hwPatchBase OBJECT IDENTIFIER ::= { hwPatch 1 }

    hwPatchFileNum OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of patches in the system."
        ::= { hwPatchBase 1 }

    hwPatchRecordReset OBJECT-TYPE
        SYNTAX INTEGER
            {
            unused(1),
            resetPatchHistory(2),
            resetPatchError(3)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Clear the patch records.
            unused(1): unused.
            resetPatchHistory(2): clears the hwPatchHistoryTable record.
            resetPatchError(3): clears the hwPatchErrorTable record."
        ::= { hwPatchBase 2 }

    hwPatchHistoryTableMax OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Set the size of hwPatchHistoryTable."
        ::= { hwPatchBase 3 }

    hwPatchTrapEnble OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The value of this object determines whether to generate the trap of HUAWEI-SYS-MAN-MIB.
            enable(1): Trap is enabled.
            disable(2): Trap is not enabled."
        ::= { hwPatchBase 4 }

    hwPatchErrorTableMax OBJECT-TYPE
        SYNTAX Integer32 (1..65535)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The value of this object identifies the maximum number of recorded errors supported by hwPatchErrorTable."
        ::= { hwPatchBase 5 }

    hwPatchId OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the patch ID on the device."
        ::= { hwPatchBase 6 }

    hwPatchLatestId OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the latest patch ID on the device."
        ::= { hwPatchBase 7 }

        
        hwPatchFailReason OBJECT-TYPE
            SYNTAX INTEGER
                {
                patchOpenErr(1),
                getPatchErr(2),
                patchSpaceShortage(3),
                patchConflict(4),
                versionErr(5),
                synchronizePatchPackageError(8),
                patchConfigInconsistError(9)
                }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This object is an index that specifies patch fail reason."
            ::= { hwPatchBase 8 }

    hwPatchFileTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwPatchFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Patch file query table."
        ::= { hwPatch 2 }

    hwPatchFileEntry OBJECT-TYPE
        SYNTAX HwPatchFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwPatchFileTable."
        INDEX { hwPatchFileIndex }
        ::= { hwPatchFileTable 1 }

    HwPatchFileEntry ::=
        SEQUENCE { 
            hwPatchFileIndex
                Unsigned32,
            hwPatchFileName
                DisplayString,
            hwPatchFileSize
                Integer32,
            hwPatchFileLocation
                DisplayString,
            hwPatchFileVersion
                DisplayString
         }

    hwPatchFileIndex OBJECT-TYPE
        SYNTAX Unsigned32 (1..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of this table."
        ::= { hwPatchFileEntry 1 }

    hwPatchFileName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the name of a patch file."
        ::= { hwPatchFileEntry 2 }

    hwPatchFileSize OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the size of a patch file."
        ::= { hwPatchFileEntry 3 }

    hwPatchFileLocation OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the position of a patch file."
        ::= { hwPatchFileEntry 4 }

    hwPatchFileVersion OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the version of the patch file."
        ::= { hwPatchFileEntry 5 }

    hwLoadPatchTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwLoadPatchEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The load table of the patch file.
            Load the patch file to the memory:
            hwSlotIndex:The slot ID of the destination device to be loaded by the patch file,
            hwPatchFileIndex:The index of the patch file,
            
            If hwSlotIndex is 128, it indicates all slots of the device."
        ::= { hwPatch 4 }

    hwLoadPatchEntry OBJECT-TYPE
        SYNTAX HwLoadPatchEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwLoadPatchTable."
        INDEX { hwPatchSlotIndex, hwPatchFileIndex }
        ::= { hwLoadPatchTable 1 }

    HwLoadPatchEntry ::=
        SEQUENCE { 
            hwPatchLoadDestType
                INTEGER,
            hwPatchLoadDestIndex
                DisplayString,
            hwPatchLoadState
                INTEGER, 
            hwLoadPatchRowState
                RowStatus
         }

    hwPatchLoadDestType OBJECT-TYPE
        SYNTAX INTEGER
            {
            all(1),
            slave(2),
            slot(3),
            chassis(4),
            unused(5)
            }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object indicates the type of the board to be loaded with the patch."
        ::= { hwLoadPatchEntry 1 }

    hwPatchLoadDestIndex OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object indicates the index of the board to be loaded with the patch."
        ::= { hwLoadPatchEntry 2 }
            
    hwPatchLoadState OBJECT-TYPE
            SYNTAX INTEGER
                {
                loading(1),
                success(2),
                failure(3),
                none(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Patch loading state:  
                loading(1):Patch is loading.
                success(2):Patch loading succeeded.
                failure(3):Patch loading failed.
                none(4):Patch and board do not match."
            ::= { hwLoadPatchEntry 3 }   
            
    hwLoadPatchRowState OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This object identifies the status of a row."
        ::= { hwLoadPatchEntry 51 }

    hwPatchInfo OBJECT IDENTIFIER ::= { hwPatch 5 }

    hwPatchTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwPatchEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Running status transfer and query of the patch.
            If hwSlotIndex is 128, it indicates all slots of the device.
            If hwPatchNum is 65535, it indicates all patches of the specified slot.
            If hwPatchNum is 0, it indicates the NP patch of the specified slot. 
            If hwPatchNum is in range from 1 to 200, it indicates the C patch of the specified slot.
            "
        ::= { hwPatchInfo 1 }

    hwPatchEntry OBJECT-TYPE
        SYNTAX HwPatchEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwPatchTable."
        INDEX { hwPatchSlotIndex, hwPatchIndex }
        ::= { hwPatchTable 1 }

    HwPatchEntry ::=
        SEQUENCE { 
            hwPatchSlotIndex
                Integer32,
            hwPatchIndex
                Unsigned32,
            hwPatchUsedFileName
                DisplayString,
            hwPatchVersion
                DisplayString,
            hwPatchDescription
                DisplayString,
            hwPatchProgramVersion
                DisplayString,
            hwPatchFuncNum
                Integer32,
            hwPatchTextLen
                Integer32,
            hwPatchDataLen
                Integer32,
            hwPatchType
                INTEGER,
            hwPatchBuildTime
                DateAndTime,
            hwPatchActiveTime
                DateAndTime,
            hwPatchAdminStatus
                INTEGER,
            hwPatchOperateState
                INTEGER,
            hwPatchOperateDestType
                INTEGER,
            hwPatchOperateDestIndex
                DisplayString
         }

    hwPatchSlotIndex OBJECT-TYPE
        SYNTAX Integer32 (0..255)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of the slot."
        ::= { hwPatchEntry 1 }

    hwPatchIndex OBJECT-TYPE
        SYNTAX Unsigned32 (0..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This object indicates the index of the patch."
        ::= { hwPatchEntry 2 }

    hwPatchUsedFileName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the name of the patch file."
        ::= { hwPatchEntry 3 }

    hwPatchVersion OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the version of the patch file."
        ::= { hwPatchEntry 4 }

    hwPatchDescription OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the description of the patch."
        ::= { hwPatchEntry 5 }

    hwPatchProgramVersion OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of the object identifies the version number of the host software."
        ::= { hwPatchEntry 6 }

    hwPatchFuncNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number functions contained in the patch."
        ::= { hwPatchEntry 7 }

    hwPatchTextLen OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the length of the patch code."
        ::= { hwPatchEntry 8 }

    hwPatchDataLen OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the length of the patch data."
        ::= { hwPatchEntry 9 }

    hwPatchType OBJECT-TYPE
        SYNTAX INTEGER
            {
            hotCommon(1),
            hotTemporary(2),
            coolCommon(3),
            coolTemporary(4)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the patch type.
            hotCommon(1): indicates the common hot patch.
            hotTemporary(2): indicates the temporary hot patch.
            coolCommon(3): indicates the common cool patch.
            coolTemporary(4): indicates the temporary cool patch."
        ::= { hwPatchEntry 10 }

    hwPatchBuildTime OBJECT-TYPE
        SYNTAX DateAndTime
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the time when a patch file is built."
        ::= { hwPatchEntry 11 }

    hwPatchActiveTime OBJECT-TYPE
        SYNTAX DateAndTime
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the time when a patch file is activated."
        ::= { hwPatchEntry 12 }

    hwPatchAdminStatus OBJECT-TYPE
        SYNTAX INTEGER
            {
            run(1),
            active(2),
            deactive(3),
            delete(4)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The value of this object identifies the operation status of a patch.
            Run (1): indicates that the patch status is Run.
            Active(2): indicates the patch status is Active.
            Deactive(3): indicates the patch status is Deactive.
            Delete(4): indicates that the patch is deleted."
        ::= { hwPatchEntry 13 }

    hwPatchOperateState OBJECT-TYPE
        SYNTAX INTEGER
            {
            patchRunning(1),
            patchActive(2),
            patchDeactive(3),
            patchDeleting(4)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "status of the patch.
            patchRunning(1): indicates that current status of the patch is Run.
            patchActive(2): indicates that current status of the patch is Active.
            patchDeactive(3): indicates that current status of the patch is Deactive."
        ::= { hwPatchEntry 14 }

    hwPatchOperateDestType OBJECT-TYPE
        SYNTAX INTEGER
            {
            all(1),
            slave(2),
            slot(3),
            chassis(4),
            unused(5)
            }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Patch operate object type,it combine with the hwPatchOperateDestIndex 
            to note the operate object."
        ::= { hwPatchEntry 15 }

    hwPatchOperateDestIndex OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Patch operate object index,it combine with chassis,the value of the hwPatchOperateDestType 
            to note the operate object.hwPatchOperateDestIndex is value such as ccc1,clc2 etc."
        ::= { hwPatchEntry 16 }

    hwPatchStateTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwPatchStateEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The statistics information of the patch area on each slot."
        ::= { hwPatchInfo 2 }

    hwPatchStateEntry OBJECT-TYPE
        SYNTAX HwPatchStateEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwPatchStateTable."
        INDEX { hwPatchSlotIndex }
        ::= { hwPatchStateTable 1 }

    HwPatchStateEntry ::=
        SEQUENCE { 
            hwPatchNumMax
                Unsigned32,
            hwPatchIdleNum
                Integer32,
            hwPatchTextMax
                Integer32,
            hwPatchDataMax
                Integer32,
            hwPatchStateTextUsed
                Integer32,
            hwPatchStateDataUsed
                Integer32,
            hwPatchStateTotalPatchNum
                Integer32,
            hwPatchStateTempPatchNum
                Integer32,
            hwPatchStateCommonPatchNum
                Integer32,
            hwPatchStateRuningPatchNum
                Integer32,
            hwPatchStateActivePatchNum
                Integer32,
            hwPatchStateDeactivePatchNum
                Integer32
         }

    hwPatchNumMax OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the maximum number of patches."
        ::= { hwPatchStateEntry 1 }

    hwPatchIdleNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of idle patches."
        ::= { hwPatchStateEntry 2 }

    hwPatchTextMax OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the size of the code in the patch area."
        ::= { hwPatchStateEntry 3 }

    hwPatchDataMax OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the size of the data in the patch area."
        ::= { hwPatchStateEntry 4 }

    hwPatchStateTextUsed OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the size of the used code in the patch area."
        ::= { hwPatchStateEntry 5 }

    hwPatchStateDataUsed OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the size of the used data in the patch area."
        ::= { hwPatchStateEntry 6 }

    hwPatchStateTotalPatchNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the total number of used patches."
        ::= { hwPatchStateEntry 7 }

    hwPatchStateTempPatchNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the total number of used temporary patches."
        ::= { hwPatchStateEntry 8 }

    hwPatchStateCommonPatchNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the total number of used common patches."
        ::= { hwPatchStateEntry 9 }

    hwPatchStateRuningPatchNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of patches in the Run state in the patch area."
        ::= { hwPatchStateEntry 10 }

    hwPatchStateActivePatchNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of patches in the Active state in the patch area."
        ::= { hwPatchStateEntry 11 }

    hwPatchStateDeactivePatchNum OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of patches in the Deactive state in the patch area."
        ::= { hwPatchStateEntry 12 }

    hwPatchHistoryTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwPatchHistoryEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Patch history table."
        ::= { hwPatchInfo 3 }

    hwPatchHistoryEntry OBJECT-TYPE
        SYNTAX HwPatchHistoryEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwPatchHistoryTable."
        INDEX { hwPatchHistoryIndex }
        ::= { hwPatchHistoryTable 1 }

    HwPatchHistoryEntry ::=
        SEQUENCE { 
            hwPatchHistoryIndex
                Unsigned32,
            hwPatchHistoryProgrameVersion
                DisplayString,
            hwPatchHistoryVersion
                DisplayString,
            hwSlotId
                Integer32,
            hwPatchBeginIndex
                Integer32,
            hwPatchEndIndex
                Integer32,
            hwPatchHistoryAction
                INTEGER,
            hwPatchHistoryBeginTime
                DateAndTime,
            hwPatchHistoryEndTime
                DateAndTime
         }

    hwPatchHistoryIndex OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This object indicates the index of the table."
        ::= { hwPatchHistoryEntry 1 }

    hwPatchHistoryProgrameVersion OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of the object identifies the version number of the image file."
        ::= { hwPatchHistoryEntry 2 }

    hwPatchHistoryVersion OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the version of the patch."
        ::= { hwPatchHistoryEntry 3 }

    hwSlotId OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of the object identifies the slot number of the patch."
        ::= { hwPatchHistoryEntry 4 }

    hwPatchBeginIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the start ID of the loaded patch."
        ::= { hwPatchHistoryEntry 5 }

    hwPatchEndIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the end ID of the loaded patch."
        ::= { hwPatchHistoryEntry 6 }

    hwPatchHistoryAction OBJECT-TYPE
        SYNTAX INTEGER
            {
            running(1),
            active(2),
            deactive(3),
            delete(4)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the patch status."
        ::= { hwPatchHistoryEntry 7 }

    hwPatchHistoryBeginTime OBJECT-TYPE
        SYNTAX DateAndTime
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the start time of running the patch."
        ::= { hwPatchHistoryEntry 8 }

    hwPatchHistoryEndTime OBJECT-TYPE
        SYNTAX DateAndTime
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the end time of running the patch."
        ::= { hwPatchHistoryEntry 9 }

    hwPatchErrorTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwPatchErrorEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The error record table of patch operation."
        ::= { hwPatchInfo 4 }

    hwPatchErrorEntry OBJECT-TYPE
        SYNTAX HwPatchErrorEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwPatchErrorTable."
        INDEX { hwPatchErrorIndex }
        ::= { hwPatchErrorTable 1 }

    HwPatchErrorEntry ::=
        SEQUENCE { 
            hwPatchErrorIndex
                Unsigned32,
            hwPatchErrorSlot
                Unsigned32,
            hwPatchErrorPatchFileName
                DisplayString,
            hwPatchErrorPatchIndex
                Unsigned32,
            hwPatchErrorCode
                HWPatchErrorType
         }

    hwPatchErrorIndex OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This object indicates the index of the patch error."
        ::= { hwPatchErrorEntry 1 }

    hwPatchErrorSlot OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the number of the slot related to a patch error."
        ::= { hwPatchErrorEntry 2 }

    hwPatchErrorPatchFileName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the index of the patch file when the patch has an error."
        ::= { hwPatchErrorEntry 3 }

    hwPatchErrorPatchIndex OBJECT-TYPE
        SYNTAX Unsigned32 (0..65535)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the index of the patch when the patch has an error."
        ::= { hwPatchErrorEntry 4 }

    hwPatchErrorCode OBJECT-TYPE
        SYNTAX HWPatchErrorType
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the flag of the patch error."
        ::= { hwPatchErrorEntry 5 }

    hwBootRom OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 11 }

    hwBootRomTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwBootRomEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Boot ROM startup parameter query table."
        ::= { hwBootRom 1 }

    hwBootRomEntry OBJECT-TYPE
        SYNTAX HwBootRomEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwBootRomTable."
        INDEX { hwBootRomIndex }
        ::= { hwBootRomTable 1 }

    HwBootRomEntry ::=
        SEQUENCE { 
            hwBootRomIndex
                INTEGER,
            hwBootRomBootDevice
                DisplayString,
            hwBootRomProcessorNo
                Integer32,
            hwBootRomHostName
                DisplayString,
            hwBootRomFileName
                DisplayString,
            hwBootRomIpOnEthernet
                IpAddress,
            hwBootRomIpOnBackPlane
                IpAddress,
            hwBootRomHostIp
                IpAddress,
            hwBootRomGatewayIp
                IpAddress,
            hwBootRomUserName
                DisplayString,
            hwBootRomPassword
                DisplayString,
            hwBootRomTargetName
                DisplayString,
            hwBootRomStartupScript
                DisplayString,
            hwBootRomXModemBaudRate
                Integer32,
              hwBootRomVersion
                Integer32
         }

    hwBootRomIndex OBJECT-TYPE
        SYNTAX INTEGER
            {
            master(1),
            slave(2)
            }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of the BootROM table.
            "
        ::= { hwBootRomEntry 1 }

    hwBootRomBootDevice OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the name of the BootROM startup device."
        ::= { hwBootRomEntry 2 }

    hwBootRomProcessorNo OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of the BootROM processor."
        ::= { hwBootRomEntry 3 }

    hwBootRomHostName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The object indicates the name of the BootROM host."
        ::= { hwBootRomEntry 4 }

    hwBootRomFileName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The object indicates the name of the BootROM file."
        ::= { hwBootRomEntry 5 }

    hwBootRomIpOnEthernet OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The object indicates the IP address of the BootROM Ethernet interface."
        ::= { hwBootRomEntry 6 }

    hwBootRomIpOnBackPlane OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The object indicates the IP address of the BootROM backplane."
        ::= { hwBootRomEntry 7 }

    hwBootRomHostIp OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The object indicates the IP address of the BootROM host."
        ::= { hwBootRomEntry 8 }

    hwBootRomGatewayIp OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The object indicates the IP address of the BootROM gateway."
        ::= { hwBootRomEntry 9 }

    hwBootRomUserName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The object indicates the name of the BootROM user."
        ::= { hwBootRomEntry 10 }

    hwBootRomPassword OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The object indicates the BootROM password."
        ::= { hwBootRomEntry 11 }

    hwBootRomTargetName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The object indicates the name of the BootROM target."
        ::= { hwBootRomEntry 12 }

    hwBootRomStartupScript OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The object indicates the BootROM startup script."
        ::= { hwBootRomEntry 13 }

    hwBootRomXModemBaudRate OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of the object identifies the baud rate for transmitting the XModem data."
        ::= { hwBootRomEntry 14 }

   hwBootRomVersion OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Boot ROM version."
        ::= { hwBootRomEntry 15 }

    hwSysUpgrade OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 12 }

    hwSysUpgradeTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysUpgradeEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "ISSU upgrade table."
        ::= { hwSysUpgrade 1 }

    hwSysUpgradeEntry OBJECT-TYPE
        SYNTAX HwSysUpgradeEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwSysUpgradeTable."
        INDEX { hwIssuIndex }
        ::= { hwSysUpgradeTable 1 }

    HwSysUpgradeEntry ::=
        SEQUENCE {
            hwIssuIndex
                Integer32, 
            hwIssuMode
                INTEGER,
            hwIssuImageFile
                DisplayString,
            hwIssuPafFile
                DisplayString,
            hwIssuLicenseFile
                DisplayString,
            hwIssuPatchFile
                DisplayString
         }

    hwIssuIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Set system issu table index."
        ::= { hwSysUpgradeEntry 1 }

    hwIssuMode OBJECT-TYPE
        SYNTAX INTEGER
        {
            issuUpgrade(1),
            issuPrecheck(2)
        }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Set system issu upgrade mode."
        ::= { hwSysUpgradeEntry 2 }

    hwIssuImageFile OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..127))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The name of the image file."
        ::= { hwSysUpgradeEntry 3 }

    hwIssuPafFile OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..127))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The name of the paf file."
        ::= { hwSysUpgradeEntry 4 }

    hwIssuLicenseFile OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..127))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The name of the license file."
        ::= { hwSysUpgradeEntry 5 }

    hwIssuPatchFile OBJECT-TYPE
        SYNTAX DisplayString (SIZE (5..127))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The name of the patch file."
        ::= { hwSysUpgradeEntry 6 }

    hwIssuState OBJECT-TYPE
        SYNTAX INTEGER
        {
            noIssuUpgrading(1),
            issuUpgrading(2),
            issuExceptional(3),
            issuRollBackByUserCancel(4),
            issuRollBackByExceptional(5)
        }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "System issu upgrade state."
        ::= { hwSysUpgrade 2 }

    hwIssuConditionCheck OBJECT-TYPE
        SYNTAX INTEGER
        {
            normal(1),
            notRealtimeBackup(2),
            slotAbnormal(3),
            configurationChange(4),
            otherAbnormal(5)        
        }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "System issu upgrade condition check.
             The default check result is normal."
        ::= { hwSysUpgrade 3 }             

    hwSysSourceIndex OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 13 }

    hwSysSourceIndexTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysSourceIndexEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "System file Index query table."
        ::= { hwSysSourceIndex 1 }

    hwSysSourceIndexEntry OBJECT-TYPE
        SYNTAX HwSysSourceIndexEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwBootRomTable."
        INDEX { hwSysFileType,hwSysFileName}
        ::= { hwSysSourceIndexTable 1 }

    HwSysSourceIndexEntry ::=
    SEQUENCE { 
        hwSysFileType
              INTEGER,
        hwSysFileName
              OCTET STRING,
         hwSysFileIndex
               Integer32
     }               

    hwSysFileType OBJECT-TYPE
        SYNTAX INTEGER
            {
            image(1),
            config(2),
            paf(3),
            license(4),
            patch(5)
            }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object is an index that indicates the type of a file."
        ::= { hwSysSourceIndexEntry 1 }      
        
    hwSysFileName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..110))
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This object is an index that indicates the name of a file on the main control board."
        ::= { hwSysSourceIndexEntry 2 }    

    hwSysFileIndex OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of a file in the specified table. 
            If the value is 0, it indicates that this file does not exist in the specified table."
        ::= { hwSysSourceIndexEntry 3 }     

    hwSysRebootInfo OBJECT IDENTIFIER     ::= { huaweiSystemManMIBObjects 14 }
    
    hwSysRebootTimes OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of the device reboot times.
            "
        ::= { hwSysRebootInfo 1 }
    
    hwSysRebootRecordTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysRebootRecordEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A reboot information record table."
        ::= { hwSysRebootInfo 2 }

    hwSysRebootRecordEntry OBJECT-TYPE
        SYNTAX HwSysRebootRecordEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Entry of hwSysReloadScheduleTable."
        INDEX { hwSysRebootRecordIndex }
        ::= { hwSysRebootRecordTable 1 }
    
    HwSysRebootRecordEntry ::=
        SEQUENCE { 
            hwSysRebootRecordIndex
                Integer32,
            hwSysRebootReason
                INTEGER,
            hwSysRebootTime
                DateAndTime
         }

    hwSysRebootRecordIndex OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The index of hwSysRebootRecordTable."
        ::= { hwSysRebootRecordEntry 1 }

    hwSysRebootReason OBJECT-TYPE
        SYNTAX INTEGER
            {
            manual(1),
            powerOff(2),
            unknown(3),
            schedule(4),
            software(5)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The reason of system's reboot."
        ::= { hwSysRebootRecordEntry 2 }

    hwSysRebootTime OBJECT-TYPE
        SYNTAX DateAndTime (SIZE (8))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The time at which the reboot action occurred.
            we will only take octet strings   
            with length 8 for this object which indicates the   
            local time of the switch. The maximum scheduled     
            time is 30 days from the current system clock time. 
            
                field  octets  contents                  range
                  1      1-2   year                      0..65536
                  2       3    month                     1..12
                  3       4    day                       1..31
                  4       5    hour                      0..23
                  5       6    minutes                   0..59
                  6       7    seconds                   0..60
                            (use 60 for leap-second)
                  7       8    deci-seconds              0..9
            "
        ::= { hwSysRebootRecordEntry 3 }

    hwSysDeviceCheck OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 15 }
     
    hwSysDeviceCheckStart OBJECT-TYPE
        SYNTAX INTEGER
        {
            checkStart(1)
        }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Set system check start."
        ::= { hwSysDeviceCheck 1 }

    hwSysDeviceCheckState OBJECT-TYPE
        SYNTAX INTEGER
        {
            done(1),
            checking(2)
        }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Get system check state."
        ::= { hwSysDeviceCheck 2 }

    hwSysSwitchoverState OBJECT IDENTIFIER  ::= { huaweiSystemManMIBObjects 19 }
    
    hwSysSwitchoverStateTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysSwitchoverStateEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Get switchover state of single-chassis"
        ::= { hwSysSwitchoverState 1 }
    
    hwSysSwitchoverStateEntry OBJECT-TYPE
        SYNTAX HwSysSwitchoverStateEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Entry of hwSysSwitchoverStateTable."
        INDEX { hwSysSwitchoverStateIndex }
        ::= { hwSysSwitchoverStateTable 1 }
    
    HwSysSwitchoverStateEntry ::=
        SEQUENCE { 
            hwSysSwitchoverStateIndex
                Integer32,
            hwSysSwitchoverSlotId
                Integer32,
            hwSysSwitchoverBoardType
                INTEGER,
            hwSysSwitchoverInfo
                OCTET STRING
             }
    
    hwSysSwitchoverStateIndex OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This object indicates the index of the table."
        ::= { hwSysSwitchoverStateEntry 1 }
    
    hwSysSwitchoverSlotId OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the slot number of the board."
        ::= { hwSysSwitchoverStateEntry 2 }
    
    hwSysSwitchoverBoardType OBJECT-TYPE
        SYNTAX INTEGER
            {
            master(1),
            slave(2),
            systemMaster(3),
            systemSlave(4),
            issuOldMaster(5),
            issuNewMaster(6)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the type of the board."
        ::= { hwSysSwitchoverStateEntry 3 }
    
    hwSysSwitchoverInfo OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..190))
        MAX-ACCESS read-only
            STATUS current
        DESCRIPTION
            "The value of this object descries the real-time information of HA status."
        ::= { hwSysSwitchoverStateEntry 4 }
           
           
           
           
           
    hwSysSwitchoverStateMultiTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysSwitchoverStateMultiEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Get switchover state of multi-chassis"
        ::= { hwSysSwitchoverState 2 }
    
    hwSysSwitchoverStateMultiEntry OBJECT-TYPE
        SYNTAX HwSysSwitchoverStateMultiEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Entry of hwSysSwitchoverStateMultiTable."
        INDEX { hwSysMultiSwtStateIndex }
        ::= { hwSysSwitchoverStateMultiTable 1 }
    
    HwSysSwitchoverStateMultiEntry ::=
        SEQUENCE { 
            hwSysMultiSwtStateIndex
                Integer32,
            hwSysMultiSwtChassisId
                OCTET STRING,
            hwSysMultiSwtSlotId
                Integer32,
            hwSysMultiSwtBoardType
                INTEGER,
            hwSysMultiSwtInfo
                OCTET STRING
             }
    
    hwSysMultiSwtStateIndex OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This object indicates the index of the table."
        ::= { hwSysSwitchoverStateMultiEntry 1 }
    
    hwSysMultiSwtChassisId OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..32))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the chassis id."
        ::= { hwSysSwitchoverStateMultiEntry 2 }
        
    hwSysMultiSwtSlotId OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the slot number of the board."
        ::= { hwSysSwitchoverStateMultiEntry 3 }
    
    hwSysMultiSwtBoardType OBJECT-TYPE
        SYNTAX INTEGER
            {
            master(1),
            slave(2),
            systemMaster(3),
            systemSlave(4),
            issuOldMaster(5),
            issuNewMaster(6)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the type of the board."
        ::= { hwSysSwitchoverStateMultiEntry 4 }
    
    hwSysMultiSwtInfo OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..190))
        MAX-ACCESS read-only
            STATUS current
        DESCRIPTION
            "The value of this object descries the real-time information of HA status."
        ::= { hwSysSwitchoverStateMultiEntry 5 }

    hwSysVoiceFile OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 20 }
        
    hwSysVoiceFileNum OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of configuration files.
            The object calculates the number of configuration files given by hwSysCFGFileTable.
            The value ranges from 0 to 2147483647.
            "
        ::= { hwSysVoiceFile 1 }
        
    hwSysVoiceFileTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysVoiceFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table of configuration files in this system."
        ::= { hwSysVoiceFile 2 }
        
    hwSysVoiceFileEntry OBJECT-TYPE
        SYNTAX HwSysVoiceFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A configuration file entry. Each entry consists of information of
            a configuration file.
            hwSysCFGFileIndex exclusively decides a configuration file."
        INDEX { hwSysVoiceFileIndex }
        ::= { hwSysVoiceFileTable 1 }
        
    HwSysVoiceFileEntry ::=
        SEQUENCE { 
            hwSysVoiceFileIndex
                Integer32,
            hwSysVoiceFileName
                DisplayString,
            hwSysVoiceFileSize
                Integer32,
            hwSysVoiceFileLocation
                DisplayString
            }

    hwSysVoiceFileIndex OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of the configuration file."
        ::= { hwSysVoiceFileEntry 1 }
        
    hwSysVoiceFileName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the name of the configuration file.
            Currently, Huawei products support two formats of configuration files, namely, .CFG and .ZIP.
            A file name containing path and suffix is a string of 4 to 64 characters.
            "
        ::= { hwSysVoiceFileEntry 2 }
        
    hwSysVoiceFileSize OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the size of the configuration file.
            The value ranges from 0 to 2147483647.
            "
        ::= { hwSysVoiceFileEntry 3 }
        
    hwSysVoiceFileLocation OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the location of the configuration file, namely, the path."
        ::= { hwSysVoiceFileEntry 4 }
		
    hwSysWlanApUpgrade OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 24 }

    hwSysWlanApUpgradeCmd OBJECT IDENTIFIER ::= { hwSysWlanApUpgrade 1 }

    hwSysWlanApUpgradeMode OBJECT-TYPE
        SYNTAX INTEGER
		{
		ftp(1),
		sftp(2),
		tftp(3)
		}
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The value of this object identifies the ap upgrade mode.
                The value ranges from 1 to 3."
	::= { hwSysWlanApUpgradeCmd 1 }

    hwSysWlanApUpgradeFileName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..127))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
		"The value of this object identifies the filename of the ap upgrade file.
                The value ranges from 1 to 127."
	::= { hwSysWlanApUpgradeCmd 2 }

    hwSysWlanApUpgradeServerIp OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "The value of this object identifies server ip address in ipv4 format."
        ::= { hwSysWlanApUpgradeCmd 3 }

    hwSysWlanApUpgradeServerUserName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (0..31))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
		"The value of this object identifies the username of server.
                The value ranges from 0 to 31."
        ::= { hwSysWlanApUpgradeCmd 4 }

    hwSysWlanApUpgradeServerPassword OBJECT-TYPE
	SYNTAX DisplayString (SIZE (0..63))
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The value of this object identifies the password of server.
                The value ranges from 0 to 63."
	::= { hwSysWlanApUpgradeCmd 5 }

    hwSysWlanApUpgradeStatus OBJECT IDENTIFIER ::= { hwSysWlanApUpgrade 2 }

    hwSysWlanApUpgradeProgressStatus OBJECT-TYPE
        SYNTAX INTEGER
		{
		updating(0),
		updateSuccessful(1),
		updateFailed(2),
		failToDownloadFile(4),
		efsAndVersionMismatched(5),
		invalidFileName(6),
		efsAndApTypeMismatched(7),
		fileContentError(8),
		writingMemoryError(9),
		noUpdateResult(10)
		}
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
		"The value of this object identifies the status of the upgrade or the last result of the upgrade.
                The value ranges from 0 to 10."
	::= { hwSysWlanApUpgradeStatus 1 }

    hwSysWlanApUpgradeLoadProgress OBJECT-TYPE
        SYNTAX Integer32 (0..100)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "The value of this object identifies the progress of file downloading.
                The value ranges from 0 to 100."
        ::= { hwSysWlanApUpgradeStatus 2 }

    hwSysWlanApUpgradeStorageProgress OBJECT-TYPE
        SYNTAX Integer32 (0..100)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "The value of this object identifies the progress of file storaging.
                The value ranges from 0 to 100."
        ::= { hwSysWlanApUpgradeStatus 3 }

    hwSysWlanApUpgradeNotifications OBJECT IDENTIFIER ::= { hwSysWlanApUpgrade 3 }

    hwSysWlanApUpgradeBeginNotify NOTIFICATION-TYPE
        STATUS current
        DESCRIPTION 
                "This notification occurs when ap begin to update."
        ::= { hwSysWlanApUpgradeNotifications 1 }

    hwSysWlanApUpgradeResultNotify NOTIFICATION-TYPE
        OBJECTS { hwSysWlanApUpgradeProgressStatus }
        STATUS current
        DESCRIPTION 
                "This notification occurs when ap has updated successfully or failed."
	::= { hwSysWlanApUpgradeNotifications 2 }

    hwSysWlanApUpgradeUbootNotMatchNotify NOTIFICATION-TYPE
        STATUS current
        DESCRIPTION 
                "This notification occurs when ap uboot not match version."
        ::= { hwSysWlanApUpgradeNotifications 3 }
        
    hwSysWlanApUpgradeAssistantPackageNotMatchNotify NOTIFICATION-TYPE
        STATUS current
        DESCRIPTION 
                "This notification occurs when ap upgrade-assistant-package not match version."
        ::= { hwSysWlanApUpgradeNotifications 4 }

    hwSysAndroidFile OBJECT IDENTIFIER ::= { huaweiSystemManMIBObjects 25 }

    hwSysAndroidFileNum OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the number of Android files.
            The object calculates the number of android files given by hwSysAndroidFileTable.
            The value ranges from 0 to 2147483647.
            "
        ::= { hwSysAndroidFile 1 }

    hwSysAndroidFileTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSysAndroidFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table of android files in this system."
        ::= { hwSysAndroidFile 2 }

    hwSysAndroidFileEntry OBJECT-TYPE
        SYNTAX HwSysAndroidFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A android file entry. Each entry consists of information of
            a android file.
            hwSysAndroidFileIndex exclusively decides a android file."
        INDEX { hwSysAndroidFileIndex }
        ::= { hwSysAndroidFileTable 1 }

    HwSysAndroidFileEntry ::=
        SEQUENCE { 
            hwSysAndroidFileIndex
                Integer32,
            hwSysAndroidFileName
                DisplayString,
            hwSysAndroidFileSize
                Integer32,
            hwSysAndroidFileLocation
                DisplayString,
            hwSysAndroidFileReason 
                DisplayString
         }

    hwSysAndroidFileIndex OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The value of this object identifies the index of the android file."
        ::= { hwSysAndroidFileEntry 1 }

    hwSysAndroidFileName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the name of the android file.
            Currently, Huawei products support one format of android files, namely, .BIN.
            A file name containing path and suffix is a string of 4 to 64 characters.
            "
        ::= { hwSysAndroidFileEntry 2 }

    hwSysAndroidFileSize OBJECT-TYPE
        SYNTAX Integer32 (0..2147483647)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this object identifies the size of the android file.
            The value ranges from 0 to 2147483647.
            "
        ::= { hwSysAndroidFileEntry 3 }

    hwSysAndroidFileLocation OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the location of the android file, namely, the path."
        ::= { hwSysAndroidFileEntry 4 }

    hwSysAndroidFileReason OBJECT-TYPE
        SYNTAX DisplayString (SIZE (0..255))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This object indicates the error cause of the android file." 
        ::= { hwSysAndroidFileEntry 5 }
    
    hwTrustStartup OBJECT IDENTIFIER  ::= { huaweiSystemManMIBObjects 26 }  
    
    hwTpmStatusTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwTpmStatusEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Tpm status query table."
        ::= { hwTrustStartup 1 }

    hwTpmStatusEntry OBJECT-TYPE
        SYNTAX HwTpmStatusEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwTpmStatusTable."
        INDEX { hwTpmPhysicalIndex }  
        ::= { hwTpmStatusTable 1 } 

    HwTpmStatusEntry ::=
        SEQUENCE {
            hwTpmPhysicalIndex
                PhysicalIndex,
            hwTpmPhysicalName
                SnmpAdminString,
            hwTpmVersion
                DisplayString,
            hwTpmManufacturer
                DisplayString,
            hwTpmStatus  
                INTEGER,
            hwSetTpmStatusRst
                INTEGER
         }
         
    hwTpmPhysicalIndex OBJECT-TYPE
        SYNTAX      PhysicalIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The index of the physical entity."
        ::= { hwTpmStatusEntry 1 }

    hwTpmPhysicalName OBJECT-TYPE
        SYNTAX      SnmpAdminString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The textual name of the physical entity."
        ::= { hwTpmStatusEntry 2 }         
    
    hwTpmVersion OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..50))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Tpm version of hwTpmStatusTable."
        ::= { hwTpmStatusEntry 3 }
    
    hwTpmManufacturer OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..50))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Tpm manufacturer of hwTpmStatusTable."
        ::= { hwTpmStatusEntry 4 }
        
    hwTpmStatus OBJECT-TYPE
        SYNTAX INTEGER
            {
            active(1),
            inactive(2),
            unknown(3)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Tpm status of hwTpmStatusTable, value can be active, inactive or unknown."
        ::= { hwTpmStatusEntry 5 }
        
    hwSetTpmStatusRst OBJECT-TYPE
        SYNTAX INTEGER
            {
            noSetting(1),
            success(2),
            failure(3),
            setting(4)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Set tpm status:
            noSetting(1): No setting tpm status. 
            success(2): Setting tpm status succeeded.
            failure(3): Setting tpm status failed.
            setting(4): Setting tpm status is processing."
        ::= { hwTpmStatusEntry 6 }   

    hwTrustStartupReportTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwTrustStartupReportEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Trust-startup report query table."
        ::= { hwTrustStartup 2 }

    hwTrustStartupReportEntry OBJECT-TYPE
        SYNTAX HwTrustStartupReportEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwTrustStartupReportTable."
        INDEX { hwTrustPhysicalIndex, hwTrustItemIndex}    
        ::= { hwTrustStartupReportTable 1 }  

    HwTrustStartupReportEntry ::=
        SEQUENCE {
            hwTrustPhysicalIndex
                PhysicalIndex,
            hwTrustItemIndex
                Integer32,
            hwTrustPhysicalName
                SnmpAdminString,
            hwTrustStartupReportItem
                DisplayString,
            hwTpmPcr
                DisplayString,
            hwTpmPcrBenchmark
                DisplayString,
            hwVerifyResult
                INTEGER
         }

    hwTrustPhysicalIndex OBJECT-TYPE
        SYNTAX      PhysicalIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The index of the physical entity."
        ::= { hwTrustStartupReportEntry 1 }
         
    hwTrustItemIndex OBJECT-TYPE
        SYNTAX Integer32 (1..2147483647)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This object indicates the index of the table."
        ::= { hwTrustStartupReportEntry 2 }
        
    hwTrustPhysicalName OBJECT-TYPE
        SYNTAX      SnmpAdminString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The textual name of the physical entity."
        ::= { hwTrustStartupReportEntry 3 } 
        
    hwTrustStartupReportItem OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..100))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Report item of hwTrustStartupReportTable."
        ::= { hwTrustStartupReportEntry 4 }
    
    hwTpmPcr OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..100))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Report tpm-pcr of hwTrustStartupReportTable."
        ::= { hwTrustStartupReportEntry 5 }
        
    hwTpmPcrBenchmark OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..100))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Tpm pcr benchmark of hwTrustStartupReportTable."
        ::= { hwTrustStartupReportEntry 6 } 

    hwVerifyResult OBJECT-TYPE
        SYNTAX INTEGER
            {
            ok(1),
            error(2),
            unknown(3),
            update(4),
            okAndUpdate(5),
            errorAndUpdate(6)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Verify result of hwTrustStartupReportTable, value can be ok, error, unknown,update,okAndUpdate or errorAndUpdate now."
        ::= { hwTrustStartupReportEntry 7 } 
		
	hwCodeSign OBJECT IDENTIFIER  ::= { huaweiSystemManMIBObjects 27 }
	
	hwSoftCrlInfoTable OBJECT-TYPE
	SYNTAX SEQUENCE OF HwSoftCrlInfoEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Software crl info query table."
	::= { hwCodeSign 1 }
	
    hwSoftCrlInfoEntry OBJECT-TYPE
        SYNTAX HwSoftCrlInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwSoftCrlInfoTable."
        INDEX { hwCrlInfoIndex }    
        ::= { hwSoftCrlInfoTable 1 } 	
    HwSoftCrlInfoEntry ::=
        SEQUENCE {
            hwCrlInfoIndex
                Integer32,
			hwCrlSlotId
				DisplayString,
            hwCrlPublisher
                DisplayString,
            hwCrlIssueDate
                DateAndTime,
            hwCrlStatus  
                INTEGER
         }

    hwCrlInfoIndex OBJECT-TYPE
        SYNTAX      Integer32 (1..64)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The value of this object identifies the index of this table."
        ::= { hwSoftCrlInfoEntry 1 } 
        
     hwCrlSlotId OBJECT-TYPE
        SYNTAX      DisplayString (SIZE (1..64))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The slot ID of board."
        ::= { hwSoftCrlInfoEntry 2 }    

	hwCrlPublisher OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..255))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Publisher of the CRL."
        ::= { hwSoftCrlInfoEntry 3 }
    
    hwCrlIssueDate OBJECT-TYPE
        SYNTAX DateAndTime
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The issue date of the CRL."
        ::= { hwSoftCrlInfoEntry 4 }
        
    hwCrlStatus OBJECT-TYPE
        SYNTAX INTEGER
            {
            invalid(0),
            valid(1)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The status of the CRL."
        ::= { hwSoftCrlInfoEntry 5 }

	hwSoftCrlFileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF HwSoftCrlFileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Software crl file query table."
	::= { hwCodeSign 2 }
	
    hwSoftCrlFileEntry OBJECT-TYPE
        SYNTAX HwSoftCrlFileEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwSoftCrlFileEntry."
        INDEX { hwCrlFileIndex }    
        ::= { hwSoftCrlFileTable 1 } 
		
    HwSoftCrlFileEntry ::=
        SEQUENCE {
            hwCrlFileIndex
                Integer32,
            hwCrlFileName
                DisplayString
         }

    hwCrlFileIndex OBJECT-TYPE
        SYNTAX      Integer32 (1..128)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The value of this object identifies the index of this table."
        ::= { hwSoftCrlFileEntry 1 }         
    
    hwCrlFileName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (5..63))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The name of crl files in MMB's home directory."
        ::= { hwSoftCrlFileEntry 2 }

	hwSoftCrlLoadTable OBJECT-TYPE
	SYNTAX SEQUENCE OF HwSoftCrlLoadEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Software crl load table."
	::= { hwCodeSign 3 }
	
    hwSoftCrlLoadEntry OBJECT-TYPE
        SYNTAX HwSoftCrlLoadEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Defines an entry in the hwSoftCrlLoadEntry."
        INDEX { hwCrlFileIndex }    
        ::= { hwSoftCrlLoadTable 1 } 
		
    HwSoftCrlLoadEntry ::=
        SEQUENCE {
            hwCrlLoadAction
                INTEGER,
			hwCrlLoadRst
				INTEGER
         }

    hwCrlLoadAction OBJECT-TYPE
        SYNTAX      INTEGER
		{
			load(1)
		}
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The action of loading software crl."
        ::= { hwSoftCrlLoadEntry 1 }
		
    hwCrlLoadRst OBJECT-TYPE
        SYNTAX      INTEGER
		{
			loadSuccess(0),
			fileNotExist(1),
			fileNotNew(2),
			publisherNotSame(3),
			nextStartupSoftwareCheckFailed(4),
			crlLoadFailed(5),
			crlFormatError(6),
			loading(7),
			crlNameInvalid(8)
		}
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The result of Loading software crl:
			loadSuccess(0): Succeeded in loading the CRL.
			fileNotExist(1): The file of CRL does not exist on the main control board.
			fileNotNew(2): The CRL file is not the latest.
			publisherNotSame(3): The publisher of the CRL file to be updated is inconsistent with that of the CRL file on the device.
			nextStartupSoftwareCheckFailed(4): The code signature verification of the next startup software package failed. Update the software package.
			crlLoadFailed(5): Loading the CRL failed.
			crlFormatError(6): The CRL format is error.
			loading(7): Loading.
			crlNameInvalid(8): The file name is invalid."
        ::= { hwSoftCrlLoadEntry 2 }		
        
--    ====================================
-- HUAWEI-SYS-MAN-MIB MIB - Notification Information
-- ====================================     
        
    huaweiSystemManMIBNotifications OBJECT IDENTIFIER ::= { huaweiSystemManMIB 2 }

    hwSysClockChangedNotification NOTIFICATION-TYPE
        OBJECTS { hwSysLocalClock }
        STATUS current
        DESCRIPTION 
            "This object indicates the notification sent when the system clock changes. 
            When the system clock changes, this trap is triggered. For example, 
            the system clock is changed through command lines.
            "
        ::= { huaweiSystemManMIBNotifications 1 }

    hwSysReloadNotification NOTIFICATION-TYPE
            OBJECTS { hwSysReloadImage, hwSysReloadCfgFile, hwSysReloadReason, hwSysReloadScheduleTime, hwSysReloadAction, 
                hwSysReloadPafFile, hwSysReloadLicenseFile, hwSysReloadPatchFile, hwSysReloadAndroidFile}
        STATUS current
        DESCRIPTION 
            "This object indicates the restart notification."
        ::= { huaweiSystemManMIBNotifications 2 }

    hwSysMasterHDError NOTIFICATION-TYPE
        STATUS current
        DESCRIPTION 
            "When the hard disk on master board cannot be read and written because of a certain error, 
            the hard disk on master board is unregistered and the notification is sent.
            "
        ::= { huaweiSystemManMIBNotifications 3 }
        
    hwSysSlaveHDError NOTIFICATION-TYPE
        STATUS current
        DESCRIPTION 
            "When the hard disk on slave board cannot be read and written because of a certain error, 
            the hard disk on slave board is unregistered and the notification is sent.
            "
        ::= { huaweiSystemManMIBNotifications 4 }

    hwPatchTrap OBJECT IDENTIFIER ::= { huaweiSystemManMIBNotifications 5 }

    hwPatchErrorTrap NOTIFICATION-TYPE
        OBJECTS { hwPatchErrorSlot, hwPatchErrorPatchIndex, hwPatchErrorCode, hwPatchErrorPatchFileName }
        STATUS current
        DESCRIPTION 
            "Notification about a patch operation failure. This trap is reported when patch installation or patch status configuration fails. 
			The trap contents include hwPatchErrorSlot, hwPatchErrorPatchIndex, hwPatchErrorCode, and hwPatchErrorPatchFileName."
        ::= { hwPatchTrap 1 }

    hwPatchActiveOverTimeTrap NOTIFICATION-TYPE
        OBJECTS { hwPatchOperateState }
        STATUS current
        DESCRIPTION 
            "The patch is not run within 24 hours after it is activated."
        ::= { hwPatchTrap 2 }

    hwPatchMalfunctionComebackTrap NOTIFICATION-TYPE
        OBJECTS { hwPatchOperateState }
        STATUS current
        DESCRIPTION 
            "The patch operation is restored."
        ::= { hwPatchTrap 3 }

    hwPatchUpdateTrap NOTIFICATION-TYPE
        OBJECTS { hwPatchVersion, hwPatchType, hwPatchOperateState}
        STATUS current
        DESCRIPTION 
            "Notification about a trap status change. This trap is reported when patch installation or patch status configuration succeeds."
        ::= { hwPatchTrap 4 }
        
    hwSysMasterCfcardError NOTIFICATION-TYPE
        STATUS current
        DESCRIPTION 
            "When the cfcard on master board can't be read and written because
            of some error, the Cfcard on master board will be unregistered and 
            the notification is sent.
            "
        ::= { huaweiSystemManMIBNotifications 6 }
        
    hwSysSlaveCfcardError NOTIFICATION-TYPE
        STATUS current
        DESCRIPTION 
            "When the cfcard on slave board can't be read and written because
            of some error, the Cfcard on slave board will be unregistered and 
            the notification is sent.
            "
        ::= { huaweiSystemManMIBNotifications 7 }

    hwSysSlaveSwitchSuccessNotification NOTIFICATION-TYPE
        OBJECTS { hwSysSlaveSwitchChassisNum, hwSysSlaveSwitchSrc, hwSysSlaveSwitchDst }
        STATUS current
        DESCRIPTION 
            "This object indicates that the hwSysSlaveSwitchChassisNum 
            chassis is successfully switched."
        ::= { huaweiSystemManMIBNotifications 8 }
        
    hwSysSlaveSwitchFailNotification NOTIFICATION-TYPE
        OBJECTS { hwSysSlaveSwitchChassisNum }
        STATUS current
        DESCRIPTION 
            "This object indicates that the hwSysSlaveSwitchChassisNum 
            chassis fails to be switched."
        ::= { huaweiSystemManMIBNotifications 9 }

    hwSysIssuNotification NOTIFICATION-TYPE
        OBJECTS { hwIssuState, hwIssuConditionCheck }
        STATUS current
        DESCRIPTION 
            "When the ISSU upgrade over, it will send success or failed message."
        ::= { huaweiSystemManMIBNotifications 10 }
        
    hwPatchInstallFail NOTIFICATION-TYPE
    OBJECTS { hwPatchUsedFileName, hwPatchVersion, hwPatchFailReason }
        STATUS current
        DESCRIPTION 
    "The patch package install fail notification."
        ::= { huaweiSystemManMIBNotifications 11 }
        
    hwPatchInstallFailClear NOTIFICATION-TYPE
    OBJECTS { hwPatchUsedFileName, hwPatchVersion, hwPatchFailReason }
        STATUS current
        DESCRIPTION 
    "The patch package install fail clear notification."
        ::= { huaweiSystemManMIBNotifications 12 }
        
    hwSumUpgradeSuccess NOTIFICATION-TYPE
        OBJECTS { hwSysImageVersion }
        STATUS current
        DESCRIPTION 
            "The patch package upgrade success notification"
        ::= { huaweiSystemManMIBNotifications 13 }     
        
    hwSysCfgFileErrorNotification NOTIFICATION-TYPE
        OBJECTS { hwSysCFGFileName,hwSysCFGFileReason}
        STATUS current
        DESCRIPTION 
            "This object notifies that some error occurs when the configuration file is specified as the next startup configuration file."
        ::= { huaweiSystemManMIBNotifications 14 }  
        
    hwSysImageErrorNotification NOTIFICATION-TYPE
        OBJECTS { hwSysImageName,hwSysImageName,hwSysImageReason }
        STATUS current
        DESCRIPTION 
            "The image file upgrade fail notification. The first hwSysImageName indicates the current image file,
            and the second hwSysImageName indicates the next startup image file."
        ::= { huaweiSystemManMIBNotifications 15 }   

    hwSysPafChangeNotification NOTIFICATION-TYPE
        OBJECTS { hwSysReloadEntity, hwSysPafFileName }
        STATUS current
        DESCRIPTION 
            "This object indicates the notification sent when the system PAF file changes.The hwSysPafFileName indicates system PAF file,
            and the hwSysReloadEntity indicates the board type(1 means main board,2 means slave main board)."
        ::= { huaweiSystemManMIBNotifications 16 }     
        
    hwSysLicenseChangeNotification  NOTIFICATION-TYPE
        OBJECTS { hwSysReloadEntity, hwSysLicenseFileName }
        STATUS current
        DESCRIPTION 
            "This object indicates the notification sent when the system license file changes.The hwSysLicenseFileName indicates the system license file,
            and the hwSysReloadEntity indicates the board type(1 means main board,2 means slave main board)."
        ::= { huaweiSystemManMIBNotifications 17 }  
 
    hwSystemBoardExclude NOTIFICATION-TYPE
        OBJECTS { entPhysicalIndex, entPhysicalName }
        STATUS current
        DESCRIPTION 
            "The board(s) excluded during software upgrading"
        ::= { huaweiSystemManMIBNotifications 18 }   
      
    hwSystemBoardExcludeClear NOTIFICATION-TYPE
        OBJECTS { entPhysicalIndex, entPhysicalName }
        STATUS current
        DESCRIPTION 
            "The board(s) excluded retrieved during software upgrading"
        ::= { huaweiSystemManMIBNotifications 19 }   
        
    hwSysEvmTraps OBJECT IDENTIFIER ::= { huaweiSystemManMIBNotifications 20 }

    hwSysEvmTrapsObject OBJECT IDENTIFIER ::= { hwSysEvmTraps 1 }

    hwSysEvmRoleName OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS accessible-for-notify
	STATUS current
	DESCRIPTION
		"The value of this object identifies the number of Android files.
		The object calculates the number of android files given by hwSysAndroidFileTable.
		The value ranges from 0 to 2147483647.
		"
	::= { hwSysEvmTrapsObject 1 }

    hwSysEvmDownloadFileName OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS accessible-for-notify
	STATUS current
	DESCRIPTION
		"The value of this object identifies the number of Android files.
		The object calculates the number of android files given by hwSysAndroidFileTable.
		The value ranges from 0 to 2147483647.
		"
	::= { hwSysEvmTrapsObject 2 }

    hwSysEvmInstallFileName OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS accessible-for-notify
	STATUS current
	DESCRIPTION
		"The value of this object identifies the number of Android files.
		The object calculates the number of android files given by hwSysAndroidFileTable.
		The value ranges from 0 to 2147483647.
		"
	::= { hwSysEvmTrapsObject 3 }

    hwSysEvmNotifications OBJECT IDENTIFIER ::= { hwSysEvmTraps 2 }
    hwEvmVmAbnormalRunNotification NOTIFICATION-TYPE
	OBJECTS { hwSysEvmRoleName }
	STATUS current
	DESCRIPTION 
		"The board(s) excluded retrieved during software upgrading"
	::= { hwSysEvmNotifications 1 }

    hwEvmVmNotRunningNotification NOTIFICATION-TYPE
	OBJECTS { hwSysEvmRoleName }
	STATUS current
	DESCRIPTION 
		"The board(s) excluded retrieved during software upgrading"
	::= { hwSysEvmNotifications 2 }


    hwEvmVmAbnormalRestartNotification NOTIFICATION-TYPE
	OBJECTS { hwSysEvmRoleName }
	STATUS current
	DESCRIPTION 
		"The board(s) excluded retrieved during software upgrading"
	::= { hwSysEvmNotifications 3 }


    hwEvmDownloadFailedNotification NOTIFICATION-TYPE
	OBJECTS { hwSysEvmDownloadFileName }
	STATUS current
	DESCRIPTION 
		"The board(s) excluded retrieved during software upgrading"
	::= { hwSysEvmNotifications 4 }


    hwEvmInstallFailedNotification NOTIFICATION-TYPE
	OBJECTS { hwSysEvmInstallFileName }
	STATUS current
	DESCRIPTION 
		"The board(s) excluded retrieved during software upgrading"
	::= { hwSysEvmNotifications 5 }

    hwTpmStaticMeasureAlarm NOTIFICATION-TYPE
    OBJECTS { hwTrustPhysicalName, hwTrustStartupReportItem}
    STATUS current
    DESCRIPTION 
        "Results of static integrity measurement mismatch during a boot"
    ::= { huaweiSystemManMIBNotifications 21 }

    hwTpmStaticMeasureAlarmClear NOTIFICATION-TYPE
    OBJECTS { hwTrustPhysicalName, hwTrustStartupReportItem}
    STATUS current
    DESCRIPTION 
        "Results of static integrity measurement resume matching during a boot"
    ::= { huaweiSystemManMIBNotifications 22 }
    
    huaweiSystemManMIBConformance OBJECT IDENTIFIER ::= { huaweiSystemManMIB 3 }

    huaweiSystemManMIBCompliances OBJECT IDENTIFIER ::= { huaweiSystemManMIBConformance 1 }

    huaweiSystemManMIBCompliance MODULE-COMPLIANCE
        STATUS current
        DESCRIPTION 
            "The compliance statement for entities which implement
            the Huawei system management MIB."
        MODULE -- this module
            MANDATORY-GROUPS { huaweiSysClockGroup, huaweiSysReloadGroup, huaweiSysImageGroup, huaweiSysCFGFileGroup, huaweiSystemManNotificationGroup
                 }
        ::= { huaweiSystemManMIBCompliances 1 }

    huaweiSystemManMIBGroups OBJECT IDENTIFIER ::= { huaweiSystemManMIBConformance 2 }

    huaweiSysClockGroup OBJECT-GROUP
        OBJECTS { hwSysLocalClock }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing mandatory system reload."
        ::= { huaweiSystemManMIBGroups 1 }

    huaweiSysReloadGroup OBJECT-GROUP
        OBJECTS { hwSysReloadSchedule, hwSysReloadAction, hwSysReloadImage, hwSysReloadCfgFile, hwSysReloadReason, 
            hwSysReloadPatchFile, hwSysReloadLicenseFile, hwSysReloadPafFile, hwSysReloadPatchState, hwSysLatestRebootErrorInfo, 
            hwSysReloadScheduleTime, hwSysReloadEntity, hwSysReloadRowStatus, hwSysReloadOperateDestType, hwSysReloadOperateDestIndex,
            hwSysSlaveSwitchChassisNum, hwSysSlaveSwitchOperType, hwSysSlaveSwitchEnableStatus,hwSysDelayReboot, hwSysReloadAndroidFile}
        STATUS current
        DESCRIPTION 
            " A collection of objects providing mandatory system clock
            information."
        ::= { huaweiSystemManMIBGroups 2 }

    huaweiSysImageGroup OBJECT-GROUP
        OBJECTS { hwSysImageNum, hwSysImageName, hwSysImageSize, hwSysImageLocation, hwSysImageVersion
             }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing mandatory system image
            information."
        ::= { huaweiSystemManMIBGroups 3 }

    huaweiSysCFGFileGroup OBJECT-GROUP
        OBJECTS { hwSysCFGFileNum, hwSysCFGFileName, hwSysCFGFileSize, hwSysCFGFileLocation }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing mandatory system configureation
            file information."
        ::= { huaweiSystemManMIBGroups 4 }

    hwSysCurGroup OBJECT-GROUP
        OBJECTS { hwSysCurCFGFileIndex, hwSysCurImageIndex, hwSysCurPafFileIndex, hwSysCurLicenseIndex, hwSysCurPatchFileIndex,
            hwSysCurVoiceFileIndex }
        STATUS current
        DESCRIPTION 
            "A collection of system current status."
        ::= { huaweiSystemManMIBGroups 5 }

    huaweiSystemManNotificationGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwSysClockChangedNotification, hwSysReloadNotification, hwSysSlaveSwitchSuccessNotification,
            hwSysSlaveSwitchFailNotification, hwSysIssuNotification, hwPatchInstallFail, hwPatchInstallFailClear, hwSumUpgradeSuccess, hwSysCfgFileErrorNotification, hwSysImageErrorNotification, hwSysPafChangeNotification, 
            hwSysLicenseChangeNotification, hwSystemBoardExclude, hwSystemBoardExcludeClear, hwEvmVmAbnormalRunNotification, hwEvmVmNotRunningNotification, hwEvmVmAbnormalRestartNotification, hwEvmDownloadFailedNotification, hwEvmInstallFailedNotification }
        STATUS current
        DESCRIPTION 
            "A collection of notification."
        ::= { huaweiSystemManMIBGroups 6 }

    huaweiSystemHDNotificationGroup NOTIFICATION-GROUP
        NOTIFICATIONS { hwSysMasterHDError, hwSysSlaveHDError }
        STATUS current
        DESCRIPTION 
            "A collection of notification about system hard disk."
        ::= { huaweiSystemManMIBGroups 7 }

    hwPatchLoadGroup OBJECT-GROUP
        OBJECTS { hwPatchLoadDestType, hwPatchLoadDestIndex, hwLoadPatchRowState }
        STATUS current
        DESCRIPTION 
            "Description."
        ::= { huaweiSystemManMIBGroups 8 }

    hwPatchTrapsGrop NOTIFICATION-GROUP
        NOTIFICATIONS { hwPatchErrorTrap, hwPatchActiveOverTimeTrap, hwPatchMalfunctionComebackTrap, hwPatchUpdateTrap }
        STATUS current
        DESCRIPTION 
            "Patch operation error."
        ::= { huaweiSystemManMIBGroups 9 }

    hwPatchInfoGroup OBJECT-GROUP
        OBJECTS { hwPatchDescription, hwPatchFuncNum, hwPatchTextLen, hwPatchDataLen, hwPatchType, 
            hwPatchAdminStatus, hwPatchStateTempPatchNum, hwPatchStateCommonPatchNum, hwPatchStateRuningPatchNum, hwPatchStateActivePatchNum, 
            hwPatchStateDeactivePatchNum, hwPatchHistoryVersion, hwPatchStateTotalPatchNum, hwPatchStateDataUsed, hwPatchStateTextUsed, 
            hwPatchDataMax, hwPatchTextMax, hwPatchIdleNum, hwPatchNumMax, hwPatchActiveTime, 
            hwPatchBuildTime, hwPatchVersion, hwPatchHistoryProgrameVersion, hwPatchFileName, hwPatchUsedFileName, 
            hwPatchErrorTableMax, hwPatchHistoryTableMax, hwPatchRecordReset, hwPatchProgramVersion, hwPatchOperateState, 
            hwPatchErrorSlot, hwPatchErrorPatchIndex, hwPatchErrorCode, hwPatchHistoryBeginTime, hwPatchHistoryEndTime, 
            hwPatchHistoryAction, hwPatchEndIndex, hwPatchTrapEnble, hwPatchBeginIndex, hwPatchId, 
            hwPatchLatestId, hwSlotId, hwPatchErrorPatchFileName, hwPatchFailReason }
        STATUS current
        DESCRIPTION 
            "Description."
        ::= { huaweiSystemManMIBGroups 10 }

    hwPatchFileGroup OBJECT-GROUP
        OBJECTS { hwPatchFileName, hwPatchFileSize, hwPatchFileLocation, hwPatchFileVersion, hwPatchFileNum
             }
        STATUS current
        DESCRIPTION 
            "Description."
        ::= { huaweiSystemManMIBGroups 11 }

    hwSysPafFileGroup OBJECT-GROUP
        OBJECTS { hwSysPafFileName, hwSysPafFileSize, hwSysPafFileLocation, hwSysPafFileVersion, hwSysPafFileNum
             }
        STATUS current
        DESCRIPTION 
            "Description."
        ::= { huaweiSystemManMIBGroups 13 }

    hwSysPafLicenseGroup OBJECT-GROUP
        OBJECTS { hwSysLicenseFileNum, hwSysLicenseFileName, hwSysLicenseFileSize, hwSysLicenseFileLocation }
        STATUS current
        DESCRIPTION 
            "Description."
        ::= { huaweiSystemManMIBGroups 14 }

    hwSysRebootAndSwitchGrop OBJECT-GROUP
        OBJECTS { hwSysReboot, hwSysSlaveSwitchEnable }
        STATUS current
        DESCRIPTION 
            "Description."
        ::= { huaweiSystemManMIBGroups 15 }

    hwBootRomGroup OBJECT-GROUP
        OBJECTS { hwBootRomBootDevice, hwBootRomHostName, hwBootRomFileName, hwBootRomIpOnEthernet, hwBootRomIpOnBackPlane, 
            hwBootRomHostIp, hwBootRomGatewayIp, hwBootRomUserName, hwBootRomPassword, hwBootRomTargetName, 
            hwBootRomStartupScript, hwBootRomXModemBaudRate, hwBootRomVersion, hwBootRomProcessorNo }
        STATUS current
        DESCRIPTION 
            "Description."
        ::= { huaweiSystemManMIBGroups 16 }

    hwSystemCfcardNotificationGroup NOTIFICATION-GROUP
        NOTIFICATIONS { hwSysMasterCfcardError, hwSysSlaveCfcardError }
        STATUS current                     
        DESCRIPTION                        
            "A collection of notification about system cfcard."
        ::= { huaweiSystemManMIBGroups 17 } 
        
    hwSysUpgradeGroup OBJECT-GROUP
        OBJECTS {hwIssuMode, hwIssuImageFile, hwIssuPafFile, hwIssuLicenseFile, hwIssuPatchFile, hwIssuState, hwIssuConditionCheck}
        STATUS current
        DESCRIPTION 
            "A collection of system upgrade."
        ::= { huaweiSystemManMIBGroups 18 }
    
    hwSysRebootInfoGroup OBJECT-GROUP
        OBJECTS { hwSysRebootTimes, hwSysRebootReason, hwSysRebootTime }
        STATUS current
        DESCRIPTION 
            "A collection of system upgrade."
        ::= { huaweiSystemManMIBGroups 19 }    

    hwSysDeviceCheckGroup OBJECT-GROUP
        OBJECTS {hwSysDeviceCheckStart, hwSysDeviceCheckState}
        STATUS current
        DESCRIPTION 
            "A collection of system device checks."
        ::= { huaweiSystemManMIBGroups 20 }
        
    huaweiSysVoiceFileGroup OBJECT-GROUP
        OBJECTS { hwSysVoiceFileNum, hwSysVoiceFileName, hwSysVoiceFileSize, hwSysVoiceFileLocation }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing mandatory system configureation
            file information."
        ::= { huaweiSystemManMIBGroups 21 }
		
    hwSysWlanApUpgradeCmdGroup OBJECT-GROUP
        OBJECTS { hwSysWlanApUpgradeMode, hwSysWlanApUpgradeFileName, hwSysWlanApUpgradeServerIp, hwSysWlanApUpgradeServerUserName, hwSysWlanApUpgradeServerPassword
		}
        STATUS current
        DESCRIPTION 
        	"A collection of system wlan ap upgrade."
        ::= { huaweiSystemManMIBGroups 22 }
		
    hwSysWlanApUpgradeStatusGroup OBJECT-GROUP
	OBJECTS { hwSysWlanApUpgradeProgressStatus, hwSysWlanApUpgradeLoadProgress, hwSysWlanApUpgradeStorageProgress }
	STATUS current
	DESCRIPTION 
		"A collection of system wlan ap upgrade status."
    	::= { huaweiSystemManMIBGroups 23 }
		
    hwSysWlanApUpgradeNotificationsGroup NOTIFICATION-GROUP
	NOTIFICATIONS { hwSysWlanApUpgradeBeginNotify, hwSysWlanApUpgradeResultNotify, hwSysWlanApUpgradeUbootNotMatchNotify, hwSysWlanApUpgradeAssistantPackageNotMatchNotify }
	STATUS current
	DESCRIPTION 
		"A collection of system wlan ap upgrade notifications."
	::= { huaweiSystemManMIBGroups 24 }
	
    huaweiSysAndroidFileGroup OBJECT-GROUP
        OBJECTS { hwSysAndroidFileNum, hwSysAndroidFileName, hwSysAndroidFileSize, hwSysAndroidFileLocation }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing mandatory system android
            file information."
        ::= { huaweiSystemManMIBGroups 25 }
    huaweihwSysEvmTrapsObjectGroup OBJECT-GROUP
        OBJECTS { hwSysEvmRoleName, hwSysEvmDownloadFileName, hwSysEvmInstallFileName }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing EVM system trap objects."
        ::= { huaweiSystemManMIBGroups 26 }
    END
