-- ============================================================================
-- Copyright (C) 2016 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- Description: The mib is used for station.
-- Reference: 
-- Version: V1.15
-- ============================================================================
-- Module definition

	HUAWEI-WLAN-STATION-MIB DEFINITIONS ::= BEGIN

		IMPORTS
			hwWlan
				FROM HUAWEI-WLAN-MIB
			hwWlanApName
		                FROM HUAWEI-WLAN-AP-MIB
		        hwWlanApMac
		                FROM HUAWEI-WLAN-AP-MIB
				hwWlanApId
						FROM HUAWEI-WLAN-AP-MIB
		        hwWlanRadioID
		                FROM HUAWEI-WLAN-AP-RADIO-MIB
			OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP
				FROM SNMPv2-CONF
			IpAddress, Integer32, Unsigned32, Counter64, OBJECT-TYPE,
			MODULE-IDENTITY, NOTIFICATION-TYPE
				FROM SNMPv2-SMI
			MacAddress, RowStatus, DateAndTime
				FROM SNMPv2-TC;
		--1.3.6.1.4.1.2011.6.139.18
		hwWlanStation MODULE-IDENTITY
			LAST-UPDATED "201612171030Z"		-- Dec 17, 2016 at 10:30 GMT
			ORGANIZATION 
				"Huawei Technologies Co.,Ltd."
			CONTACT-INFO 
                                  "Huawei Industrial Base
				   Bantian, Longgang
				   Shenzhen 518129
				   People's Republic of China
				   Website: http://www.huawei.com
				   Email: support@huawei.com
                                                                                        "
                        DESCRIPTION 
				"V1.15, Modify the description of hwWlanStaStatOperMode and hwWlanStaApId."
			REVISION "201612171030Z"		-- Dec 17, 2016 at 10:30 GMT
                        DESCRIPTION 
				"V1.14, Modify the description of hwWlanStaStatOperMode and hwWlanStaApId."
			REVISION "201609141030Z"		-- Sep 14, 2016 at 10:30 GMT

                                                                DESCRIPTION 
				"V1.13, Add the nodes ofhwWlanStaGetIPFailedCount and hwWlanStaGetIPSuccessCount."
			REVISION "201608161400Z"		-- Aug 16, 2016 at 14:00 GMT

                                                                DESCRIPTION 
				"V1.12, Modify the nodes of hwWlanStaAssocStartTime, hwWlanStaAssocSuccessTime and so on."
			REVISION "201608080915Z"		-- Aug 8, 2016 at 09:15 GMT
                
			DESCRIPTION 
				"V1.11, Add the node of hwWlanStaRoamTraceEntry  in the hwWlanStaRoamTraceInfo."
			REVISION "201607291130Z"		-- Jul 18, 2016 at 11:30 GMT
                                          			   
                                                                DESCRIPTION 
				"V1.10, Add the node of hwWlanStaAcL3RoamStatisticAcDescription  in the hwWlanStaAcL3RoamStatisticsTable."
			REVISION "201607181130Z"		-- Jul 18, 2016 at 11:30 GMT
                                                  
   
                                                                DESCRIPTION 
				"V1.09, Add the nodes of  hwWlanStaVHTCapable,hwWlanStaVHTTxBFCapable,hwWlanStaMUMIMOCapable, 
                                                                                  hwWlanStaWpaStartTime and hwWlanStaWpaSuccessTime in the hwWlanStationTable."
			REVISION "201606010930Z"		-- Jun 1, 2016 at 09:30 GMT

                                                     DESCRIPTION 
				"V1.08, Add the nodes of  hwWlanStaAssocStartTime,hwWlanStaAssocSuccesTime,hwWlanStaAuthStartTime, 
                                                                                  hwWlanStaAuthSuccesTime,hwWlanStaDhcpStartTime and hwWlanStaDhcpSuccesTime in the hwWlanStationTable."
			REVISION "201602260910Z"		-- Feb 26, 2016 at 09:10 GMT
     
			DESCRIPTION 
				"V1.07, Add the nodes of hwWlanStationApStatApId in the hwWlanStationApStatTable."
			REVISION "201602161110Z"		-- Feb 16, 2016 at 11:10 GMT
		    DESCRIPTION 
				"V1.06, Add the nodes of hwWlanStationUapsdCapacity and hwWlanStationPowerSavePercent in the hwWlanStationTable."
			REVISION "201511301110Z"		-- Nov 30, 2015 at 11:10 GMT
			DESCRIPTION 
				"V1.05, Add Value list in the hwWlanStaAuthenMethod node."
			REVISION "201511052030Z"		-- Oct 05, 2015 at 20:30 GMT 
			DESCRIPTION 
				"V1.04, Add AP ID in the trap node."
			REVISION "201509151030Z"		-- Sept 15, 2015 at 10:30 GMT 
			DESCRIPTION 
				"The MIB module defines the station operation."
				REVISION "201508271815Z"		-- Aug 27, 2015 at 18:15 GMT
			DESCRIPTION 
				"V1.02, Add the node of hwWlanStaApId in the hwWlanStationTable."
			REVISION "201506271815Z"		-- June 27, 2015 at 18:15 GMT
			DESCRIPTION 
				"V1.02, Modify the hwWlanStaEncryptMethod node."
			REVISION "201505111452Z"		-- May 11, 2015 at 14:52 GMT
			DESCRIPTION 
				"
				V1.01, Add the description of mib nodes.
				"
			REVISION "201502021452Z"		-- February 2, 2015 at 14:52 GMT
			DESCRIPTION 
				"
				V1.00, Inital version.
				"
			::= { hwWlan 18 }

--
--Node definitions
--

		--1.3.6.1.4.1.2011.6.139.18.1
		hwWlanStationObjects OBJECT IDENTIFIER ::= { hwWlanStation 1 }

		--1.3.6.1.4.1.2011.6.139.18.1.1
		hwWlanStaTraps OBJECT IDENTIFIER ::= { hwWlanStationObjects 1 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1
		hwWlanStaTrap OBJECT IDENTIFIER ::= { hwWlanStaTraps 1 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1.1
		hwWlanStaAuthErrorTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanApMac, hwWlanRadioID, hwWlanStaMac, hwWlanApName, hwWlanStaAssocBssid, hwWlanStaSsid, hwWlanStaAuthenticationMode, hwWlanStaFailCodeType, hwWlanStaAuthenticationFailCause, hwWlanStaAuthenticationFailCauseStr, hwWlanApId }
			STATUS current
			DESCRIPTION 
				"STA authentication fails."
			::= { hwWlanStaTrap 1 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1.2
		hwWlanStaAssoFailTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanApMac, hwWlanRadioID, hwWlanStaMac, hwWlanApName, hwWlanStaAssocBssid, hwWlanStaSsid, hwWlanStaFailCodeType, hwWlanStaAuthenticationFailCause, hwWlanStaAuthenticationFailCauseStr, hwWlanApId }
			STATUS current
			DESCRIPTION 
				"STA association fails."
			::= { hwWlanStaTrap 2 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1.3
		hwWlanUserInvalidCerficationTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanApMac, hwWlanRadioID, hwWlanStaMac, hwWlanApName, hwWlanStaAssocBssid, hwWlanStaSsid, hwWlanApId }
			STATUS current
			DESCRIPTION 
				"A user with an invalid certificate attempts to access the network."
			::= { hwWlanStaTrap 3 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1.4
		hwWlanStaRepititiveAttackTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanApMac, hwWlanRadioID, hwWlanStaMac, hwWlanApName, hwWlanStaAssocBssid, hwWlanStaSsid, hwWlanApId }
			STATUS current
			DESCRIPTION 
				"The STA undergoes a replay attack."
			::= { hwWlanStaTrap 4 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1.5
		hwWlanStaTamperAttackTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanApMac, hwWlanRadioID, hwWlanStaMac, hwWlanApName, hwWlanStaAssocBssid, hwWlanStaSsid, hwWlanApId }
			STATUS current
			DESCRIPTION 
				"A tamper attack occurs."
			::= { hwWlanStaTrap 5 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1.6
		hwWlanStaLowLevelSecAttackTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanApMac, hwWlanRadioID, hwWlanStaMac, hwWlanApName, hwWlanStaAssocBssid, hwWlanStaSsid, hwWlanApId }
			STATUS current
			DESCRIPTION 
				"The AP security level was lowered."
			::= { hwWlanStaTrap 6 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1.7
		hwWlanStaAddressRedirectionAttackTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanApMac, hwWlanRadioID, hwWlanStaMac, hwWlanApName, hwWlanStaAssocBssid, hwWlanStaSsid, hwWlanApId }
			STATUS current
			DESCRIPTION 
				"An address redirection attack occurs."
			::= { hwWlanStaTrap 7 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1.8
		hwWlanStaWepIdConflictTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanWepIDConflictTrapAPMAC, hwWlanWepIDConflictTrapAPName, hwWlanWepIDConflictTrapRadioId, hwWlanWepIDConflictTrapPreSSID, hwWlanWepIDConflictTrapCurrSSID, 
			hwWlanWepIDConflictTrapCipherIdx, hwWlanApId }
			STATUS current
			DESCRIPTION 
				"SSID keys conflict"
			::= { hwWlanStaTrap 8 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1.9
		hwStationOnlineTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanApMac, hwWlanStaMac, hwWlanStaRadioId, hwWlanApName, hwWlanStaAccessChannel, 
			hwWlanStaRssi, hwWlanStaTrapOccurTime, hwWlanApId }
			STATUS current
			DESCRIPTION 
				"A STA goes online."
			::= { hwWlanStaTrap 9 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1.10
		hwStationOfflineTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanApMac, hwWlanStaMac, hwWlanStaRadioId, hwWlanApName, hwWlanStaAccessChannel, 
			hwWlanStaRssi, hwWlanStaTrapOccurTime, hwWlanApId }
			STATUS current
			DESCRIPTION 
				"A STA goes offline."
			::= { hwWlanStaTrap 10 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.1.11
		hwStationSignalStrengthLowThanThresholdTrap NOTIFICATION-TYPE
			OBJECTS { hwWlanApMac, hwWlanStaMac, hwWlanStaRadioId, hwWlanApName, hwWlanStaAccessChannel, 
			hwWlanStaRssi, hwWlanSignalStrengthThreshold, hwWlanApId }
			STATUS current
			DESCRIPTION 
				"The STA signal strength is lower than the threshold."
			::= { hwWlanStaTrap 11 }

		--1.3.6.1.4.1.2011.6.139.18.1.1.2
		hwWlanStaTrapObjects OBJECT IDENTIFIER ::= { hwWlanStaTraps 2 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.1
		hwWlanStaAuthenticationMode OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the STA authentication mode."
			::= { hwWlanStaTrapObjects 1 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.2
		hwWlanStaAuthenticationFailCause OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the STA authentication failure reason."
			::= { hwWlanStaTrapObjects 2 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.3
		hwWlanStaAssociationFailCause OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the STA association failure reason."
			::= { hwWlanStaTrapObjects 3 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.4
		hwWlanStaAssocBssid OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the BSSID with which the STA associates."
			::= { hwWlanStaTrapObjects 4 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.5
		hwWlanStaFailCodeType OBJECT-TYPE
			SYNTAX INTEGER
			{
			    reasonCode(1),
			    statusCode(2)			
			}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the error codes for STA association and authentication failures."
			::= { hwWlanStaTrapObjects 5 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.6
		hwWlanWepIDConflictTrapAPMAC OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the AP MAC."
			::= { hwWlanStaTrapObjects 6 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.7
		hwWlanWepIDConflictTrapAPName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the AP name."
			::= { hwWlanStaTrapObjects 7 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.8
		hwWlanWepIDConflictTrapRadioId OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the radio id."
			::= { hwWlanStaTrapObjects 8 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.9
		hwWlanWepIDConflictTrapPreSSID OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the previous SSID."
			::= { hwWlanStaTrapObjects 9 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.10
		hwWlanWepIDConflictTrapCurrSSID OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the current SSID."
			::= { hwWlanStaTrapObjects 10 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.11
		hwWlanWepIDConflictTrapCipherIdx OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the cipher index."
			::= { hwWlanStaTrapObjects 11 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.12
		hwWlanWlanStaAuthEncryptMode OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the authentication and encryption modes for STAs."
			::= { hwWlanStaTrapObjects 12 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.13
		hwWlanWlanVapAuthEncryptMode OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the authentication and encryption modes for VAPs."
			::= { hwWlanStaTrapObjects 13 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.14
		hwWlanStaAuthenticationFailCauseStr OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the character string indicating the STA authentication failure reason."
			::= { hwWlanStaTrapObjects 14 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.15
		hwWlanStaAssociationFailCauseStr OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the character string indicating the STA association failure reason."
			::= { hwWlanStaTrapObjects 15 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.16
		hwWlanSignalStrengthThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"This object indicates the RSSI threshold."
			::= { hwWlanStaTrapObjects 16 }

		 --1.3.6.1.4.1.2011.6.139.18.1.1.2.17
		hwWlanStaTrapOccurTime OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the time when a STA alarm is generated."
			::= { hwWlanStaTrapObjects 17 }

		--1.3.6.1.4.1.2011.6.139.18.1.2
		hwWlanStationTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwWlanStationEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This table is used to describe access information about terminals."
			::= { hwWlanStationObjects 2 }

		--1.3.6.1.4.1.2011.6.139.18.1.2.1
		hwWlanStationEntry OBJECT-TYPE
			SYNTAX HwWlanStationEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"The index of this table is hwWlanStaMac."
			INDEX { hwWlanStaMac }
			::= { hwWlanStationTable 1 }


		HwWlanStationEntry ::=
			SEQUENCE {				
				hwWlanStaMac
					MacAddress,
				hwWlanStaUsername
					OCTET STRING,
				hwWlanStaApMac
					MacAddress,
				hwWlanStaApName
					OCTET STRING,
				hwWlanStaApGroup
					OCTET STRING,
				hwWlanStaRadioId
					Unsigned32,
				hwWlanStaAssocBand
					Unsigned32,
				hwWlanStaSupportBand
					Unsigned32,
				hwWlanStaAccessChannel
					Integer32,
				hwWlanStaRfMode
					INTEGER,
				hwWlanStaHtMode
					INTEGER,
				hwWlanStaMcsVal
					Unsigned32,
				hwWlanStaShortGIStatus
					INTEGER,
				hwWlanStaConnectRxRate
					Unsigned32,
				hwWlanStaConnectTxRate
					Unsigned32,
				hwWlanStaEssName
					OCTET STRING,
				hwWlanStaBSSID
					MacAddress,
				hwWlanStaSsid
					OCTET STRING,
				hwWlanStaStatus
					INTEGER,
				hwWlanStaAuthenMethod
					INTEGER,
				hwWlanStaEncryptMethod
					INTEGER,
				hwWlanStaQosMode
					INTEGER,
				hwWlanStaRoamStatus
					INTEGER,
				hwWlanStaVlan
					Unsigned32,
				hwWlanStaIP
					IpAddress,
				hwWlanStaIPv6
					OCTET STRING,
				hwWlanStaGateway
					IpAddress,
				hwWlanStaAssocTime
					Integer32,
				hwWlanStaAccessTime
					Integer32,
				hwWlanStaOnlineTime
					Integer32,
				hwWlanStaAccessOnlineTime
					Integer32,
				hwWlanStaStatOperMode
					INTEGER,
				hwWlanStaWirelessStatRxFrames
					Counter64,
				hwWlanStaWirelessRxBytes
					Counter64,
				hwWlanStaWirelessRxRate
					Unsigned32,
				hwWlanStaWirelessStatTxFrames
					Counter64,
				hwWlanStaWirelessTxBytes
					Counter64,
				hwWlanStaWirelessTxRate
					Unsigned32,
				hwWlanStaPeriodSendDropFrames
					Counter64,
				hwWlanStaPeriodReSendFrames
					Counter64,
				hwWlanStaPeriodReSendBytes
					Counter64,
				hwWlanStaRssi
					Integer32,
				hwWlanStaNoise
					Integer32,
				hwWlanStaSnrUs
					Integer32,
				hwWlanStaRxPowerUs
					Integer32,
				hwWlanStaChannelUtilRate
					Unsigned32,
				hwWlanStaChannelBusyRate
					Unsigned32,
				hwWlanStaChannelTxRatio
					Unsigned32,
				hwWlanStaChannelRxRatio
					Unsigned32,
				hwWlanStaChannelFreeRate
					Unsigned32,
				hwWlanStaChannelInterfRate
					Unsigned32,
				hwWlanStaPeriodSendFrames
					Unsigned32,
				hwWlanStaApId
					Unsigned32,
				hwWlanStationUapsdCapacity
					Integer32,
				hwWlanStationPowerSavePercent
					Integer32,
                hwWlanStaAssocStartTime
					Unsigned32,
				hwWlanStaAssocSuccessTime
					Unsigned32,
				hwWlanStaAuthStartTime
					Unsigned32,
				hwWlanStaAuthSuccessTime 
					Unsigned32,
				hwWlanStaDhcpStartTime
					Unsigned32,
				hwWlanStaDhcpSuccessTime
					Unsigned32,
				hwWlanStaVHTCapable
					INTEGER,
				hwWlanStaVHTTxBFCapable
					INTEGER,
				hwWlanStaMUMIMOCapable
					INTEGER,
				hwWlanStaWpaStartTime 
		        	Unsigned32,   
				hwWlanStaWpaSuccessTime 
					Unsigned32
			 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.1
		hwWlanStaMac OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION 
				"This object indicates the MAC address of a STA, which identifies the STA and functions as the index for querying information associated with the STA."
			::= { hwWlanStationEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.2
		hwWlanStaUsername OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the user name."
			::= { hwWlanStationEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.3
		hwWlanStaApMac OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the MAC address of the AP connected to users."
			::= { hwWlanStationEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.4
		hwWlanStaApName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the name of the AP connected to users."
			::= { hwWlanStationEntry 4 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.5
		hwWlanStaApGroup OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the AP group to which users belong."
			::= { hwWlanStationEntry 5 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.6
		hwWlanStaRadioId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the radio ID with which the STA associates."
			::= { hwWlanStationEntry 6 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.7
		hwWlanStaAssocBand OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the frequency band where users reside.	2.4G(1): 2.4G frequency band 5G(2): 5G frequency band."
			::= { hwWlanStationEntry 7 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.8
		hwWlanStaSupportBand OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the frequency band supported by STA, in bits. bit0: 2.4G.  bit1: 5G"
			::= { hwWlanStationEntry 8 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.9
		hwWlanStaAccessChannel OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the channel connected to users."
			::= { hwWlanStationEntry 9 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.10
		hwWlanStaRfMode OBJECT-TYPE
			SYNTAX INTEGER
				{
				dotb(1),
				dotg(2),
				dotn(3),
				dota(4),
				dotac(5)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the user radio mode."
			::= { hwWlanStationEntry 10 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.11
		hwWlanStaHtMode OBJECT-TYPE
			SYNTAX INTEGER
				{
				invalid(1) ,
				ht40(2) ,
				ht20(3) ,
				vht80(4)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the HT mode of STAs."
			::= { hwWlanStationEntry 11 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.12
		hwWlanStaMcsVal OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the MCS value."
			::= { hwWlanStationEntry 12 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.13
		hwWlanStaShortGIStatus OBJECT-TYPE
			SYNTAX INTEGER
				{
				nonsupport(1) ,
				support(2)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates whether the STA supports short GI."
			::= { hwWlanStationEntry 13 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.14
		hwWlanStaConnectRxRate OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the rate at which the AP receives user packets."
			::= { hwWlanStationEntry 14 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.15
		hwWlanStaConnectTxRate OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the rate at which the AP sends packets to users."
			::= { hwWlanStationEntry 15 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.16
		hwWlanStaEssName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the ESS associated with the STA."
			::= { hwWlanStationEntry 16 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.17
		hwWlanStaBSSID OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the air interface address for STA management."
			::= { hwWlanStationEntry 17 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.18
		hwWlanStaSsid OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the SSID assocaited with the STA."
			::= { hwWlanStationEntry 18 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.19
		hwWlanStaStatus OBJECT-TYPE
			SYNTAX INTEGER
				{
				age(1),
				associatedNotAuthenticated(2),
				associatedAndAuthenticated(3),
				roam(4),
				backup(5)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the user online status."
			::= { hwWlanStationEntry 19 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.20
		hwWlanStaAuthenMethod OBJECT-TYPE
			SYNTAX INTEGER
				{
				wepOpenSystem(1),
				wepOpenSystemMac(2),
				wepOpenSystem8021X(3),
				wepOpenSystemPortal(4),
				wepShareKey(5), 
				wepShareKeyMac(6),
				wepShareKey8021X(7),
				wepShareKeyPortal(8),
				wpa8021X(9),
				wpaPreShareKey(10),
				wpaPskMac(11),
				wpaPskPortal(12),
				wpa2Dot1x(13),
				wpa2PreShareKey(14),
				wpa2PskMac(15),
				wpa2PskPortal(16),  
				wapiCertification(17),
				wapiPreShareKey(18), 
				wpaWpa2PreShareKey(19),
				wpaWpa2PskMac(20),
				wpaWpa2PskPortal(21),
				wpaWpa2Dot1x(22),
				wapiPskPortal(23)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the user authentication method."
			::= { hwWlanStationEntry 20 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.21
		hwWlanStaEncryptMethod OBJECT-TYPE
			SYNTAX INTEGER
				{
				wpiSms4(1),
				wep40(2),
				wep104(3),
				tkip(4),
				aes(5),
				none(6)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the encryption method."
			::= { hwWlanStationEntry 21 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.22
		hwWlanStaQosMode OBJECT-TYPE
			SYNTAX INTEGER
				{
				wmm(1) ,
				null(2)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the QoS mode of the STA."
			::= { hwWlanStationEntry 22 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.23
		hwWlanStaRoamStatus OBJECT-TYPE
			SYNTAX INTEGER
				{
				no(1) ,
				yes(2)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the roaming status of the STA."
			::= { hwWlanStationEntry 23 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.24
		hwWlanStaVlan OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the VLAN connected to users."
			::= { hwWlanStationEntry 24 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.25
		hwWlanStaIP OBJECT-TYPE
			SYNTAX IpAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the connected user's IP address."
			::= { hwWlanStationEntry 25 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.26
		hwWlanStaIPv6 OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the IPv6 address of a user."
			::= { hwWlanStationEntry 26 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.27
		hwWlanStaGateway OBJECT-TYPE
			SYNTAX IpAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the user gateway."
			::= { hwWlanStationEntry 27 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.28
		hwWlanStaAssocTime OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the initial association time of a user."
			::= { hwWlanStationEntry 28 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.29
		hwWlanStaAccessTime OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the time when user authentication starts.If non-authentication is configured, the value of this object is equal to hwStaAssociateTime. If other authentication modes, especially, Portal authentication, are configured, the value of this object is larger than hwStaAssociateTime."
			::= { hwWlanStationEntry 29 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.30
		hwWlanStaOnlineTime OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the association time of the STA (online time), which is timed from the first association.The unit is second. 1:When the STA switches another AP, the online time is not cleared, and is accumulated. 2:	When the STA is disassociated from the AP, the STA data is cleared. New statistics of the STA will be collected when the STA goes online the next time."
			::= { hwWlanStationEntry 30 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.31
		hwWlanStaAccessOnlineTime OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the time elapsed since the user passes the authentication. This object applies only to Portal authentication users."
			::= { hwWlanStationEntry 31 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.32
		hwWlanStaStatOperMode OBJECT-TYPE
			SYNTAX INTEGER
				{
				invalid(1),
				clearstatistic(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"This object indicates that STA statistics are cleared."
			::= { hwWlanStationEntry 32 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.33
		hwWlanStaWirelessStatRxFrames OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of upstream frames received."
			::= { hwWlanStationEntry 33 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.34
		hwWlanStaWirelessRxBytes OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of upstream bytes received."
			::= { hwWlanStationEntry 34 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.35
		hwWlanStaWirelessRxRate OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the upstream Committed Information Rate (CIR), in bit/s."
			::= { hwWlanStationEntry 35 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.36
		hwWlanStaWirelessStatTxFrames OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of downstream frames received."
			::= { hwWlanStationEntry 36 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.37
		hwWlanStaWirelessTxBytes OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of downstream bytes received."
			::= { hwWlanStationEntry 37 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.38
		hwWlanStaWirelessTxRate OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the downstream Committed Information Rate (CIR), in bit/s."
			::= { hwWlanStationEntry 38 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.39
		hwWlanStaPeriodSendDropFrames OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of downstream packets (frames) discarded at the wireless side within the echo interval."
			::= { hwWlanStationEntry 39 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.40
		hwWlanStaPeriodReSendFrames OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of downstream packets (frames) retransmitted at the wireless side within the echo interval."
			::= { hwWlanStationEntry 40 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.41
		hwWlanStaPeriodReSendBytes OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of downstream bytes retransmitted at the wireless side within the echo interval."
			::= { hwWlanStationEntry 41 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.42
		hwWlanStaRssi OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the received signal strength indicator (RSSI) of a STA."
			::= { hwWlanStationEntry 42 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.43
		hwWlanStaNoise OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the noise from a connected STA."
			::= { hwWlanStationEntry 43 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.44
		hwWlanStaSnrUs OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the upstream SNR of the STA (AP measured), in 0.1 dB. Special value 0x7FFFFFFF indicates that the value exceeds the threshold and 0x7FFFFFFE indicates that the value cannot be obtained at present."
			::= { hwWlanStationEntry 44 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.45
		hwWlanStaRxPowerUs OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the upstream input power of the STA. The value is measured by the AP, in 0.1 dB. Special value 0x7FFFFFFF indicates that the value exceeds the threshold and 0x7FFFFFFE indicates that the value cannot be obtained at present."
			::= { hwWlanStationEntry 45 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.46
		hwWlanStaChannelUtilRate OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the channel usage of the STA."
			::= { hwWlanStationEntry 46 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.47
		hwWlanStaChannelBusyRate OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the busy rate of the STA channel."
			::= { hwWlanStationEntry 47 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.48
		hwWlanStaChannelTxRatio OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the packet sending ratio of the STA channel."
			::= { hwWlanStationEntry 48 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.49
		hwWlanStaChannelRxRatio OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the packet receiving ratio of the STA channel."
			::= { hwWlanStationEntry 49 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.50
		hwWlanStaChannelFreeRate OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the idle rate of the STA channel."
			::= { hwWlanStationEntry 50 }

		 --1.3.6.1.4.1.2011.6.139.18.1.2.1.51
		hwWlanStaChannelInterfRate OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the interference ratio of the STA channel."
			::= { hwWlanStationEntry 51 }

		
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.52
		hwWlanStaPeriodSendFrames OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the number of downstream frames received within the echo interval."
			::= { hwWlanStationEntry 52 }

		
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.53
		hwWlanStaApId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the AP ID with which the STA associates."
			::= { hwWlanStationEntry 53 }
		
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.54
		hwWlanStationUapsdCapacity OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the uapsd capacity of a STA."
			DEFVAL { '0'b }
			::= { hwWlanStationEntry 54 }
		
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.55
		hwWlanStationPowerSavePercent OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the power save percent of a STA."
			DEFVAL { '0'b }
			::= { hwWlanStationEntry 55 }

                                   
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.56
		hwWlanStaAssocStartTime OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the association start time of the station."
			::= { hwWlanStationEntry 56 }
		
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.57
		hwWlanStaAssocSuccessTime OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the association success time of the station."
			::= { hwWlanStationEntry 57 }
		
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.58
		hwWlanStaAuthStartTime OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the auth start time of the station."
			::= { hwWlanStationEntry 58 }

        -- 1.3.6.1.4.1.2011.6.139.18.1.2.1.59
		hwWlanStaAuthSuccessTime  OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the auth success time of the station."
			::= { hwWlanStationEntry 59 }
		
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.60
		hwWlanStaDhcpStartTime OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the dhcp start time of the station."
			::= { hwWlanStationEntry 60 }
		
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.61
		hwWlanStaDhcpSuccessTime  OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the dhcp success time of the station."
			::= { hwWlanStationEntry 61 }
		
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.62
		hwWlanStaVHTCapable OBJECT-TYPE
			SYNTAX INTEGER
				{
				nonsupport(1),
				support(2)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the capability of VHT."
			::= { hwWlanStationEntry 62 }

		
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.63
		hwWlanStaVHTTxBFCapable OBJECT-TYPE
			SYNTAX INTEGER
				{
				nonsupport(1),
				support(2)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the capability of VHTTxBF."
			::= { hwWlanStationEntry 63 }

		
		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.64
		hwWlanStaMUMIMOCapable OBJECT-TYPE
			SYNTAX INTEGER
				{
				nonsupport(1),
				support(2)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the capability of MUMIMO."
			::= { hwWlanStationEntry 64 }

		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.65
		hwWlanStaWpaStartTime  OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the wpa start time of the station."
			::= { hwWlanStationEntry 65 }

		-- 1.3.6.1.4.1.2011.6.139.18.1.2.1.66
		hwWlanStaWpaSuccessTime  OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the wpa success time of the station."
                                                    ::= { hwWlanStationEntry 66 }


		-- 1.3.6.1.4.1.2011.6.139.18.1.3
		hwWlanStationApStatTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwWlanStationApStatEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This table is used to describe the terminal access information on APs."
			::= { hwWlanStationObjects 3 }

		--1.3.6.1.4.1.2011.6.139.18.1.3.1
		hwWlanStationApStatEntry OBJECT-TYPE
			SYNTAX HwWlanStationApStatEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"The index of this table is hwWlanApAssocStatApMac."
			INDEX { hwWlanApAssocStatApMac }
			::= { hwWlanStationApStatTable 1 }


		HwWlanStationApStatEntry ::=
			SEQUENCE {				
				hwWlanApAssocStatApMac
					MacAddress,
				hwWlanTotalOnlineTime
					Unsigned32,
				hwWlanTotalAssociatedStationCount
					Unsigned32,
				hwWlanCurrAssociatedStationCount
					Unsigned32,
				hwWlanAssociationRequestCount
					Unsigned32,
				hwWlanAssociationRejectCount
					Unsigned32,
				hwWlanAssociationFailedCount
					Unsigned32,
				hwWlanReAssociationRequestCount
					Unsigned32,
				hwWlanReAssociationRejectCount
					Unsigned32,
				hwWlanReAssociationFailedCount
					Unsigned32,
				hwWlanDisAssocOfUserNotifiedCount
					Unsigned32,
				hwWlanDisAssocOfStaRoamCount
					Unsigned32,
				hwWlanDisAssocOfStaAgeCount
					Unsigned32,
				hwWlanDisAssocOfApUnableHandleCount
					Unsigned32,
				hwWlanDisAssocOfOtherReasonsCount
					Unsigned32,
				hwWlanAssocRequestCntByResource
					Unsigned32,
				hwWlanStaExceptionalOfflineCnt
					Unsigned32,
				hwWlanReAssociationSuccessCount
					Unsigned32,
				hwWlanBSSNotSupportAssocFailCount
					Unsigned32,
				hwWlanStaAccessRequestCount
					Unsigned32,
				hwWlanStaAccessRequestFailedCount
					Unsigned32,
				hwWlanStaAuthenRequestCount
					Unsigned32,
				hwWlanStaAuthenRequestFailedCount
					Unsigned32,
				hwWlanRefusedStaNumByResource
					Unsigned32,
				hwWlanStaAssocAndReAssocRequestCount
					Unsigned32,
				hwWlanStaAuthenRequestSuccessCount
					Unsigned32,
				hwWlanStationApStatApId
					Unsigned32,  
				hwWlanStaGetIPFailedCount
					Unsigned32,
				hwWlanStaGetIPSuccessCount
					Unsigned32
			 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.1
		hwWlanApAssocStatApMac OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This object indicates the MAC address of the AP."
			::= { hwWlanStationApStatEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.2
		hwWlanTotalOnlineTime OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total accumulated online time of the STAs that have ever associated with the AP, in seconds."
			::= { hwWlanStationApStatEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.3
		hwWlanTotalAssociatedStationCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs that have ever associated with the AP."
			::= { hwWlanStationApStatEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.4
		hwWlanCurrAssociatedStationCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STAs that are being associated with the AP."
			::= { hwWlanStationApStatEntry 4 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.5
		hwWlanAssociationRequestCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of association requirements received by the AP."
			::= { hwWlanStationApStatEntry 5 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.6
		hwWlanAssociationRejectCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of association requirements rejected by the AP."
			::= { hwWlanStationApStatEntry 6 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.7
		hwWlanAssociationFailedCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of association failures on the AP, excluding rejected association requirements."
			::= { hwWlanStationApStatEntry 7 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.8
		hwWlanReAssociationRequestCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of re-association requirements received by the AP."
			::= { hwWlanStationApStatEntry 8 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.9
		hwWlanReAssociationRejectCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of re-association requirements rejected by the AP."
			::= { hwWlanStationApStatEntry 9 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.10
		hwWlanReAssociationFailedCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of re-association failures on the AP, excluding rejected re-association requirements."
			::= { hwWlanStationApStatEntry 10 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.11
		hwWlanDisAssocOfUserNotifiedCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of associations removed because a STA goes offline."
			::= { hwWlanStationApStatEntry 11 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.12
		hwWlanDisAssocOfStaRoamCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of associations removed because a STA roams to another AP."
			::= { hwWlanStationApStatEntry 12 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.13
		hwWlanDisAssocOfStaAgeCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of associations removed because a STA goes offline unexpectedly."
			::= { hwWlanStationApStatEntry 13 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.14
		hwWlanDisAssocOfApUnableHandleCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of associations removed due to insufficient AP capability."
			::= { hwWlanStationApStatEntry 14 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.15
		hwWlanDisAssocOfOtherReasonsCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of associations removed due to other reasons."
			::= { hwWlanStationApStatEntry 15 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.16
		hwWlanAssocRequestCntByResource OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of STA association requests rejected by the AP because of insufficient resources."
			::= { hwWlanStationApStatEntry 16 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.17
		hwWlanStaExceptionalOfflineCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of times STAs are forced offline."
			::= { hwWlanStationApStatEntry 17 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.18
		hwWlanReAssociationSuccessCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of successful re-association attempts."
			::= { hwWlanStationApStatEntry 18 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.19
		hwWlanBSSNotSupportAssocFailCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of association requests rejected because the rate of STA does not meet the basic rate requirement."
			::= { hwWlanStationApStatEntry 19 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.20
		hwWlanStaAccessRequestCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total number of access attempts."
			::= { hwWlanStationApStatEntry 20 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.21
		hwWlanStaAccessRequestFailedCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total number of access failures."
			::= { hwWlanStationApStatEntry 21 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.22
		hwWlanStaAuthenRequestCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total number of authentication attempts."
			::= { hwWlanStationApStatEntry 22 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.23
		hwWlanStaAuthenRequestFailedCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total number of authentication failures."
			::= { hwWlanStationApStatEntry 23 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.24
		hwWlanRefusedStaNumByResource OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of rejected STA requests."
			::= { hwWlanStationApStatEntry 24 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.25
		hwWlanStaAssocAndReAssocRequestCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the total number of association and re-association requirements received by the AP."
			::= { hwWlanStationApStatEntry 25 }

		 --1.3.6.1.4.1.2011.6.139.18.1.3.1.26
		hwWlanStaAuthenRequestSuccessCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of successful authentication requirements."
			::= { hwWlanStationApStatEntry 26 }

		
		-- 1.3.6.1.4.1.2011.6.139.18.1.3.1.27
		hwWlanStationApStatApId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the AP ID."
			::= { hwWlanStationApStatEntry 27 }
   
   		-- 1.3.6.1.4.1.2011.6.139.18.1.3.1.28
		hwWlanStaGetIPFailedCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the number of times STAs get IP failed."
			::= { hwWlanStationApStatEntry 28 }        
			
		-- 1.3.6.1.4.1.2011.6.139.18.1.3.1.29
		hwWlanStaGetIPSuccessCount OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the number of times STAs get IP successfully."
			::= { hwWlanStationApStatEntry 29 }
		
		-- 1.3.6.1.4.1.2011.6.139.18.1.4
		hwWlanStaOnlineFailInfo OBJECT IDENTIFIER ::= { hwWlanStationObjects 4 }

		--1.3.6.1.4.1.2011.6.139.18.1.4.1
		hwWlanStaOnlineFailTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwWlanStaOnlineFailEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This table is used to describe information about failures of terminals to get online."
			::= { hwWlanStaOnlineFailInfo 1 }

		--1.3.6.1.4.1.2011.6.139.18.1.4.1.1
		hwWlanStaOnlineFailEntry OBJECT-TYPE
			SYNTAX HwWlanStaOnlineFailEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"The indexes of this table are hwStaOnlineFailMacAddress and hwStaOnlineFailReasonIndex."
			INDEX { hwWlanStaOnlineFailMacAddress, hwWlanStaOnlineFailReasonIndex }
			::= { hwWlanStaOnlineFailTable 1 }


		HwWlanStaOnlineFailEntry ::=
			SEQUENCE {				
				hwWlanStaOnlineFailMacAddress
					MacAddress,
				hwWlanStaOnlineFailReasonIndex
					Unsigned32,
				hwWlanStaOnlineFailApMac
					MacAddress,
				hwWlanStaOnlineFailApName
					OCTET STRING,
				hwWlanStaOnlineFailRadioId
					Unsigned32,
				hwWlanStaOnlineFailWlanId
					Unsigned32,
				hwWlanStaOnlineFailLastFailTime
					OCTET STRING,
				hwWlanStaOnlineFailReason
					OCTET STRING,
				hwWlanStaOnlineFailSsid
					OCTET STRING,
				hwWlanStaOnlineFailRowStatus
					RowStatus,
				hwWlanStaOnlineFailApId
					Unsigned32
			 }

		 --1.3.6.1.4.1.2011.6.139.18.1.4.1.1.1
		hwWlanStaOnlineFailMacAddress OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This object indicates the user MAC address."
			::= { hwWlanStaOnlineFailEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.18.1.4.1.1.2
		hwWlanStaOnlineFailReasonIndex OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This object indicates the reason ID."
			::= { hwWlanStaOnlineFailEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.18.1.4.1.1.3
		hwWlanStaOnlineFailApMac OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the MAC address of the AP."
			::= { hwWlanStaOnlineFailEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.18.1.4.1.1.4
		hwWlanStaOnlineFailApName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the AP name."
			::= { hwWlanStaOnlineFailEntry 4 }

		 --1.3.6.1.4.1.2011.6.139.18.1.4.1.1.5
		hwWlanStaOnlineFailRadioId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the radio ID."
			::= { hwWlanStaOnlineFailEntry 5 }

		 --1.3.6.1.4.1.2011.6.139.18.1.4.1.1.6
		hwWlanStaOnlineFailWlanId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the WLAN ID."
			::= { hwWlanStaOnlineFailEntry 6 }

		 --1.3.6.1.4.1.2011.6.139.18.1.4.1.1.7
		hwWlanStaOnlineFailLastFailTime OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the last time when a user failed to go online."
			::= { hwWlanStaOnlineFailEntry 7 }

		 --1.3.6.1.4.1.2011.6.139.18.1.4.1.1.8
		hwWlanStaOnlineFailReason OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the failure reason."
			::= { hwWlanStaOnlineFailEntry 8 }

		 --1.3.6.1.4.1.2011.6.139.18.1.4.1.1.9
		hwWlanStaOnlineFailSsid OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the SSID."
			::= { hwWlanStaOnlineFailEntry 9 }

		 --1.3.6.1.4.1.2011.6.139.18.1.4.1.1.10
		hwWlanStaOnlineFailRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"This object indicates the row status."
			::= { hwWlanStaOnlineFailEntry 10 }


		-- 1.3.6.1.4.1.2011.6.139.18.1.4.1.1.11
		hwWlanStaOnlineFailApId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the AP ID."
			::= { hwWlanStaOnlineFailEntry 11 }
			
		--1.3.6.1.4.1.2011.6.139.18.1.5
		hwWlanStaOfflineInfo OBJECT IDENTIFIER ::= { hwWlanStationObjects 5 }

		--1.3.6.1.4.1.2011.6.139.18.1.5.1
		hwWlanStaOfflineTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwWlanStaOfflineEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This table is used to describe offline information."
			::= { hwWlanStaOfflineInfo 1 }

		--1.3.6.1.4.1.2011.6.139.18.1.5.1.1
		hwWlanStaOfflineEntry OBJECT-TYPE
			SYNTAX HwWlanStaOfflineEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"The indexes of this table are hwWlanStaOfflineMacAddress and hwWlanStaOfflineReasonIndex."
			INDEX { hwWlanStaOfflineMacAddress, hwWlanStaOfflineReasonIndex }
			::= { hwWlanStaOfflineTable 1 }


		HwWlanStaOfflineEntry ::=
			SEQUENCE {				
				hwWlanStaOfflineMacAddress
					MacAddress,
				hwWlanStaOfflineReasonIndex
					Unsigned32,
				hwWlanStaOfflineApMac
					MacAddress,
				hwWlanStaOfflineApName
					OCTET STRING,
				hwWlanStaOfflineRadioId
					Unsigned32,
				hwWlanStaOfflineWlanId
					Unsigned32,
				hwWlanStaOfflineLastFailTime
					OCTET STRING,
				hwWlanStaOfflineReason
					OCTET STRING,
				hwWlanStaOfflineSsid
					OCTET STRING,
				hwWlanStaOfflineFailRowStatus
					RowStatus,
				hwWlanStaOfflineApId
					Unsigned32
			 }

		 --1.3.6.1.4.1.2011.6.139.18.1.5.1.1.1
		hwWlanStaOfflineMacAddress OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This object indicates the user MAC address."
			::= { hwWlanStaOfflineEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.18.1.5.1.1.2
		hwWlanStaOfflineReasonIndex OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This object indicates the reason ID."
			::= { hwWlanStaOfflineEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.18.1.5.1.1.3
		hwWlanStaOfflineApMac OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the MAC address of the AP."
			::= { hwWlanStaOfflineEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.18.1.5.1.1.4
		hwWlanStaOfflineApName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the AP name."
			::= { hwWlanStaOfflineEntry 4 }

		 --1.3.6.1.4.1.2011.6.139.18.1.5.1.1.5
		hwWlanStaOfflineRadioId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the radio ID."
			::= { hwWlanStaOfflineEntry 5 }

		 --1.3.6.1.4.1.2011.6.139.18.1.5.1.1.6
		hwWlanStaOfflineWlanId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the WLAN ID."
			::= { hwWlanStaOfflineEntry 6 }

		 --1.3.6.1.4.1.2011.6.139.18.1.5.1.1.7
		hwWlanStaOfflineLastFailTime OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the last time when a user went offline."
			::= { hwWlanStaOfflineEntry 7 }

		 --1.3.6.1.4.1.2011.6.139.18.1.5.1.1.8
		hwWlanStaOfflineReason OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the failure reason."
			::= { hwWlanStaOfflineEntry 8 }

		 --1.3.6.1.4.1.2011.6.139.18.1.5.1.1.9
		hwWlanStaOfflineSsid OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the SSID."
			::= { hwWlanStaOfflineEntry 9 }

		 --1.3.6.1.4.1.2011.6.139.18.1.5.1.1.10
		hwWlanStaOfflineFailRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"This object indicates the row status."
			::= { hwWlanStaOfflineEntry 10 }


		-- 1.3.6.1.4.1.2011.6.139.18.1.5.1.1.11
		hwWlanStaOfflineApId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the AP ID."
			::= { hwWlanStaOfflineEntry 11 }
			
			
		--1.3.6.1.4.1.2011.6.139.18.1.6
		hwWlanStaRoamInfo OBJECT IDENTIFIER ::= { hwWlanStationObjects 6 }

		--1.3.6.1.4.1.2011.6.139.18.1.6.1
		hwWlanStaRoamTraceTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwWlanStaRoamTraceEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This table describes the roaming track of a STA."
			::= { hwWlanStaRoamInfo 1 }

		--1.3.6.1.4.1.2011.6.139.18.1.6.1.1
		hwWlanStaRoamTraceEntry OBJECT-TYPE
			SYNTAX HwWlanStaRoamTraceEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"The indexes of this table are hwWlanStaRoamTraceStaMac and hwWlanStaRoamTraceIndex."
			INDEX { hwWlanStaRoamTraceStaMac, hwWlanStaRoamTraceIndex }
			::= { hwWlanStaRoamTraceTable 1 }


		HwWlanStaRoamTraceEntry ::=
			SEQUENCE {				
				hwWlanStaRoamTraceStaMac
					MacAddress,
				hwWlanStaRoamTraceIndex
					Integer32,
				hwWlanStaRoamTraceTime
					Unsigned32,
				hwWlanStaRoamTraceAcIP
					IpAddress,
				hwWlanStaRoamTraceAcIPv6
					OCTET STRING,
				hwWlanStaRoamTraceApName
					OCTET STRING,
				hwWlanStaRoamTraceRadioId
					Integer32,
				hwWlanStaRoamTraceBssid
					MacAddress,
				hwWlanStaRoamTraceInRate
					Integer32,
				hwWlanStaRoamTraceOutRate
					Integer32,
				hwWlanStaRoamTraceInRssi
					Integer32,
				hwWlanStaRoamTraceOutRssi
					Integer32,
				hwWlanStaRoamTraceRoamType
					INTEGER,
				hwWlanStaRoamTraceApId
					Unsigned32,
				hwWlanStaRoamTraceInfo
					INTEGER
			 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.1
		hwWlanStaRoamTraceStaMac OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This object indicates the STA's MAC address."
			::= { hwWlanStaRoamTraceEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.2
		hwWlanStaRoamTraceIndex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This object indicates the internal ID."
			::= { hwWlanStaRoamTraceEntry 2 }

		
		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.3
		hwWlanStaRoamTraceTime OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the roaming time."
			::= { hwWlanStaRoamTraceEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.4
		hwWlanStaRoamTraceAcIP OBJECT-TYPE
			SYNTAX IpAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the IP address of the AC with which the STA associates."
			::= { hwWlanStaRoamTraceEntry 4 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.5
		hwWlanStaRoamTraceAcIPv6 OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the IPv6 address of the AC with which the STA associates."
			::= { hwWlanStaRoamTraceEntry 5 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.6
		hwWlanStaRoamTraceApName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the name of the AP with which the STA associates."
			::= { hwWlanStaRoamTraceEntry 6 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.7
		hwWlanStaRoamTraceRadioId OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the ID of the radio which which the STA associates."
			::= { hwWlanStaRoamTraceEntry 7 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.8
		hwWlanStaRoamTraceBssid OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the BSSID of the STA."
			::= { hwWlanStaRoamTraceEntry 8 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.9
		hwWlanStaRoamTraceInRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates roam-in rate."
			::= { hwWlanStaRoamTraceEntry 9 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.10
		hwWlanStaRoamTraceOutRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates roam-out rate."
			::= { hwWlanStaRoamTraceEntry 10 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.11
		hwWlanStaRoamTraceInRssi OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the roam-in RSSI."
			::= { hwWlanStaRoamTraceEntry 11 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.12
		hwWlanStaRoamTraceOutRssi OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates roam-out RSSI."
			::= { hwWlanStaRoamTraceEntry 12 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.1.1.13
		hwWlanStaRoamTraceRoamType OBJECT-TYPE
			SYNTAX INTEGER
				{
				l2(1),
				l3(2),
				none(3)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the roaming type. 1: Layer 2 roaming 2: Layer 3 Roaming 3: Not roaming."
			::= { hwWlanStaRoamTraceEntry 13 }


		-- 1.3.6.1.4.1.2011.6.139.18.1.6.1.1.14
		hwWlanStaRoamTraceApId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the AP ID."
			::= { hwWlanStaRoamTraceEntry 14 }
		
			
		-- 1.3.6.1.4.1.2011.6.139.18.1.6.1.1.15
		hwWlanStaRoamTraceInfo OBJECT-TYPE
			SYNTAX INTEGER
				{
				normal(0),
				zeroRoam(1),
				pmkCacheRoam(2),
				ftRoam(3)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the roam type information."
			::= { hwWlanStaRoamTraceEntry 15 }	
		--1.3.6.1.4.1.2011.6.139.18.1.6.2
		hwWlanStaAcL3RoamStatisticsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwWlanStaAcL3RoamStatisticsEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This table describes statistics on Layer 3 roaming STAs based on ACs."
			::= { hwWlanStaRoamInfo 2 }

		--1.3.6.1.4.1.2011.6.139.18.1.6.2.1
		hwWlanStaAcL3RoamStatisticsEntry OBJECT-TYPE
			SYNTAX HwWlanStaAcL3RoamStatisticsEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"The index of this table is hwWlanStaAcL3RoamStatisticAcIndex."
			INDEX { hwWlanStaAcL3RoamStatisticAcIndex }
			::= { hwWlanStaAcL3RoamStatisticsTable 1 }


		HwWlanStaAcL3RoamStatisticsEntry ::=
			SEQUENCE {				
				hwWlanStaAcL3RoamStatisticAcIndex
					Integer32,
				hwWlanStaAcL3RoamStatisticAcIP
					IpAddress,
				hwWlanStaAcL3RoamStatisticAcIPv6
					OCTET STRING,
				hwWlanStaAcL3RoamStatisticRoamInCnt
					Unsigned32,
				hwWlanStaAcL3RoamStatisticRoamOutCnt
					Unsigned32, 
				hwWlanStaAcL3RoamStatisticAcDescription
					OCTET STRING
			 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.2.1.1
		hwWlanStaAcL3RoamStatisticAcIndex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This object indicates the peer AC ID."
			::= { hwWlanStaAcL3RoamStatisticsEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.2.1.2
		hwWlanStaAcL3RoamStatisticAcIP OBJECT-TYPE
			SYNTAX IpAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the peer AC IP address."
			::= { hwWlanStaAcL3RoamStatisticsEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.2.1.3
		hwWlanStaAcL3RoamStatisticAcIPv6 OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the peer AC IPv6 address."
			::= { hwWlanStaAcL3RoamStatisticsEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.2.1.4
		hwWlanStaAcL3RoamStatisticRoamInCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of users who roam from peer AC to local AC."
			::= { hwWlanStaAcL3RoamStatisticsEntry 4 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.2.1.5
		hwWlanStaAcL3RoamStatisticRoamOutCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of users who roam from local AC to peer AC."
			::= { hwWlanStaAcL3RoamStatisticsEntry 5 }
			
		 --1.3.6.1.4.1.2011.6.139.18.1.6.2.1.6
		hwWlanStaAcL3RoamStatisticAcDescription OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the AC description."
			::= { hwWlanStaAcL3RoamStatisticsEntry 6 }


		--1.3.6.1.4.1.2011.6.139.18.1.6.3
		hwWlanStaApL3RoamStatisticsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwWlanStaApL3RoamStatisticsEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This table describes statistics on Layer 3 roaming STAs based on APs."
			::= { hwWlanStaRoamInfo 3 }

		--1.3.6.1.4.1.2011.6.139.18.1.6.3.1
		hwWlanStaApL3RoamStatisticsEntry OBJECT-TYPE
			SYNTAX HwWlanStaApL3RoamStatisticsEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"The index of this table is hwWlanStaApL3RoamStatisticApMac."
			INDEX { hwWlanStaApL3RoamStatisticApMac }
			::= { hwWlanStaApL3RoamStatisticsTable 1 }


		HwWlanStaApL3RoamStatisticsEntry ::=
			SEQUENCE {				
				hwWlanStaApL3RoamStatisticApMac
					MacAddress,
				hwWlanStaApL3RoamStatisticApName
					OCTET STRING,
				hwWlanStaApL3RoamStatisticRoamInCnt
					Unsigned32,
				hwWlanStaApL3RoamStatisticRoamOutCnt
					Unsigned32,
				hwWlanStaApL3RoamStatisticApId
					Unsigned32
			 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.3.1.1
		hwWlanStaApL3RoamStatisticApMac OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"This object indicates the MAC address of the AP."
			::= { hwWlanStaApL3RoamStatisticsEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.3.1.2
		hwWlanStaApL3RoamStatisticApName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the AP name."
			::= { hwWlanStaApL3RoamStatisticsEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.3.1.3
		hwWlanStaApL3RoamStatisticRoamInCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of roam-in users."
			::= { hwWlanStaApL3RoamStatisticsEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.18.1.6.3.1.4
		hwWlanStaApL3RoamStatisticRoamOutCnt OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"This object indicates the number of roam-out users."
			::= { hwWlanStaApL3RoamStatisticsEntry 4 }

		-- 1.3.6.1.4.1.2011.6.139.18.1.6.3.1.5
		hwWlanStaApL3RoamStatisticApId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the AP ID."
			::= { hwWlanStaApL3RoamStatisticsEntry 5 }

		--1.3.6.1.4.1.2011.6.139.18.2
		hwWlanStationConformance OBJECT IDENTIFIER ::= { hwWlanStation 2 }

		--1.3.6.1.4.1.2011.6.139.18.2.1
		hwWlanStationCompliances OBJECT IDENTIFIER ::= { hwWlanStationConformance 1 }

		--1.3.6.1.4.1.2011.6.139.18.2.1.1
		hwWlanStationCompliance MODULE-COMPLIANCE
			STATUS current
			DESCRIPTION 
				"Description."
			MODULE
					MANDATORY-GROUPS { hwWlanStationGroup, hwWlanApAssocStatGroup, hwWlanStaOnlineFailInfoGroup, hwWlanStaOfflineInfoGroup, hwWlanStaRoamInfoGroup }
			::= { hwWlanStationCompliances 1 }

		--1.3.6.1.4.1.2011.6.139.18.2.2
		hwWlanStationObjectGroups OBJECT IDENTIFIER ::= { hwWlanStationConformance 2 }

		--1.3.6.1.4.1.2011.6.139.18.2.2.1
		hwWlanStaTrapsGroup NOTIFICATION-GROUP
			NOTIFICATIONS { hwWlanStaAuthErrorTrap, hwWlanStaAssoFailTrap, hwWlanUserInvalidCerficationTrap, hwWlanStaRepititiveAttackTrap, hwWlanStaTamperAttackTrap, 
			hwWlanStaLowLevelSecAttackTrap, hwWlanStaAddressRedirectionAttackTrap, hwWlanStaWepIdConflictTrap, hwStationOnlineTrap, hwStationOfflineTrap, 
			hwStationSignalStrengthLowThanThresholdTrap }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanStationObjectGroups 1 }
                
                --1.3.6.1.4.1.2011.6.139.18.2.2.2
		hwWlanStaTrapsObjectGroup OBJECT-GROUP
			OBJECTS { hwWlanStaAuthenticationMode,hwWlanStaTrapOccurTime,hwWlanStaFailCodeType,hwWlanSignalStrengthThreshold,hwWlanWepIDConflictTrapRadioId,
			hwWlanWepIDConflictTrapAPMAC,hwWlanStaAuthenticationFailCause,hwWlanWepIDConflictTrapPreSSID,hwWlanWlanVapAuthEncryptMode,hwWlanWlanStaAuthEncryptMode,
			hwWlanWepIDConflictTrapCurrSSID,hwWlanStaAuthenticationFailCauseStr,hwWlanWepIDConflictTrapCipherIdx,hwWlanWepIDConflictTrapAPName,hwWlanStaAssociationFailCauseStr,
			hwWlanStaAssociationFailCause,hwWlanStaAssocBssid }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanStationObjectGroups 2 }
			
		--1.3.6.1.4.1.2011.6.139.18.2.2.3
		hwWlanStationGroup OBJECT-GROUP
			OBJECTS { hwWlanStaMac, hwWlanStaUsername, hwWlanStaApMac, hwWlanStaApName, hwWlanStaApGroup, 
				hwWlanStaRadioId, hwWlanStaAssocBand, hwWlanStaSupportBand, hwWlanStaAccessChannel, hwWlanStaRfMode, 
				hwWlanStaHtMode, hwWlanStaMcsVal, hwWlanStaShortGIStatus, hwWlanStaConnectRxRate, hwWlanStaConnectTxRate, 
				hwWlanStaEssName, hwWlanStaBSSID, hwWlanStaSsid, hwWlanStaStatus, hwWlanStaAuthenMethod, 
				hwWlanStaEncryptMethod, hwWlanStaQosMode, hwWlanStaRoamStatus, hwWlanStaVlan, hwWlanStaIP, 
				hwWlanStaIPv6, hwWlanStaGateway, hwWlanStaAssocTime, hwWlanStaAccessTime, hwWlanStaOnlineTime, 
				hwWlanStaAccessOnlineTime, hwWlanStaStatOperMode, hwWlanStaWirelessStatRxFrames, hwWlanStaWirelessRxBytes, hwWlanStaWirelessRxRate, 
				hwWlanStaWirelessStatTxFrames, hwWlanStaWirelessTxBytes, hwWlanStaWirelessTxRate, hwWlanStaPeriodSendDropFrames, hwWlanStaPeriodReSendFrames, 
				hwWlanStaPeriodReSendBytes, hwWlanStaRssi, hwWlanStaNoise, hwWlanStaSnrUs, hwWlanStaRxPowerUs, 
				hwWlanStaChannelUtilRate, hwWlanStaChannelBusyRate, hwWlanStaChannelTxRatio, hwWlanStaChannelRxRatio, hwWlanStaChannelFreeRate, 
				hwWlanStaChannelInterfRate, hwWlanStaPeriodSendFrames, hwWlanStaApId, 
				hwWlanStationUapsdCapacity, hwWlanStationPowerSavePercent, hwWlanStaAssocStartTime, hwWlanStaAuthStartTime, hwWlanStaDhcpStartTime, hwWlanStaVHTCapable, hwWlanStaVHTTxBFCapable, hwWlanStaMUMIMOCapable, hwWlanStaWpaStartTime, hwWlanStaWpaSuccessTime}
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanStationObjectGroups 3 }

		--1.3.6.1.4.1.2011.6.139.18.2.2.4
		hwWlanApAssocStatGroup OBJECT-GROUP
			OBJECTS { hwWlanTotalOnlineTime, hwWlanTotalAssociatedStationCount, hwWlanCurrAssociatedStationCount, hwWlanAssociationRequestCount, 
			hwWlanAssociationRejectCount, hwWlanAssociationFailedCount, hwWlanReAssociationRequestCount, hwWlanReAssociationRejectCount, hwWlanReAssociationFailedCount, 
			hwWlanDisAssocOfUserNotifiedCount, hwWlanDisAssocOfStaRoamCount, hwWlanDisAssocOfStaAgeCount, hwWlanDisAssocOfApUnableHandleCount, hwWlanDisAssocOfOtherReasonsCount, 
			hwWlanAssocRequestCntByResource, hwWlanStaExceptionalOfflineCnt, hwWlanReAssociationSuccessCount, hwWlanBSSNotSupportAssocFailCount, hwWlanStaAccessRequestCount, 
			hwWlanStaAccessRequestFailedCount, hwWlanStaAuthenRequestCount, hwWlanStaAuthenRequestFailedCount, hwWlanRefusedStaNumByResource, hwWlanStaAssocAndReAssocRequestCount, 
			hwWlanStaAuthenRequestSuccessCount, hwWlanStationApStatApId, hwWlanStaGetIPFailedCount, hwWlanStaGetIPSuccessCount}
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanStationObjectGroups 4 }

		--1.3.6.1.4.1.2011.6.139.18.2.2.5
		hwWlanStaOnlineFailInfoGroup OBJECT-GROUP
			OBJECTS { hwWlanStaOnlineFailApMac, hwWlanStaOnlineFailApName, hwWlanStaOnlineFailRadioId, 
			hwWlanStaOnlineFailWlanId, hwWlanStaOnlineFailLastFailTime, hwWlanStaOnlineFailReason, hwWlanStaOnlineFailSsid, hwWlanStaOnlineFailRowStatus, hwWlanStaOnlineFailApId }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanStationObjectGroups 5 }

		--1.3.6.1.4.1.2011.6.139.18.2.2.6
		hwWlanStaOfflineInfoGroup OBJECT-GROUP
			OBJECTS { hwWlanStaOfflineApMac, hwWlanStaOfflineApName, hwWlanStaOfflineRadioId, 
			hwWlanStaOfflineWlanId, hwWlanStaOfflineLastFailTime, hwWlanStaOfflineReason, hwWlanStaOfflineSsid, hwWlanStaOfflineFailRowStatus, hwWlanStaOfflineApId }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanStationObjectGroups 6 }

		--1.3.6.1.4.1.2011.6.139.18.2.2.7
		hwWlanStaRoamInfoGroup OBJECT-GROUP
			OBJECTS { hwWlanStaRoamTraceTime, hwWlanStaRoamTraceAcIP, 
			hwWlanStaRoamTraceAcIPv6, hwWlanStaRoamTraceApName, hwWlanStaRoamTraceRadioId, hwWlanStaRoamTraceBssid, 
			hwWlanStaRoamTraceInRate, hwWlanStaRoamTraceOutRate, hwWlanStaRoamTraceInRssi, hwWlanStaRoamTraceOutRssi, hwWlanStaRoamTraceRoamType, 
			hwWlanStaRoamTraceApId, hwWlanStaRoamTraceInfo,hwWlanStaAcL3RoamStatisticAcIP, hwWlanStaAcL3RoamStatisticAcIPv6, hwWlanStaAcL3RoamStatisticRoamInCnt, hwWlanStaAcL3RoamStatisticRoamOutCnt, 
			hwWlanStaApL3RoamStatisticApName, hwWlanStaApL3RoamStatisticRoamInCnt, hwWlanStaApL3RoamStatisticRoamOutCnt, hwWlanStaApL3RoamStatisticApId }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanStationObjectGroups 7 }


	END
--
-- HUAWEI-WLAN-STATION-MIB.mib
--
