-- Copyright (C) 2018 by HUAWEI TECHNOLOGIES. All rights reserved.
-- Description: HUAWEI Private Extended Interface MIB
-- Reference:
-- Version: V2.21
-- History:
-- Version: V2.0
-- History:
--              Yang Jishang,2009-05-04, Add one table for Mdn compliance.       
-- ==================================================================
-- ==================================================================
-- 
-- Varibles and types be imported
--
-- ==================================================================
HUAWEI-LLDP-MIB DEFINITIONS ::= BEGIN
	IMPORTS
	
     TruthValue, TEXTUAL-CONVENTION, DisplayString, MacAddress
        FROM SNMPv2-TC
        
     MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
        FROM SNMPv2-CONF

    MODULE-IDENTITY, OBJECT-TYPE, Integer32, IpAddress,
    OBJECT-IDENTITY, Unsigned32, NOTIFICATION-TYPE
        FROM SNMPv2-SMI

     InterfaceIndex
        FROM IF-MIB

    lldpPortConfigPortNum,lldpLocSysCapSupported,lldpLocSysCapEnabled,
    LldpPortNumber,LldpPortId,lldpRemEntry,LldpManAddress,LldpManAddrIfSubtype,
    lldpRemTimeMark,lldpRemLocalPortNum,lldpRemIndex,LldpChassisId,LldpSystemCapabilitiesMap
      	FROM LLDP-MIB  
    
    AddressFamilyNumbers
        FROM IANA-ADDRESS-FAMILY-NUMBERS-MIB
        
    hwDatacomm
        FROM HUAWEI-MIB;
 
    hwLldpMIB MODULE-IDENTITY
        LAST-UPDATED "201808300000Z"

        ORGANIZATION 
            "Huawei Technologies Co.,Ltd."
        CONTACT-INFO 
            "Huawei Industrial Base
              Bantian, Longgang
               Shenzhen 518129
               People's Republic of China
               Website: http://www.huawei.com
               Email: support@huawei.com
             "
        DESCRIPTION
            "This file is an extension of LLDP-MIB. It provides such functions of 
           globally enabling or disabling the LLDP protocol, enabling the global
           alarm, clearing statistics on ports and configuring network management 
           IP addresses and some alarms."
        REVISION "201808300000Z"
        DESCRIPTION "add trap hwLldpInterfaceParaChange"

        REVISION  "201804070000Z"
        DESCRIPTION "add hwLldpRemManAddrTable"

        REVISION  "201803270000Z"
        DESCRIPTION "modify decription of hwLldpNotificationEnable"

        REVISION  "201708172019Z"
        DESCRIPTION "modify decription of hwLldpMdnRemTable"

        REVISION  "201707200000Z"
        DESCRIPTION "add trap hwLldpDdpTrapObjects"

        REVISION "201707130000Z"
        DESCRIPTION "edit hwLldpEnable  description"

        REVISION "201705220000Z"
        DESCRIPTION "add hwLldpDdpFilterType"

        REVISION "201612240000Z"
        DESCRIPTION "add hwLldpRemNetworkIdTable"

        REVISION "201605160000Z"
        DESCRIPTION "add trap hwLldpInterfaceRemTablesChange"
	
        REVISION  "201503311730Z"
        DESCRIPTION "add trap hwLldpRateExcessive"
        
        REVISION  "201503101558Z"
        DESCRIPTION "modify hwLldpCounterReset" 
        


            ::= { hwDatacomm 134 }  
         
      -- Textual Convention

		EnabledStatus ::= TEXTUAL-CONVENTION
    		STATUS    current
    		DESCRIPTION
       		 "A simple status value for the object."
    		SYNTAX   INTEGER 
   				 { 
      				enabled(1),
      				disabled(2)
    			}
 		    
    -- ============================================================================
    -- Node definitions
    -- ============================================================================ 

    -- 1.3.6.1.4.1.2011.5.25.134
 
    hwLldpObjects  OBJECT IDENTIFIER ::= { hwLldpMIB 1} 

    hwLldpTraps OBJECT IDENTIFIER ::= { hwLldpMIB 2 }  
    
    hwLldpConformance  OBJECT IDENTIFIER ::= { hwLldpMIB 3 }
 

  -- ============================================================================
  --
  -- ======================= Objects definitions=================================
  --
  -- ============================================================================  

  hwLldpConfiguration  OBJECT IDENTIFIER ::= { hwLldpObjects 1}      
  hwLldpRemoteSystemData  OBJECT IDENTIFIER ::= { hwLldpObjects 2} 
  hwLldpInterfaceRemData  OBJECT IDENTIFIER ::= { hwLldpObjects 3} 
  hwLldpTrapObjects OBJECT IDENTIFIER ::= { hwLldpObjects 51 }
  hwLldpDdpFilterType OBJECT IDENTIFIER ::= { hwLldpObjects 53 }

  hwLldpDdpFilterTypeTable OBJECT-TYPE
	SYNTAX SEQUENCE OF HwLldpDdpFilterTypeEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Description."
			::= { hwLldpDdpFilterType 1 }

  hwLldpDdpFilterTypeEntry OBJECT-TYPE
	SYNTAX HwLldpDdpFilterTypeEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Description."
	INDEX { hwLldpDdpIfIndex }
			::= { hwLldpDdpFilterTypeTable 1 }

		
  HwLldpDdpFilterTypeEntry ::=
	SEQUENCE { 
		hwLldpDdpIfIndex
			Integer32,
		hwLldpDdpSetFilterType
			Integer32
			 }
  hwLldpDdpIfIndex OBJECT-TYPE
		SYNTAX Integer32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwLldpDdpFilterTypeEntry 1 }

  hwLldpDdpSetFilterType OBJECT-TYPE
			SYNTAX Integer32 (0..2)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwLldpDdpFilterTypeEntry 2 }

  hwLldpEnable OBJECT-TYPE 
	SYNTAX EnabledStatus
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"Globally enable or disable the LLDP configuration. If the hwLldpEnable 
        is 1, LLDP is enabled. If the hwLldpEnable is 2, LLDP is disabled. "   
	::= { hwLldpConfiguration 1 }   

  hwLldpLocManIPAddr OBJECT-TYPE 
	SYNTAX IpAddress
	MAX-ACCESS read-write
	STATUS  current
	DESCRIPTION
		"Specifies the management IP address of the local device. The management IP
        address is carried in the management address TLV of LLDP packet and is used
        to identify NM devices in network management. The management IP address 
        configured here must be a valid one and must be an IP address in the address
        chain. If the IP address is not valid or is not configured, the management IP 
        address will be chosen from default IP addressees of the system. The sequence
        of address searching is: loopback interface, management network interface, VLANIF
        port and IP address chain (The smallest IP is chosen). If the default IP is not 
        found, the bridge MAC of the system is used."
		
	::= { hwLldpConfiguration 2 }     
	
    hwLldpCounterReset OBJECT-TYPE 
		SYNTAX EnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Clears the statistics of neighbours received and sent for trap informations."   
		::= { hwLldpConfiguration 3 } 
		
	hwLldpNotificationEnable OBJECT-TYPE 
		SYNTAX EnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The global alarming that is used to control alarms on all ports.
             If it is 1, the global alarming is enabled. If it is 2, the global
             alarming is disabled."     
		::= { hwLldpConfiguration 4 } 

   hwLldpPortConfigTable  OBJECT-TYPE
      SYNTAX SEQUENCE OF HwLldpPortConfigEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
			"LLDP port congfiguration table."
      ::= { hwLldpConfiguration  5 }

   hwLldpPortConfigEntry OBJECT-TYPE
        SYNTAX HwLldpPortConfigEntry
		MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           	"Entries of the LLDP port congfiguration table."
        INDEX{ lldpPortConfigPortNum}
        ::= { hwLldpPortConfigTable 1}  
   
   HwLldpPortConfigEntry ::=
    	SEQUENCE  {    
    	    hwLldpPortConfigIfIndex  
    	    	    InterfaceIndex,
    		hwLldpPortConfigCounterReset
    				EnabledStatus
        			}
    				
   hwLldpPortConfigIfIndex  OBJECT-TYPE
    	SYNTAX InterfaceIndex
    	MAX-ACCESS read-only
    	STATUS current
   		DESCRIPTION 
   				"Port index."     
   		::= {hwLldpPortConfigEntry 11}
 
   hwLldpPortConfigCounterReset OBJECT-TYPE
    	SYNTAX EnabledStatus
    	MAX-ACCESS read-write
    	STATUS current
   		DESCRIPTION 
   			"Clears the statistics of packets received and sent on the current port."     
   		::= {hwLldpPortConfigEntry 12}
		
   hwLldpRemProtoTypeTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwLldpRemProtoTypeEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
	 	 	"LLDP remote neighbour protocol version table."
        ::= { hwLldpRemoteSystemData  1 }

   hwLldpRemProtoTypeEntry OBJECT-TYPE
        SYNTAX HwLldpRemProtoTypeEntry
		MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           	"Entries of the LLDP remote neighbour protocol version table."
 	    INDEX {
	    lldpPortConfigPortNum
	    }
        ::= { hwLldpRemProtoTypeTable 1}  
   
   HwLldpRemProtoTypeEntry ::=
    	SEQUENCE  {    
   hwLldpRemProtoType INTEGER
   }
    				 
   hwLldpRemProtoType  OBJECT-TYPE
        SYNTAX INTEGER
            {
            lldp(1),
            mdn(2),
            unknown(255)
            }
    	MAX-ACCESS read-only
    	STATUS current
   		DESCRIPTION 
   				"Protocol type of the remote neighbour."     
   		::= {hwLldpRemProtoTypeEntry 1}
   		
   hwLldpMdnRemTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwLldpMdnRemEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
       "Remote MDN neighbor query table."
        ::= { hwLldpRemoteSystemData  2 }

   hwLldpMdnRemEntry OBJECT-TYPE
        SYNTAX HwLldpMdnRemEntry
		MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           	"Entries of the MacAddress discovery neighbour remote table."
 	    INDEX {
	    hwLldpMdnRemLocalPortNum,
	    hwLldpMdnRemIndex
	    }
        ::= { hwLldpMdnRemTable 1}  
   
   HwLldpMdnRemEntry ::=
    	SEQUENCE  {    
   hwLldpMdnRemLocalPortNum LldpPortNumber,
   hwLldpMdnRemIndex Integer32,  
   hwLldpMdnRemLocalPortId LldpPortId,  
   hwLldpMdnRemMacAddr MacAddress
   }
    				 
   hwLldpMdnRemLocalPortNum  OBJECT-TYPE
      SYNTAX LldpPortNumber
    	MAX-ACCESS not-accessible
    	STATUS current
   		DESCRIPTION 
   				"The index value used to identify the local port associated with 
   				this entry."     
   		::= {hwLldpMdnRemEntry 1} 
   		   		
   hwLldpMdnRemIndex  OBJECT-TYPE
      SYNTAX Integer32
    	MAX-ACCESS not-accessible
    	STATUS current
   		DESCRIPTION 
   				"This object represents an arbitrary local integer value used to 
   				identify a particular connection instance, unique only for the 
   				indicated remote system."     
   		::= {hwLldpMdnRemEntry 2}   
   		
   hwLldpMdnRemLocalPortId  OBJECT-TYPE
      SYNTAX LldpPortId
    	MAX-ACCESS read-only
    	STATUS current
   		DESCRIPTION 
		        "The string value used to identify the port component
		        associated with a given port in the local system."   
   		::= {hwLldpMdnRemEntry 3} 
   		     		
   hwLldpMdnRemMacAddr  OBJECT-TYPE
      SYNTAX MacAddress
    	MAX-ACCESS read-only
    	STATUS current
   		DESCRIPTION 
   				"The MacAddress of LLDP MacAddress discovery neighbor."     
   		::= {hwLldpMdnRemEntry 8}  
    --hwLldpRemManAddrTable : Management addresses of the remote system
    --
    hwLldpRemManAddrTable OBJECT-TYPE
    SYNTAX SEQUENCE OF HwLldpRemManAddrEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table contains one or more rows per management address
        information on the remote system learned on a particular port
        contained in the local chassis known to this agent."
    ::= { hwLldpRemoteSystemData 4 } 
    
    hwLldpRemManAddrEntry OBJECT-TYPE
    SYNTAX HwLldpRemManAddrEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Management address information about a particular chassis
        component. There may be multiple management addresses
        configured on the remote system identified by a particular
        lldpRemIndex whose information is received on
        lldpRemLocalPortNum of the local system. Each management
        address should have distinct 'management address
        type' (hwLldpRemManAddrSubtype) and 'management address'
        (hwLldpRemManAddr.)
        Entries may be created and deleted in this table by the
        agent."
    INDEX { lldpRemTimeMark,
    lldpRemLocalPortNum,
    lldpRemIndex,
    hwLldpRemManAddrSubtype,
    hwLldpRemManAddr
    }
    ::= { hwLldpRemManAddrTable 1 }   
    
    HwLldpRemManAddrEntry ::= SEQUENCE {
    hwLldpRemManAddrSubtype AddressFamilyNumbers,
    hwLldpRemManAddr LldpManAddress,
    hwLldpRemManAddrIfSubtype LldpManAddrIfSubtype,
    hwLldpRemManAddrIfId Integer32,
    hwLldpRemManAddrOID OBJECT IDENTIFIER
    }                       
    
    hwLldpRemManAddrSubtype OBJECT-TYPE
    SYNTAX AddressFamilyNumbers
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The type of management address identifier encoding used in
        the associated 'lldpRemManagmentAddr' object."
    REFERENCE
        "IEEE Std 802.1AB-2005 9.5.9.3"
    ::= { hwLldpRemManAddrEntry 1 }    
    
    hwLldpRemManAddr OBJECT-TYPE
    SYNTAX LldpManAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The string value used to identify the management address
        component associated with the remote system. The purpose
        of this address is to contact the management entity."
    REFERENCE
        "IEEE Std 802.1AB-2005 9.5.9.4"
    ::= { hwLldpRemManAddrEntry 2 }     
    
    hwLldpRemManAddrIfSubtype OBJECT-TYPE
    SYNTAX LldpManAddrIfSubtype
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The enumeration value that identifies the interface numbering
        method used for defining the interface number, associated
        with the remote system."
    REFERENCE
        "IEEE Std 802.1AB-2005 9.5.9.5"
    ::= { hwLldpRemManAddrEntry 3 }    
    
    hwLldpRemManAddrIfId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The integer value used to identify the interface number
        regarding the management address component associated with
        the remote system."
    REFERENCE
        "IEEE Std 802.1AB-2005 9.5.9.6"
    ::= { hwLldpRemManAddrEntry 4 }   
    
    hwLldpRemManAddrOID OBJECT-TYPE
    SYNTAX OBJECT IDENTIFIER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The OID value used to identify the type of hardware component
        or protocol entity associated with the management address
        advertised by the remote system agent."
    REFERENCE
        "IEEE Std 802.1AB-2005 9.5.9.8"
    ::= { hwLldpRemManAddrEntry 5 }     
   hwLldpRemNetworkIdTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwLldpRemNetworkIdEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "LLDP remote neighbour network id table."
        ::= { hwLldpRemoteSystemData  3 }	
   	
	hwLldpRemNetworkIdEntry OBJECT-TYPE
        SYNTAX HwLldpRemNetworkIdEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
           "Entries of the LLDP remote neighbour network id table."
        AUGMENTS  {   lldpRemEntry  }
        ::= { hwLldpRemNetworkIdTable 1}
		
    HwLldpRemNetworkIdEntry ::=
            SEQUENCE  {				  
                      hwLldpRemNetworkId OCTET STRING
                      }
	
    hwLldpRemNetworkId  OBJECT-TYPE
        SYNTAX OCTET STRING
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Network id of the remote neighbour."
        ::= {hwLldpRemNetworkIdEntry 1}
	
   hwLldpInterfaceRemTable  OBJECT-TYPE
      SYNTAX SEQUENCE OF HwLldpInterfaceRemEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
	 	 	"The LLDP remote table."
        ::= { hwLldpInterfaceRemData  1 }
		
   hwLldpInterfaceRemEntry OBJECT-TYPE
      SYNTAX HwLldpInterfaceRemEntry
		MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           	"Entries of the LLDP remote table."
 	    INDEX {
	        hwLldpRemTablesChangeIfIndex
	    }
        ::= { hwLldpInterfaceRemTable 1}  
		
  HwLldpInterfaceRemEntry ::=
	  SEQUENCE  { 
			   hwLldpRemTablesChangeIfIndex InterfaceIndex,
			   hwLldpRemTablesChangeType INTEGER,  
			   hwLldpInterfaceRemAdds Integer32,  
			   hwLldpInterfaceRemDeletes Integer32
			   }

   hwLldpRemTablesChangeIfIndex OBJECT-TYPE 
	  SYNTAX InterfaceIndex
	    MAX-ACCESS not-accessible
	    STATUS current
	    DESCRIPTION
		      "The LLDP neighbors of this interface was changed."   
	    ::= { hwLldpInterfaceRemEntry 1 }  
		
   hwLldpRemTablesChangeType OBJECT-TYPE 
	  SYNTAX INTEGER {
        added(1),
        deleted(2)
        }    
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		      "The change type of LLDP remote tables."   
	    ::= { hwLldpInterfaceRemEntry 2 }  

   hwLldpInterfaceRemAdds OBJECT-TYPE 
	  SYNTAX Integer32
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		      "The number of LLDP neighbors inserted."   
	    ::= { hwLldpInterfaceRemEntry 3 }

   hwLldpInterfaceRemDeletes OBJECT-TYPE 
	  SYNTAX Integer32
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		      "The number of LLDP neighbors deleted."   
	    ::= { hwLldpInterfaceRemEntry 4 }

  hwLldpDdpTrapObjects OBJECT IDENTIFIER ::= { hwLldpObjects 52 }	 
  hwLldpDdpTrapLocalSN OBJECT-TYPE
		SYNTAX OCTET STRING
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpDdpTrapObjects 1 }	
  hwLldpDdpTrapLocalIfindex OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpDdpTrapObjects 2 }
  hwLldpDdpTrapLocalIP OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpDdpTrapObjects 3 }
  hwLldpDdpTrapLocalMAC OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpDdpTrapObjects 4 }
  hwLldpDdpTrapNbrSN OBJECT-TYPE
		SYNTAX OCTET STRING
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpDdpTrapObjects 5 }
hwLldpDdpTrapNbrIfindex OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpDdpTrapObjects 6 }
	hwLldpDdpTrapNbrIP OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpDdpTrapObjects 7 }
	hwLldpDdpTrapNbrMAC OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpDdpTrapObjects 8 }

   	-- define trap VB
	  hwLldpTrapIfName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..64))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Lldp trap message interface name."
			::= { hwLldpTrapObjects 1 } 		   		    		  		  		   		   		
                                
    --- define paramet trap   
    hwLldpTrapParaObjects OBJECT IDENTIFIER ::= { hwLldpObjects 54 }	 
    hwLldpParaTrapLocPortId OBJECT-TYPE
			SYNTAX LldpPortId
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Lldp trap interface name."
		::= { hwLldpTrapParaObjects 1 }	
    hwLldpParaTrapPeerPortId OBJECT-TYPE
		SYNTAX LldpPortId
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpTrapParaObjects 2 }	
    hwLldpParaTrapLocStatus OBJECT-TYPE
		SYNTAX EnabledStatus
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpTrapParaObjects 3 }	
    hwLldpParaTrapLocChassisId OBJECT-TYPE
		SYNTAX LldpChassisId
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpTrapParaObjects 4 }	
    hwLldpParaTrapLocTTL OBJECT-TYPE
    		SYNTAX Integer32
		MAX-ACCESS accessible-for-notify
		STATUS current		
		DESCRIPTION
			"Description."
		::= { hwLldpTrapParaObjects 5 }	
    hwLldpParaTrapLocMngIp OBJECT-TYPE
		SYNTAX LldpManAddress
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpTrapParaObjects 6 }	
    hwLldpParaTrapPeerChassisId OBJECT-TYPE
		SYNTAX LldpChassisId
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpTrapParaObjects 7 }	
    hwLldpParaTrapPeerPortDesc OBJECT-TYPE
		SYNTAX OCTET STRING
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpTrapParaObjects 8 }	
    hwLldpParaTrapPeerSysName OBJECT-TYPE
		SYNTAX OCTET STRING
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpTrapParaObjects 9 }	
    hwLldpParaTrapPeerSysDesc OBJECT-TYPE
		SYNTAX OCTET STRING
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpTrapParaObjects 10 }	
    hwLldpParaTrapPeerSysCap OBJECT-TYPE
		SYNTAX LldpSystemCapabilitiesMap
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpTrapParaObjects 11 }	
    hwLldpParaTrapPeerMngIp OBJECT-TYPE
		SYNTAX LldpManAddress
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
			"Description."
		::= { hwLldpTrapParaObjects 12 }
		                         
                                
  	hwLldpEnabled  NOTIFICATION-TYPE
  	STATUS current	
	DESCRIPTION 
      	"Notify the NMS that the LLDP is globally enabled. This alarm is not 
        restricted by the alarm delay."
	::= { hwLldpTraps 1}

  	hwLldpDisabled  NOTIFICATION-TYPE
 	STATUS current	
	DESCRIPTION 
      	"Notify the NMS that the LLDP is globally disabled. This alarm is not 
        restricted by the alarm delay."
	::= { hwLldpTraps 2}  
	
  hwLldpLocSysCapSupportedChange  NOTIFICATION-TYPE
	OBJECTS {lldpLocSysCapSupported}
	STATUS current	
	DESCRIPTION 
      	"Alarm on the change of capabilities supported of a local device."
   	::= { hwLldpTraps 3}  
	
	hwLldpLocSysCapEnabledChange  NOTIFICATION-TYPE
	OBJECTS {lldpLocSysCapEnabled}
	STATUS current	
	DESCRIPTION 
      	"Alarm on the change of capabilities enabled of a local device."
     ::= { hwLldpTraps 4}                      
                         
  hwLldpLocManIPAddrChange  NOTIFICATION-TYPE
	OBJECTS {hwLldpLocManIPAddr}
	STATUS current	
	DESCRIPTION 
      	"Alarm on the change of management IP address of a local device."
	::= { hwLldpTraps 5} 
	
  hwLldpMdnRemTablesChange  NOTIFICATION-TYPE
	STATUS current	
	DESCRIPTION 
      	"Notify the NMS that the MacAddress discovery neighbor is changed."
	::= { hwLldpTraps 6}	 
	
	hwLldpRateExcessive  NOTIFICATION-TYPE
	OBJECTS { hwLldpTrapIfName }
	STATUS current	
	DESCRIPTION 
      	"Notify the NMS that the received PDU rate has exceeded the threshold."
	::= { hwLldpTraps 7}
	
  hwLldpInterfaceRemTablesChange  NOTIFICATION-TYPE
	OBJECTS {
    hwLldpRemTablesChangeType,
    hwLldpInterfaceRemAdds,
    hwLldpInterfaceRemDeletes
    }
	STATUS current	
	DESCRIPTION 
      	"Notify the NMS that the LLDP neighbor information of the interface was changed."
	::= { hwLldpTraps 8}
 
  hwLldpDdpNotifyDeviceAuthenTrap NOTIFICATION-TYPE
		OBJECTS { hwLldpDdpTrapLocalSN, hwLldpDdpTrapLocalIfindex, hwLldpDdpTrapLocalIP, hwLldpDdpTrapLocalMAC, hwLldpDdpTrapNbrSN, 
			hwLldpDdpTrapNbrIfindex, hwLldpDdpTrapNbrIP, hwLldpDdpTrapNbrMAC }
		STATUS current
		DESCRIPTION 
			"Description."
		::= { hwLldpTraps 9 }	
            
                   
  hwLldpInterfaceParaChange  NOTIFICATION-TYPE
	OBJECTS {
	hwLldpParaTrapLocPortId, hwLldpParaTrapPeerPortId, hwLldpParaTrapLocStatus, hwLldpParaTrapLocChassisId, hwLldpParaTrapLocTTL,
	hwLldpParaTrapLocMngIp, hwLldpParaTrapPeerChassisId, hwLldpParaTrapPeerPortDesc, hwLldpParaTrapPeerSysName, hwLldpParaTrapPeerSysDesc,
    hwLldpParaTrapPeerSysCap, hwLldpParaTrapPeerMngIp }
	STATUS current	
	DESCRIPTION 
      	"Notify the NMS that the LLDP parament of the interface was changed."
	::= { hwLldpTraps 10}
		
  --
	-- ***********************************************************
	--
	-- HAUWEILLDPMIBCONFORMANCE
	--
	-- ***********************************************************
	--
     
    hwLldpCompliances OBJECT IDENTIFIER ::= { hwLldpConformance 1 }
	hwLldpGroups OBJECT IDENTIFIER ::= { hwLldpConformance 2 }
	-- compliance statements
	lldpCompliance MODULE-COMPLIANCE
	STATUS current
	DESCRIPTION
		"The compliance statement for SNMP entities which implement
		the HUAWEI-LLDP-MIB."
	MODULE -- this module
	MANDATORY-GROUPS { 
	hwLldpConfigGroup,
	hwLldpStatsGroup,
	hwLldpPortGroup,
	hwLldpTrapGroup
	}
	::= { hwLldpCompliances 1 }    
	   
	-- MIB groupings
	hwLldpConfigGroup OBJECT-GROUP
	OBJECTS {  
	hwLldpEnable,
	hwLldpLocManIPAddr,
	hwLldpNotificationEnable,
	hwLldpDdpSetFilterType }
	STATUS current
	DESCRIPTION
		"The collection of objects which are used to configure the
		LLDP implementation behavior.
		This group is mandatory for agents which implement the LLDP."
	::= { hwLldpGroups 1 }     
	
	hwLldpStatsGroup OBJECT-GROUP
	OBJECTS {  
	hwLldpCounterReset,
	
	hwLldpPortConfigCounterReset	
	}
	STATUS current
	DESCRIPTION
		"The collection of objects which are used to represent LLDP
		 statistics.
		This group is mandatory for agents which implement the LLDP
		and have the capability of receiving and transmitting LLDP frames."
	::= { hwLldpGroups 2 } 
     
    
    hwLldpPortGroup OBJECT-GROUP
	OBJECTS {  
	hwLldpPortConfigIfIndex ,
	hwLldpRemProtoType
	}
	STATUS current
	DESCRIPTION
		"The collection of objects indicate index of port."
	::= { hwLldpGroups 3 }    
		
   	hwLldpTrapGroup NOTIFICATION-GROUP
	NOTIFICATIONS {  
	hwLldpEnabled,
	hwLldpDisabled,
	hwLldpLocSysCapSupportedChange,
	hwLldpLocSysCapEnabledChange,
	hwLldpLocManIPAddrChange,
	hwLldpMdnRemTablesChange,
	hwLldpRateExcessive,
	hwLldpInterfaceRemTablesChange,
	hwLldpInterfaceParaChange
	}
	STATUS current
	DESCRIPTION
		"The collection of notifications used to indicate HUAWEI-LLDP-MIB
		data consistency and general status information.
		This group is mandatory for agents which implement the LLDP
		and have the capability of receiving LLDP frames."
	::= { hwLldpGroups 4 }  

    hwLldpMdnRemGroup OBJECT-GROUP
	OBJECTS {  
	hwLldpMdnRemLocalPortId,	
	hwLldpMdnRemMacAddr
	}
	STATUS current
	DESCRIPTION
        "The collection of objects which are used to represent
        LLDP MacAddress discovery neighbor remote systems information. 
        The objects represent the information associated with the basic 
        TLV set. Please note that even the agent doesn't implement some 
        of the optional TLVs, it shall recognize all the optional TLV 
        information that the remote system may advertise."
	::= { hwLldpGroups 5 }
	
	hwLldpTrapObjectsGroup OBJECT-GROUP
			OBJECTS { hwLldpTrapIfName }
			STATUS current
			DESCRIPTION 
				"The collection of objects used as trap parameters."
			::= { hwLldpGroups 6 }
			
	hwLldpInterfaceRemGroup OBJECT-GROUP
			OBJECTS {  
			hwLldpRemTablesChangeType,  
			hwLldpInterfaceRemAdds,	
			hwLldpInterfaceRemDeletes
			 }
			STATUS current
			DESCRIPTION 
				"The LLDP remote table."
			::= { hwLldpGroups 7 }

                 hwLldpRemNetworkIdGroup OBJECT-GROUP
			OBJECTS {  
			hwLldpRemNetworkId
			 }
			STATUS current
			DESCRIPTION 
				"The LLDP remote networkId table."
			::= { hwLldpGroups 8 }
			  	
			  	
END
