-- ==================================================================
-- Copyright (C) 2017 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description: HUAWEI-OSPFV3-MIB.mib, The HUAWEI-OSPFV3-MIB provides information about OSPFv3
-- Reference: draft-ietf-ospf-ospfv3-mib-11
-- Version:    V2.19
-- History:
-- ==================================================================

       HUAWEI-OSPFV3-MIB DEFINITIONS ::= BEGIN 
 
    IMPORTS 
            hwDatacomm            
            FROM HUAWEI-MIB  
            
            MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE, mib-2, 
            Counter32, Gauge32, Integer32, Unsigned32 
                    FROM SNMPv2-SMI  
            TEXTUAL-CONVENTION, TruthValue, RowStatus 
                    FROM SNMPv2-TC 
            MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP 
                    FROM SNMPv2-CONF 
            InterfaceIndex 
                    FROM IF-MIB 
            InetAddressType, InetAddress, InetAddressPrefixLength 
                    FROM INET-ADDRESS-MIB 
            Metric, BigMetric, Status,  
            HelloRange, DesignatedRouterPriority 
                    FROM OSPF-MIB; 
    
    hwOspfv3 MODULE-IDENTITY 
            LAST-UPDATED "201708172015Z" 
        ORGANIZATION 
                 "Huawei Technologies Co.,Ltd."
            CONTACT-INFO 
                 "Huawei Industrial Base
                   Bantian, Longgang
                    Shenzhen 518129
                    People's Republic of China
                    Website: http://www.huawei.com
                    Email: support@huawei.com
                  "
             DESCRIPTION 
                 "The MIB module for OSPF version 3. 
                  Copyright (C) The Internet Society (2006). 
                  This version of this MIB module is part of 
                  RFC draft-ietf-ospf-ospfv3-mib-11;  
                  see the RFC itself for full legal 
                  notices." 


            REVISION "201708172015Z"
            DESCRIPTION "modify hwOspfv3PeerFlappingSuppressStatus discription"

            REVISION "201608041521Z"
            DESCRIPTION "Added 		            
	                hwOspfv3DeleteRouteByPurge,
		            hwOspfv3DeleteRouteByPurgeClear,
		            hwOspfv3RouteBeDeletedByPurgeExact,
		            hwOspfv3RouteBeDeletedByPurgeExactClear,
		            hwOspfv3RouteBeDeletedByPurgeInexact,
		            hwOspfv3RouteBeDeletedByPurgeInexactClear,
		            hwOspfv3RouteBeDeletedByPurge,
		            hwOspfv3RouteBeDeletedByPurgeClear,
		            hwOspfv3ThirdPartRouteBeDeletedByPurgeExact,
		            hwOspfv3ThirdPartRouteBeDeletedByPurgeExactClear,
		            hwOspfv3ThirdPartRouteBeDeletedByPurgeInexact,
		            hwOspfv3ThirdPartRouteBeDeletedByPurgeInexactClear,
		            hwOspfv3ThirdPartRouteBeDeletedByPurge,
		            hwOspfv3ThirdPartRouteBeDeletedByPurgeClear " 

            REVISION "201605251110Z"
            DESCRIPTION "Added a trap hwOspfv3GreaterAgeLsaRecived"
            
            REVISION "201605251110Z"
            DESCRIPTION "Added hwOspfv3LsaId to indicates the link-id of recived lsa"
            
            REVISION "201605251110Z"
            DESCRIPTION "Added hwOspfv3LsaAge to indicates the age of recived lsa"                  
                  
	    REVISION "201603231750Z"
            DESCRIPTION "Changed the type of hwOspfv3ProcessId from Integer32 to Unsigned32" 
			    
	    REVISION "201603181750Z"
            DESCRIPTION "Added 
	                    hwOspfv3ImportAseRouteThreshold,
                            hwOspfv3ImportAseRouteThresholdClear,
                            hwOspfv3ImportAseRouteExceed,
                            hwOspfv3ImportAseRouteExceedClear,
                            hwOspfv3ImportNssaRouteThreshold,
                            hwOspfv3ImportNssaRouteThresholdClear,
                            hwOspfv3ImportNssaRouteExceed,
                            hwOspfv3ImportNssaRouteExceedClear" 

            REVISION "201603011750Z"
            DESCRIPTION "Deleted hwOspfv3PeerFlappingSuppressInterval, Added hwOspfv3PeerFlappingSuppressReason to indicates the suppress status change reason, change hwOspfv3PeerFlappingSuppressInterval of hwOspfv3PeerFlappingSuppressStatusChange to hwOspfv3PeerFlappingSuppressReason" 

            REVISION "201603011750Z"
            DESCRIPTION "Modified hwOspfv2PeerFlappingSuppressStatusChange status currentdescription"                   
                  
 						 REVISION "201507081110Z"
             DESCRIPTION "Added hwOspfv3PeerFlappingSuppressStatus to indicates the suppress status of peer flapping" 
 
             REVISION "201505031110Z"
             DESCRIPTION "Added hwOspfv3IntraAreaRouterIdConflictRecovered to indicates process id" 
                              
             REVISION "201504031110Z"
             DESCRIPTION "Added hwOspfv3IntraAreaRouterIdConflictRecovered to indicates the routerid conflict recovered" 
            
             REVISION "200706122100Z" 
             DESCRIPTION -- RFC Editor assigns RFC xxxx 
                 "Initial version, published as RFC xxxx" 
             ::= { hwDatacomm 147 }  
 
    -- Texual conventions 
 
    HWOspfv3UpToRefreshIntervalTc ::= TEXTUAL-CONVENTION 
             DISPLAY-HINT "d" 
             STATUS        current 
             DESCRIPTION 
                "The values one might be able to configure for                  
                variables bounded by the Refresh Interval" 
             SYNTAX      Unsigned32 (0..3600) 
 
    HWOspfv3DeadIntRangeTc ::= TEXTUAL-CONVENTION 
             DISPLAY-HINT "d" 
             STATUS        current 
             DESCRIPTION 
                "The range, in seconds, of dead interval value." 
             SYNTAX      Unsigned32 (0..'FFFF'h) 
    
    HWOspfv3RouterIdTc ::= TEXTUAL-CONVENTION 
             DISPLAY-HINT "d" 
             STATUS      current 
             DESCRIPTION 
                "A 32-bit, unsigned integer uniquely identifying the 
                router in the Autonomous System. To ensure uniqueness, 
                this may default to the value of one of the router's 
                IPv4 host addresses if IPv4 is configured on the 
                router." 
             SYNTAX      Unsigned32 (0..'FFFFFFFF'h) 

    HWOspfv3LsIdTC ::= TEXTUAL-CONVENTION
             DISPLAY-HINT "d"
             STATUS      current
             DESCRIPTION
                  "A unique 32-bit identifier of the piece of the
                  routing domain that is being described by a link
                  state advertisement.  In contrast to OSPFv2, the
                  Link State ID (LSID) has no addressing semantics."
             REFERENCE
                  "OSPF Version 2, Section 12.1.4, Link State ID"
             SYNTAX      Unsigned32 (1..'FFFFFFFF'h)

    HWOspfv3AreaIdTc ::= TEXTUAL-CONVENTION 
             DISPLAY-HINT "d" 
             STATUS      current 
             DESCRIPTION 
                "An OSPFv3 Area Identifier" 
             SYNTAX      Unsigned32 (0..'FFFFFFFF'h) 
 
    HWOspfv3IfInstIdTc ::= TEXTUAL-CONVENTION 
             DISPLAY-HINT "d" 
             STATUS      current 
             DESCRIPTION 
                "An OSPFv3 interface instance ID" 
             SYNTAX      Unsigned32 (0..255) 

    HWOspfv3LsaSequenceTC ::= TEXTUAL-CONVENTION
             DISPLAY-HINT "d"
             STATUS      current
             DESCRIPTION
                "The sequence number field is a signed 32-bit
                integer.  It is used to detect old and duplicate
                link state advertisements.  The space of
                sequence numbers is linearly ordered.  The
                larger the sequence number, the more recent the
                advertisement."
             REFERENCE
                "OSPF Version 2, Section 12.1.6, LS sequence
                number"
             SYNTAX      Integer32
             
    HWOspfv3LsaAgeTC ::= TEXTUAL-CONVENTION
             DISPLAY-HINT "d"
             STATUS      current
             DESCRIPTION
                "The age of the link state advertisement in
                seconds.  The high-order bit of the LS age
                field is considered the DoNotAge bit for
                support of on-demand circuits."
             REFERENCE
                "OSPF Version 2, Section 12.1.1, LS age;
                 Extending OSPF to Support Demand Circuits,
                 Section 2.2, The LS age field"
             SYNTAX      Unsigned32 (0..3600 | 32768..36368)             

   HWHelloRange ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                "The range of intervals on which hello messages are
                exchanged."
            SYNTAX Integer32 (0..65535)

    
 
    -- Top-level structure of MIB 
    hwOspfv3Notifications  OBJECT IDENTIFIER ::= { hwOspfv3 0 } 
    hwOspfv3Objects        OBJECT IDENTIFIER ::= { hwOspfv3 1 } 
    hwOspfv3Conformance    OBJECT IDENTIFIER ::= { hwOspfv3 2 } 
 
    -- OSPFv3 General Variables 
 
    -- These parameters apply globally to the Router's 
    -- OSPFv3 Process. 
 
    hwOspfv3GeneralGroup OBJECT IDENTIFIER ::= { hwOspfv3Objects 1 } 
 
    hwOspfv3RouterId OBJECT-TYPE 
            SYNTAX         HWOspfv3RouterIdTc 
            MAX-ACCESS     read-write 
            STATUS         current  
            DESCRIPTION 
                "A 32-bit integer uniquely identifying the 
                router in the Autonomous System. To ensure 
                uniqueness, this may default to the value of 
                one of the router's IPv4 host addresses, 
                represented as a 32-bit unsigned integer, 
                if IPv4 is configured on the router." 
            ::= { hwOspfv3GeneralGroup 1 } 
 
    hwOspfv3AdminStatus OBJECT-TYPE 
            SYNTAX          Status 
            MAX-ACCESS      read-write 
            STATUS          current 
            DESCRIPTION 
                "The administrative status of OSPFv3 in the 
                router. The value 'enabled' denotes that the 
                OSPFv3 Process is active on at least one 
                interface; 'disabled' disables it on all 
                interfaces." 
            ::= { hwOspfv3GeneralGroup 2 } 
 
    hwOspfv3VersionNumber OBJECT-TYPE 
            SYNTAX          INTEGER { version3 (3) } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The version number of OSPF for IPv6 is 3." 
            ::= { hwOspfv3GeneralGroup 3 } 
 
    hwOspfv3AreaBdrRtrStatus OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "A flag to note whether this router is an area 
                border router." 
            REFERENCE 
                "OSPF Version 2, Section 3 Splitting the AS into 
                Areas" 
            ::= { hwOspfv3GeneralGroup 4 } 
 
    hwOspfv3AsBdrRtrStatus OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-write 
            STATUS          current 
            DESCRIPTION 
                "A flag to note whether this router is  
                configured as an Autonomous System border router." 
            REFERENCE 
                "OSPF Version 2, Section 3.3 Classification of 
                routers" 
            ::= { hwOspfv3GeneralGroup 5 } 

    hwOspfv3AsScopeLsaCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of AS-Scope (e.g. AS-External) link state 
                advertisements in the link state database." 
            ::= { hwOspfv3GeneralGroup 6 } 
 
    hwOspfv3AsScopeLsaCksumSum OBJECT-TYPE 
            SYNTAX          Unsigned32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit unsigned sum of the LS checksums of 
                the AS-scoped link state advertisements  
                contained in the link state database. This sum 
                can be used to determine if there has been a 
                change in a router's link state database, and 
                to compare the link state database of two 
                routers." 
            ::= { hwOspfv3GeneralGroup 7 } 
 
    hwOspfv3OriginateNewLsas OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of new link-state advertisements 
                that have been originated. This number is 
                incremented each time the router originates a new 
                LSA." 
            ::= { hwOspfv3GeneralGroup 8 } 
 
    hwOspfv3RxNewLsas OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of link state advertisements  
                received determined to be new instantiations. 
                This number does not include newer  
                instantiations of self-originated link state 
                advertisements." 
            ::= { hwOspfv3GeneralGroup 9 } 
 
    hwOspfv3ExtLsaCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of AS-Scope External(LS type 0x4005) link state 
                advertisements in the link state database" 

            ::= { hwOspfv3GeneralGroup 10 } 
 
 
    hwOspfv3ExtAreaLsdbLimit OBJECT-TYPE 
            SYNTAX          Integer32 (-1..'7FFFFFFF'h) 
            MAX-ACCESS      read-write 
            STATUS          current 
            DESCRIPTION 
                "The maximum number of non-default  
                AS-external-LSAs entries that can be stored in the 
                link state database. If the value is -1, then 
                there is no limit. 
 
                When the number of non-default AS-external-LSAs 
                in a router's link-state database reaches 
                ospfv3ExtAreaLsdbLimit, the router enters Overflow 
                state. The router never holds more than 
                ospfv3ExtAreaLsdbLimit non-default AS-external-LSAs 
                in its database. Ospfv3ExtAreaLsdbLimit MUST be set 
                identically in all routers attached to the OSPFv3 
                backbone and/or any regular OSPFv3 area. (i.e., 
                OSPFv3 stub areas and NSSAs are excluded)." 
            ::= { hwOspfv3GeneralGroup 11 } 
 
  hwOspfv3RestartSupport OBJECT-TYPE  
           SYNTAX       INTEGER { none (1),  
                                  plannedOnly (2),  
                                  plannedAndUnplanned (3)  
                             } 
           MAX-ACCESS   read-write  
           STATUS       current  
           DESCRIPTION  
              "The router's support for OSPFv3 Graceful restart.  
              Options include: no restart support, only planned  
              restarts or both planned and unplanned restarts."  
           ::= { hwOspfv3GeneralGroup 12 }  
        
    hwOspfv3RestartInterval OBJECT-TYPE  
           SYNTAX       HWOspfv3UpToRefreshIntervalTc 
           UNITS        "seconds"  
           MAX-ACCESS   read-write  
           STATUS       current  
           DESCRIPTION  
              "Configured OSPFv3 Graceful restart timeout interval."  
           ::= { hwOspfv3GeneralGroup 13 }  
        
    hwOspfv3RestartStatus OBJECT-TYPE  
           SYNTAX       INTEGER { notRestarting (1),  
                                  plannedRestart (2),  
                                  unplannedRestart (3)  
                                }  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "The current status of OSPFv3 Graceful restart capability."  
           ::= { hwOspfv3GeneralGroup 14 }  
        
    hwOspfv3RestartAge OBJECT-TYPE  
           SYNTAX       HWOspfv3UpToRefreshIntervalTc 
           UNITS        "seconds"  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Remaining time in current OSPFv3 Graceful restart  
              interval."  
           ::= { hwOspfv3GeneralGroup 15 }  
        
    hwOspfv3RestartExitRc OBJECT-TYPE  
           SYNTAX       INTEGER { none (1),  
                                  inProgress (2),  
                                  completed (3), 
                                  timedOut (4), 
                                  topologyChanged (5) 
                                }  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Describes the outcome of the last attempt at a  
              Graceful restart. 
     
              none:............no restart has yet been attempted. 
              inProgress:......a restart attempt is currently underway. 
              completed:.......the last restart completed successfully. 
              timedOut:........the last restart timed out. 
              topologyChanged:.the last restart was aborted due to 
                               a topology change."  
        ::= { hwOspfv3GeneralGroup 16 } 
 
    hwOspfv3NotificationEnable OBJECT-TYPE 
           SYNTAX TruthValue 
           MAX-ACCESS read-write 
           STATUS current 
           DESCRIPTION 
               "If this object is set to true(1), then it enables 
                the generation of OSPFv3 Notifications. If it is 
                set to false(2), these notifications are not 
                generated. 
    
                Configured values MUST survive an agent reboot." 
       ::= { hwOspfv3GeneralGroup 17 } 
 
    hwOspfv3ReferenceBandwidth OBJECT-TYPE   
           SYNTAX       Unsigned32 
           MAX-ACCESS   read-write  
           STATUS       current  
           DESCRIPTION
               "Reference bandwidth in kilobits per second for
               calculating default interface metrics.  The
               default value is 100,000 KBPS (100 MBPS).

               This object is persistent, and when written, the
               entity SHOULD save the change to non-volatile
               storage."
           DEFVAL { 100000 }    
           ::= { hwOspfv3GeneralGroup 18 }

    -- The OSPFv3 Area Data Structure contains information 
    -- regarding the various areas. The interfaces and 
    -- virtual links are configured as part of these areas. 
    -- Area 0, by definition, is the Backbone Area 
 
    hwOspfv3AreaTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF HwOspfv3AreaEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Information describing the configured  
                parameters and cumulative statistics of the router's 
                attached areas." 
            REFERENCE 
                "OSPF Version 2, Section 6 The Area Data  
                Structure" 
            ::= { hwOspfv3Objects 2 } 
 
    hwOspfv3AreaEntry OBJECT-TYPE 
            SYNTAX          HwOspfv3AreaEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Information describing the configured  
                parameters and cumulative statistics of one of the 
                router's attached areas." 
            INDEX           { hwOspfv3AreaId } 
            ::= { hwOspfv3AreaTable 1 } 
 
    HwOspfv3AreaEntry ::= SEQUENCE { 
            hwOspfv3AreaId 
                    HWOspfv3AreaIdTc, 
            hwOspfv3AreaImportAsExtern 
                    INTEGER, 
            hwOspfv3AreaSpfRuns 
                    Counter32, 
            hwOspfv3AreaBdrRtrCount 
                    Gauge32, 
            hwOspfv3AreaAsBdrRtrCount 
                    Gauge32, 
            hwOspfv3AreaScopeLsaCount 
                    Gauge32, 
            hwOspfv3AreaScopeLsaCksumSum 
                    Unsigned32, 
            hwOspfv3AreaSummary 
                    INTEGER, 
            hwOspfv3AreaRowStatus 
                    RowStatus, 
            hwOspfv3AreaStubMetric 
                    BigMetric,
            hwOspfv3AreaNssaTranslatorRole
                    INTEGER,
            hwOspfv3AreaNssaTranslatorState
                    INTEGER,
            hwOspfv3AreaNssaTranslatorStabInterval
                    Unsigned32,
            hwOspfv3AreaNssaTranslatorEvents
                    Counter32
             } 
 
    hwOspfv3AreaId OBJECT-TYPE 
            SYNTAX          HWOspfv3AreaIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A 32-bit integer uniquely identifying an area. 
                Area ID 0 is used for the OSPFv3 backbone." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            ::= { hwOspfv3AreaEntry 1 } 
 
    hwOspfv3AreaImportAsExtern OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            importExternal(1),   -- normal area 
                            importNoExternal(2), -- stub area 
                            importNssa(3)        -- not-so-stubby-area 
                            } 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether an area is a Stub area, NSSA, or 
                standard area. AS-scope LSAs are not imported into Stub 
                Areas or NSSAs. NSSAs import AS-External data as NSSA 
                LSAs which have Area-scope" 
            REFERENCE  
                "OSPF Version 2, Appendix C.2 Area parameters" 
            DEFVAL { importExternal } 
            ::= { hwOspfv3AreaEntry 2 } 
 
    hwOspfv3AreaSpfRuns OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of times that the intra-area route 
                table has been calculated using this area's 
                link state database. This is typically done 
                using Dijkstra's algorithm." 
            ::= { hwOspfv3AreaEntry 3 } 
 
    hwOspfv3AreaBdrRtrCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The total number of area border routers 
                reachable within this area. This is initially zero, 
                and is calculated in each SPF Pass." 
            DEFVAL { 0 } 
            ::= { hwOspfv3AreaEntry 4 } 
 
    hwOspfv3AreaAsBdrRtrCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The total number of Autonomous System border 
                routers reachable within this area. This is 
                initially zero, and is calculated in each SPF 
                Pass." 
            DEFVAL { 0 }               
            ::= { hwOspfv3AreaEntry 5 } 
 
    hwOspfv3AreaScopeLsaCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The total number of Area-Scope link state  
                advertisements in this area's link state  
                database." 
             DEFVAL { 0 }                 
            ::= { hwOspfv3AreaEntry 6 } 
 
    hwOspfv3AreaScopeLsaCksumSum OBJECT-TYPE 
            SYNTAX          Unsigned32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit unsigned sum of the Area-Scope link state 
                advertisements' LS checksums contained in this 
                area's link state database. The sum can be used 
                to determine if there has been a change in a 
                router's link state database, and to compare the 
                link-state database of two routers." 
            ::= { hwOspfv3AreaEntry 7 } 
 
    hwOspfv3AreaSummary OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            noAreaSummary(1), 
                            sendAreaSummary(2) 
                            } 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The variable ospfv3AreaSummary controls the 
                import of Inter-Area LSAs into stub and 
                NSSA areas. It has no effect on other areas. 
 
                If it is noAreaSummary, the router will neither 
                originate nor propagate Inter-Area LSAs into the 
                stub or NSSA area. It will rely entirely on its 
                default route. 
 
                If it is sendAreaSummary, the router will both 
                summarize and propagate Inter-Area LSAs." 
            DEFVAL   { sendAreaSummary } 
            ::= { hwOspfv3AreaEntry 8 } 
 
    hwOspfv3AreaRowStatus OBJECT-TYPE 
            SYNTAX          RowStatus 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This object permits management of the table by 
                facilitating actions such as row creation, 
                construction and destruction. 
 
                The value of this object has no effect on 
                whether other objects in this conceptual row can be 
                modified." 
            ::= { hwOspfv3AreaEntry 9 } 
 
    hwOspfv3AreaStubMetric OBJECT-TYPE 
            SYNTAX          BigMetric 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The metric value advertised for the default route 
                 into Stub and NSSA areas." 
            ::= { hwOspfv3AreaEntry 10 } 
 
    hwOspfv3AreaNssaTranslatorRole OBJECT-TYPE
            SYNTAX          INTEGER { always(1), candidate(2) }
            MAX-ACCESS      read-create
            STATUS          current
            DESCRIPTION
                "Indicates an NSSA border router's policy to
                perform NSSA translation of NSSA-LSAs into
                AS-External-LSAs."
            DEFVAL { candidate }
            ::= { hwOspfv3AreaEntry 11 }
            
    hwOspfv3AreaNssaTranslatorState OBJECT-TYPE
            SYNTAX          INTEGER {
                            enabled(1),
                            elected(2),
                            disabled(3)
                            }
            MAX-ACCESS      read-only
            STATUS          current
            DESCRIPTION
                 "Indicates if and how an NSSA border router is
                 performing NSSA translation of NSSA-LSAs into
                 AS-External-LSAs.  When this object is set to
                 'enabled', the NSSA border router's
                 ospfv3AreaNssaTranslatorRole has been set to 'always'.
                 When this object is set to 'elected', a candidate
                 NSSA border router is translating NSSA-LSAs into
                 AS-External-LSAs.  When this object is set to
                 'disabled', a candidate NSSA Border router is NOT
                 translating NSSA-LSAs into AS-External-LSAs."
            ::= { hwOspfv3AreaEntry 12 }
            
    hwOspfv3AreaNssaTranslatorStabInterval OBJECT-TYPE 
            SYNTAX          Unsigned32 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION
                "The stability interval defined as the number of
                seconds after an elected translator determines its
                services are no longer required that it should
                continue to perform its translation duties."
            DEFVAL { 40 }
            ::= { hwOspfv3AreaEntry 13 }
            
    hwOspfv3AreaNssaTranslatorEvents OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION
                "Indicates the number of Translator state changes
                that have occurred since the last start-up of the
                OSPFv3 routing process.

                Discontinuities in the value of this counter
                can occur at re-initialization of the management
                system and at other times as indicated by the
                value of ospfv3DiscontinuityTime."
            ::= { hwOspfv3AreaEntry 14 }
            
    -- OSPFv3 AS-Scope Link State Database 
    -- The Link State Database contains the AS-Scope Link State 
    -- Advertisements from throughout the areas that the 
    -- device is attached to. 
 
    hwOspfv3AsLsdbTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF HwOspfv3AsLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Process's AS-Scope Link State Database." 
            ::= { hwOspfv3Objects 3 } 
 
    hwOspfv3AsLsdbEntry OBJECT-TYPE 
            SYNTAX          HwOspfv3AsLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A single AS-Scope Link State Advertisement." 
            INDEX           { hwOspfv3AsLsdbType, 
                              hwOspfv3AsLsdbRouterId, 
                              hwOspfv3AsLsdbLsId } 
            ::= { hwOspfv3AsLsdbTable 1 } 
 
    HwOspfv3AsLsdbEntry ::= SEQUENCE { 
            hwOspfv3AsLsdbType 
                    Unsigned32, 
            hwOspfv3AsLsdbRouterId 
                    HWOspfv3RouterIdTc, 
            hwOspfv3AsLsdbLsId 
                    Unsigned32, 
            hwOspfv3AsLsdbSequence 
                    HWOspfv3LsaSequenceTC,
            hwOspfv3AsLsdbAge 
                    HWOspfv3LsaAgeTC,
            hwOspfv3AsLsdbChecksum 
                    Integer32, 
            hwOspfv3AsLsdbAdvertisement 
                    OCTET STRING, 
            hwOspfv3AsLsdbTypeKnown 
                    TruthValue 
            } 
 
    hwOspfv3AsLsdbType OBJECT-TYPE 
            SYNTAX          Unsigned32(0..'FFFFFFFF'h) 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The type of the link state advertisement. 
                Each link state type has a separate  
                advertisement format. AS-Scope LSAs not recognized 
                by the router may be stored in the database." 
            ::= { hwOspfv3AsLsdbEntry 1 } 
 
    hwOspfv3AsLsdbRouterId OBJECT-TYPE 
            SYNTAX          HWOspfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The 32 bit number that uniquely identifies the 
                originating router in the Autonomous System." 
            REFERENCE 
                "OSPF Version 2, Appendix C.1 Global parameters" 
            ::= { hwOspfv3AsLsdbEntry 2 } 
 
    hwOspfv3AsLsdbLsId OBJECT-TYPE 
            SYNTAX          Unsigned32 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Link State ID is an LS Type Specific field 
                containing a unique identifier; 
                it identifies the piece of the routing domain 
                that is being described by the advertisement. 
                In contrast to OSPFv2, the LSID has no 
                addressing semantics." 
            ::= { hwOspfv3AsLsdbEntry 3 } 
 
    -- Note that the OSPF Sequence Number is a 32 bit signed 
    -- integer. It starts with the value '80000001'h, 
    -- or -'7FFFFFFF'h, and increments until '7FFFFFFF'h 
    -- Thus, a typical sequence number will be very negative. 
 
    hwOspfv3AsLsdbSequence OBJECT-TYPE 
            SYNTAX          HWOspfv3LsaSequenceTC
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The sequence number field is a signed 32-bit 
                integer. It is used to detect old and duplicate 
                link state advertisements. The space of 
                sequence numbers is linearly ordered. The 
                larger the sequence number the more recent the 
                advertisement."  
            REFERENCE 
                "OSPF Version  2,  Section  12.1.6  LS  sequence 
                number" 
            ::= { hwOspfv3AsLsdbEntry 4 } 
 
    hwOspfv3AsLsdbAge OBJECT-TYPE 
            SYNTAX          HWOspfv3LsaAgeTC -- Should be 0..MaxAge 
                                           -- unless DoNotAge bit is set 
            UNITS           "seconds" 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the age of the link state  
                advertisement in seconds." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.1 LS age" 
            ::= { hwOspfv3AsLsdbEntry 5 } 
 
    hwOspfv3AsLsdbChecksum OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the checksum of the complete 
                contents of the advertisement, excepting the 
                age field. The age field is excepted so that 
                an advertisement's age can be incremented 
                without updating the checksum. The checksum 
                used is the same that is used for ISO 
                connectionless datagrams; it is commonly 
                referred to as the Fletcher checksum." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.7 LS checksum" 
            ::= { hwOspfv3AsLsdbEntry 6 } 
 
    hwOspfv3AsLsdbAdvertisement OBJECT-TYPE 
            SYNTAX          OCTET STRING (SIZE (1..65535)) 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The entire Link State Advertisement, including 
                its header." 
            ::= { hwOspfv3AsLsdbEntry 7 } 
 
    hwOspfv3AsLsdbTypeKnown OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether the LSA type is recognized by 
                this Router." 
            ::= { hwOspfv3AsLsdbEntry 8 } 

    -- OSPFv3 Area-Scope Link State Database 
 
    -- The Link State Database contains the Area-Scope Link State 
    -- Advertisements from throughout the area that the 
    -- device is attached to. 
 
    hwOspfv3AreaLsdbTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF HwOspfv3AreaLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Process's Area-Scope Link State Database." 
            ::= { hwOspfv3Objects 4 } 
 
    hwOspfv3AreaLsdbEntry OBJECT-TYPE 
            SYNTAX          HwOspfv3AreaLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A single Area-Scope Link State Advertisement." 
            INDEX           { hwOspfv3AreaLsdbAreaId, 
                              hwOspfv3AreaLsdbType, 
                              hwOspfv3AreaLsdbRouterId, 
                              hwOspfv3AreaLsdbLsId } 
            ::= { hwOspfv3AreaLsdbTable 1 } 
 
    HwOspfv3AreaLsdbEntry ::= SEQUENCE { 
            hwOspfv3AreaLsdbAreaId 
                    HWOspfv3AreaIdTc, 
            hwOspfv3AreaLsdbType 
                    Unsigned32, 
            hwOspfv3AreaLsdbRouterId 
                    HWOspfv3RouterIdTc, 
            hwOspfv3AreaLsdbLsId 
                    Unsigned32, 
            hwOspfv3AreaLsdbSequence 
                    HWOspfv3LsaSequenceTC,
            hwOspfv3AreaLsdbAge 
                    HWOspfv3LsaAgeTC,
            hwOspfv3AreaLsdbChecksum 
                    Integer32, 
            hwOspfv3AreaLsdbAdvertisement 
                    OCTET STRING, 
            hwOspfv3AreaLsdbTypeKnown 
                    TruthValue 
            } 
 
    hwOspfv3AreaLsdbAreaId OBJECT-TYPE 
            SYNTAX          HWOspfv3AreaIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit identifier of the Area from which the 
                LSA was received." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            ::= { hwOspfv3AreaLsdbEntry 1 } 
 
    hwOspfv3AreaLsdbType OBJECT-TYPE 
            SYNTAX          Unsigned32(0..'FFFFFFFF'h) 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The type of the link state advertisement. 
                Each link state type has a separate 
                advertisement format. Area-Scope LSAs unrecognized 
                by the router are also stored in this database." 
            ::= { hwOspfv3AreaLsdbEntry 2 } 
 
    hwOspfv3AreaLsdbRouterId OBJECT-TYPE 
            SYNTAX          HWOspfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit number that uniquely identifies the 
                originating router in the Autonomous System." 
            REFERENCE 
                "OSPF Version 2, Appendix C.1 Global parameters" 
            ::= { hwOspfv3AreaLsdbEntry 3 } 
 
    hwOspfv3AreaLsdbLsId OBJECT-TYPE 
            SYNTAX          Unsigned32 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Link State ID is an LS Type Specific field 
                containing a unique identifier; 
                it identifies the piece of the routing domain 
                that is being described by the advertisement. 
                In contrast to OSPFv2, the LSID has no 
                addressing semantics." 
            ::= { hwOspfv3AreaLsdbEntry 4 } 
 
    -- Note that the OSPF Sequence Number is a 32 bit signed 
    -- integer.  It starts with the value '80000001'h, 
    -- or -'7FFFFFFF'h, and increments until '7FFFFFFF'h 
    -- Thus, a typical sequence number will be very negative. 
 
    hwOspfv3AreaLsdbSequence OBJECT-TYPE 
            SYNTAX          HWOspfv3LsaSequenceTC
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The sequence number field is a signed 32-bit 
                integer. It is used to detect old and  
                duplicate link state advertisements. The space 
                of sequence numbers is linearly ordered. The 
                larger the sequence number the more recent the 
                advertisement." 
            REFERENCE 
                "OSPF Version  2,  Section  12.1.6  LS  sequence 
                number" 
            ::= { hwOspfv3AreaLsdbEntry 5 } 
 
    hwOspfv3AreaLsdbAge OBJECT-TYPE 
            SYNTAX          HWOspfv3LsaAgeTC -- Should be 0..MaxAge 
                                           -- unless DoNotAge bit is set 
            UNITS           "seconds" 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the age of the link state 
                advertisement in seconds." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.1 LS age" 
            ::= { hwOspfv3AreaLsdbEntry 6 } 
 
    hwOspfv3AreaLsdbChecksum OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the checksum of the complete 
                contents of the advertisement, excepting the 
                age field. The age field is excepted so that 
                an advertisement's age can be incremented 
                without updating the checksum. The checksum 
                used is the same that is used for ISO  
                connectionless datagrams; it is commonly 
                referred to as the Fletcher checksum." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.7 LS checksum" 
            ::= { hwOspfv3AreaLsdbEntry 7 } 
 
    hwOspfv3AreaLsdbAdvertisement OBJECT-TYPE 
            SYNTAX          OCTET STRING (SIZE (1..65535)) 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The entire Link State Advertisement, including 
                its header." 
            ::= { hwOspfv3AreaLsdbEntry 8 } 
 
    hwOspfv3AreaLsdbTypeKnown OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether the LSA type is recognized 
                by this Router." 
            ::= { hwOspfv3AreaLsdbEntry 9 } 
 
    -- OSPFv3 Link-Scope Link State Database 
 
    -- The Link State Database contains the Link-Scope Link State 
    -- Advertisements from the links that the 
    -- device is attached to. 
 
    hwOspfv3LinkLsdbTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF HwOspfv3LinkLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Process's Link-Scope Link State Database." 
            ::= { hwOspfv3Objects 5 } 
 
    hwOspfv3LinkLsdbEntry OBJECT-TYPE 
            SYNTAX          HwOspfv3LinkLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A single Link-Scope Link State Advertisement." 
            INDEX           { hwOspfv3LinkLsdbIfIndex, 
                              hwOspfv3LinkLsdbIfInstId, 
                              hwOspfv3LinkLsdbType, 
                              hwOspfv3LinkLsdbRouterId, 
                              hwOspfv3LinkLsdbLsId } 
            ::= { hwOspfv3LinkLsdbTable 1 } 
 
    HwOspfv3LinkLsdbEntry ::= SEQUENCE { 
            hwOspfv3LinkLsdbIfIndex 
                    InterfaceIndex,
            hwOspfv3LinkLsdbIfInstId 
                    HWOspfv3IfInstIdTc, 
            hwOspfv3LinkLsdbType 
                    Unsigned32, 
            hwOspfv3LinkLsdbRouterId 
                    HWOspfv3RouterIdTc, 
            hwOspfv3LinkLsdbLsId 
                    HWOspfv3LsIdTC,
            hwOspfv3LinkLsdbSequence 
                    HWOspfv3LsaSequenceTC,
            hwOspfv3LinkLsdbAge 
                    HWOspfv3LsaAgeTC,
            hwOspfv3LinkLsdbChecksum 
                    Integer32, 
            hwOspfv3LinkLsdbAdvertisement 
                    OCTET STRING, 
            hwOspfv3LinkLsdbTypeKnown 
                    TruthValue 
            } 

    hwOspfv3LinkLsdbIfIndex OBJECT-TYPE 
            SYNTAX         InterfaceIndex
            MAX-ACCESS     not-accessible 
            STATUS         current 
            DESCRIPTION 
                "The identifier of the link from which the LSA 
                was received." 
            ::= { hwOspfv3LinkLsdbEntry 1 } 
 
    hwOspfv3LinkLsdbIfInstId OBJECT-TYPE 
            SYNTAX         HWOspfv3IfInstIdTc 
            MAX-ACCESS     not-accessible 
            STATUS         current 
            DESCRIPTION 
                "The identifier of the interface instance from 
                which the LSA was received." 
            ::= { hwOspfv3LinkLsdbEntry 2 } 
 
    hwOspfv3LinkLsdbType OBJECT-TYPE 
            SYNTAX          Unsigned32(0..'FFFFFFFF'h) 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The type of the link state advertisement. 
                Each link state type has a separate 
                advertisement format. Link-Scope LSAs unrecognized 
                by the router are also stored in this database." 
            ::= { hwOspfv3LinkLsdbEntry 3 } 
 
    hwOspfv3LinkLsdbRouterId OBJECT-TYPE 
            SYNTAX          HWOspfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The 32 bit number that uniquely identifies the 
                originating router in the Autonomous System." 
            REFERENCE 
                "OSPF Version 2, Appendix C.1 Global parameters" 
            ::= { hwOspfv3LinkLsdbEntry 4 } 
 
    hwOspfv3LinkLsdbLsId OBJECT-TYPE 
            SYNTAX        HWOspfv3LsIdTC
            MAX-ACCESS    not-accessible 
            STATUS        current 
            DESCRIPTION 
                "The Link State ID is an LS Type Specific field 
                containing a unique identifier; 
                it identifies the piece of the routing domain 
                that is being described by the advertisement. 
                In contrast to OSPFv2, the LSID has no 
                addressing semantics." 
            ::= { hwOspfv3LinkLsdbEntry 5 } 

    -- Note that the OSPF Sequence Number is a 32 bit signed 
    -- integer.  It starts with the value '80000001'h, 
    -- or -'7FFFFFFF'h, and increments until '7FFFFFFF'h 
    -- Thus, a typical sequence number will be very negative. 
 
    hwOspfv3LinkLsdbSequence OBJECT-TYPE 
            SYNTAX          HWOspfv3LsaSequenceTC
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The sequence number field is a signed 32-bit 
                integer. It is used to detect old and duplicate 
                link state advertisements. The space of 
                sequence numbers is linearly ordered. The 
                larger the sequence number the more recent the 
                advertisement." 
            REFERENCE 
                "OSPF Version  2,  Section  12.1.6  LS  sequence 
                number" 
            ::= { hwOspfv3LinkLsdbEntry 6 } 
 
    hwOspfv3LinkLsdbAge OBJECT-TYPE 
            SYNTAX          HWOspfv3LsaAgeTC -- Should be 0..MaxAge 
                                             -- unless DoNotAge bit is set 
            UNITS           "seconds" 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the age of the link state 
                advertisement in seconds." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.1 LS age" 
            ::= { hwOspfv3LinkLsdbEntry 7 } 
 
    hwOspfv3LinkLsdbChecksum OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the checksum of the complete 
                contents of the advertisement, excepting the 
                age field. The age field is excepted so that 
                an advertisement's age can be incremented 
                without updating the checksum. The checksum 
                used is the same that is used for ISO 
                connectionless datagrams; it is commonly 
                referred to as the Fletcher checksum." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.7 LS checksum" 
            ::= { hwOspfv3LinkLsdbEntry 8 } 
 
    hwOspfv3LinkLsdbAdvertisement OBJECT-TYPE 
            SYNTAX          OCTET STRING (SIZE (1..65535)) 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The entire Link State Advertisement, including 
                its header." 
            ::= { hwOspfv3LinkLsdbEntry 9 } 
 
    hwOspfv3LinkLsdbTypeKnown OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether the LSA type is recognized by this 
                 Router." 
            ::= { hwOspfv3LinkLsdbEntry 10 } 
 
 
 
 
    -- OSPFv3 Interface Table 
 
    hwOspfv3IfTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF HwOspfv3IfEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Interface Table describes the  
                interfaces from the viewpoint of OSPFv3." 
            REFERENCE 
                "OSPF Version 2, Appendix C.3 Router interface 
                parameters" 
            ::= { hwOspfv3Objects 6 } 
 
    hwOspfv3IfEntry OBJECT-TYPE 
            SYNTAX          HwOspfv3IfEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Interface Entry describes one 
                interface from the viewpoint of OSPFv3." 
            INDEX           { hwOspfv3IfIndex, 
                              hwOspfv3IfInstId } 
            ::= { hwOspfv3IfTable 1 } 
 
 
    HwOspfv3IfEntry ::= SEQUENCE { 
            hwOspfv3IfIndex 
                    InterfaceIndex, 
            hwOspfv3IfInstId 
                    HWOspfv3IfInstIdTc, 
            hwOspfv3IfAreaId 
                    HWOspfv3AreaIdTc, 
            hwOspfv3IfType 
                    INTEGER, 
            hwOspfv3IfAdminStatus 
                    Status, 
            hwOspfv3IfRtrPriority 
                    DesignatedRouterPriority, 
            hwOspfv3IfTransitDelay 
                    HWOspfv3UpToRefreshIntervalTc, 
            hwOspfv3IfRetransInterval 
                    HWOspfv3UpToRefreshIntervalTc, 
            hwOspfv3IfHelloInterval 
                    HWHelloRange, 
            hwOspfv3IfRtrDeadInterval 
                     HWOspfv3DeadIntRangeTc, 
            hwOspfv3IfState 
                    INTEGER, 
            hwOspfv3IfDesignatedRouter 
                    HWOspfv3RouterIdTc, 
            hwOspfv3IfBackupDesignatedRouter 
                    HWOspfv3RouterIdTc, 
            hwOspfv3IfEvents 
                    Counter32, 
            hwOspfv3IfRowStatus 
                    RowStatus, 
            hwOspfv3IfMetricValue 
                    Metric, 
            hwOspfv3IfLinkScopeLsaCount 
                    Gauge32, 
            hwOspfv3IfLinkLsaCksumSum 
                    Unsigned32,
            hwOspfv3IfPollInterval 
                    Unsigned32,
            hwOspfv3IfMulticastForwarding 
                    INTEGER
            } 
 
    hwOspfv3IfIndex OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The interface index of this OSPFv3 interface. 
                 It corresponds to the interface index of the 
                 IPv6 interface on which OSPFv3 is configured." 
            ::= { hwOspfv3IfEntry 1 } 
 
    hwOspfv3IfInstId OBJECT-TYPE 
            SYNTAX          HWOspfv3IfInstIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Enables multiple interface instances of OSPFv3 
                to be run over a single link. Each protocol 
                instance would be assigned a separate ID. This ID 
                has local link significance only." 
            ::= { hwOspfv3IfEntry 2 } 
 
    hwOspfv3IfAreaId OBJECT-TYPE 
            SYNTAX          HWOspfv3AreaIdTc 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "A 32-bit integer uniquely identifying the area 
                to which the interface connects. Area ID 
                0 is used for the OSPFv3 backbone." 
            DEFVAL          { 0 } 
            ::= { hwOspfv3IfEntry 3 } 
 
    hwOspfv3IfType OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            broadcast(1), 
                            nbma(2), 
                            pointToPoint(3), 
                            loopback(4),
                            pointToMultipoint(5),
                            p2mpNonbroadcast(6) 
                            } 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 interface type." 
            ::= { hwOspfv3IfEntry 4 } 
 
    hwOspfv3IfAdminStatus OBJECT-TYPE 
            SYNTAX          Status 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 interface's administrative status. 
                The value formed on the interface, and the 
                interface will be advertised as an internal route 
                to some area. The value 'disabled' denotes 
                that the interface is external to OSPFv3." 
            DEFVAL          { enabled } 
            ::= { hwOspfv3IfEntry 5 } 
 
    hwOspfv3IfRtrPriority OBJECT-TYPE 
            SYNTAX          DesignatedRouterPriority 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The priority of this interface. Used in 
                multi-access networks, this field is used in 
                the designated router election algorithm. The 
                value 0 signifies that the router is not  
                eligible to become the designated router on this 
                particular network. In the event of a tie in 
                this value, routers will use their Router ID as 
                a tie breaker." 
            DEFVAL          { 1 } 
            ::= { hwOspfv3IfEntry 6 } 
 
    hwOspfv3IfTransitDelay OBJECT-TYPE 
            SYNTAX          HWOspfv3UpToRefreshIntervalTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The estimated number of seconds it takes to 
                transmit a link state update packet over this 
                interface." 
            DEFVAL          { 1 } 
            ::= { hwOspfv3IfEntry 7 } 
 
    hwOspfv3IfRetransInterval OBJECT-TYPE 
            SYNTAX          HWOspfv3UpToRefreshIntervalTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The number of seconds between link state 
                advertisement retransmissions, for adjacencies 
                belonging to this interface. This value is 
                also used when retransmitting database  
                description and link state request packets." 
            DEFVAL          { 5 } 
            ::= { hwOspfv3IfEntry 8 } 
 
    hwOspfv3IfHelloInterval OBJECT-TYPE 
            SYNTAX          HWHelloRange 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The length of time, in seconds, between the 
                Hello packets that the router sends on the 
                interface. This value must be the same for all 
                routers attached to a common network." 
            DEFVAL          { 10 } 
            ::= { hwOspfv3IfEntry 9 } 
 
    hwOspfv3IfRtrDeadInterval OBJECT-TYPE 
            SYNTAX          HWOspfv3DeadIntRangeTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The number of seconds that a router's Hello 
                packets have not been seen before its  
                neighbors declare the router down on the interface. 
                This should be some multiple of the Hello interval. 
                This value must be the same for all routers attached 
                to a common network." 
            DEFVAL          { 40 } 
            ::= { hwOspfv3IfEntry 10 } 
 
   hwOspfv3IfState OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            down(1), 
                            loopback(2), 
                            waiting(3), 
                            pointToPoint(4), 
                            designatedRouter(5), 
                            backupDesignatedRouter(6), 
                            otherDesignatedRouter(7) 
                            } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Interface State." 
            ::= { hwOspfv3IfEntry 11 } 
 
    hwOspfv3IfDesignatedRouter OBJECT-TYPE 
            SYNTAX          HWOspfv3RouterIdTc 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The Router ID of the Designated Router." 
            ::= { hwOspfv3IfEntry 12 } 
 
    hwOspfv3IfBackupDesignatedRouter OBJECT-TYPE 
            SYNTAX          HWOspfv3RouterIdTc 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The Router ID of the Backup Designated 
                Router." 
            ::= { hwOspfv3IfEntry 13 } 

    hwOspfv3IfEvents OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of times this OSPFv3 interface has 
                changed its state, or an error has occurred." 
            ::= { hwOspfv3IfEntry 14 } 
 
     hwOspfv3IfRowStatus OBJECT-TYPE 
            SYNTAX          RowStatus 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This object permits management of the table by 
                facilitating actions such as row creation, 
                construction and destruction. 
 
                The value of this object has no effect on 
                whether other objects in this conceptual row can be 
                modified." 
            ::= { hwOspfv3IfEntry 15 } 
 

 
    hwOspfv3IfMetricValue OBJECT-TYPE 
            SYNTAX          Metric 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The metric assigned to this interface. 
                 The default value of the Metric is 
                Reference Bandwidth / ifSpeed. The value 
                of the reference bandwidth is configured 
                by the ospfv3ReferenceBandwidth object." 
            ::= { hwOspfv3IfEntry 16 } 
 
     hwOspfv3IfLinkScopeLsaCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The total number of Link-Scope link state 
                advertisements in this link's link state 
                database." 
            ::= { hwOspfv3IfEntry 17 } 
 
     hwOspfv3IfLinkLsaCksumSum OBJECT-TYPE 
            SYNTAX          Unsigned32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit unsigned sum of the Link-Scope link state 
                advertisements' LS checksums contained in this 
                link's link state database. The sum can be used 
                to determine if there has been a change in a 
                router's link state database, and to compare the 
                link state database of two routers." 
            ::= { hwOspfv3IfEntry 18 } 
 
    hwOspfv3IfPollInterval OBJECT-TYPE 
            SYNTAX          Unsigned32 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The larger time interval, in seconds, between 
                the Hello packets sent to an inactive  
                non-broadcast multi-access neighbor." 
            DEFVAL          { 120 } 
            ::= { hwOspfv3IfEntry 19 } 
 
    hwOspfv3IfMulticastForwarding OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            blocked(1),   -- no multicast forwarding 
                            multicast(2), -- using multicast address 
                            unicast(3)    -- to each OSPFv3 neighbor 
                            } 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The way multicasts should forwarded on this 
                interface; not forwarded, forwarded as data 
                link multicasts, or forwarded as data link  
                unicasts. Data link multicasting is not  
                meaningful on point to point and NBMA interfaces, 
                and setting ospfv3MulticastForwarding to 0 
                effectively disables all multicast forwarding." 
            DEFVAL { blocked } 
            ::= { hwOspfv3IfEntry 20 }  
 
 
    -- OSPFv3 Virtual Interface Table 
 
    -- The Virtual Interface Table describes the virtual 
    -- links that the OSPFv3 Process is configured to 
    -- carry on. 
 
    hwOspfv3VirtIfTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF HwOspfv3VirtIfEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Information about this router's virtual 
                interfaces." 
            REFERENCE 
                "OSPF Version 2, Appendix C.4 Virtual link 
                parameters" 
            ::= { hwOspfv3Objects 7 } 
 
    hwOspfv3VirtIfEntry OBJECT-TYPE 
            SYNTAX          HwOspfv3VirtIfEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Information about a single Virtual Interface." 
            INDEX           { hwOspfv3VirtIfAreaId, 
                              hwOspfv3VirtIfNeighbor } 
            ::= { hwOspfv3VirtIfTable 1 } 
 
    HwOspfv3VirtIfEntry ::= SEQUENCE { 
            hwOspfv3VirtIfAreaId 
                    HWOspfv3AreaIdTc, 
            hwOspfv3VirtIfNeighbor 
                    HWOspfv3RouterIdTc, 
            hwOspfv3VirtIfIndex 
                    InterfaceIndex,
            hwOspfv3VirtIfInstId 
                    HWOspfv3IfInstIdTc, 
            hwOspfv3VirtIfTransitDelay 
                    HWOspfv3UpToRefreshIntervalTc, 
            hwOspfv3VirtIfRetransInterval 
                    HWOspfv3UpToRefreshIntervalTc, 
            hwOspfv3VirtIfHelloInterval 
                    HelloRange, 
            hwOspfv3VirtIfRtrDeadInterval 
                    HWOspfv3DeadIntRangeTc, 
            hwOspfv3VirtIfState 
                    INTEGER, 
            hwOspfv3VirtIfEvents 
                    Counter32, 
            hwOspfv3VirtIfRowStatus 
                    RowStatus, 
            hwOspfv3VirtIfLinkScopeLsaCount 
                    Gauge32, 
            hwOspfv3VirtIfLinkLsaCksumSum 
                    Unsigned32
            } 
 
    hwOspfv3VirtIfAreaId OBJECT-TYPE 
            SYNTAX          HWOspfv3AreaIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Transit Area that the Virtual Link 
                traverses. By definition, this is not 
                Area 0" 
            ::= { hwOspfv3VirtIfEntry 1 } 
 
    hwOspfv3VirtIfNeighbor OBJECT-TYPE 
            SYNTAX          HWOspfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Router ID of the Virtual Neighbor." 
            ::= { hwOspfv3VirtIfEntry 2 } 
 
    hwOspfv3VirtIfIndex OBJECT-TYPE 
            SYNTAX          InterfaceIndex
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The local interface index assigned to this 
                OSPFv3 virtual interface. It is advertised in 
                Hello's sent over the virtual link and in the 
                router's router-LSAs." 
            ::= { hwOspfv3VirtIfEntry 3 } 
 
    hwOspfv3VirtIfInstId OBJECT-TYPE 
            SYNTAX          HWOspfv3IfInstIdTc 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Specifies the interface instance ID to be used 
                for the virtual interface. This ID has local link 
                significance only." 
            ::= { hwOspfv3VirtIfEntry 4 } 
 
    hwOspfv3VirtIfTransitDelay OBJECT-TYPE 
            SYNTAX          HWOspfv3UpToRefreshIntervalTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The estimated number of seconds it takes to 
                transmit a link state update packet over this 
                interface." 
            DEFVAL          { 1 } 
            ::= { hwOspfv3VirtIfEntry 5 } 
 
    hwOspfv3VirtIfRetransInterval OBJECT-TYPE 
            SYNTAX          HWOspfv3UpToRefreshIntervalTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The number of seconds between link state 
                advertisement retransmissions, for adjacencies 
                belonging to this interface. This value is 
                also used when retransmitting database 
                description and link state request packets. This 
                value should be well over the expected 
                round-trip time." 
            DEFVAL          { 5 } 
            ::= { hwOspfv3VirtIfEntry 6 } 
 
    hwOspfv3VirtIfHelloInterval OBJECT-TYPE 
            SYNTAX          HelloRange 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The length of time, in seconds, between the 
                Hello packets that the router sends on the 
                interface.  This value must be the same for the 
                virtual neighbor." 
            DEFVAL          { 10 } 
            ::= { hwOspfv3VirtIfEntry 7 } 
 
    hwOspfv3VirtIfRtrDeadInterval OBJECT-TYPE 
            SYNTAX          HWOspfv3DeadIntRangeTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The number of seconds that a router's Hello 
                packets have not been seen before its 
                neighbors declare the router down. This should 
                be some multiple of the Hello interval. This 
                value must be the same for the virtual 
                neighbor." 
            DEFVAL          { 40 } 
            ::= { hwOspfv3VirtIfEntry 8 } 
 
    hwOspfv3VirtIfState OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            down(1), 
                            pointToPoint(4) 
                            } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "OSPFv3 virtual interface states. The same encoding 
                as the hwOspfv3IfTable is used." 
            ::= { hwOspfv3VirtIfEntry 9 } 
 
    hwOspfv3VirtIfEvents OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of state changes or error events on 
                this Virtual Link" 
            ::= { hwOspfv3VirtIfEntry 10 } 
 
    hwOspfv3VirtIfRowStatus OBJECT-TYPE 
            SYNTAX          RowStatus 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This object permits management of the table by 
                facilitating actions such as row creation, 
                construction and destruction. 
 
                The value of this object has no effect on 
                whether other objects in this conceptual row can be 
                modified." 
            ::= { hwOspfv3VirtIfEntry 11 } 
 
    hwOspfv3VirtIfLinkScopeLsaCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The total number of Link-Scope link state 
                advertisements in this virtual link's link state 
                database." 
            ::= { hwOspfv3VirtIfEntry 12 } 
 
    hwOspfv3VirtIfLinkLsaCksumSum OBJECT-TYPE 
            SYNTAX          Unsigned32
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit unsigned sum of the Link-Scope link-state 
                advertisements' LS checksums contained in this 
                virtual link's link-state database. The sum can be used 
                to determine if there has been a change in a 
                router's link state database, and to compare the 
                link state database of two routers." 
            ::= { hwOspfv3VirtIfEntry 13 } 
 
 
    -- OSPFv3 Neighbor Table 
 
    -- The OSPFv3 Neighbor Table describes all neighbors in 
    -- the locality of the subject router. 
 
    hwOspfv3NbrTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF HwOspfv3NbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A table of non-virtual neighbor information." 
            REFERENCE 
                "OSPF Version 2, Section 10 The Neighbor Data 
                Structure" 
            ::= { hwOspfv3Objects 8 } 
 
    hwOspfv3NbrEntry OBJECT-TYPE 
            SYNTAX          HwOspfv3NbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The information regarding a single neighbor." 
            REFERENCE 
                "OSPF Version 2, Section 10 The Neighbor Data 
                Structure" 
            INDEX           { hwOspfv3NbrIfIndex, 
                              hwOspfv3NbrIfInstId, 
                              hwOspfv3NbrRtrId } 
            ::= { hwOspfv3NbrTable 1 } 
 
    HwOspfv3NbrEntry ::= SEQUENCE { 
            hwOspfv3NbrIfIndex 
                    InterfaceIndex, 
            hwOspfv3NbrIfInstId 
                    HWOspfv3IfInstIdTc, 
            hwOspfv3NbrRtrId 
                    HWOspfv3RouterIdTc, 
            hwOspfv3NbrAddressType 
                    InetAddressType, 
            hwOspfv3NbrAddress 
                    InetAddress,             
            hwOspfv3NbrOptions 
                    Integer32, 
            hwOspfv3NbrPriority 
                    DesignatedRouterPriority, 
            hwOspfv3NbrState 
                    INTEGER, 
            hwOspfv3NbrEvents 
                    Counter32, 
            hwOspfv3NbrLsRetransQLen 
                    Gauge32, 
            hwOspfv3NbrHelloSuppressed 
                    TruthValue, 
            hwOspfv3NbrIfId 
                    InterfaceIndex, 
            hwOspfv3NbrRestartHelperStatus  
                    INTEGER,  
            hwOspfv3NbrRestartHelperAge  
                    HWOspfv3UpToRefreshIntervalTc,  
            hwOspfv3NbrRestartHelperExitRc  
                    INTEGER 
            } 
 
    hwOspfv3NbrIfIndex OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The local link ID of the link over which the 
                 neighbor can be reached." 
            ::= { hwOspfv3NbrEntry 1 } 
 
    hwOspfv3NbrIfInstId OBJECT-TYPE 
            SYNTAX          HWOspfv3IfInstIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Interface instance over which the neighbor 
                can be reached. This ID has local link 
                significance only." 
            ::= { hwOspfv3NbrEntry 2 } 
 
    hwOspfv3NbrRtrId OBJECT-TYPE 
            SYNTAX          HWOspfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
               "A 32-bit integer uniquely identifying the neighboring 
               router in the Autonomous System." 
            ::= { hwOspfv3NbrEntry 3 } 
 
    hwOspfv3NbrAddressType OBJECT-TYPE 
            SYNTAX          InetAddressType 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The address type of ospfv3NbrAddress. Only IPv6 
                addresses without zone index are expected." 
            ::= { hwOspfv3NbrEntry 4 } 
 
    hwOspfv3NbrAddress OBJECT-TYPE 
            SYNTAX          InetAddress 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The IPv6 address of the neighbor associated with 
                the local link." 
            ::= { hwOspfv3NbrEntry 5 } 
 
    hwOspfv3NbrOptions OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "A Bit Mask corresponding to the neighbor's 
                options field." 
            REFERENCE 
                "OSPF Version 3, Appendix A.2 the Options field" 
            ::= { hwOspfv3NbrEntry 6 } 
 
    hwOspfv3NbrPriority OBJECT-TYPE 
            SYNTAX          DesignatedRouterPriority 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The priority of this neighbor in the designated 
                router election algorithm. The value 0 signifies 
                that the neighbor is not eligible to become the 
                designated router on this particular network." 
            ::= { hwOspfv3NbrEntry 7 } 
 
    hwOspfv3NbrState OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            down(1), 
                            attempt(2), 
                            init(3), 
                            twoWay(4), 
                            exchangeStart(5), 
                            exchange(6), 
                            loading(7), 
                            full(8) 
                            } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The State of the relationship with this 
                Neighbor." 
            REFERENCE 
                "OSPF Version 2, Section 10.1 Neighbor States" 
            ::= { hwOspfv3NbrEntry 8 } 
 
    hwOspfv3NbrEvents OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of times this neighbor relationship 
                has changed state, or an error has occurred." 
            ::= { hwOspfv3NbrEntry 9 } 
 
    hwOspfv3NbrLsRetransQLen OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The current length of the retransmission 
                queue." 
            ::= { hwOspfv3NbrEntry 10 } 
 
    hwOspfv3NbrHelloSuppressed OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether Hellos are being suppressed 
                to the neighbor" 
            ::= { hwOspfv3NbrEntry 11 } 
 
    hwOspfv3NbrIfId OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The interface ID that the neighbor advertises 
                in its Hello Packets on this link, that is, the 
                neighbor's local interface index." 
            ::= { hwOspfv3NbrEntry 12 } 
 
    hwOspfv3NbrRestartHelperStatus OBJECT-TYPE  
           SYNTAX       INTEGER { notHelping (1),  
                                  helping (2)  
                                }   
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Indicates whether the router is acting  
              as a Graceful restart helper for the neighbor."  
              ::= { hwOspfv3NbrEntry 13 }  
        
    hwOspfv3NbrRestartHelperAge OBJECT-TYPE  
           SYNTAX       HWOspfv3UpToRefreshIntervalTc 
           UNITS        "seconds"  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Remaining time in current OSPFv3 Graceful restart  
              interval, if the router is acting as a restart  
              helper for the neighbor."  
           ::= { hwOspfv3NbrEntry 14 }  
        
    hwOspfv3NbrRestartHelperExitRc OBJECT-TYPE  
           SYNTAX       INTEGER { none (1), 
                                  inProgress (2),  
                                  completed (3),  
                                  timedOut (4),  
                                  topologyChanged (5) 
                                }  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Describes the outcome of the last attempt at acting  
              as a Graceful restart helper for the neighbor. 
    
              none:............no restart has yet been attempted. 
              inProgress:......a restart attempt is currently underway. 
              completed:.......the last restart completed successfully. 
              timedOut:........the last restart timed out. 
              topologyChanged:.the last restart was aborted due to 
                               a topology change."  
        ::= { hwOspfv3NbrEntry 15 } 
 
 
    -- OSPFv3 Configured Neighbor Table 
 
    -- The OSPFv3 Configured Neighbor Table describes all configured 
    -- neighbors 
 
    hwOspfv3CfgNbrTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF HwOspfv3CfgNbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A table of configured, non-virtual neighbor 
                information." 
            REFERENCE 
                "OSPF Version 2, Section 10 The Neighbor Data 
                Structure" 
            ::= { hwOspfv3Objects 9 } 
 
    hwOspfv3CfgNbrEntry OBJECT-TYPE 
            SYNTAX          HwOspfv3CfgNbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The information regarding a single configured 
                neighbor or neighbor discovered by lower-level 
                protocols such as Inverse Neighbor Discovery." 
            REFERENCE 
                "OSPF Version 2, Section 10 The Neighbor Data 
                Structure" 
            INDEX           { hwOspfv3CfgNbrIfIndex, 
                              hwOspfv3CfgNbrIfInstId,                                
                              hwOspfv3CfgNbrRtrId } 
            ::= { hwOspfv3CfgNbrTable 1 } 
 
    HwOspfv3CfgNbrEntry ::= SEQUENCE { 
            hwOspfv3CfgNbrIfIndex 
                    InterfaceIndex, 
            hwOspfv3CfgNbrIfInstId 
                    HWOspfv3IfInstIdTc, 
            hwOspfv3CfgNbrRtrId 
                    HWOspfv3RouterIdTc, 
            hwOspfv3CfgNbrPriority 
                    DesignatedRouterPriority, 
            hwOspfv3CfgNbrRowStatus 
                    RowStatus 
            } 
 
    hwOspfv3CfgNbrIfIndex OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The local link ID of the link over which the 
                 neighbor can be reached." 
            ::= { hwOspfv3CfgNbrEntry 1 } 
 
    hwOspfv3CfgNbrIfInstId OBJECT-TYPE 
            SYNTAX          HWOspfv3IfInstIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Interface instance over which the neighbor 
                can be reached. This ID has local link 
                significance only." 
            ::= { hwOspfv3CfgNbrEntry 2 }     
 
    hwOspfv3CfgNbrRtrId OBJECT-TYPE 
            SYNTAX          HWOspfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A 32-bit integer uniquely identifying the static neighbor 
               router in the Autonomous System."  
            ::= { hwOspfv3CfgNbrEntry 3 } 
 
    hwOspfv3CfgNbrPriority OBJECT-TYPE 
            SYNTAX          DesignatedRouterPriority 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The priority of this neighbor in the designated 
                router election algorithm. The value 0 signifies 
                that the neighbor is not eligible to become the 
                designated router on this particular network." 
            DEFVAL          { 1 } 
            ::= { hwOspfv3CfgNbrEntry 4 } 
 
    hwOspfv3CfgNbrRowStatus OBJECT-TYPE 
            SYNTAX          RowStatus 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This object permits management of the table by 
                facilitating actions such as row creation, 
                construction and destruction. 
 
                The value of this object has no effect on 
                whether other objects in this conceptual row can be 
                modified." 
            ::= { hwOspfv3CfgNbrEntry 5 } 
 
    -- OSPFv3 Virtual Neighbor Table 
 
    -- This table describes all virtual neighbors. 
    -- Since Virtual Links are configured in the 
    -- virtual interface table, this table is read-only. 
 
    hwOspfv3VirtNbrTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF HwOspfv3VirtNbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A table of virtual neighbor information." 
            REFERENCE 
                "OSPF Version 2, Section 15 Virtual Links" 
            ::= { hwOspfv3Objects 10 } 
 
    hwOspfv3VirtNbrEntry OBJECT-TYPE 
            SYNTAX          HwOspfv3VirtNbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Virtual neighbor information." 
            INDEX           { hwOspfv3VirtNbrArea, 
                              hwOspfv3VirtNbrRtrId } 
            ::= { hwOspfv3VirtNbrTable 1 } 
 
    HwOspfv3VirtNbrEntry ::= SEQUENCE { 
            hwOspfv3VirtNbrArea 
                    HWOspfv3AreaIdTc, 
            hwOspfv3VirtNbrRtrId 
                    HWOspfv3RouterIdTc, 
            hwOspfv3VirtNbrIfIndex 
                    InterfaceIndex, 
            hwOspfv3VirtNbrIfInstId 
                    HWOspfv3IfInstIdTc, 
            hwOspfv3VirtNbrAddressType 
                    InetAddressType, 
            hwOspfv3VirtNbrAddress 
                    InetAddress, 
            hwOspfv3VirtNbrOptions 
                    Integer32, 
            hwOspfv3VirtNbrState 
                    INTEGER, 
            hwOspfv3VirtNbrEvents 
                    Counter32, 
            hwOspfv3VirtNbrLsRetransQLen 
                    Gauge32, 
            hwOspfv3VirtNbrHelloSuppressed 
                    TruthValue, 
            hwOspfv3VirtNbrIfId 
                    InterfaceIndex,
            hwOspfv3VirtNbrRestartHelperStatus  
                    INTEGER,  
            hwOspfv3VirtNbrRestartHelperAge  
                    HWOspfv3UpToRefreshIntervalTc,  
            hwOspfv3VirtNbrRestartHelperExitRc  
                    INTEGER 
            } 
 
    hwOspfv3VirtNbrArea OBJECT-TYPE 
            SYNTAX          HWOspfv3AreaIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Transit Area Identifier." 
            ::= { hwOspfv3VirtNbrEntry 1 } 
 
    hwOspfv3VirtNbrRtrId OBJECT-TYPE 
            SYNTAX          HWOspfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A 32-bit integer uniquely identifying the 
                neighboring router in the Autonomous System." 
            ::= { hwOspfv3VirtNbrEntry 2 } 
 
    hwOspfv3VirtNbrIfIndex OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The local interface ID for the virtual link over 
                which the neighbor can be reached." 
            ::= { hwOspfv3VirtNbrEntry 3 } 
 
    hwOspfv3VirtNbrIfInstId OBJECT-TYPE 
            SYNTAX          HWOspfv3IfInstIdTc 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The interface instance for the virtual link over 
                which the neighbor can be reached." 
            ::= { hwOspfv3VirtNbrEntry 4 } 
 
    hwOspfv3VirtNbrAddressType OBJECT-TYPE 
            SYNTAX          InetAddressType 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The address type of ospfv3VirtNbrAddress. Only IPv6 
                addresses without zone index are expected." 
            ::= { hwOspfv3VirtNbrEntry 5 } 
 
    hwOspfv3VirtNbrAddress OBJECT-TYPE 
            SYNTAX          InetAddress  
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The IPv6 address advertised by this Virtual Neighbor. 
                It must be a Global scope address." 
            ::= { hwOspfv3VirtNbrEntry 6 } 
 
    hwOspfv3VirtNbrOptions OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "A Bit Mask corresponding to the neighbor's options 
                field." 
            REFERENCE 
                "OSPF Version 3, Appendix A.2 the Options field" 
            ::= { hwOspfv3VirtNbrEntry 7 } 
 
    hwOspfv3VirtNbrState OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            down(1), 
                            attempt(2), 
                            init(3), 
                            twoWay(4), 
                            exchangeStart(5), 
                            exchange(6), 
                            loading(7), 
                            full(8) 
                            } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The state of the Virtual Neighbor Relationship." 
            ::= { hwOspfv3VirtNbrEntry 8 } 
 
    hwOspfv3VirtNbrEvents OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of times this virtual link has 
                changed its state, or an error has occurred." 
            ::= { hwOspfv3VirtNbrEntry 9 } 
 
    hwOspfv3VirtNbrLsRetransQLen OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The current length of the retransmission 
                queue." 
            ::= { hwOspfv3VirtNbrEntry 10 } 
 
    hwOspfv3VirtNbrHelloSuppressed OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether Hellos are being suppressed 
                to the neighbor" 
            ::= { hwOspfv3VirtNbrEntry 11 } 
             
    hwOspfv3VirtNbrIfId OBJECT-TYPE 
            SYNTAX          InterfaceIndex
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The interface ID that the neighbor advertises 
                in its Hello Packets on this virtual link, that is, 
                the neighbor's local interface ID." 
            ::= { hwOspfv3VirtNbrEntry 12 } 
 
   hwOspfv3VirtNbrRestartHelperStatus OBJECT-TYPE  
           SYNTAX       INTEGER { notHelping (1),  
                                  helping (2)  
                                }  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Indicates whether the router is acting  
              as a Graceful restart helper for the neighbor."  
              ::= { hwOspfv3VirtNbrEntry 13 }  
        
    hwOspfv3VirtNbrRestartHelperAge OBJECT-TYPE  
           SYNTAX       HWOspfv3UpToRefreshIntervalTc 
           UNITS        "seconds"  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Remaining time in current OSPFv3 Graceful restart  
              interval, if the router is acting as a restart  
              helper for the neighbor."  
           ::= { hwOspfv3VirtNbrEntry 14 }  
        
    hwOspfv3VirtNbrRestartHelperExitRc OBJECT-TYPE  
           SYNTAX       INTEGER { none (1),  
                                  inProgress (2),  
                                  completed (3),  
                                  timedOut (4),  
                                  topologyChanged (5)  
                                }  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Describes the outcome of the last attempt at acting  
               as a Graceful restart helper for the neighbor. 
    
              none:............no restart has yet been attempted. 
              inProgress:......a restart attempt is currently underway. 
              completed:.......the last restart completed successfully. 
              timedOut:........the last restart timed out. 
              topologyChanged:.the last restart was aborted due to 
                               a topology change."  
        ::= { hwOspfv3VirtNbrEntry 15 } 
    -- 
    -- The OSPFv3 Area Aggregate Table 
    -- 
 
    hwOspfv3AreaAggregateTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF HwOspfv3AreaAggregateEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A range of IPv6 prefixes specified by a 
                prefix/prefix length pair. Note that if 
                ranges are configured such that one range 
                subsumes another range the most specific 
                match is the preferred one." 
            ::= { hwOspfv3Objects 11 } 
 
    hwOspfv3AreaAggregateEntry OBJECT-TYPE 
            SYNTAX          HwOspfv3AreaAggregateEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A range of IPv6 prefixes specified by a 
                prefix/prefix length pair. Note that if 
                ranges are configured such that one range 
                subsumes another range the most specific match is 
                the preferred one." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2  Area parameters" 
            INDEX           { hwOspfv3AreaAggregateAreaId,  
                              hwOspfv3AreaAggregateAreaLsdbType, 
                              hwOspfv3AreaAggregatePrefixType, 
                              hwOspfv3AreaAggregatePrefix, 
                              hwOspfv3AreaAggregatePrefixLength } 
            ::= { hwOspfv3AreaAggregateTable 1 } 
 
    HwOspfv3AreaAggregateEntry ::= SEQUENCE { 
            hwOspfv3AreaAggregateAreaId 
                    HWOspfv3AreaIdTc, 
            hwOspfv3AreaAggregateAreaLsdbType 
                    INTEGER, 
            hwOspfv3AreaAggregatePrefixType 
                    InetAddressType, 
            hwOspfv3AreaAggregatePrefix 
                    InetAddress, 
            hwOspfv3AreaAggregatePrefixLength 
                    InetAddressPrefixLength, 
            hwOspfv3AreaAggregateRowStatus 
                    RowStatus, 
            hwOspfv3AreaAggregateEffect 
                    INTEGER
            } 
 
    hwOspfv3AreaAggregateAreaId OBJECT-TYPE 
            SYNTAX          HWOspfv3AreaIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Area the Address Aggregate is to be found 
                within." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            ::= { hwOspfv3AreaAggregateEntry 1 } 
 
    hwOspfv3AreaAggregateAreaLsdbType OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            interAreaPrefixLsa(8195), -- 0x2003 
                            nssaExternalLsa(8199)     -- 0x2007 
                            } 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The type of the Address Aggregate.  This field 
                specifies the Area Lsdb type that this Address 
                Aggregate applies to." 
            REFERENCE 
                "OSPF Version 2, Appendix A.4.1 The Link State 
                Advertisement header" 
            ::= { hwOspfv3AreaAggregateEntry 2 } 
 
    hwOspfv3AreaAggregatePrefixType OBJECT-TYPE 
            SYNTAX          InetAddressType --{ ipv6(2) } 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The prefix type of ospfv3AreaAggregatePrefix. Only 
                IPv6 addresses are expected." 
            ::= { hwOspfv3AreaAggregateEntry 4 } 
 
    hwOspfv3AreaAggregatePrefix OBJECT-TYPE 
            SYNTAX          InetAddress  
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The IPv6 Prefix." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            ::= { hwOspfv3AreaAggregateEntry 5 } 
 
    hwOspfv3AreaAggregatePrefixLength OBJECT-TYPE 
            SYNTAX          InetAddressPrefixLength (1..128) 
            UNITS           "bits" 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The length of the prefix (in bits). A prefix can 
                not be shorter than 0 bits." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            ::= { hwOspfv3AreaAggregateEntry 6 } 
 
    hwOspfv3AreaAggregateRowStatus OBJECT-TYPE 
            SYNTAX          RowStatus 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This object permits management of the table by 
                facilitating actions such as row creation, 
                construction and destruction. 
 
                The value of this object has no effect on 
                whether other objects in this conceptual row can be 
                modified." 
            ::= { hwOspfv3AreaAggregateEntry 7 } 
 
    hwOspfv3AreaAggregateEffect OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            advertiseMatching(1), 
                            doNotAdvertiseMatching(2) 
                            } 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "Prefixes subsumed by ranges either trigger the 
                advertisement of the indicated aggregate 
                (advertiseMatching), or result in the prefix not 
                being advertised at all outside the area." 
            DEFVAL          { advertiseMatching } 
            ::= { hwOspfv3AreaAggregateEntry 8 } 
 
 
 
 
    -- The Ospfv3 Notification Table 
    
    -- The Ospfv3 Notification Table records fields that are 

    -- required for notifications 
    
    hwOspfv3NotificationEntry OBJECT IDENTIFIER 
            ::= { hwOspfv3Objects 12 } 
    
    hwOspfv3ConfigErrorType OBJECT-TYPE 
        SYNTAX       INTEGER { 
                        badVersion (1), 
                        areaMismatch (2), 
                        unknownNbmaNbr (3), -- Router is DR eligible 
                        unknownVirtualNbr (4), 
                        helloIntervalMismatch (5), 
                        deadIntervalMismatch (6), 
                        optionMismatch (7), 
                        mtuMismatch (8), 
                        duplicateRouterId (9), 
                        noError (10) } 
        MAX-ACCESS   accessible-for-notify 
        STATUS   current 
        DESCRIPTION 
           "Potential types of configuration conflicts. 
           Used by the ospfv3ConfigError and  
           ospfv3ConfigVirtError notifications. When the last value 
           of a notification using this object is needed, but no 
           notifications of that type have been sent, this value 
           pertaining to this object should be returned as 
           noError" 
        ::= { hwOspfv3NotificationEntry 1 } 
 
    hwOspfv3PacketType OBJECT-TYPE 
        SYNTAX       INTEGER { 
                        hello (1), 
                        dbDescript (2), 
                        lsReq (3), 
                        lsUpdate (4), 
                        lsAck (5), 
                        nullPacket (6) } 
        MAX-ACCESS   accessible-for-notify 
        STATUS       current 
        DESCRIPTION 
           "OSPFv3 packet types. When the last value of a notification 
           using this object is needed, but no notifications of 
           that type have been sent, the value pertaining 
           to this object should be returned as nullPacket" 
        ::= { hwOspfv3NotificationEntry 2 } 
 
    hwOspfv3PacketSrc      OBJECT-TYPE 
            SYNTAX       InetAddress 
            MAX-ACCESS   accessible-for-notify 
            STATUS       current 
            DESCRIPTION 
               "The IPv6 address of an inbound packet that cannot 
               be identified by a neighbor instance. When 
               the last value of a notification using this object is 
               needed, but no notifications of that type have been sent, 
               the value pertaining to this object should 
               be returned as 0. 
 
               Only IPv6 addresses without zone index are expected." 
        ::= { hwOspfv3NotificationEntry 3 } 
 
    hwOspfv3IfName OBJECT-TYPE 
            SYNTAX          OCTET STRING (SIZE (1..64)) 
            MAX-ACCESS      accessible-for-notify 
            STATUS          current 
            DESCRIPTION 
                "The interface name" 
            ::= { hwOspfv3NotificationEntry 4 } 
            
    hwOspfv3IfStateChgReason OBJECT-TYPE
        SYNTAX       INTEGER {
        		noEvent(1),
			interfaceUp(2),
			waitTimerExpired(3),
			backupSeenOccured(4),
			neighborChangeEventOccured(5),
			loopInd(6),
			unloopInd(7),
			interfaceDown(8)
                        }
        MAX-ACCESS   accessible-for-notify
        STATUS   current
        DESCRIPTION
            "Interface state change reason."
        ::= { hwOspfv3NotificationEntry 5 }      
        
   hwOspfv3NbrStateChgReason OBJECT-TYPE
        SYNTAX       INTEGER {
                        noEvent(1),
			receivedHelloPacket(2),
			start(3),
			receivedTwoWay(4),
			negotiationDone(5),
			exchangeDone(6),
			receivedBadLSRequest(7),
			loadingDone(8),
			establishedAdjacency(9),
			mismatchInSeqNumber(10),
			receivedOneWay(11),
			nbrKilled(12),
			inactivityTimerExpired(13),
			linkDown(14)
			}
        MAX-ACCESS   accessible-for-notify
        STATUS   current
        DESCRIPTION
            "Neighbor state change reason."
        ::= { hwOspfv3NotificationEntry 6 }           
    
    hwOspfv3ProcessId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The process ID indicates the OSPFv3 process number. The value ranges from 1 to 4294967295."
            ::= { hwOspfv3NotificationEntry 7 }
            
    hwOspfv3AreaIdIndex OBJECT-TYPE
            SYNTAX          HWOspfv3AreaIdTc 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "A 32-bit integer uniquely identifying an area. 
                Area ID 0 is used for the OSPFv3 backbone." 
            ::= { hwOspfv3NotificationEntry 8 }
                  
     hwOspfv3NewRouterId OBJECT-TYPE
            SYNTAX         HWOspfv3RouterIdTc 
            MAX-ACCESS     read-only 
            STATUS         current 
            DESCRIPTION
                "A 32-bit integer uniquely identifying the 
                router in the Autonomous System. To ensure 
                uniqueness, this may default to the value of 
                one of the router's IPv4 host addresses, 
                represented as a 32-bit unsigned integer, 
                if IPv4 is configured on the router." 
            ::= { hwOspfv3NotificationEntry 9 }
    
     hwOspfv3PeerFlappingSuppressStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                none(1),
                holddown(2),
                holdmaxcost(3)
                }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "his object indicates the mode of the OSPFv3 neighbor relationship flapping suppression.
none(1): OSPFv3 neighbor relationship flapping suppression is not started yet.
holddown(2): OSPFv3 neighbor relationship flapping suppression works in Hold-down mode.
holdmaxcost(3): OSPFv3 neighbor relationship flapping suppression works in Hold-max-cost mode.
"
     ::= { hwOspfv3NotificationEntry 10 }

     hwOspfv3PeerFlappingSuppressReason OBJECT-TYPE
            SYNTAX INTEGER
                {
                resumeTimerExpired(1),
                configureChange(2),
                resetSuppressFlapping(3),
                neighbourFlapping(4),
                holddownToHoldmaxcost(5)
                }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The reason of peer flapping suppress status change."
            ::= { hwOspfv3NotificationEntry 11 }

        hwOspfv3LsaId OBJECT-TYPE
            SYNTAX HWOspfv3RouterIdTc
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                  "A 32-bit integer uniquely identifies an area.
                LSA-ID 0.0.0.0 is used for the OSPF LSA."
            ::= { hwOspfv3NotificationEntry 12 } 

        hwOspfv3LsaAge OBJECT-TYPE
            SYNTAX Integer32 (0..3600)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This age of the ospf lsa."
            ::= { hwOspfv3NotificationEntry 13 } 
            
     hwOspfv3PurgeHostName OBJECT-TYPE
            SYNTAX     OCTET STRING (SIZE (1..64)) 
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the name of an OSPFv3 router which purge OSPFv3 routes."
            ::= { hwOspfv3NotificationEntry 14 }
             
     hwOspfv3PurgeIpAddress OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the IP address of an OSPFv3 router which purge OSPFv3 routes."
            ::= { hwOspfv3NotificationEntry 15 }
             
     hwOspfv3PurgeRouterId OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the 32-bit integer that uniquely identifies the router in the Autonomous System."
            ::= { hwOspfv3NotificationEntry 16 }
             
     hwOspfv3FlushLsaNum OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the number of LSAs deleted by the local device or another device."
            ::= { hwOspfv3NotificationEntry 17 }
             
     hwOspfv3AffectedNodeNum OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the number of affected node when OSPFv3 routes were deleted."
            ::= { hwOspfv3NotificationEntry 18 }
             
     hwOspfv3TotalNodeNum OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the total number of node in the System."
            ::= { hwOspfv3NotificationEntry 19 }
             
     hwOspfv3PurgeStatPeriod OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the period interval for purge statistic."
            ::= { hwOspfv3NotificationEntry 20 }
             
     hwOspfv3RuledOutDeviceNum OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the number of node ruled out when checking faulty device."
            ::= { hwOspfv3NotificationEntry 21 }
             
     hwOspfv3PurgeHostName1 OBJECT-TYPE
            SYNTAX     OCTET STRING (SIZE (1..64)) 
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the name of an OSPFv3 router which maybe purge OSPFv3 routes."
            ::= { hwOspfv3NotificationEntry 22 }
             
     hwOspfv3PurgeHostName2 OBJECT-TYPE
            SYNTAX     OCTET STRING (SIZE (1..64)) 
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the name of an OSPFv3 router which maybe purge OSPFv3 routes."
            ::= { hwOspfv3NotificationEntry 23 }
             
     hwOspfv3PurgeHostName3 OBJECT-TYPE
            SYNTAX     OCTET STRING (SIZE (1..64)) 
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the name of an OSPFv3 router which maybe purge OSPFv3 routes."
            ::= { hwOspfv3NotificationEntry 24 }
             
     hwOspfv3PurgeIpAddress1 OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the IP address of an OSPFv3 router which maybe purge OSPFv3 routes."
            ::= { hwOspfv3NotificationEntry 25 }
             
     hwOspfv3PurgeIpAddress2 OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the IP address of an OSPFv3 router which maybe purge OSPFv3 routes."
            ::= { hwOspfv3NotificationEntry 26 }
             
     hwOspfv3PurgeIpAddress3 OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the IP address of an OSPFv3 router which maybe purge OSPFv3 routes."
            ::= { hwOspfv3NotificationEntry 27 }
             
     hwOspfv3PurgeRouterId1 OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the 32-bit integer that uniquely identifies the router in the Autonomous System."
            ::= { hwOspfv3NotificationEntry 28 }
             
     hwOspfv3PurgeRouterId2 OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the 32-bit integer that uniquely identifies the router in the Autonomous System."
            ::= { hwOspfv3NotificationEntry 29 }
             
     hwOspfv3PurgeRouterId3 OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                  "This object indicates the 32-bit integer that uniquely identifies the router in the Autonomous System."
            ::= { hwOspfv3NotificationEntry 30 }

    -- Notification definitions  
 
   hwOspfv3VirtIfStateChange NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId,  -- The originator of the notification 
                  hwOspfv3VirtIfState,  -- The new state 
                  hwOspfv3IfStateChgReason -- The interface state change reason
           } 
        STATUS       current 
        DESCRIPTION 
           "An ospfv3VirtIfStateChange notification signifies that there 
           has been a change in the state of an OSPFv3 virtual 
           interface. 
 
           This notification should be generated when the interface 
           state regresses (e.g., goes from Point-to-Point to Down) 
           or progresses to a terminal state (i.e., Point-to-Point)." 
        ::= { hwOspfv3Notifications 1 } 
 
   hwOspfv3NbrStateChange NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId,   -- The originator of the notification 
                  hwOspfv3NbrState,    -- The new state                   
                  hwOspfv3IfName,   -- The interface name
                  hwOspfv3NbrStateChgReason -- The neighbor state change reason
           } 
        STATUS       current 
        DESCRIPTION 
           "An ospfv3NbrStateChange notification signifies that 
           there has been a change in the state of a 
           non-virtual OSPFv3 neighbor. This notification should be 
           generated when the neighbor state regresses 
           (e.g., goes from Attempt or Full to 1-Way or 
           Down) or progresses to a terminal state (e.g., 
           2-Way or Full). When an neighbor transitions 
           from or to Full on non-broadcast multi-access 
           and broadcast networks, the notification should be 
           generated by the designated router. A designated 
           router transitioning to Down will be noted by 
           ospfIfStateChange." 
        ::= { hwOspfv3Notifications 2 } 
 
   hwOspfv3VirtNbrStateChange NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification 
                  hwOspfv3VirtNbrState,  -- The new state 
                  hwOspfv3NbrStateChgReason -- The neighbor state change reason
           } 
        STATUS       current 
        DESCRIPTION 
           "An ospfv3VirtNbrStateChange notification signifies 
           that there has been a change in the state of an OSPFv3 
           virtual neighbor. This notification should be generated 
           when the neighbor state regresses (e.g., goes 
           from Attempt or Full to 1-Way or Down) or 
           progresses to a terminal state (e.g., Full)." 
        ::= { hwOspfv3Notifications 3 } 
 
   hwOspfv3IfConfigError NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification 
           hwOspfv3IfState,         -- State of the interface 
           hwOspfv3PacketSrc,       -- IPv6 address of source 
           hwOspfv3ConfigErrorType, -- Type of error 
           hwOspfv3PacketType       -- Type of packet 
           } 
        STATUS       current 
        DESCRIPTION 
           "An ospfv3IfConfigError notification signifies that a 
           packet has been received on a non-virtual 
           interface from a router whose configuration 
           parameters conflict with this router's 
           configuration parameters. Note that the event 
           optionMismatch should cause a notification only if it 
           prevents an adjacency from forming." 
        ::= { hwOspfv3Notifications 4 } 
 
   hwOspfv3VirtIfConfigError NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification 
           hwOspfv3VirtIfState,     -- State of the interface 
           hwOspfv3ConfigErrorType, -- Type of error 
           hwOspfv3PacketType 
           } 
        STATUS       current 
        DESCRIPTION 
           "An ospfv3VirtIfConfigError notification signifies that a 
           packet has been received on a virtual interface 
           from a router whose configuration parameters 
           conflict with this router's configuration 
           parameters. Note that the event optionMismatch 
           should cause a notification only if it prevents an 
           adjacency from forming." 
        ::= { hwOspfv3Notifications 5 } 
 
 
   hwOspfv3IfRxBadPacket NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification 
           hwOspfv3IfState,         -- State of the interface 
           hwOspfv3PacketSrc,       -- The source IPv6 address 
           hwOspfv3PacketType       -- Type of packet 
           } 
        STATUS       current 
        DESCRIPTION 
           "An ospfv3IfRxBadPacket notification signifies that an 
           OSPFv3 packet that cannot be parsed has been received on a 
           non-virtual interface." 
        ::= { hwOspfv3Notifications 6 } 
 
   hwOspfv3VirtIfRxBadPacket NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification 
          hwOspfv3VirtIfState,      -- State of the interface 
          hwOspfv3PacketType        -- Type of packet 
          } 
        STATUS       current 
        DESCRIPTION 
           "An ospfv3VirtIfRxBadPacket notification signifies 
           that an OSPFv3 packet that cannot be parsed has been received 
           on a virtual interface." 
        ::= { hwOspfv3Notifications 7 } 
 
 
   
   
   hwOspfv3IfStateChange NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification 
           hwOspfv3IfState,   -- The new state           
           hwOspfv3IfName,   -- The interface name
           hwOspfv3IfStateChgReason -- The interface state change reason
           } 
        STATUS       current 
        DESCRIPTION 
           "An ospfv3IfStateChange notification signifies that there 
           has been a change in the state of a non-virtual 
           OSPFv3 interface. This notification should be generated 
           when the interface state regresses (e.g., goes 
           from Dr to Down) or progresses to a terminal 
           state (i.e., Point-to-Point, DR Other, Dr, or 
           Backup)." 
        ::= { hwOspfv3Notifications 8 } 
 
   
 
   hwOspfv3RestartStatusChange NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification 
                  hwOspfv3RestartStatus,  -- new status 
                  hwOspfv3RestartInterval, 
                  hwOspfv3RestartExitRc 
                } 
        STATUS       current 
        DESCRIPTION 
           "An ospfv3RestartStatusChange notification signifies that 
           there has been a change in the graceful restart 
           state for the router. This notification should be 
           generated when the router restart status 
           changes." 
        ::= { hwOspfv3Notifications 9 } 
    
   hwOspfv3NbrRestartHelperStatusChange NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification 
                  hwOspfv3NbrRestartHelperStatus,  -- new status 
                  hwOspfv3NbrRestartHelperAge, 
                  hwOspfv3NbrRestartHelperExitRc 
                } 
        STATUS       current 
        DESCRIPTION 
           "An ospfv3NbrRestartHelperStatusChange notification 
           signifies that there has been a change in the 
           graceful restart helper state for the neighbor. 
           This notification should be generated when the 
           neighbor restart helper status transitions for a neighbor." 
        ::= { hwOspfv3Notifications 10 } 
    
   hwOspfv3VirtNbrRestartHelperStatusChange NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification 
                  hwOspfv3VirtNbrRestartHelperStatus,  -- new status 
                  hwOspfv3VirtNbrRestartHelperAge, 
                  hwOspfv3VirtNbrRestartHelperExitRc 
                }  
        STATUS       current 
        DESCRIPTION 
           "An ospfv3VirtNbrRestartHelperStatusChange 
           notification signifies that there has been a 
           change in the graceful restart helper state for 
           the virtual neighbor. This notification should be 
           generated when the virtual neighbor restart helper status 
           transitions for a virtual neighbor." 
        ::= { hwOspfv3Notifications 11 } 
 
   hwOspfv3NssaTranslatorStatusChange NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification 
                  hwOspfv3AreaNssaTranslatorState  -- new status                    
                }  
        STATUS       current 
        DESCRIPTION 
           "An ospfv3NssaTranslatorStatusChange notification 
            indicates that there has been a change in the router's ability 
            to translate OSPFv3 NSSA LSAs into OSPFv3 External LSAs. 
            This notification should be generated when the Translator Status 
            transitions from or to any defined status on a per area basis." 
        ::= { hwOspfv3Notifications 12 } 
             
   hwOspfv3LastAuthKeyExpiry NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification 
                  hwOspfv3IfName    -- The interface name
                }  
        STATUS       current 
        DESCRIPTION 
           "An hwOspfv3LastAuthKeyExpiry notification 
            indicates that the last key associated with an interface has expired.
            When this notification is received, either the lifetime of the key should be extended
            or a new key should be configured." 
        ::= { hwOspfv3Notifications 13 }   
        
   hwOspfv3AuthSequenceNumWrap NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3RouterId, -- The originator of the notification
                  hwOspfv3IfName    -- The interface name                  
                }  
        STATUS       current 
        DESCRIPTION 
           "An hwOspfv3AuthSequenceNumWrap notification 
            indicates that the 64-bit authentication sequence number has wrapped.
            When this notification is received, all the keys must be reset
            to avoid the possibility of replay attacks." 
        ::= { hwOspfv3Notifications 14 }                  

   hwOspfv3IntraAreaRouterIdConflictRecovered NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3ProcessId, hwOspfv3AreaIdIndex, hwOspfv3RouterId, hwOspfv3NewRouterId }  
        STATUS       current 
        DESCRIPTION 
           "The object is used to monitor router ID conflict recovery in an intra area." 
        ::= { hwOspfv3Notifications 15 } 

   hwOspfv3PeerFlappingSuppressStatusChange NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3ProcessId, hwOspfv3RouterId, hwOspfv3AreaIdIndex, hwOspfv3IfName, hwOspfv3PeerFlappingSuppressStatus, hwOspfv3PeerFlappingSuppressReason }  
        STATUS       current 
        DESCRIPTION 
           "These objects are used to monitor changed OSPFv3 peer flapping suppress status." 
        ::= { hwOspfv3Notifications 16 } 
        
   hwOspfv3ImportAseRouteThreshold NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3ProcessId }  
        STATUS       current 
        DESCRIPTION 
           "This object indicates that the number of AS-external LSAs generated when an OSPFv3 process imports external routes exceeds the configured alarm threshold." 
        ::= { hwOspfv3Notifications 17 } 
        
   hwOspfv3ImportAseRouteThresholdClear NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3ProcessId }  
        STATUS       current 
        DESCRIPTION 
           "This object indicates that the number of AS-external LSAs generated when an OSPFv3 process imports external routes has been less than the configured alarm threshold." 
        ::= { hwOspfv3Notifications 18 } 
        
   hwOspfv3ImportAseRouteExceed NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3ProcessId }  
        STATUS       current 
        DESCRIPTION 
           "This object indicates that the number of AS-external LSAs generated when an OSPFv3 process imports external routes exceeds the configured maximum number." 
        ::= { hwOspfv3Notifications 19 } 
        
   hwOspfv3ImportAseRouteExceedClear NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3ProcessId }  
        STATUS       current 
        DESCRIPTION 
           "This object indicates that the number of AS-external LSAs generated when an OSPFv3 process imports external routes has been less than the configured maximum number." 
        ::= { hwOspfv3Notifications 20 }        
                
   hwOspfv3ImportNssaRouteThreshold NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3ProcessId, hwOspfv3AreaIdIndex }  
        STATUS       current 
        DESCRIPTION 
           "This object indicates that the number of NSSA LSAs generated when an OSPFv3 process imports external routes exceeds the configured alarm threshold." 
        ::= { hwOspfv3Notifications 21 } 
        
   hwOspfv3ImportNssaRouteThresholdClear NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3ProcessId, hwOspfv3AreaIdIndex }  
        STATUS       current 
        DESCRIPTION 
           "This object indicates that the number of NSSA LSAs generated when an OSPFv3 process imports external routes has been less than the configured alarm threshold." 
        ::= { hwOspfv3Notifications 22 } 
        
   hwOspfv3ImportNssaRouteExceed NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3ProcessId, hwOspfv3AreaIdIndex }
        STATUS       current 
        DESCRIPTION 
           "This object indicates that the number of NSSA LSAs generated when an OSPFv3 process imports external routes exceeds the configured maximum number." 
        ::= { hwOspfv3Notifications 23 } 
        
   hwOspfv3ImportNssaRouteExceedClear NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3ProcessId, hwOspfv3AreaIdIndex }  
        STATUS       current 
        DESCRIPTION 
           "This object indicates that the number of NSSA LSAs generated when an OSPFv3 process imports external routes has been less than the configured maximum number." 
        ::= { hwOspfv3Notifications 24 }

   hwOspfv3GreaterAgeLsaRecived NOTIFICATION-TYPE 
        OBJECTS { hwOspfv3ProcessId, hwOspfv3RouterId, hwOspfv3AreaIdIndex, hwOspfv3IfName, hwOspfv3LsaId, hwOspfv3LsaAge }  
        STATUS       current 
        DESCRIPTION 
           "This object is used to monitor the router recive a greater age lsa in ospfv3." 
        ::= { hwOspfv3Notifications 25 }
        
   hwOspfv3DeleteRouteByPurge NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex, 
                hwOspfv3FlushLsaNum, hwOspfv3AffectedNodeNum, hwOspfv3TotalNodeNum, hwOspfv3PurgeStatPeriod }
        STATUS current
        DESCRIPTION
            "This object indicates that the local device deleted OSPFv3 routes advertised by other devices. 
            Reset or isolate the device from the network."
        ::= { hwOspfv3Notifications 26 }
        
   hwOspfv3DeleteRouteByPurgeClear NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex }
        STATUS current
        DESCRIPTION
            "This object indicates that the local device did not delete OSPFv3 routes advertised by other devices."
        ::= { hwOspfv3Notifications 27 }
        
   hwOspfv3RouteBeDeletedByPurgeExact NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex, 
                hwOspfv3FlushLsaNum, hwOspfv3AffectedNodeNum, hwOspfv3TotalNodeNum, hwOspfv3PurgeStatPeriod }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by the local device were deleted by another device. 
            Reset or isolate the faulty device from the network."
        ::= { hwOspfv3Notifications 28 }
        
   hwOspfv3RouteBeDeletedByPurgeExactClear NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by the local device were not deleted by another device."
        ::= { hwOspfv3Notifications 29 }
        
   hwOspfv3RouteBeDeletedByPurgeInexact NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex, 
                hwOspfv3FlushLsaNum, hwOspfv3AffectedNodeNum, hwOspfv3TotalNodeNum, hwOspfv3RuledOutDeviceNum, hwOspfv3PurgeStatPeriod }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by the local device were deleted by another device, 
            and the possibly faulty device did not support OSPFv3 flush LSA source trace. Log in to the possibly faulty device. 
            If the device is deleting routes, reset or isolate it from the network. Otherwise, check other devices. 
            Neither of the devices displayed in the display ospfv3 purge-source-trace analysis-info  command output is the faulty device."
        ::= { hwOspfv3Notifications 30 }
        
   hwOspfv3RouteBeDeletedByPurgeInexactClear NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by the local device were not deleted by another device."
        ::= { hwOspfv3Notifications 31 }
        
   hwOspfv3RouteBeDeletedByPurge NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex, hwOspfv3TotalNodeNum, 
                hwOspfv3PurgeHostName1, hwOspfv3PurgeIpAddress1, hwOspfv3PurgeRouterId1, 
                hwOspfv3PurgeHostName2, hwOspfv3PurgeIpAddress2, hwOspfv3PurgeRouterId2, 
                hwOspfv3PurgeHostName3, hwOspfv3PurgeIpAddress3, hwOspfv3PurgeRouterId3 }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by the local device were deleted by another device. 
            Log in to the possibly faulty device. If the device is deleting routes, reset or isolate it from the network. 
            Otherwise, check other devices."
        ::= { hwOspfv3Notifications 32 }
        
   hwOspfv3RouteBeDeletedByPurgeClear NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by the local device were not deleted by another device."
        ::= { hwOspfv3Notifications 33 }
        
   hwOspfv3ThirdPartRouteBeDeletedByPurgeExact NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex, 
                hwOspfv3FlushLsaNum, hwOspfv3AffectedNodeNum, hwOspfv3TotalNodeNum, hwOspfv3PurgeStatPeriod }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by another device were deleted. 
            Reset or isolate the faulty device from the network."
        ::= { hwOspfv3Notifications 34 }
        
   hwOspfv3ThirdPartRouteBeDeletedByPurgeExactClear NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by another device were not deleted."
        ::= { hwOspfv3Notifications 35 }
        
   hwOspfv3ThirdPartRouteBeDeletedByPurgeInexact NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex, 
                hwOspfv3FlushLsaNum, hwOspfv3AffectedNodeNum, hwOspfv3TotalNodeNum, hwOspfv3RuledOutDeviceNum, hwOspfv3PurgeStatPeriod }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by another device were deleted, 
            and the possibly faulty device did not support OSPFv3 flush LSA source trace. 
            Log in to the possibly faulty device. If the device is deleting routes, reset or isolate it from the network. 
            Otherwise, check other devices. Neither of the devices displayed in the display ospfv3 purge-source-trace analysis-info 
            command output is the faulty device."
        ::= { hwOspfv3Notifications 36 }
        
   hwOspfv3ThirdPartRouteBeDeletedByPurgeInexactClear NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by another device were not deleted."
        ::= { hwOspfv3Notifications 37 }
        
   hwOspfv3ThirdPartRouteBeDeletedByPurge NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex, hwOspfv3TotalNodeNum, 
                hwOspfv3PurgeHostName1, hwOspfv3PurgeIpAddress1, hwOspfv3PurgeRouterId1, 
                hwOspfv3PurgeHostName2, hwOspfv3PurgeIpAddress2, hwOspfv3PurgeRouterId2, 
                hwOspfv3PurgeHostName3, hwOspfv3PurgeIpAddress3, hwOspfv3PurgeRouterId3 }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by another device were deleted. Log in to the possibly faulty device. 
            If the device is deleting routes, reset or isolate it from the network. Otherwise, check other devices."
        ::= { hwOspfv3Notifications 38 }
        
   hwOspfv3ThirdPartRouteBeDeletedByPurgeClear NOTIFICATION-TYPE
        OBJECTS { hwOspfv3ProcessId, hwOspfv3PurgeHostName, hwOspfv3PurgeIpAddress, hwOspfv3PurgeRouterId, hwOspfv3AreaIdIndex }
        STATUS current
        DESCRIPTION
            "This object indicates that OSPFv3 routes advertised by another device were not deleted."
        ::= { hwOspfv3Notifications 39 }

    -- conformance information 
 
    hwOspfv3Groups      OBJECT IDENTIFIER ::= { hwOspfv3Conformance 1 } 
    hwOspfv3Compliances OBJECT IDENTIFIER ::= { hwOspfv3Conformance 2 } 
 
    -- compliance statements 
 
    hwOspfv3Compliance MODULE-COMPLIANCE 
            STATUS          current 
            DESCRIPTION     "The compliance statement" 
            MODULE          -- this module 
            MANDATORY-GROUPS { 
                            hwOspfv3BasicGroup, 
                            hwOspfv3AreaGroup, 
                            hwOspfv3IfGroup, 
                            hwOspfv3VirtIfGroup, 
                            hwOspfv3NbrGroup,
                            hwOspfv3CfgNbrGroup,                             
                            hwOspfv3VirtNbrGroup, 
                            hwOspfv3AreaAggregateGroup
                            } 
 
            GROUP           hwOspfv3AsLsdbGroup 
            DESCRIPTION 
                "This group is required for OSPFv3 systems that 
                display their AS-scope link state database." 
 
            GROUP           hwOspfv3AreaLsdbGroup 
            DESCRIPTION 
                "This group is required for OSPFv3 systems that 
                display their Area-scope link state database." 
 
            GROUP           hwOspfv3LinkLsdbGroup 
            DESCRIPTION 
                "This group is required for OSPFv3 systems that 
                display their Link-scope link state database." 
 
            GROUP           hwOspfv3NotificationObjectGroup
            DESCRIPTION
                "This group is required for OSPFv3 systems that
                support OSPFv3 notifications."

            GROUP           hwOspfv3NotificationGroup
            DESCRIPTION
                "This group is required for OSPFv3 systems that
                support OSPFv3 notifications."
                
            OBJECT          hwOspfv3NbrAddressType 
            SYNTAX          InetAddressType -- { ipv6(2) }
            DESCRIPTION 
                "An implementation is only required to support IPv6 
                address without zone index." 
                
            OBJECT          hwOspfv3NbrAddress
            SYNTAX          InetAddress (SIZE (16))
            DESCRIPTION
                "An implementation is only required to support IPv6
                address without zone index."                
 
            OBJECT          hwOspfv3VirtNbrAddressType 
            SYNTAX          InetAddressType --{ ipv6(2) } 
            DESCRIPTION 
                "An implementation is only required to support IPv6 
                address without zone index." 
                
            OBJECT          hwOspfv3VirtNbrAddress
            SYNTAX          InetAddress (SIZE (16))
            DESCRIPTION
                "An implementation is only required to support IPv6
                address without zone index."                
 
            ::= { hwOspfv3Compliances 1 } 
            
        hwOspfv3ReadOnlyCompliance MODULE-COMPLIANCE
          STATUS     current
          DESCRIPTION
                  "When this MIB module is implemented without
                  support for read-create (i.e., in read-only
                  mode), the implementation can claim read-only
                  compliance.  Such a device can then be monitored,
                  but cannot be configured with this MIB."

          MODULE -- this module
               MANDATORY-GROUPS {
                       hwOspfv3BasicGroup,
                       hwOspfv3AreaGroup,
                       hwOspfv3IfGroup,
                       hwOspfv3VirtIfGroup,
                       hwOspfv3NbrGroup,
                       hwOspfv3CfgNbrGroup,
                       hwOspfv3VirtNbrGroup,
                       hwOspfv3AreaAggregateGroup
                       }

          GROUP           hwOspfv3AsLsdbGroup
          DESCRIPTION
              "This group is required for OSPFv3 systems that
              display their AS-scope link state database."

          GROUP           hwOspfv3AreaLsdbGroup
          DESCRIPTION
              "This group is required for OSPFv3 systems that
              display their Area-scope link state database."

          GROUP           hwOspfv3LinkLsdbGroup
          DESCRIPTION
              "This group is required for OSPFv3 systems that
              display their Link-scope link state database
              for non-virtual interfaces."

          GROUP           hwOspfv3NotificationObjectGroup
          DESCRIPTION
              "This group is required for OSPFv3 systems that
              support OSPFv3 notifications."

          GROUP           hwOspfv3NotificationGroup
          DESCRIPTION
              "This group is required for OSPFv3 systems that
              support OSPFv3 notifications."

          OBJECT hwOspfv3RouterId
          MIN-ACCESS read-only

          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3AdminStatus
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3ExtAreaLsdbLimit
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3ReferenceBandwidth
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3RestartSupport
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3RestartInterval
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."


          OBJECT hwOspfv3NotificationEnable
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."


          OBJECT hwOspfv3AreaSummary
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3AreaRowStatus
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3AreaStubMetric
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3AreaNssaTranslatorRole
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3AreaNssaTranslatorStabInterval
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."


          OBJECT hwOspfv3IfAreaId
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3IfType
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3IfAdminStatus
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3IfRtrPriority
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3IfTransitDelay
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3IfRetransInterval
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3IfHelloInterval
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3IfRtrDeadInterval
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3IfPollInterval
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3IfRowStatus
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3IfMetricValue
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3VirtIfTransitDelay
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3VirtIfRetransInterval
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3VirtIfHelloInterval
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3VirtIfRtrDeadInterval
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3VirtIfRowStatus
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3CfgNbrPriority
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3CfgNbrRowStatus
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3AreaAggregateRowStatus
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

          OBJECT hwOspfv3AreaAggregateEffect
          MIN-ACCESS read-only
          DESCRIPTION
               "Write access is not required."

       ::= { hwOspfv3Compliances 2 }
       
       
    -- units of conformance 
 
    hwOspfv3BasicGroup OBJECT-GROUP 
            OBJECTS         { 
                            hwOspfv3RouterId, 
                            hwOspfv3AdminStatus, 
                            hwOspfv3VersionNumber, 
                            hwOspfv3AreaBdrRtrStatus, 
                            hwOspfv3AsBdrRtrStatus, 
                            hwOspfv3AsScopeLsaCount, 
                            hwOspfv3AsScopeLsaCksumSum, 
                            hwOspfv3OriginateNewLsas, 
                            hwOspfv3RxNewLsas, 
                            hwOspfv3ExtLsaCount, 
                            hwOspfv3ExtAreaLsdbLimit,                 
                            hwOspfv3RestartSupport, 
                            hwOspfv3RestartInterval, 
                            hwOspfv3RestartStatus, 
                            hwOspfv3RestartAge, 
                            hwOspfv3RestartExitRc, 
                            hwOspfv3NotificationEnable, 
                            hwOspfv3ReferenceBandwidth
                            } 
            STATUS          current 
            DESCRIPTION 
                "These objects are used for managing/monitoring 
                OSPFv3 global parameters." 
            ::= { hwOspfv3Groups 1 } 
 
 
    hwOspfv3AreaGroup OBJECT-GROUP 
            OBJECTS         {                       
                            hwOspfv3AreaImportAsExtern, 
                            hwOspfv3AreaSpfRuns, 
                            hwOspfv3AreaBdrRtrCount, 
                            hwOspfv3AreaAsBdrRtrCount, 
                            hwOspfv3AreaScopeLsaCount, 
                            hwOspfv3AreaScopeLsaCksumSum, 
                            hwOspfv3AreaSummary, 
                            hwOspfv3AreaRowStatus, 
                            hwOspfv3AreaStubMetric,
                            hwOspfv3AreaNssaTranslatorRole,
                            hwOspfv3AreaNssaTranslatorState,
                            hwOspfv3AreaNssaTranslatorStabInterval,
                            hwOspfv3AreaNssaTranslatorEvents
                               } 
            STATUS          current 
            DESCRIPTION 
                "These objects are used for OSPFv3 systems 
                supporting areas." 
            ::= { hwOspfv3Groups 2 } 
 
    hwOspfv3AsLsdbGroup OBJECT-GROUP 
            OBJECTS         { 
                            hwOspfv3AsLsdbSequence, 
                            hwOspfv3AsLsdbAge, 
                            hwOspfv3AsLsdbChecksum, 
                            hwOspfv3AsLsdbAdvertisement, 
                            hwOspfv3AsLsdbTypeKnown 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These objects are used for OSPFv3 systems 
                that display their AS-scope link state database." 
            ::= { hwOspfv3Groups 3 } 
 
    hwOspfv3AreaLsdbGroup OBJECT-GROUP 
            OBJECTS         { 
                            hwOspfv3AreaLsdbSequence, 
                            hwOspfv3AreaLsdbAge, 
                            hwOspfv3AreaLsdbChecksum, 
                            hwOspfv3AreaLsdbAdvertisement, 
                            hwOspfv3AreaLsdbTypeKnown 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These objects are used for OSPFv3 systems 
                that display their Area-scope link state database." 
            ::= { hwOspfv3Groups 4 } 
 
    hwOspfv3LinkLsdbGroup OBJECT-GROUP 
            OBJECTS         { 
                            hwOspfv3LinkLsdbSequence, 
                            hwOspfv3LinkLsdbAge, 
                            hwOspfv3LinkLsdbChecksum, 
                            hwOspfv3LinkLsdbAdvertisement, 
                            hwOspfv3LinkLsdbTypeKnown 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These objects are used for OSPFv3 systems 
                that display their Link-scope link state database." 
            ::= { hwOspfv3Groups 5 } 
 

 
    hwOspfv3IfGroup OBJECT-GROUP 
            OBJECTS         { 
                            hwOspfv3IfAreaId, 
                            hwOspfv3IfType, 
                            hwOspfv3IfAdminStatus, 
                            hwOspfv3IfRtrPriority, 
                            hwOspfv3IfTransitDelay, 
                            hwOspfv3IfRetransInterval, 
                            hwOspfv3IfHelloInterval, 
                            hwOspfv3IfRtrDeadInterval,                             
                            hwOspfv3IfState, 
                            hwOspfv3IfDesignatedRouter, 
                            hwOspfv3IfBackupDesignatedRouter, 
                            hwOspfv3IfEvents, 
                            hwOspfv3IfRowStatus,                             
                            hwOspfv3IfMetricValue, 
                            hwOspfv3IfLinkScopeLsaCount, 
                            hwOspfv3IfLinkLsaCksumSum,
                            hwOspfv3IfPollInterval, 
                            hwOspfv3IfMulticastForwarding                          
                            } 
            STATUS          current 
            DESCRIPTION 
                "These interface objects used for  
                managing/monitoring OSPFv3 interfaces." 
            ::= { hwOspfv3Groups 6 } 
 
    hwOspfv3VirtIfGroup OBJECT-GROUP 
            OBJECTS         { 
                            hwOspfv3VirtIfIndex, 
                            hwOspfv3VirtIfInstId, 
                            hwOspfv3VirtIfTransitDelay, 
                            hwOspfv3VirtIfRetransInterval, 
                            hwOspfv3VirtIfHelloInterval, 
                            hwOspfv3VirtIfRtrDeadInterval, 
                            hwOspfv3VirtIfState, 
                            hwOspfv3VirtIfEvents, 
                            hwOspfv3VirtIfRowStatus, 
                            hwOspfv3VirtIfLinkScopeLsaCount, 
                            hwOspfv3VirtIfLinkLsaCksumSum  
                            } 
            STATUS          current 
            DESCRIPTION 
                "These virtual interface objects are used for  
                managing/monitoring OSPFv3 virtual interfaces." 
            ::= { hwOspfv3Groups 7 } 
 
    hwOspfv3NbrGroup OBJECT-GROUP 
            OBJECTS         { 
                            hwOspfv3NbrAddressType, 
                            hwOspfv3NbrAddress, 
                            hwOspfv3NbrOptions, 
                            hwOspfv3NbrPriority, 
                            hwOspfv3NbrState, 
                            hwOspfv3NbrEvents, 
                            hwOspfv3NbrLsRetransQLen, 
                            hwOspfv3NbrHelloSuppressed, 
                            hwOspfv3NbrIfId, 
                            hwOspfv3NbrRestartHelperStatus,  
                            hwOspfv3NbrRestartHelperAge,  
                            hwOspfv3NbrRestartHelperExitRc 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These neighbor objects are used for 
                managing/monitoring OSPFv3 neighbors." 
            ::= { hwOspfv3Groups 8 } 
 
    hwOspfv3CfgNbrGroup OBJECT-GROUP 
            OBJECTS         { 
                            hwOspfv3CfgNbrPriority, 
                            hwOspfv3CfgNbrRowStatus 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These configured neighbor objects are used for 
                managing/monitoring OSPFv3 configured neighbors." 
            ::= { hwOspfv3Groups 9 } 
 
    hwOspfv3VirtNbrGroup OBJECT-GROUP 
            OBJECTS         { 
                            hwOspfv3VirtNbrIfIndex, 
                            hwOspfv3VirtNbrIfInstId, 
                            hwOspfv3VirtNbrAddressType,  
                            hwOspfv3VirtNbrAddress, 
                            hwOspfv3VirtNbrOptions, 
                            hwOspfv3VirtNbrState, 
                            hwOspfv3VirtNbrEvents, 
                            hwOspfv3VirtNbrLsRetransQLen, 
                            hwOspfv3VirtNbrHelloSuppressed, 
                            hwOspfv3VirtNbrIfId, 
                            hwOspfv3VirtNbrRestartHelperStatus,  
                            hwOspfv3VirtNbrRestartHelperAge,  
                            hwOspfv3VirtNbrRestartHelperExitRc 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These virtual neighbor objects are used for 
                managing/monitoring OSPFv3 virtual neighbors." 
            ::= { hwOspfv3Groups 10 } 
 
    hwOspfv3AreaAggregateGroup OBJECT-GROUP 
            OBJECTS         { 
                            hwOspfv3AreaAggregateRowStatus, 
                            hwOspfv3AreaAggregateEffect                            
                            } 
            STATUS          current 
            DESCRIPTION 
                "These area aggregate objects used required for 
                aggregating OSPFv3 prefixes for summarization  
                across areas." 
            ::= { hwOspfv3Groups 11 } 
 
    hwOspfv3NotificationObjectGroup OBJECT-GROUP 
            OBJECTS         { 
                            hwOspfv3ConfigErrorType, 
                            hwOspfv3PacketType, 
                            hwOspfv3PacketSrc, 
                            hwOspfv3IfName,
                            hwOspfv3IfStateChgReason,
                            hwOspfv3NbrStateChgReason,
                            hwOspfv3ProcessId,
                            hwOspfv3AreaIdIndex,
                            hwOspfv3NewRouterId                            
                            } 
            STATUS          current 
            DESCRIPTION 
                "These objects are used to record notification 
                parameters" 
            ::= { hwOspfv3Groups 12 } 
 
    hwOspfv3NotificationGroup NOTIFICATION-GROUP 
            NOTIFICATIONS   { 
                            hwOspfv3VirtIfStateChange, 
                            hwOspfv3NbrStateChange, 
                            hwOspfv3VirtNbrStateChange, 
                            hwOspfv3IfConfigError, 
                            hwOspfv3VirtIfConfigError, 
                            hwOspfv3IfRxBadPacket, 
                            hwOspfv3VirtIfRxBadPacket,                             
                            hwOspfv3IfStateChange,                             
                            hwOspfv3RestartStatusChange, 
                            hwOspfv3NbrRestartHelperStatusChange, 
                            hwOspfv3VirtNbrRestartHelperStatusChange,
                            hwOspfv3NssaTranslatorStatusChange,
                            hwOspfv3LastAuthKeyExpiry,
                            hwOspfv3AuthSequenceNumWrap,
                            hwOspfv3IntraAreaRouterIdConflictRecovered,
                            hwOspfv3PeerFlappingSuppressStatusChange,
                            hwOspfv3ImportAseRouteThreshold,
                            hwOspfv3ImportAseRouteThresholdClear,
                            hwOspfv3ImportAseRouteExceed,
                            hwOspfv3ImportAseRouteExceedClear,
                            hwOspfv3ImportNssaRouteThreshold,
                            hwOspfv3ImportNssaRouteThresholdClear,
                            hwOspfv3ImportNssaRouteExceed,
                            hwOspfv3ImportNssaRouteExceedClear,
                            hwOspfv3GreaterAgeLsaRecived,
                            hwOspfv3DeleteRouteByPurge,
                            hwOspfv3DeleteRouteByPurgeClear,
                            hwOspfv3RouteBeDeletedByPurgeExact,
                            hwOspfv3RouteBeDeletedByPurgeExactClear,
                            hwOspfv3RouteBeDeletedByPurgeInexact,
                            hwOspfv3RouteBeDeletedByPurgeInexactClear,
                            hwOspfv3RouteBeDeletedByPurge,
                            hwOspfv3RouteBeDeletedByPurgeClear,
                            hwOspfv3ThirdPartRouteBeDeletedByPurgeExact,
                            hwOspfv3ThirdPartRouteBeDeletedByPurgeExactClear,
                            hwOspfv3ThirdPartRouteBeDeletedByPurgeInexact,
                            hwOspfv3ThirdPartRouteBeDeletedByPurgeInexactClear,
                            hwOspfv3ThirdPartRouteBeDeletedByPurge,
                            hwOspfv3ThirdPartRouteBeDeletedByPurgeClear
                            } 
            STATUS          current 
            DESCRIPTION 
                "This group is used for OSPFv3 notifications" 
            ::= { hwOspfv3Groups 13 } 
 
    END  