-- ==================================================================
-- Copyright (C) 2017 by HUAWEI TECHNOLOGIES. All rights reserved.
-- Description:   This MIB is used for defining the HUAWEI private   
--                extended Multiprotocol Label Switching (MPLS) MIB 
--                object. All MIB objects are used to describe private
--                managed objects and trap definitions for MPLS.
-- Reference:
-- Version: V2.46
-- History:
-- V2.45 Siju Samuel, 2017-4-25, modify for hwMplsTunnelDelegationReturn/hwMplsTunnelDelegationReturnClear alarm
-- V2.44 jiangweisheng, 2017-3-4, modify for hwMplsLspBfdDown/hwMplsLspBfdDownClear add te keyword in the name
-- V2.43 zhangka, 2016-12-13, modify for hwMplsLspBfdDown/hwMplsLspBfdDownClear
-- V2.42 chujianping, 2016-06-13, modify for hwMplsTunnelBfdPathMismatch/hwMplsTunnelBfdPathMismatchClear bind VB
-- V2.41 liujialei, 2016-01-11, delete for type BITS
-- V2.40 zhangtan, 2016-01-06, modify for hwMplsTunnelBfdPathMismatch/hwMplsTunnelBfdPathMismatchClear
-- V2.39 zhangtan, 2015-09-08, modify for hwMplsTunnelHotstandbySwitch/hwMplsTunnelHotstandbyResume
-- V2.38 zhangtan, 2015-04-11, modify for hwMplsResourceType
-- V2.37 xuejianguo, 2015-03-31, add for hwMplsTunnelStatisticsTable
-- V2.36 zhangtan, 2015-03-19, modify for hwMplsResourceType
-- V2.35 wangbin, 2015-01-22, modify for hwMplsIngressLsrId, hwMplsEgressLsrId
-- V2.34 wangbin, 2015-01-12, modify for TE OPT
-- V2.33 zhangtan, 2014-11-21, modify for mpls te commit
-- V2.32 wangbin, 2014-11-14, modify for BiStatic Lsp LoopBack
-- V2.31 wangxinhai, 2014-11-06, modify for hwMplsResourceType
-- V2.30 hanyeting, 2014-08-12, modify for hwMplsResourceType
-- V2.29 zhangka, 2014-07-21, modify for private network bgp lsp threshold trap
-- V2.28 longyong, 2014-06-16, add for hwMplsResourceThresholdExceed, hwMplsResourceThresholdExceedClear, hwMplsResourceTotalCountExceed, hwMplsResourceTotalCountExceedClear 
-- V2.27 denghuan, 2014-02-17, modify for hwStaticLspDownReason add reason for ring invalid 
-- V2.26 wangxinhai, 2014-02-07, modify for hwStaticLspDownReason add reason for static lsp configure update
-- V2.25 wangxinhai, 2014-01-27, modify for static LSP/CR-LSP down-reason for  tunnel down
-- V2.24 wangxinhai, 2014-01-13, modify for ldp frr/rsvp lsp/total lsp/total cr lsp threshold trap
-- V2.23 zhangaifen, 2013-11-07, modify for bgp lsp threshold trap
-- V2.09 DouZongxin, 2012-09-14, modify for TE last error vb type
-- V2.08 DouZongxin, 2012-08-24, modify for TE last error opt project
-- V2.07 WangHonglei, 2012-07-05, revision

-- ==================================================================
-- ==================================================================
-- 
-- Variables and types be imported
-- 
-- ==================================================================

    HUAWEI-MPLS-EXTEND-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            hwDatacomm            
                FROM HUAWEI-MIB            
            ifIndex, ifName           
                FROM IF-MIB            
            MplsIndexType            
                FROM MPLS-LSR-STD-MIB            
            MplsTunnelIndex, MplsTunnelInstanceIndex, MplsExtendedTunnelId, MplsLsrIdentifier       
                FROM MPLS-TC-STD-MIB            
            SnmpAdminString            
                FROM SNMP-FRAMEWORK-MIB            
            OBJECT-GROUP, NOTIFICATION-GROUP, MODULE-COMPLIANCE            
                FROM SNMPv2-CONF            
            Integer32, Unsigned32, Counter32, IpAddress, Counter64, OBJECT-TYPE, 
            MODULE-IDENTITY, NOTIFICATION-TYPE            
                FROM SNMPv2-SMI
            mplsTunnelAdminStatus, mplsTunnelOperStatus
                FROM MPLS-TE-STD-MIB
            InetAddressType, InetAddress
                FROM INET-ADDRESS-MIB;
    
    

        -- 1.3.6.1.4.1.2011.5.25.121
        hwMplsExtendMib MODULE-IDENTITY 
            LAST-UPDATED "201708171640Z"        
            ORGANIZATION 
                "Huawei Technologies Co.,Ltd."
            CONTACT-INFO 
                "Huawei Industrial Base
                  Bantian, Longgang
                   Shenzhen 518129
                   People's Republic of China
                   Website: http://www.huawei.com
                   Email: support@huawei.com
                 "
            DESCRIPTION 
                "This MIB is used for defining the HUAWEI private   
                 extended Multiprotocol Label Switching (MPLS) MIB
                 object. All MIB objects are used to describe private
                 managed objects and trap definitions for MPLS."

            --  Revision history
            REVISION   "201708171640Z"
            DESCRIPTION "V2.46, modify descroption of three item"

            REVISION   "201704251600Z"
            DESCRIPTION "V2.45, modify for hwMplsTunnelDelegationReturn/hwMplsTunnelDelegationReturnClear alarm."

            REVISION   "201703041600Z"
            DESCRIPTION "V2.44,  change alarm name hwMplsLspBfdDown hwMplsLspBfdDownClear to hwMplsTeLspBfdDown hwMplsTeLspBfdDownClear."

            REVISION   "201612131600Z"
            DESCRIPTION "V2.43,  add a new alarm, hwMplsLspBfdDown hwMplsLspBfdDownClear."
			
            REVISION   "201606131600Z"
            DESCRIPTION "V2.42, modify hwMplsTunnelBfdPathMismatch hwMplsTunnelBfdPathMismatchClear bind VB."

            REVISION   "201601111600Z"
            DESCRIPTION "V2.41, delete a type BITS. It is a basic type now."

            REVISION   "201601061200Z"
            DESCRIPTION "V2.40, add a new alarm, hwMplsTunnelBfdPathMismatch hwMplsTunnelBfdPathMismatchClear."
            
            REVISION   "201508011200Z"
            DESCRIPTION "V2.39, add a new alarm, hwMplsTunnelHotstandbySwitch hwMplsTunnelHotstandbyResume."

            REVISION   "201504111200Z"
            DESCRIPTION "V2.38, modify enum hwMplsResourceType for supporting MPLS CSPF resource total exceed alarm."

            REVISION   "201503311419Z"
            DESCRIPTION "V2.37, add for hwMplsTunnelStatisticsTable."
                                
            REVISION   "201503191700Z"
            DESCRIPTION "V2.36, add enum hwMplsResourceType for supporting MPLS CSPF resource total exceed alarm."
            
            REVISION   "201501221916Z"
            DESCRIPTION "V2.35, modify hwMplsIngressLsrId hwMplsEgressLsrId."
			
            REVISION   "201501122016Z"
            DESCRIPTION "V2.34, modify hwMplsTeFrrSwitch."
			
            REVISION   "201411211800Z"
            DESCRIPTION "V2.33, add  hwMplsTunnelCommitLost hwMplsTunnelCommitLostClear."

            REVISION   "201411141800Z"
            DESCRIPTION "V2.32, add  hwMplsLspLoopBack hwMplsLspLoopBackClear hwMplsSessionTunnelId hwMplsLocalLspId hwMplsIngressLsrId hwMplsEgressLsrId hwMplsLspName."

            REVISION   "201411061630Z"
            DESCRIPTION "V2.31, add  enum ldpTotalLocalAdjacency to hwMplsResourceType for supporting MPLS resource total and threshold exceed alarm."

            REVISION   "201408121450Z"
            DESCRIPTION "V2.30, add  enum outSegment and autoPrimaryTunnelIf to hwMplsResourceType for supporting MPLS resource total exceed alarm."

            REVISION   "201407211427Z"
            DESCRIPTION "V2.29, add  enum privateNetBgp to hwMplsLspProtocol for supporting private network bgp lsp threshold alarm."

            REVISION   "201406161417Z"
            DESCRIPTION "V2.28, add traps: hwMplsResourceThresholdExceed, hwMplsResourceThresholdExceedClear, hwMplsResourceTotalCountExceed, hwMplsResourceTotalCountExceedClear."

            REVISION   "201402171905Z"
            DESCRIPTION "V2.27,  modify hwStaticLspDownReason for add invalid ring reason ."            

            REVISION   "201402071100Z"
            DESCRIPTION "V2.26,  modify  hwStaticLspDownReason  for configure update."

            REVISION   "201401271100Z"
            DESCRIPTION "V2.25,  modify  hwStaticLspDownReason  for tunnel dowm."

            REVISION   "201401131345Z"
            DESCRIPTION "V2.24,  add  enum ldpfrr, rsvp, totalLsp and totalCrLsp to hwMplsLspProtocol for supporting ldp frr, rsvp lsp, total lsp, total cr lsp threshold alarm."

            REVISION   "201311071745Z"
            DESCRIPTION "V2.23, add  enum bgp and bgpv6 to hwMplsLspProtocol for supporting bgp and bgp ipv6 lsp threshold alarm."
         
            REVISION   "201309111745Z"
            DESCRIPTION "V2.22, add table: hwMplsTrafficStatisticsStaticLspTable."

            REVISION   "201304131652Z"
            DESCRIPTION "V2.21, modify hwMplsRingSwitch, hwMplsRingResume."

            REVISION   "201301141525Z"
            DESCRIPTION "V2.20, add the description of hwmplsDynamicLabelThresholdexceed,hwmplsDynamicLabelThresholdexceedClear,hwmplsDynamicLabeltotalcountexceed,hwmplsDynamicLabeltotalcountexceedClear."

            REVISION   "201207052025Z"
            DESCRIPTION "V2.07, modify the description of hwMplsLspTotalCountExceed."

            REVISION   "201206081405Z"
            DESCRIPTION "V2.06, add traps: hwmplslspThresholdexceed, hwmplslspthresholdexceedclear, hwmplslsptotalcountexceed, hwmplslsptotalcountexceedclear."

            REVISION    "201206051100Z"  
            DESCRIPTION "V2.05, add traps: hwmplstunneldelete; modify hwmplsoamtunnellock to hwmplsoamlocallock; modify hwmplstunnellockrecovery to hwmplslocallockrecovery."


            REVISION    "201205091100Z"  
            DESCRIPTION "V2.05, add traps: from hwMplsRingWestOamLoss to hwMplsRingEastOamUnexpectedMepClear."

            REVISION    "201205041100Z"  
            DESCRIPTION "V2.04, add traps: hwMplsoamTunnellock, hwMplsoamTunnellockRecovery."


            REVISION    "201111291100Z"  
            DESCRIPTION "V2.03, add traps: hwMplsExtTunnelDown, hwMplsExtTunnelDownClear."

            REVISION    "201111181100Z"  
            DESCRIPTION "V2.02, add traps: hwMplsTunnelBBSwitch, hwMplsTunnelBBResume."
            
            REVISION    "201110241100Z"  
            DESCRIPTION "V2.01, add traps: hwMplsTeAutoTunnelDownClear, hwMplsTeAutoTunnelPrimaryDownClear."

            REVISION    "201107301100Z"  
            DESCRIPTION "V2.00, delete Defval clause in these nodes: hwMplsTunnelDownReason, hwMplsTunnelLspType."
            
            REVISION     "201011231155Z"        
            DESCRIPTION  "V1.02, modified the MIB description."
                                        
            REVISION     "201007131535Z"        
            DESCRIPTION  "V1.01, modified the MIB description."
            
            REVISION     "200606301554Z"       
            DESCRIPTION  "V1.00, initial LSPM MIB."
            ::= { hwDatacomm 121 }
    
--
-- Node definitions
--
    
-- 1.3.6.1.4.1.2011.5.25.121.1
        hwMplsExtendMibTunnel OBJECT IDENTIFIER ::= { hwMplsExtendMib 1 }

--   1.3.6.1.4.1.2011.5.25.121.1.1
        hwMplsTunnelTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwMplsTunnelEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A tunnel needs to be uniquely identified across  
                 an MPLS network. Indexes hwMplsTunnelIndex and       
                 hwMplsTunnelInstance uniquely identify a tunnel 
                 on the LSR originating the tunnel. 
                 hwMplsTunnelIngressLSRId uniquely identifies a 
                 tunnel across an MPLS network. The last index     
                 hwMplsTunnelEgressLSRId is useful in identifying
                 all instances of a tunnel that are terminated on
                 the same egress LSR.                                       
                 The indexes of this table are hwMplsTunnelIndex,    
                 hwMplsTunnelInstance, hwMplsTunnelIngressLSRId and  
                 hwMplsTunnelEgressLSRId."
            ::= { hwMplsExtendMibTunnel 1 }

--   1.3.6.1.4.1.2011.5.25.121.1.1.1
        hwMplsTunnelEntry OBJECT-TYPE
            SYNTAX HwMplsTunnelEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A tunnel needs to be uniquely identified across  
                 an MPLS network. Indexes hwMplsTunnelIndex and       
                 hwMplsTunnelInstance uniquely identify a tunnel 
                 on the LSR originating the tunnel. 
                 hwMplsTunnelIngressLSRId uniquely identifies a 
                 tunnel across an MPLS network. The last index     
                 hwMplsTunnelEgressLSRId is useful in identifying
                 all instances of a tunnel that are terminated on
                 the same egress LSR.                                       
                 The indexes of this entry are hwMplsTunnelIndex,    
                 hwMplsTunnelInstance, hwMplsTunnelIngressLSRId and  
                 hwMplsTunnelEgressLSRId."
            REFERENCE
                "1. RFC 2863 - The Interfaces Group MIB, McCloghrie,
                K., and F. Kastenholtz, June 2000 "
            INDEX { hwMplsTunnelIndex, hwMplsTunnelInstance, hwMplsTunnelIngressLSRId, hwMplsTunnelEgressLSRId }
            ::= { hwMplsTunnelTable 1 }

        
        HwMplsTunnelEntry ::=
            SEQUENCE { 
                hwMplsTunnelIndex
                    MplsTunnelIndex,
                hwMplsTunnelInstance
                    MplsTunnelInstanceIndex,
                hwMplsTunnelIngressLSRId
                    MplsExtendedTunnelId,
                hwMplsTunnelEgressLSRId
                    MplsExtendedTunnelId,
                hwMplsTunnelClassType
                    INTEGER,
                hwMplsTunnelBandwidth
                    Integer32,
                hwMplsTunnelAdminStatus
                    INTEGER,
                hwMplsTunnelOperStatus
                    INTEGER,
                hwMplsTunnelSessionAttr
                    BITS,
                hwMplsTunnelFrrSetupPrio
                    Unsigned32,
                hwMplsTunnelFrrHoldingPrio
                    Unsigned32,
                hwMplsTunnelFrrBandwidth
                    Unsigned32,
                hwMplsTunnelFrrSwitchover
                    Counter32,
                hwMplsTunnelFrrBypassTableIndex
                    Unsigned32,
                hwMplsTunnelFrrARHopTableIndex
                    Unsigned32,
                hwMplsTunnelName
                    SnmpAdminString,
                hwMplsTunnelIfIndex
                    Unsigned32,
                hwMplsTunnelPreBandwidth
                    Unsigned32,
                hwMplsTunnelNextBandwidth
                    Unsigned32,
                hwMplsTunnelCt0Bandwidth
                    Unsigned32,
                hwMplsTunnelCt1Bandwidth
                    Unsigned32,
                hwMplsTunnelCt2Bandwidth
                    Unsigned32,
                hwMplsTunnelCt3Bandwidth
                    Unsigned32,
                hwMplsTunnelCt4Bandwidth
                    Unsigned32,
                hwMplsTunnelCt5Bandwidth
                    Unsigned32,
                hwMplsTunnelCt6Bandwidth
                    Unsigned32,
                hwMplsTunnelCt7Bandwidth
                    Unsigned32,
                hwMplsTunnelLspType
                    INTEGER,
                hwMplsTunnelInterfaceName
                    SnmpAdminString,
                hwMplsTunnelSignalProto
                    INTEGER,
                hwMplsTunnelType
                    INTEGER
             }

--   1.3.6.1.4.1.2011.5.25.121.1.1.1.1
        hwMplsTunnelIndex OBJECT-TYPE
            SYNTAX MplsTunnelIndex
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Uniquely identifies a set of tunnel instances 
                between a pair of ingress and egress LSRs. 
                When the MPLS signalling protocol is rsvp(2), this value 
                equals to the value signaled in the Tunnel ID 
                of the SESSION object. When the MPLS signalling protocol 
                is crldp(3), this value equals to the value 
                signaled in the LSP ID. Reference to MPLS-TE-STD-MIB."
            ::= { hwMplsTunnelEntry 1 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.2
        hwMplsTunnelInstance OBJECT-TYPE
            SYNTAX MplsTunnelInstanceIndex
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Uniquely identifies a particular instance of a 
                tunnel between a pair of ingress and egress LSRs. 
                It is used to identify multiple instances of 
                tunnels for backup and parallel tunnels. 
                When the MPLS signaling protocol is 
                rsvp(2), this value equals to the LSP ID 
                of the Sender Template object. When the signaling 
                protocol is crldp(3) there is no equivalent 
                signaling object. Reference to MPLS-TE-STD-MIB."
            ::= { hwMplsTunnelEntry 2 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.3
        hwMplsTunnelIngressLSRId OBJECT-TYPE
            SYNTAX MplsExtendedTunnelId
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the ingress LSR ID of this tunnel. 
                When the MPLS signalling protocol 
                is rsvp(2), this value equals to the Tunnel 
                Sender Address in the Sender Template object and may 
                equal to the Extended Tunnel ID in the 
                SESSION object. When the MPLS signalling protocol is 
                crldp(3), this value equals to the Ingress 
                LSR Router ID in the LSPID TLV object. 
                Reference to MPLS-TE-STD-MIB."
            ::= { hwMplsTunnelEntry 3 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.4
        hwMplsTunnelEgressLSRId OBJECT-TYPE
            SYNTAX MplsExtendedTunnelId
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the egress LSR ID of this 
                tunnel. Reference to MPLS-TE-STD-MIB."
            ::= { hwMplsTunnelEntry 4 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.5
        hwMplsTunnelClassType OBJECT-TYPE
            SYNTAX INTEGER
                {
                bc0(1),
                bc1(2),
                invalidValue(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the bandwidth type used by this tunnel. 
                Options:
                1. bc0(1)          -indicates the bandwidth type is bc0.
                2. bc1(2)          -indicates the bandwidth type is bc1.
                3. invalidValue(3) -indicates the invalid value.
                "
            ::= { hwMplsTunnelEntry 5 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.6
        hwMplsTunnelBandwidth OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the bandwidth used by this tunnel.
                Unit: kbit/s
                "
            ::= { hwMplsTunnelEntry 6 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.7
        hwMplsTunnelAdminStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                up(1),
                down(2),
                testing(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the management status of this 
                tunnel.Reference to MPLS-TE-STD-MIB.
                Options:
                1. up(1)      -indicates the management status of this tunnel is up.
                2. down(2)    -indicates the management status of this tunnel is down.
                3. testing(3) -indicates the tunnel is used in some test mode.         
                "
            ::= { hwMplsTunnelEntry 7 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.8
        hwMplsTunnelOperStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                up(1),
                down(2),
                testing(3),
                unknown(4),
                dormant(5),
                notPresent(6),
                lowerLayerDown(7)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the actual operational status of this tunnel, 
                which is but not limited to the status of this tunnel of
                a certain period.Reference to MPLS-TE-STD-MIB.
                Options:
                1. up(1)             -indicates that the operational status of this tunnel is up.          
                2. down(2)           -indicates that the operational status of this tunnel is down.
                3. testing(3)        -indicates that the tunnel is used in some test mode.
                4. unknown(4)        -indicates the invalid value.
                5. dormant(5)        -indicates that the status cannot be determined.
                6. notPresent(6)     -indicates that some component is missing
                7. lowerLayerDown(7) -indicates the Down state due to the state of lower layer interfaces.
                "
            ::= { hwMplsTunnelEntry 8 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.9
        hwMplsTunnelSessionAttr OBJECT-TYPE
            SYNTAX BITS
                {
                localProtectionDesired(0),
                nodeProtectionDesired(1),
                bandwidthProtectionDesired(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates protection types desired by the primary 
                tunnel, such as node protection, link protection or 
                bandwidth protection.
                Options:
                1. localProtectionDesired(0)     -indicates link protection.
                2. nodeProtectionDesired(1)      -indicates node protection.
                3. bandwidthProtectionDesired(2) -indicates bandwidth protection.              
                "
            ::= { hwMplsTunnelEntry 9 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.10
        hwMplsTunnelFrrSetupPrio OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the setup PRI of auto-bypass tunnel.
                Range: 0-7
                Default: 7
                "
            ::= { hwMplsTunnelEntry 10 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.11
        hwMplsTunnelFrrHoldingPrio OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the holding PRI of auto-bypass tunnel.
                Range: 0-7
                Default: 7
                "
            ::= { hwMplsTunnelEntry 11 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.12
        hwMplsTunnelFrrBandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the protecting bandwidth of auto-bypass tunnel. 
                Its value is defined by the configuration on the primary 
                tunnel.
                Unit: kbit/s"
            ::= { hwMplsTunnelEntry 12 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.13
        hwMplsTunnelFrrSwitchover OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates FRR switching times"
            ::= { hwMplsTunnelEntry 13 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.14
        hwMplsTunnelFrrBypassTableIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the index of the bypass tunnel table, that is, 
                the LSP ID of the bypass tunnel. The bypass table shows 
                interfaces protected by specified bypass tunnel."
            ::= { hwMplsTunnelEntry 14 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.15
        hwMplsTunnelFrrARHopTableIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the table index of the protection type adopted 
                by each hop of the primary tunnel."
            ::= { hwMplsTunnelEntry 15 }
        
        hwMplsTunnelName OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the tunnel name. The name can refer to the tunnel 
                on the console port of the LSR. If mplsTunnelIsIf is set to 
                True, the IfName of the interface corresponding to this tunnel 
                should have a value equal to hwMplsTunnelName. 
                Reference to the description of IfName in RFC 2863."
            ::= { hwMplsTunnelEntry 16 }
        
        hwMplsTunnelIfIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the interface index of the tunnel. It uniquely 
                identifies the tunnel name."
            ::= { hwMplsTunnelEntry 17 }

        
        hwMplsTunnelPreBandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the original bandwidth of the tunnel 
                when the tunnel is in the Modify state.
                Unit: kbit/s"
            ::= { hwMplsTunnelEntry 18 }

        
        hwMplsTunnelNextBandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the bandwidth of the tunnel that is to be changed 
                when the tunnel is in the Modify state.
                Unit: kbit/s"
            ::= { hwMplsTunnelEntry 19 }

        
        hwMplsTunnelCt0Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 0 (CT0) in this tunnel, in kbit/s.                
                If all CT bandwidths are 0s, it means that this tunnel's Class-Type
                is CT0, and bandwidth is 0 kbit/s.
                Unit: kbit/s"
            ::= { hwMplsTunnelEntry 20 }

        
        hwMplsTunnelCt1Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 1 (CT1) in this tunnel, in kbit/s.
                Unit: kbit/s"
            ::= { hwMplsTunnelEntry 21 }

        
        hwMplsTunnelCt2Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 2 (CT2) in this tunnel, in kbit/s.
                Unit: kbit/s"
            ::= { hwMplsTunnelEntry 22 }

        
        hwMplsTunnelCt3Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 3 (CT3) in this tunnel, in kbit/s.
                Unit: kbit/s"
            ::= { hwMplsTunnelEntry 23 }

        
        hwMplsTunnelCt4Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 4 (CT4) in this tunnel, in kbit/s.
                Unit: kbit/s"
            ::= { hwMplsTunnelEntry 24 }

        
        hwMplsTunnelCt5Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 5 (CT5) in this tunnel, in kbit/s.
                Unit: kbit/s"
            ::= { hwMplsTunnelEntry 25 }

        
        hwMplsTunnelCt6Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 6 (CT6) in this tunnel, in kbit/s.
                Unit: kbit/s"
            ::= { hwMplsTunnelEntry 26 }

        
        hwMplsTunnelCt7Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 7 (CT7) in this tunnel, in kbit/s.
                Unit: kbit/s"
            ::= { hwMplsTunnelEntry 27 }

        hwMplsTunnelLspType OBJECT-TYPE
            SYNTAX INTEGER
            {
            invalid(0),
            primary(1),
            primaryModifing(2),
            hotStandby(3),
            hotStandbyModifing(4),
            ordinary(5),
            ordinaryModifing(6),
            bestEffort(7),
            bestEffortModifing(8)
            }
            
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object is meaningful only at the ingress of the tunnel. It indicates LSP types.                                                                 
                Options: 
                0. invalid(0) -indicates that the LSP type is invalid, the possible cause is that the LSP is not created at an ingress. 
                1. primary(1) -indicates the primary LSP
                2. primaryModifing(2) -indicates the LSP that will replace the primary LSP
                3. hotStandby(3) -indicates the hot-standby LSP
                4. hotStandbyModifing(4) -indicates the LSP that will replace the hot-standby LSP
                5. ordinary(5) -indicates the ordinary LSP
                6. ordinaryModifing(6) -indicates the LSP that will replace the ordinary LSP
                7. bestEffort(7) -indicates the Best-Effort LSP
                8. bestEffortModifing(8) -indicates the LSP that will replace the Best-Effort LSP
                Modifying LSPs are created when users modify the make-before-break attribute of the corresponding LSP types. After being created, modifying LSPs replace the corresponding LSPs to transmit traffic.              
                "
            ::= { hwMplsTunnelEntry 28 }

        hwMplsTunnelInterfaceName OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the tunnel interface name. The object is 
                only valid at the ingress."
            ::= { hwMplsTunnelEntry 29 }
                 
--   1.3.6.1.4.1.2011.5.25.121.1.1.1.30
        hwMplsTunnelSignalProto OBJECT-TYPE
            SYNTAX INTEGER
                {
                rsvpTE(1),
                static(2),
                staticCR(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the signal protocol of this tunnel"
            ::= { hwMplsTunnelEntry 30 }

--   1.3.6.1.4.1.2011.5.25.121.1.1.1.31
        hwMplsTunnelType OBJECT-TYPE
            SYNTAX INTEGER
                { 
                invalid(1),               
                primaryTunnel(2),
                bypassTunnel(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object is meaningful only at the ingress of the tunnel. It indicates tunnel types.                                                                 
                Options: 
                1. invalid(1) -indicates that the tunnel type is invalid, the possible cause is that it is not ingress node of this tunnel
                2. primaryTunnel(2) -indicates that this is a primary tunnel
                3. bypassTunnel(3) -indicates that this is a bypass tunnel
                "        
            ::= { hwMplsTunnelEntry 31 }

--   1.3.6.1.4.1.2011.5.25.121.1.2
        hwTunnelFrrBypassTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwTunnelFrrBypassEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the bypass tunnel. The indexes of this table are 
                hwTunnelFrrBypassListIndex and hwTunnelFrrBypassIndex."
            ::= { hwMplsExtendMibTunnel 2 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.2.1
        hwTunnelFrrBypassEntry OBJECT-TYPE
            SYNTAX HwTunnelFrrBypassEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the bypass tunnel.The indexes of this entry are 
                hwTunnelFrrBypassListIndex and hwTunnelFrrBypassIndex."
            INDEX { hwTunnelFrrBypassListIndex, hwTunnelFrrBypassIndex }
            ::= { hwTunnelFrrBypassTable 1 }

        
        HwTunnelFrrBypassEntry ::=
            SEQUENCE { 
                hwTunnelFrrBypassListIndex
                    Unsigned32,
                hwTunnelFrrBypassIndex
                    Unsigned32,
                hwTunnelFrrBypassProtIfIndex
                    Unsigned32
             }

--    1.3.6.1.4.1.2011.5.25.121.1.2.1.1
        hwTunnelFrrBypassListIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the index of the bypass tunnel table, that is, the LSP ID of the bypass tunnel."
            ::= { hwTunnelFrrBypassEntry 1 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.2.1.2
        hwTunnelFrrBypassIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the index of the bypass tunnel interface."
            ::= { hwTunnelFrrBypassEntry 2 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.2.1.3
        hwTunnelFrrBypassProtIfIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the index of the interface protected by the bypass tunnel."
            ::= { hwTunnelFrrBypassEntry 3 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.3
        hwTunnelFrrARHopTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwTunnelFrrARHopEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the FrrARHopTable, which will show every hop's frr 
                protect information of the tunnel.
                The indexes of this table are hwTunnelFrrARHopListIndex and hwTunnelFrrARHopIndex."
            ::= { hwMplsExtendMibTunnel 3 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.3.1
        hwTunnelFrrARHopEntry OBJECT-TYPE
            SYNTAX HwTunnelFrrARHopEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the FrrARHopTable, which will show every hop's frr 
                protect information of the tunnel.
                The indexes of this entry are hwTunnelFrrARHopListIndex and hwTunnelFrrARHopIndex."
            INDEX { hwTunnelFrrARHopListIndex, hwTunnelFrrARHopIndex }
            ::= { hwTunnelFrrARHopTable 1 }

        
        HwTunnelFrrARHopEntry ::=
            SEQUENCE { 
                hwTunnelFrrARHopListIndex
                    Unsigned32,
                hwTunnelFrrARHopIndex
                    Unsigned32,
                hwTunnelFrrARHopProtDesired
                    BITS,
                hwTunnelFrrARHopProtActual
                    BITS
             }

--    1.3.6.1.4.1.2011.5.25.121.1.3.1.1
        hwTunnelFrrARHopListIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the table index of each hop along the primary tunnel."
            ::= { hwTunnelFrrARHopEntry 1 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.3.1.2
        hwTunnelFrrARHopIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the index of each hop along the primary tunnel."
            ::= { hwTunnelFrrARHopEntry 2 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.3.1.3
        hwTunnelFrrARHopProtDesired OBJECT-TYPE
            SYNTAX BITS
                {
                localProtection(0),
                nodeProtection(1),
                bandwidthProtection(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the FRR protection types desired by the primary tunnel interface, including:
                0: link protection,
                1: node protection,
                2: bandwidth protection
                "
            ::= { hwTunnelFrrARHopEntry 3 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.3.1.4
        hwTunnelFrrARHopProtActual OBJECT-TYPE
            SYNTAX BITS
                {
                localProtection(0),
                nodeProtection(1),
                bandwidthProtection(2),
                protectionInuse(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the actual FRR protection types of the primary tunnel interface, including:
                0: link protection,
                1: node protection,
                2: bandwidth protection,
                3: primary tunnel protection in use
                "
            ::= { hwTunnelFrrARHopEntry 4 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.4
        hwTunnelFrrRouteDBTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwTunnelFrrRouteDBEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the primary tunnel is protected by which bypass tunnel. The indexes of this
                table are hwTunnelFrrRouteDBTunnelIndex, hwTunnelFrrRouteDBTunnelInstance, 
                hwTunnelFrrRouteDBTunnelIngressLSRId and hwTunnelFrrRouteDBTunnelEngressLSRId."
            ::= { hwMplsExtendMibTunnel 4 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.4.1
        hwTunnelFrrRouteDBEntry OBJECT-TYPE
            SYNTAX HwTunnelFrrRouteDBEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the primary tunnel is protected by which bypass tunnel. The indexes of this
                entry are hwTunnelFrrRouteDBTunnelIndex, hwTunnelFrrRouteDBTunnelInstance, 
                hwTunnelFrrRouteDBTunnelIngressLSRId and hwTunnelFrrRouteDBTunnelEngressLSRId."
            INDEX { hwTunnelFrrRouteDBTunnelIndex, hwTunnelFrrRouteDBTunnelInstance, hwTunnelFrrRouteDBTunnelIngressLSRId, hwTunnelFrrRouteDBTunnelEngressLSRId }
            ::= { hwTunnelFrrRouteDBTable 1 }

        
        HwTunnelFrrRouteDBEntry ::=
            SEQUENCE { 
                hwTunnelFrrRouteDBTunnelIndex
                    Unsigned32,
                hwTunnelFrrRouteDBTunnelInstance
                    Unsigned32,
                hwTunnelFrrRouteDBTunnelIngressLSRId
                    Unsigned32,
                hwTunnelFrrRouteDBTunnelEngressLSRId
                    Unsigned32,
                hwTunnelFrrRouteDBBypassIfIndex
                    Unsigned32,
                hwTunnelFrrRouteDBInnerLabel
                    Unsigned32
             }

--    1.3.6.1.4.1.2011.5.25.121.1.4.1.1
        hwTunnelFrrRouteDBTunnelIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Identifies the index of the primary. Manager obtains new index 
                values for row creation in this table by reading mplsTunnelIndexNext. 
                When the MPLS signaling protocol is rsvp(2), this value equals to 
                the value signaled in the Tunnel ID of the SESSION object. When 
                the MPLS signaling protocol is crldp(3), this value equals to the 
                value signaled in the LSP ID. Reference to MPLS-TE-STD-MIB."
            ::= { hwTunnelFrrRouteDBEntry 1 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.4.1.2
        hwTunnelFrrRouteDBTunnelInstance OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Uniquely identifies a particular instance of a
                tunnel between a pair of ingress and egress LSRs. 
                It is the object identifies multiple instances of 
                tunnels for the purposes of backup and parallel 
                tunnels. When the MPLS signaling protocol is 
                rsvp(2), this value equals to the LSP ID
                of the Sender Template object. When the signaling
                protocol is crldp(3), there is no equivalent
                signaling object. Reference to MPLS-TE-STD-MIB."
            ::= { hwTunnelFrrRouteDBEntry 2 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.4.1.3
        hwTunnelFrrRouteDBTunnelIngressLSRId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Identifies the ingress LSR ID of the primary tunnel. 
                When the MPLS signalling protocol is rsvp(2),LSR ID 
                equals to the Tunnel Sender Address in the Sender 
                Template object or the Extended Tunnel Id in the 
                SESSION object. When the MPLS signalling protocol is 
                crldp(3),  LSR ID equals to the Ingress 
                LSR Router ID in the LSPID TLV object."
            ::= { hwTunnelFrrRouteDBEntry 3 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.4.1.4
        hwTunnelFrrRouteDBTunnelEngressLSRId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Identifies the egress LSR ID of the primary tunnel. 
                Reference to MPLS-TE-STD-MIB."
            ::= { hwTunnelFrrRouteDBEntry 4 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.4.1.5
        hwTunnelFrrRouteDBBypassIfIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the interface index of the bypass tunnel."
            ::= { hwTunnelFrrRouteDBEntry 5 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.4.1.6
        hwTunnelFrrRouteDBInnerLabel OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the inner label of the primary tunnel and bypass tunnel."
            ::= { hwTunnelFrrRouteDBEntry 6 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.5
        hwStaticLspTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwStaticLspEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A static LSP is created by a network administrator by using 
                static MPLS. Note that only point-to-point static LSP segments
                are supported. Each static MPLS LSP can thus have one out-segment
                originating at this LSR and/or one in-segment terminating at
                this LSR. The indexes of this table are hwStaticLspIndex, 
                hwStaticLspInSegmentIndex, and hwStaticLspOutSegmentIndex."
            ::= { hwMplsExtendMibTunnel 5 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.5.1
        hwStaticLspEntry OBJECT-TYPE
            SYNTAX HwStaticLspEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A static LSP is created by a network administrator by using 
                static MPLS. Note that only point-to-point static LSP segments
                are supported. Each static MPLS LSP can thus have one out-segment
                originating at this LSR and/or one in-segment terminating at
                this LSR. The indexes of this entry are hwStaticLspIndex, 
                hwStaticLspInSegmentIndex, and hwStaticLspOutSegmentIndex."
            INDEX { hwStaticLspIndex, hwStaticLspInSegmentIndex, hwStaticLspOutSegmentIndex }
            ::= { hwStaticLspTable 1 }

        
        HwStaticLspEntry ::=
            SEQUENCE { 
                hwStaticLspIndex
                    MplsIndexType,
                hwStaticLspInSegmentIndex
                    MplsIndexType,
                hwStaticLspOutSegmentIndex
                    MplsIndexType,
                hwStaticLspOwner
                    INTEGER,
                hwStaticLspName
                    SnmpAdminString,
                hwStaticLspStatus
                    INTEGER,
                hwStaticLspClassType
                    INTEGER,
                hwStaticLspBandwidth
                    Unsigned32
             }

--    1.3.6.1.4.1.2011.5.25.121.1.5.1.1
        hwStaticLspIndex OBJECT-TYPE
            SYNTAX MplsIndexType
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the index of the static LSP. If the string is 0x00, 
                it means that the index is invalid."
            ::= { hwStaticLspEntry 1 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.5.1.2
        hwStaticLspInSegmentIndex OBJECT-TYPE
            SYNTAX MplsIndexType
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the incoming label index of the static LSP/CR-LSP. 
                If the string is 0x00, it means that the index is invalid. 
                In this case, no corresponding mplsInSegmentEntry exists. 
                Reference to MPLS-LSR-STD-MIB."
            ::= { hwStaticLspEntry 2 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.5.1.3
        hwStaticLspOutSegmentIndex OBJECT-TYPE
            SYNTAX MplsIndexType
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the outgoing index of the static LSP/CR-LSP. 
                If the entry is used to identify the incoming node or 
                intermediate node of the LSP, this object cannot be set 
                to the string 0x00. Because corresponding mplsOutSegmentEntry 
                exists. If the entry is used to identify the outgoing node 
                of the LSP, this object must be set to the string 0x00. Because  
                no corresponding mplsOutSegmentEntry exists. 
                Reference to MPLS-LSR-STD-MIB."
            ::= { hwStaticLspEntry 3 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.5.1.4
        hwStaticLspOwner OBJECT-TYPE
            SYNTAX INTEGER
                {
                static(1),
                crstatic(2),
                other(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Denotes the entity that creates and manages the static LSP. See MPLS-LSR-STD-MIB.
                Options:
                1. static(1)          -indicates the static LSP. 
                2. crstatic(2)        -indicates the static CR-LSP. 
                3. other(3)           -indicates the LSP of another type.
                "
            ::= { hwStaticLspEntry 4 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.5.1.5
        hwStaticLspName OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the name of the static LSP or CR-LSP. 
                The name is appointed when the static LSP or CR-LSP 
                is created."
            REFERENCE
                "RFC 2863 - The Interfaces Group MIB, McCloghrie, K.,
                and F. Kastenholtz, June 2000"
            ::= { hwStaticLspEntry 5 }

        
--    1.3.6.1.4.1.2011.5.25.121.1.5.1.6
        hwStaticLspStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                up(1),
                down(2),
                testing(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the actual operation status of the static LSP/CR-LSP. 
                Options: 
                1. up(1)        -indicates that the static LSP/CR-LSP is in Up state.
                2. down(2)      -indicates that the static LSP/CR-LSP is in down state.
                3. testing(3)   -indicates that the static LSP/CR-LSP is used in test mode.
                "
            ::= { hwStaticLspEntry 6 }

        
        hwStaticLspClassType OBJECT-TYPE
            SYNTAX INTEGER
                {
                ct0(1),
                ct1(2),
                ct2(3),
                ct3(4),
                ct4(5),
                ct5(6),
                ct6(7),
                ct7(8),
                none(9)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Class-Type of this static lsp.
                Options:                                                         
                1. ct0(1)       -indicates that the class type is ct0. 
                2. ct1(2)       -indicates that the class type is ct1.
                3. ct2(3)       -indicates that the class type is ct2.
                4. ct3(4)       -indicates that the class type is ct3.
                5. ct4(5)       -indicates that the class type is ct4.
                6. ct5(6)       -indicates that the class type is ct5.
                7. ct6(7)       -indicates that the class type is ct6.
                8. ct7(8)       -indicates that the class type is ct7.  
                9. none(9)      -indicates that the class type is unconfiged.              
                "        
            ::= { hwStaticLspEntry 7 }
                         
                         
        hwStaticLspBandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of this static lsp.
                Unit: kbit/s"
            ::= { hwStaticLspEntry 8 }

        
        hwMplsTeClassTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwMplsTeClassEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "TE-class mapping is a set of a maximum of eight TE-class items.          
                TE-class is a <Class-Type, Priority> pair, such as TE-Class[1] = <CT0, 5>.              
                A (setup/holding) priority associated with an LSP valid only if it appears
                as a pair with the Class-Type. Class-Types and priorities can be randomly
                paired up. You can define a maximum of eight <Class-Type, Priority> pairs.     
                The LSR is considered to support a particular Class-Type only if it appears 
                in the definition of the eight possible TE-Classes. It is suggested that all
                the LSRs in the domain use the same TE-Class mapping. The index of this table
                is hwMplsTeClassId."
            ::= { hwMplsExtendMibTunnel 6 }

        
        hwMplsTeClassEntry OBJECT-TYPE
            SYNTAX HwMplsTeClassEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "TE-class mapping is a set of a maximum of eight TE-class items.          
                TE-class is a <Class-Type, Priority> pair, such as TE-Class[1] = <CT0, 5>.              
                A (setup/holding) priority associated with an LSP valid only if it appears
                as a pair with the Class-Type. Class-Types and priorities can be randomly
                paired up. You can define a maximum of eight <Class-Type, Priority> pairs.     
                The LSR is considered to support a particular Class-Type only if it appears 
                in the definition of the eight possible TE-Classes. It is suggested that all
                the LSRs in the domain use the same TE-Class mapping. The index of this entry
                is hwMplsTeClassId."
            INDEX { hwMplsTeClassId }
            ::= { hwMplsTeClassTable 1 }

        
        HwMplsTeClassEntry ::=
            SEQUENCE { 
                hwMplsTeClassId
                    Unsigned32,
                hwMplsTeClassClassType
                    INTEGER,
                hwMplsTeClassPriority
                    Unsigned32,
                hwMplsTeClassDescription
                    OCTET STRING
             }

        hwMplsTeClassId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This value represents the index of the TE-Class configured
                on this LSR."
            ::= { hwMplsTeClassEntry 1 }

        
        hwMplsTeClassClassType OBJECT-TYPE
            SYNTAX INTEGER
                {
                ct0(1),
                ct1(2),
                ct2(3),
                ct3(4),
                ct4(5),
                ct5(6),
                ct6(7),
                ct7(8)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This value represents a Class-Type supported on the LSR.
                Options:                                                          
                1. ct0(1)   -indicates that the class type of static CR-LSP is ct0.
                2. ct1(2)   -indicates that the class type of static CR-LSP is ct1.
                3. ct2(3)   -indicates that the class type of static CR-LSP is ct2.
                4. ct3(4)   -indicates that the class type of static CR-LSP is ct3.
                5. ct4(5)   -indicates that the class type of static CR-LSP is ct4.
                6. ct5(6)   -indicates that the class type of static CR-LSP is ct5.
                7. ct6(7)   -indicates that the class type of static CR-LSP is ct6.
                8. ct7(8)   -indicates that the class type of static CR-LSP is ct7.
                "
            ::= { hwMplsTeClassEntry 2 }

        
        hwMplsTeClassPriority OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This value represents the preemption priority (setup or holding) 
                supported for a particular class-type, on the LSR.
                Range: 0-7
                Default: 7
                "
            ::= { hwMplsTeClassEntry 3 }

        
        hwMplsTeClassDescription OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Textual description of the TE-Class defined by this row."
            ::= { hwMplsTeClassEntry 4 }

        
        hwMplsIfBcTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwMplsIfBcEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes bandwidth constraints associated with MPLS TE
                enabled interfaces. The index of this table is ifIndex."
            ::= { hwMplsExtendMibTunnel 7 }

        
        hwMplsIfBcEntry OBJECT-TYPE
            SYNTAX HwMplsIfBcEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes bandwidth constraints associated with MPLS TE
                enabled interfaces. The index of this entry is ifIndex."
            INDEX { ifIndex }
            ::= { hwMplsIfBcTable 1 }

        
        HwMplsIfBcEntry ::=
            SEQUENCE { 
                hwMplsIfMaxResvBandwidth
                    Unsigned32,
                hwMplsIfBc0Bandwidth
                    Unsigned32,
                hwMplsIfBc1Bandwidth
                    Unsigned32,
                hwMplsIfBc2Bandwidth
                    Unsigned32,
                hwMplsIfBc3Bandwidth
                    Unsigned32,
                hwMplsIfBc4Bandwidth
                    Unsigned32,
                hwMplsIfBc5Bandwidth
                    Unsigned32,
                hwMplsIfBc6Bandwidth
                    Unsigned32,
                hwMplsIfBc7Bandwidth
                    Unsigned32
             }

        hwMplsIfMaxResvBandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The maximum reservable bandwidth on this interface.
                Unit: kbit/s 
                "
            ::= { hwMplsIfBcEntry 1 }

        
        hwMplsIfBc0Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 0 (CT0) in this tunnel.
                Unit: kbit/s
                "
            ::= { hwMplsIfBcEntry 2 }

        
        
        hwMplsIfBc1Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 1 (CT1) in this tunnel.
                Unit: kbit/s
                "
            ::= { hwMplsIfBcEntry 3 }

        
        hwMplsIfBc2Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 2 (CT2) in this tunnel.
                Unit: kbit/s
                "
            ::= { hwMplsIfBcEntry 4 }

        
        hwMplsIfBc3Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 3 (CT3) in this tunnel.
                Unit: kbit/s
                "
            ::= { hwMplsIfBcEntry 5 }

        
        hwMplsIfBc4Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 4 (CT4) in this tunnel.
                Unit: kbit/s
                "
            ::= { hwMplsIfBcEntry 6 }

        
        hwMplsIfBc5Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 5 (CT5) in this tunnel.
                Unit: kbit/s
                "
            ::= { hwMplsIfBcEntry 7 }

        
        hwMplsIfBc6Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 6 (CT6) in this tunnel.
                Unit: kbit/s
                "
            ::= { hwMplsIfBcEntry 8 }
                
        
        hwMplsIfBc7Bandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "kilobits per second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bandwidth of Class-Type 7 (CT7) in this tunnel.
                Unit: kbit/s
                "               
            ::= { hwMplsIfBcEntry 9 }
        
        hwStaticLspTnlTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwStaticLspTnlEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "hwStaticLspTnlTable is used to display static LSP token of   
                 a static LSP of a specified name. The index of this table 
                 is hwStaticLspTnlName."
            ::= { hwMplsExtendMibTunnel 8 }
        
        hwStaticLspTnlEntry OBJECT-TYPE
            SYNTAX HwStaticLspTnlEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "hwStaticLspTnlTable is used to display static LSP token of   
                 a static LSP of a specified name. The index of this entry 
                 is hwStaticLspTnlName."
            INDEX { hwStaticLspTnlName }
            ::= { hwStaticLspTnlTable 1 }
        
        HwStaticLspTnlEntry ::=
            SEQUENCE { 
                hwStaticLspTnlName
                    SnmpAdminString,
                hwStaticLspTnlToken
                    Unsigned32
             }

        hwStaticLspTnlName OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the name of the Static Lsp."
            ::= { hwStaticLspTnlEntry 1 }
        
        hwStaticLspTnlToken OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the token of the Static Lsp."
            ::= { hwStaticLspTnlEntry 2 }
        
        hwMplsTeVpnQosTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwMplsTeVpnQosEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is used to display VPN QoS information of a specified TE Tunnel according to TunnelID.
                 The index of this table is hwMplsTnlID."
            ::= { hwMplsExtendMibTunnel 9 }
            
        hwMplsTeVpnQosEntry OBJECT-TYPE
            SYNTAX HwMplsTeVpnQosEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is used to display VPN QoS information of a specified TE Tunnel according to TunnelID.
                 The index of this entry is hwMplsTnlID."
            INDEX { hwMplsTnlID }
            ::= { hwMplsTeVpnQosTable 1 } 
            
        HwMplsTeVpnQosEntry ::=
             SEQUENCE { 
                hwMplsTnlID
                    Unsigned32,             
                hwMplsTeVpnMaxBandwidth
                    Unsigned32,
                hwMplsTeVpnAllocatedBandwidth
                    Unsigned32
             }
             
        hwMplsTnlID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The value of this object identifies the TE tunnel ID."
            ::= { hwMplsTeVpnQosEntry 1 } 
            
       hwMplsTeVpnMaxBandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the bandwidth the TE tunnel can provide for VPN QoS.
                Unit: kbit/s"
            ::= { hwMplsTeVpnQosEntry 2 }         
                    
       hwMplsTeVpnAllocatedBandwidth OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the bandwidth used by VPN QoS, in Kbps.
                Unit: kbit/s"
            ::= { hwMplsTeVpnQosEntry 3 }

       hwStaticLspInIfIndex OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Indicates the inbound interface index of a static LSP/CR-LSP."
            ::= { hwMplsExtendMibTunnel 11 }

        -- 1.3.6.1.4.1.2011.5.25.121.1.12
        hwStaticLspInIfName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Indicates the name of an inbound interface of a static LSP/CR-LSP."
            ::= { hwMplsExtendMibTunnel 12 }

        -- 1.3.6.1.4.1.2011.5.25.121.1.13
        hwStaticLspDownReason OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Indicates the reason for static LSP/CR-LSP Down:
                0. Other
                1. Static LSP/CR-LSP up
                2. MPLS disabled on an interface
                3. MPLS TE disabled on an interface
                4. Route change
                5. Tunnel binding associated with the static LSP/CR-LSP deleted
                6. Static LSP/CR-LSP configuration delete
                7. Inbound interface Down
                8. Outbound interface Down
                9. Tunnel associated with the static LSP/CR-LSP has been shut down
                10. Static LSP/CR-LSP configuration update
                11. The bound ring is invalid."                
            ::= { hwMplsExtendMibTunnel 13 }

--   1.3.6.1.4.1.2011.5.25.121.1.14
        hwMplsTunnelStatisticsTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwMplsTunnelStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A tunnel needs to be uniquely identified across  
                 an MPLS network. hwMplsTunnelStatisticsTunnelIndex 
                 uniquely identifies a tunnel on the LSR originating 
                 the tunnel. hwMplsTunnelStatisticsIngressLSRId 
                 uniquely identifies a tunnel across an MPLS network. 
                 The last index hwMplsTunnelStatisticsEgressLSRId is 
                 useful in identifying all instances of a tunnel that
                 are terminated on the same egress LSR. 

                 The indexes of this table are 
                 hwMplsTunnelStatisticsTunnelIndex,    
                 hwMplsTunnelStatisticsIngressLSRId and  
                 hwMplsTunnelStatisticsEgressLSRId."
            ::= { hwMplsExtendMibTunnel 14 }

--   1.3.6.1.4.1.2011.5.25.121.1.14.1
        hwMplsTunnelStatisticsEntry OBJECT-TYPE
            SYNTAX HwMplsTunnelStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A tunnel needs to be uniquely identified across 
                 an MPLS network. hwMplsTunnelStatisticsTunnelIndex 
                 uniquely identifies a tunnel on the LSR originating 
                 the tunnel. hwMplsTunnelStatisticsIngressLSRId uniquely 
                 identifies a tunnel across an MPLS network. The last 
                 index hwMplsTunnelStatisticsEgressLSRId is useful in 
                 identifying all instances of a tunnel that are terminated
                 on the same egress LSR.

                 The indexes of this table are 
                 hwMplsTunnelStatisticsTunnelIndex,    
                 hwMplsTunnelStatisticsIngressLSRId and  
                 hwMplsTunnelStatisticsEgressLSRId."
            REFERENCE
                "1. RFC 2863 - The Interfaces Group MIB, McCloghrie,
                K., and F. Kastenholtz, June 2000 "
            INDEX { hwMplsTunnelStatisticsTunnelIndex, hwMplsTunnelStatisticsIngressLSRId, hwMplsTunnelStatisticsEgressLSRId }
            ::= { hwMplsTunnelStatisticsTable 1 }

        
        HwMplsTunnelStatisticsEntry ::=
            SEQUENCE { 
                hwMplsTunnelStatisticsTunnelIndex
                    Unsigned32,
                hwMplsTunnelStatisticsIngressLSRId
                    IpAddress,
                hwMplsTunnelStatisticsEgressLSRId
                    IpAddress,
                hwMplsTunnelStatisticsHCInOctets 
                    Counter64,
                hwMplsTunnelStatisticsHCOutOctets
                    Counter64
             }

--   1.3.6.1.4.1.2011.5.25.121.1.14.1.1
        hwMplsTunnelStatisticsTunnelIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Uniquely identifies a set of tunnel instances 
                 between a pair of ingress and egress LSRs. 
                 When the MPLS signalling protocol is rsvp(2), this value 
                 equals to the value signaled in the Tunnel ID 
                 of the SESSION object. When the MPLS signalling protocol 
                 is crldp(3), this value equals to the value 
                 signaled in the LSP ID. Reference to MPLS-TE-STD-MIB."
            ::= { hwMplsTunnelStatisticsEntry 1 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.14.1.2
        hwMplsTunnelStatisticsIngressLSRId OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the ingress LSR ID of this tunnel. 
                 When the MPLS signalling protocol 
                 is rsvp(2), this value equals to the Tunnel 
                 Sender Address in the Sender Template object and may 
                 equal to the Extended Tunnel ID in the 
                 SESSION object. When the MPLS signalling protocol is 
                 crldp(3), this value equals to the Ingress 
                 LSR Router ID in the LSPID TLV object. 
                 Reference to MPLS-TE-STD-MIB."
            ::= { hwMplsTunnelStatisticsEntry 2 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.14.1.3
        hwMplsTunnelStatisticsEgressLSRId OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the egress LSR ID of this 
                 tunnel. Reference to MPLS-TE-STD-MIB."
            ::= { hwMplsTunnelStatisticsEntry 3 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.14.1.4
        hwMplsTunnelStatisticsHCInOctets OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of octets received on the interface,
                 including framing characters."
            ::= { hwMplsTunnelStatisticsEntry 4 }

        
--   1.3.6.1.4.1.2011.5.25.121.1.14.1.5
        hwMplsTunnelStatisticsHCOutOctets OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total number of octets transmitted out of the
                 interface, including framing characters."
            ::= { hwMplsTunnelStatisticsEntry 5 }

                                                         
--   1.3.6.1.4.1.2011.5.25.121.2
        hwMplsExtendTrap OBJECT IDENTIFIER ::= { hwMplsExtendMib 2 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1
        hwLspTrap OBJECT IDENTIFIER ::= { hwMplsExtendTrap 1 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.1
        hwMplsStaticLspUp NOTIFICATION-TYPE
            OBJECTS { hwStaticLspName, hwStaticLspStatus, ifName, hwStaticLspInIfIndex, hwStaticLspInIfName, hwStaticLspDownReason }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of referred static LSP changes to Up."
            ::= { hwLspTrap 1 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.2
        hwMplsStaticLspDown NOTIFICATION-TYPE
            OBJECTS { hwStaticLspName, hwStaticLspStatus, ifName, hwStaticLspInIfIndex, hwStaticLspInIfName, hwStaticLspDownReason }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of referred static LSP changes to Down."
            ::= { hwLspTrap 2 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.3
        hwMplsStaticCRLspUp NOTIFICATION-TYPE
            OBJECTS { hwStaticLspName, hwStaticLspStatus, ifName, hwStaticLspInIfIndex, hwStaticLspInIfName, hwStaticLspDownReason }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of referred static CR-LSP changes to Up."
            ::= { hwLspTrap 3 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.4
        hwMplsStaticCRLspDown NOTIFICATION-TYPE
            OBJECTS { hwStaticLspName, hwStaticLspStatus, ifName, hwStaticLspInIfIndex, hwStaticLspInIfName, hwStaticLspDownReason }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of referred static CR-LSP changes to Down."
            ::= { hwLspTrap 4 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.5
        hwMplsTeFrrProtAval NOTIFICATION-TYPE
            OBJECTS { hwTunnelFrrRouteDBBypassIfIndex, hwTunnelFrrRouteDBInnerLabel }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the primary tunnel is bound to TE FRR bypass tunnel."
            ::= { hwLspTrap 5 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.6
        hwMplsTeFrrProtNotAval NOTIFICATION-TYPE
            OBJECTS { hwTunnelFrrRouteDBBypassIfIndex }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the primary tunnel is unbound to bypass tunnel."
            ::= { hwLspTrap 6 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.7
        hwMplsTeFrrSwitch NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus, hwMplsSessionTunnelId, hwMplsLocalLspId, hwMplsIngressLsrId, hwMplsEgressLsrId}
            STATUS current
            DESCRIPTION 
                "This notification indicates that the primary tunnel is switches to the TE FRR bypass tunnel."
            ::= { hwLspTrap 7 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.8
        hwMplsTeFrrResume NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the primary tunnel is switched back from the TE FRR bypass tunnel."
            ::= { hwLspTrap 8 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.9
        hwMplsTunnelHSBSwitch NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the data is switched from the primary CR-LSP to the HSB CR-LSP."
            ::= { hwLspTrap 9 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.10
        hwMplsTunnelHSBResume NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the data is switched from the HSB CR-LSP to the primary CR-LSP."
            ::= { hwLspTrap 10 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.11
        hwMplsTunnelOBSwitch NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the primary CR-LSP is down and the Ordinary backup CR-LSP is up."
            ::= { hwLspTrap 11 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.12
        hwMplsTunnelOBResume NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the data is switched from the Ordinary backup CR-LSP to the primary CR-LSP."
            ::= { hwLspTrap 12 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.13
        hwMplsTunnelUp NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus }
            STATUS obsolete
            DESCRIPTION 
                "The hwMplsTunnelUp trap indicates that the staus of the tunnel changes into Up."
            ::= { hwLspTrap 13 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.14        
        hwMplsTunnelDown NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus }
            STATUS obsolete
            DESCRIPTION 
                "The hwMplsTunnelDown trap indicates that the staus of the tunnel changes into Down."
            ::= { hwLspTrap 14 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.15
        hwMplsTunnelChangeBw NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelIfIndex, hwMplsTunnelPreBandwidth, hwMplsTunnelNextBandwidth }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the bandwidth of the tunnel is changed."
            ::= { hwLspTrap 15 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.16
        hwMplsTunnelTpOamLossSD NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "This object indicates that the loss ratio of the packets carried by the tunnel exceeded the first threshold."
            ::= { hwLspTrap 16 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.17
        hwMplsOamSDRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto  }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that the loss ratio of the packets carried by the tunnel dropped below the first threshold.
                "
            ::= { hwLspTrap 17 } 

--   1.3.6.1.4.1.2011.5.25.121.2.1.18
        hwMplsOamLoss NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto, ifName}
            STATUS current
            DESCRIPTION 
                "
                This object indicates that TP OAM detected tunnel connectivity faults.
                "
            ::= { hwLspTrap 18 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.19
        hwMplsOamLossRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto  }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that TP OAM did not detect tunnel connectivity faults.
                "
            ::= { hwLspTrap 19 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.20
        hwMplsOamAis NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto  }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that TP OAM detected an alarm indication signal.
                "
            ::= { hwLspTrap 20 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.21
        hwMplsOamAisRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto  }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that TP OAM no longer detected alarm indication signals.
                "
            ::= { hwLspTrap 21 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.22
        hwMplsOamRdi NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto, ifName}
            STATUS current
            DESCRIPTION 
                "
                This object indicates that TP OAM detected remote defects.
                "
            ::= { hwLspTrap 22 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.23
        hwMplsOamRdiRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto  }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that the remote defects detected by TP OAM were removed.
                "
            ::= { hwLspTrap 23 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.24
        hwMplsOamMeg NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto  }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that the names configured on the two ends of the tunnel are inconsistent.
                "
            ::= { hwLspTrap 24 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.25
        hwMplsOamMegRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that the names configured on the two ends of the tunnel now are consistent.
                "
            ::= { hwLspTrap 25 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.26
        hwMplsOamMep NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that the MEP-IDs configured on the two ends of the tunnel are inconsistent.
                "
            ::= { hwLspTrap 26 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.27
        hwMplsOamMepRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that the MEP-IDs configured on the two ends of the tunnel now are consistent.
                "
            ::= { hwLspTrap 27 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.28
        hwMplsOamSF NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that the loss ratio of the packets carried by the tunnel exceeded the second threshold in the local link.
                "
            ::= { hwLspTrap 28 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.29
        hwMplsOamSFRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that the loss ratio of the packets carried by the tunnel dropped below the second threshold in the local link.
                "
            ::= { hwLspTrap 29 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.30
        hwMplsOamPeriod NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that the TP OAM detection periods on the two ends of the tunnel are inconsistent.
                "
            ::= { hwLspTrap 30 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.31
        hwMplsOamPeriodRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that the TP OAM detection periods on the two ends of the tunnel now are consistent.
                "
            ::= { hwLspTrap 31 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.32
        hwMplsOamLck NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that TP OAM detected the service level of the tunnel has been locked.                
                "
            ::= { hwLspTrap 32 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.33
        hwMplsOamLckRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that TP OAM detected the service level of the tunnel has not been locked.
                "
            ::= { hwLspTrap 33 }
                      
--   1.3.6.1.4.1.2011.5.25.121.2.1.34
        hwMplsOamExcess NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received excess alarm.
                "
            ::= { hwLspTrap 34 } 
            
--   1.3.6.1.4.1.2011.5.25.121.2.1.35
        hwMplsOamExcessRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received excess alarm end.
                "
            ::= { hwLspTrap 35 } 
        
--   1.3.6.1.4.1.2011.5.25.121.2.1.36
        hwMplsOamMisMatch NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received MisMatch alarm.
                "
            ::= { hwLspTrap 36 } 

--   1.3.6.1.4.1.2011.5.25.121.2.1.37
        hwMplsOamMisMatchRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received MisMatch alarm end.
                "
            ::= { hwLspTrap 37 } 

--   1.3.6.1.4.1.2011.5.25.121.2.1.38
        hwMplsOamMisMerge NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received MisMerge alarm.
                "
            ::= { hwLspTrap 38 } 

--   1.3.6.1.4.1.2011.5.25.121.2.1.39
        hwMplsOamMisMergeRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received MisMerge alarm end.
                "
            ::= { hwLspTrap 39 } 

--   1.3.6.1.4.1.2011.5.25.121.2.1.40
        hwMplsOamUnknown NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received Unknown alarm.
                "
            ::= { hwLspTrap 40 } 

--   1.3.6.1.4.1.2011.5.25.121.2.1.41
        hwMplsOamUnknownRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received Unknown alarm end.
                "
            ::= { hwLspTrap 41 } 

--   1.3.6.1.4.1.2011.5.25.121.2.1.42
        hwMplsOamBDI NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto, ifName}
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received BDI alarm.
                "
            ::= { hwLspTrap 42 } 

--   1.3.6.1.4.1.2011.5.25.121.2.1.43
        hwMplsOamBDIRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received BDI alarm end.
                "
            ::= { hwLspTrap 43 } 

--   1.3.6.1.4.1.2011.5.25.121.2.1.44
        hwMplsOamFail NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto, ifName}
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received OAMFAIL alarm.
                "
            ::= { hwLspTrap 44 } 

--   1.3.6.1.4.1.2011.5.25.121.2.1.45
        hwMplsOamFailRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that MPLS OAM detected the tunnel received OAMFAIL alarm end.
                "
            ::= { hwLspTrap 45 } 

--   1.3.6.1.4.1.2011.5.25.121.2.1.46
        hwMplsTunnelPrimaryUp NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of the RSVP-TE Primary LSP changes to Up."
            ::= { hwLspTrap 46 }
            
--   1.3.6.1.4.1.2011.5.25.121.2.1.47
        hwMplsTunnelPrimaryDown NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelDownReason, hwMplsTunnelDownLSRID, hwMplsTunnelDownIfIpAddrType, hwMplsTunnelDownIfIpAddr }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of the RSVP-TE Primary LSP changes to Down."
            ::= { hwLspTrap 47 }
            
--   1.3.6.1.4.1.2011.5.25.121.2.1.48
        hwMplsTunnelHotstandbyUp NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of the RSVP-TE Hot-standby LSP changes to Up."
            ::= { hwLspTrap 48 }
            
--   1.3.6.1.4.1.2011.5.25.121.2.1.49
        hwMplsTunnelHotstandbyDown NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelDownReason, hwMplsTunnelDownLSRID, hwMplsTunnelDownIfIpAddrType, hwMplsTunnelDownIfIpAddr}
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of the RSVP-TE Hot-standby LSP changes to Down."
            ::= { hwLspTrap 49 }
            
--   1.3.6.1.4.1.2011.5.25.121.2.1.50
        hwMplsTunnelOrdinaryUp NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of the RSVP-TE Ordinary LSP changes to Up."
            ::= { hwLspTrap 50 }
            
--   1.3.6.1.4.1.2011.5.25.121.2.1.51
        hwMplsTunnelOrdinaryDown NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelDownReason, hwMplsTunnelDownLSRID, hwMplsTunnelDownIfIpAddrType, hwMplsTunnelDownIfIpAddr }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of the RSVP-TE Ordinary LSP changes to Down."
            ::= { hwLspTrap 51 }
            
--   1.3.6.1.4.1.2011.5.25.121.2.1.52
        hwMplsTunnelBesteffortUp NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of the RSVP-TE Best-effort LSP changes to Up."
            ::= { hwLspTrap 52 }
            
--   1.3.6.1.4.1.2011.5.25.121.2.1.53
        hwMplsTunnelBesteffortDown NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelDownReason, hwMplsTunnelDownLSRID, hwMplsTunnelDownIfIpAddrType, hwMplsTunnelDownIfIpAddr }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of the RSVP-TE Best-effort LSP changes to Down."
            ::= { hwLspTrap 53 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.54
        hwMplsTeAutoTunnelDownClear NOTIFICATION-TYPE
            OBJECTS { mplsTunnelAdminStatus, mplsTunnelOperStatus, hwMplsTunnelIfName }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the TE Auto tunnel Down alarm was cleared."
            ::= { hwLspTrap 54 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.55
        hwMplsTeAutoTunnelPrimaryDownClear NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the Down alarm about the primary LSP in the TE Auto tunnel was cleared."
            ::= { hwLspTrap 55 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.56
        hwMplsTunnelBBSwitch NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the primary CR-LSP is Down and the Best-effort backup CR-LSP is Up."
            ::= { hwLspTrap 56 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.57
        hwMplsTunnelBBResume NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus }
            STATUS current
            DESCRIPTION 
                "This notification indicates that data is switched from the Best-effort backup CR-LSP to the primary CR-LSP."
            ::= { hwLspTrap 57 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.58
        hwMplsExtTunnelDown NOTIFICATION-TYPE
            OBJECTS {hwMplsTunnelInterfaceName, hwMplsTunnelType, hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus, hwMplsTunnelDownReason, ifName, hwMplsTunnelDownLSRID, hwMplsTunnelDownIfIpAddrType, hwMplsTunnelDownIfIpAddr}
            STATUS current
            DESCRIPTION 
                "This notification indicates that the status of te tunnel changes to Down."
            ::= { hwLspTrap 58 }
            
--   1.3.6.1.4.1.2011.5.25.121.2.1.59
        hwMplsExtTunnelDownClear NOTIFICATION-TYPE
            OBJECTS {hwMplsTunnelInterfaceName, hwMplsTunnelType, hwMplsTunnelAdminStatus, hwMplsTunnelOperStatus, hwMplsTunnelDownReason, ifName}
            STATUS current
            DESCRIPTION 
                "This notification indicates that the down alarm of te tunnel was cleared."
            ::= { hwLspTrap 59 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.60
        hwMplsOamLocalLock NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that TP OAM detected the tunnel has been locked.
                "
            ::= { hwLspTrap 60 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.61
        hwMplsOamLocalLockRecovery NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto }
            STATUS current
            DESCRIPTION 
                "
                This object indicates that TP OAM detected the tunnel has not been locked.
                "
            ::= { hwLspTrap 61 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.62
        hwMplsTunnelDelete NOTIFICATION-TYPE
            OBJECTS {mplsTunnelAdminStatus,mplsTunnelOperStatus,hwMplsTunnelIfName}
            STATUS current
            DESCRIPTION 
                "This notification indicates that the mpls te tunnel was deleted."
            ::= { hwLspTrap 62 }

--  1.3.6.1.4.1.2011.5.25.121.2.1.63
       hwMplsLspThresholdExceed NOTIFICATION-TYPE
            OBJECTS { hwMplsLspProtocol, hwMplsLspCurrentCount, hwMplsLspThreshold, hwMplsLspTotalCount }
            STATUS current
            DESCRIPTION
                "
                This object indicates that lsp count has exceeded the threshold.
                "
            ::= { hwLspTrap 63 }

--  1.3.6.1.4.1.2011.5.25.121.2.1.64
       hwMplsLspThresholdExceedClear NOTIFICATION-TYPE
            OBJECTS { hwMplsLspProtocol }
            STATUS current
            DESCRIPTION
                "
                This object indicates that lsp count has resumed from exceeding the threshold.
                " 
            ::= { hwLspTrap 64 }               

--  1.3.6.1.4.1.2011.5.25.121.2.1.65
       hwMplsLspTotalCountExceed NOTIFICATION-TYPE
            OBJECTS { hwMplsLspProtocol, hwMplsLspTotalCount }
            STATUS current
            DESCRIPTION
                "
                This object indicates that lsp count has reached the total count.
                "    
            ::= { hwLspTrap 65 }     
                                        
--  1.3.6.1.4.1.2011.5.25.121.2.1.66
       hwMplsLspTotalCountExceedClear NOTIFICATION-TYPE
            OBJECTS { hwMplsLspProtocol }
            STATUS current
            DESCRIPTION
                "
                This object indicates that lsp count has resumed from reaching the total count.
                " 
            ::= { hwLspTrap 66 }    

--  1.3.6.1.4.1.2011.5.25.121.2.1.67
       hwMplsDynamicLabelThresholdExceed NOTIFICATION-TYPE
            OBJECTS { hwMplsDynamicLabelTotalCount, hwMplsDynamicLabelCurrentCount, hwMplsDynamicLabelThresholdUpperLimit, hwMplsDynamicLabelThresholdLowerLimit }
            STATUS current
            DESCRIPTION
                "
                This object indicates that label usage has exceeded the threshold.
                "
            ::= { hwLspTrap 67 }

--  1.3.6.1.4.1.2011.5.25.121.2.1.68
       hwMplsDynamicLabelThresholdExceedClear NOTIFICATION-TYPE
            OBJECTS { hwMplsDynamicLabelTotalCount, hwMplsDynamicLabelCurrentCount, hwMplsDynamicLabelThresholdUpperLimit, hwMplsDynamicLabelThresholdLowerLimit }
            STATUS current
            DESCRIPTION
                "
                This object indicates that label usage has resumed from exceeding the threshold.
                " 
            ::= { hwLspTrap 68 }               

--  1.3.6.1.4.1.2011.5.25.121.2.1.69
       hwMplsDynamicLabelTotalCountExceed NOTIFICATION-TYPE
            OBJECTS { hwMplsDynamicLabelTotalCount, hwMplsDynamicLabelCurrentCount }
            STATUS current
            DESCRIPTION
                "
                This object indicates that label count has reached the total count.
                "    
            ::= { hwLspTrap 69 }     
                                        
--  1.3.6.1.4.1.2011.5.25.121.2.1.70
       hwMplsDynamicLabelTotalCountExceedClear NOTIFICATION-TYPE
            OBJECTS { hwMplsDynamicLabelTotalCount, hwMplsDynamicLabelCurrentCount }
            STATUS current
            DESCRIPTION
                "
                This object indicates that label usage count has resumed from reaching the total count.
                " 
            ::= { hwLspTrap 70 }

--  1.3.6.1.4.1.2011.5.25.121.2.1.71
       hwMplsResourceThresholdExceed NOTIFICATION-TYPE
            OBJECTS { hwMplsResourceType, hwMplsResourceCurrentCount, hwMplsResourceThreshold, hwMplsResourceTotalCount }
            STATUS current
            DESCRIPTION
                "
                This object indicates that the number of MPLS resources has exceeded the upper threshold.
                "
            ::= { hwLspTrap 71 }

--  1.3.6.1.4.1.2011.5.25.121.2.1.72
       hwMplsResourceThresholdExceedClear NOTIFICATION-TYPE
            OBJECTS { hwMplsResourceType }
            STATUS current
            DESCRIPTION
                "
                This object indicates that the number of MPLS resources has fallen below the lower threshold.
                " 
            ::= { hwLspTrap 72 }               

--  1.3.6.1.4.1.2011.5.25.121.2.1.73
       hwMplsResourceTotalCountExceed NOTIFICATION-TYPE
            OBJECTS { hwMplsResourceType, hwMplsResourceTotalCount }
            STATUS current
            DESCRIPTION
                "
                This object indicates that the number of MPLS resources has reached the maximum number.
                "    
            ::= { hwLspTrap 73 }     
                                        
--  1.3.6.1.4.1.2011.5.25.121.2.1.74
       hwMplsResourceTotalCountExceedClear NOTIFICATION-TYPE
            OBJECTS { hwMplsResourceType }
            STATUS current
            DESCRIPTION
                "
                This object indicates that the number of MPLS resources fallen below the recovery number.
                " 
            ::= { hwLspTrap 74 }

--  1.3.6.1.4.1.2011.5.25.121.2.1.75
       hwMplsLspLoopBack NOTIFICATION-TYPE
            OBJECTS { hwMplsSessionTunnelId, hwMplsLocalLspId, hwMplsIngressLsrId, hwMplsEgressLsrId, hwMplsLspName }
            STATUS current
            DESCRIPTION
                "
                This object indicates that the lsp was looped back.
                " 
            ::= { hwLspTrap 75 }

--  1.3.6.1.4.1.2011.5.25.121.2.1.76
       hwMplsLspLoopBackClear NOTIFICATION-TYPE
            OBJECTS { hwMplsSessionTunnelId, hwMplsLocalLspId, hwMplsIngressLsrId, hwMplsEgressLsrId, hwMplsLspName }
            STATUS current
            DESCRIPTION
                "
                This object indicates that loopback of the LSP is restored.
                " 
            ::= { hwLspTrap 76 }

--  1.3.6.1.4.1.2011.5.25.121.2.1.77
       hwMplsTunnelCommitLost NOTIFICATION-TYPE
            STATUS current
            DESCRIPTION
                "
                This object indicates that, after the device saves MPLS TE tunnel configurations, the device commits only some MPLS tunnel configurations.
                " 
            ::= { hwLspTrap 77 } 

--  1.3.6.1.4.1.2011.5.25.121.2.1.78
       hwMplsTunnelCommitLostClear NOTIFICATION-TYPE
            STATUS current
            DESCRIPTION
                "
                This object indicates that, after the device saves MPLS TE tunnel configurations, the device commits all MPLS tunnel configurations.
                " 
            ::= { hwLspTrap 78 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.79
        hwMplsTunnelHotstandbySwitch NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the data is switched from the primary CR-LSP to the HSB CR-LSP."
            ::= { hwLspTrap 79 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.80
        hwMplsTunnelHotstandbyResume NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the data is switched from the HSB CR-LSP to the primary CR-LSP."
            ::= { hwLspTrap 80 }


--   1.3.6.1.4.1.2011.5.25.121.2.1.81
        hwMplsTunnelBfdPathMismatch NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsSessionTunnelId, hwMplsLocalLspId, hwMplsIngressLsrId, hwMplsEgressLsrId, hwMplsTunnelIfName }
            STATUS current
            DESCRIPTION 
                "This notification indicates the forward primary LSP path is the same as the reverse hot-standby LSP path, and the reverse primary LSP path is the same as the forward hot-standby LSP path, causing path mismatches."
            ::= { hwLspTrap 81 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.82
        hwMplsTunnelBfdPathMismatchClear NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsSessionTunnelId, hwMplsLocalLspId, hwMplsIngressLsrId, hwMplsEgressLsrId, hwMplsTunnelIfName }
            STATUS current
            DESCRIPTION 
                "This notification indicates that either or both path mismatches were rectified."
            ::= { hwLspTrap 82 }
    
--   1.3.6.1.4.1.2011.5.25.121.2.1.83
        hwMplsTeLspBfdDown NOTIFICATION-TYPE
            OBJECTS {hwMplsTunnelInterfaceName, hwMplsTunnelLspType }
            STATUS current
            DESCRIPTION 
                "This notification indicates the bfd status of te-lsp changes to down. "
            ::= { hwLspTrap 83 }

        
--   1.3.6.1.4.1.2011.5.25.121.2.1.84
        hwMplsTeLspBfdDownClear NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName, hwMplsTunnelLspType }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the down alarm of bfd was cleared."
            ::= { hwLspTrap 84 }

--   1.3.6.1.4.1.2011.5.25.121.2.1.85 
        hwMplsTunnelDelegationReturn NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the delegation of Tunnel LSP is returned by server."
            ::= { hwLspTrap 85 }


--   1.3.6.1.4.1.2011.5.25.121.2.1.85 
        hwMplsTunnelDelegationReturnClear NOTIFICATION-TYPE
            OBJECTS { hwMplsTunnelInterfaceName }
            STATUS current
            DESCRIPTION 
                "This notification indicates that the delegation of Tunnel LSP is returned by server."
            ::= { hwLspTrap 86 }
            
-- 1.3.6.1.4.1.2011.5.25.121.2.2
        hwMplsTrapObjects OBJECT IDENTIFIER ::= { hwMplsExtendTrap 2 }
        
         hwMplsTunnelIfName OBJECT-TYPE
         SYNTAX           SnmpAdminString
         MAX-ACCESS     accessible-for-notify
         STATUS           obsolete
         DESCRIPTION
             "The Tunnel Interface name."
         ::= { hwMplsTrapObjects 1 }  
             
            
        hwMplsTunnelFrrConfigOper OBJECT-TYPE
        SYNTAX  INTEGER
             {
             unconfig(0),
             config(1),
             unknow(2)
             }
        MAX-ACCESS     accessible-for-notify
        STATUS           obsolete
        DESCRIPTION
            "The value of this object identifies the operation that an FRR configuration is committed on the tunnel.
            Options:                                                       
            1.unconfig(0) -indicates the configuration of the undo mpls te fast-reroute command is committed.  
            2.config(1)   -indicates the configuration of the mpls te fast-reroute command is committed.      
            3.unknow(2)   -indicates an unknown operation."
        ::= { hwMplsTrapObjects 2 }

        hwMplsTunnelDownReason OBJECT-TYPE
            SYNTAX INTEGER
            {
            other(1),
            staticLspDown(2),
            staticCrlspDown(3),
            outIfDown(4),
            resourcePreempted(5),
            rsvpMessageTimeout(6),
            rsvpNeighborLost(7),
            bypassTunnelDownOrUnbinded(8),
            cspfComputeFail(9),
            userShutdown(10),
            tpoamLossOfContinuity(11),
            tpoamAlarmIndicationSignal(12),
            tpoamRemoteDefectIndication(13),
            tpoamUnexpectedMEG(14),
            tpoamUnexpectedMEP(15),
            tpoamLossSF(16),
            tpoamPeriod(17),
            mplsOamLocv(18),
            mplsOamExcess(19),
            mplsOamMisMatch(20),
            mplsOamMisMerge(21),
            mplsOamUnknown(22),
            mplsOamBdi(23),
            mplsOamFdi(24),
            mplsOamSF(25),
            mplsOamSD(26),
            mplsOamDOamFail(27),
            serviceResume(28),
            serviceDelete(29),
            clear(100)
            }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Indicates the alarm reason as below:
                1. Other;
                2. Static LSP down;
                3. Static CR-LSP down;
                4. The out interface of the RSVP LSP ingress is down; 
                5. The resource of RSVP LSP is preempted;
                6. RSVP message timeout;
                7. RSVP neighbor lost;
                8. The bypass-tunnel is down or is unbinded with main tunnel, as bypass-tunnel is in used;
                9. CSPF compute fail;
                10.User shutdown the tunnel;
                11.TPOAM indicates the connectivity fault of the link;
                12.TPOAM indicates receive alarm indication signal defect of the link;
                13.TPOAM indicates the remote defect of the link;
                14.TPOAM indicates receive unexpected MEG-ID defect of the link;
                15.TPOAM indicates receive unexpected MEP-ID defect of the link;
                16.TPOAM indicates packet lost exceed signal fault threshold in the local link;
                17.TPOAM indicates packet unexpected period defect of the link;
                18.MPLS OAM connectivity fault;
                19.MPLS OAM TTSI excess;
                20.MPLS OAM TTSI mismatch;
                21.MPLS OAM TTSI merge error;
                22.MPLS OAM unknown error;
                23.MPLS OAM BDI;
                24.MPLS OAM FDI;
                25.MPLS OAM signal fail;
                26.MPLS OAM signal degrade;
                27.MPLS OAM fail;
                28.Service resume;
                29.Service delete;
                100. Clear."
            ::= { hwMplsTrapObjects 3 }

     hwMplsLspProtocol OBJECT-TYPE
        SYNTAX  INTEGER
             {
             ldp(1),
             bgp(2),
             bgpv6(3),
             ldpfrr(4),
             rsvp(5),
             totalLsp(6),
             totalCrLsp(7),
             ldpIngress(8),
             ldpTransit(9),
             ldpEgress(10),
             bgpIngress(11),
             bgpEgress(12),
             bgpv6Ingress(13),
             bgpv6Egress(14),
             rsvpIngress(15),
             rsvpTransit(16),
             rsvpEgress(17),
             totalLspIngress(18),
             totalLspTransit(19),
             totalLspEgress(20),
             totalCrLspIngress(21),
             totalCrLspTransit(22),
             totalCrLspEgress(23),
             totalPublicNetLspIngressTransit(24),
             totalPublicNetLspTransitEgress(25),
             privateNetBgp(26),             
             unknown(100)
             }
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the protocol of the lsp which exceeds the threshold or total count.
            Options:                                                       
            1.ldp(1)         -indicates the lsp is ldp lsp.  
            2.bgp(2)         -indicates the lsp is bgp lsp.
            3.bgpv6(3)         -indicates the lsp is bgpv6 lsp.
            4.ldpfrr(4)         -indicates the lsp is ldp frr lsp.
            5.rsvp(5)         -indicates the lsp is rsvp te lsp.
            6.totalLsp(6)         -indicates the lsp is total lsp.
            7.totalCrLsp(7)         -indicates the lsp is total cr-lsp.
            8.ldpIngress(8)         -indicates the lsp is ldp ingress lsp.
            9.ldpTransit(9)         -indicates the lsp is ldp transit lsp.
            10.ldpEgress(10)         -indicates the lsp is ldp egress lsp.
            11.bgpIngress(11)         -indicates the lsp is bgp ingress lsp.
            12.bgpEgress(12)         -indicates the lsp is bgp egress lsp.
            13.bgpv6Ingress(13)         -indicates the lsp is bgpv6 ingress lsp.
            14.bgpv6Egress(14)         -indicates the lsp is bgpv6 egress lsp.
            15.rsvpIngress(15)         -indicates the lsp is rsvp te ingress lsp.
            16.rsvpTransit(16)         -indicates the lsp is rsvp te transit lsp.
            17.rsvpEgress(17)         -indicates the lsp is rsvp te egress lsp.
            18.totalLspIngress(18)         -indicates the lsp is total ingress lsp.
            19.totalLspTransit(19)         -indicates the lsp is total transit lsp.
            20.totalLspEgress(20)         -indicates the lsp is total egress lsp.
            21.totalCrLspIngress(21)         -indicates the lsp is total ingress cr-lsp.
            22.totalCrLspTransit(22)         -indicates the lsp is total transit cr-lsp.
            23.totalCrLspEgress(23)         -indicates the lsp is total egress cr-lsp.
            24.totalPublicNetLspIngressTransit(24)         -indicates the lsp is total ingress and transit public netwrok lsp.
            25.totalPublicNetLspTransitEgress(25)         -indicates the lsp is total transit and egress public network cr-lsp.
            26.privateNetBgp(26)         -indicates the lsp is private network bgp lsp.    
            27.unknown(100)   -indicates the lsp type is unknown. "
        ::= { hwMplsTrapObjects 4 }
     
     hwMplsLspThreshold OBJECT-TYPE
        SYNTAX  Integer32
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the threshold of the lsp."
        ::= { hwMplsTrapObjects 5 }
        
     hwMplsLspTotalCount OBJECT-TYPE
        SYNTAX  Integer32
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the total permit count of lsp."
        ::= { hwMplsTrapObjects 6 }

     hwMplsLspCurrentCount OBJECT-TYPE
        SYNTAX  Integer32
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the current count of the lsp."
        ::= { hwMplsTrapObjects 7 }

     hwMplsTunnelDownLSRID OBJECT-TYPE
        SYNTAX  MplsLsrIdentifier
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the LSR ID of the error node on a tunnel."
        ::= { hwMplsTrapObjects 8 }   
        
     hwMplsTunnelDownIfIpAddr OBJECT-TYPE
        SYNTAX  InetAddress
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the IP address of the error interface on a tunnel."
        ::= { hwMplsTrapObjects 9 }

     hwMplsTunnelDownIfIpAddrType OBJECT-TYPE
        SYNTAX  InetAddressType
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the IP address type of the error interface on a tunnel."
        ::= { hwMplsTrapObjects 10 }
        
     hwMplsResourceType OBJECT-TYPE
        SYNTAX  INTEGER
             {
             autoBypassTunnelIf(1),
             p2mpAutoTunnelIf(2),
             teBfd(3),
             ldpBfd(4),
             mldpTotalTree(5),
             mldpTotalBranch(6),
             ldpTotalRemoteAdjacency(7),
             outSegment(8),
             autoPrimaryTunnelIf(9),
             ldpTotalLocalAdjacency(10),
             cspfNode(11),
             cspfLink(12),
             cspfNlsa(13),
             cspfSrlg(14),
             unknown(100)
             }
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies that the number of MPLS resources has exceeded the threshold or the maximum number.
            Options:                                                       
            1.autoBypassTunnelIf(1)         -Indicates that the resource is auto bypass tunnel interface.  
            2.p2mpAutoTunnelIf(2)         -Indicates that the resource is P2MP auto tunnel interface.
            3.teBfd(3)         -Indicates that the resource is dynamic BFD for TE LSP.
            4.ldpBfd(4)         -Indicates that the resource is dynamic BFD for LDP LSP.
            5.mldpTotalTree(5)         -Indicates that the resource is the total number of MLDP trees.
            6.mldpTotalBranch(6)         -Indicates that the resource is the total number of MLDP branches.
            7.ldpTotalRemoteAdjacency(7)         -Indicates that the resource is LDP total remote adjacency.
            8.outSegment(8)         -Indicates that the resource is LDP outSegment.
            9.autoPrimaryTunnelIf(9)         -Indicates that the resource is auto primary tunnel interface.
            10.ldpTotalLocalAdjacency(10)         -Indicates that the resource is LDP total local adjacency.
            11.cspfNode(11)                       -Indicates that the resource is cspf node.
            12.cspfLink(12)                       -Indicates that the resource is cspf link.
            13.cspfNlsa(13)                       -Indicates that the resource is cspf nlsa.
            14.cspfSrlg(14)                       -Indicates that the resource is cspf srlg.
            15.unknown(100)   -Indicates that the resource type is unknown. "
        ::= { hwMplsTrapObjects 11 }
        
     hwMplsResourceCurrentCount OBJECT-TYPE
        SYNTAX  Integer32
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the number of the resources."
        ::= { hwMplsTrapObjects 12 }
        
     hwMplsResourceThreshold OBJECT-TYPE
        SYNTAX  Integer32
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the threshold for the number of the resources."
        ::= { hwMplsTrapObjects 13 }
        
     hwMplsResourceTotalCount OBJECT-TYPE
        SYNTAX  Integer32
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the maximum number of allowed resources."
        ::= { hwMplsTrapObjects 14 }
 
      hwMplsSessionTunnelId OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the Tunnel ID."
        ::= { hwMplsTrapObjects 15 }

      hwMplsLocalLspId OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the LSP ID."
        ::= { hwMplsTrapObjects 16 }

      hwMplsIngressLsrId OBJECT-TYPE
        SYNTAX  MplsLsrIdentifier
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the ingress LSR ID."
        ::= { hwMplsTrapObjects 17 }

      hwMplsEgressLsrId OBJECT-TYPE
        SYNTAX  MplsLsrIdentifier
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "The value of this object identifies the egress LSR ID."
        ::= { hwMplsTrapObjects 18 }

      hwMplsLspName OBJECT-TYPE
        SYNTAX  SnmpAdminString
        MAX-ACCESS     accessible-for-notify
        STATUS           current
        DESCRIPTION
            "This object indicates the name of an bidirectional static CR-LSP."
        ::= { hwMplsTrapObjects 19 }
                                        
     hwMplsTunnelFrrConfigChange NOTIFICATION-TYPE
        OBJECTS { hwMplsTunnelIfName, hwMplsTunnelFrrConfigOper }
        STATUS obsolete
        DESCRIPTION
            "When the trap indicating that TE-Frr configuration of Tunnel is changed is sent, the cause for the change of TE-FRR configuration of Tunnel is displayed."
        ::= { hwMplsExtendTrap 3 }
        
        hwMplsGlobalObject OBJECT IDENTIFIER ::= { hwMplsExtendMib 3 }

        hwMplsGlobalWorkMode OBJECT-TYPE
            SYNTAX INTEGER
                {
                standard(1),
                nonstandard(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The work mode of DS-TE system, default mode is nonstandard.
                Options:
                1. standard(1)       -indicates work mode of DS-TE system is standard
                2. nonstandard(2)    -indicates work mode of DS-TE system is nonstandard"
            ::= { hwMplsGlobalObject 1 }

        hwMplsGlobalBcModel OBJECT-TYPE
            SYNTAX INTEGER
                {
                rdm(1),
                mam(2),
                extendMam(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Bandwidth Constraint Model currently used by this LSR.
                Options: 
                1. rdm(1)          -indicates that the bandwidth constraint model is RDM.
                2. mam(2)          -indicates that the bandwidth constraint model is MAM.   
                3. extendMam(3)    -indicates that the bandwidth constraint model is ExtendMam."
            ::= { hwMplsGlobalObject 2 }

       hwMplsDynamicLabelTotalCount OBJECT-TYPE
            SYNTAX  Unsigned32
            MAX-ACCESS     read-only
            STATUS         current
            DESCRIPTION
                "The value of this object identifies the total permit count of dynamic label."
            ::= { hwMplsGlobalObject 3 }

        hwMplsDynamicLabelCurrentCount OBJECT-TYPE
            SYNTAX  Unsigned32
            MAX-ACCESS     read-only
            STATUS         current
            DESCRIPTION
                "The value of this object identifies the current count of the dynamic label."
            ::= { hwMplsGlobalObject 4 }
            
        hwMplsDynamicLabelThresholdUpperLimit OBJECT-TYPE
            SYNTAX  Unsigned32
            MAX-ACCESS     read-only
            STATUS         current
            DESCRIPTION
                "The upper limit threshold value (%) of dynamic label, default value is 80." 
            ::= { hwMplsGlobalObject 5 }
            
        hwMplsDynamicLabelThresholdLowerLimit OBJECT-TYPE
            SYNTAX  Unsigned32
            MAX-ACCESS     read-only
            STATUS         current
            DESCRIPTION
                "The lower limit threshold value (%) of dynamic label, default value is 70."
            ::= { hwMplsGlobalObject 6 }
        
        hwMplsLspStatistics OBJECT IDENTIFIER ::= { hwMplsExtendMib 4 }
        
        hwMplsLspStatisticsTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwMplsLspStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "hwMplsLspStatisticsTable is used to display the number of ingress LSPs,  
                transit LSPs, or egress LSPs of specified types. The index of this table 
                is hwMplsLspStatisticsLspType."
            ::= { hwMplsLspStatistics 1 }
        
        hwMplsLspStatisticsEntry OBJECT-TYPE
            SYNTAX HwMplsLspStatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "hwMplsLspStatisticsTable is used to display the number of ingress LSPs,  
                transit LSPs, or egress LSPs of specified types. The index of this entry 
                is hwMplsLspStatisticsLspType."
            INDEX { hwMplsLspStatisticsLspType }
            ::= { hwMplsLspStatisticsTable 1 }
        
        HwMplsLspStatisticsEntry ::=
            SEQUENCE { 
                hwMplsLspStatisticsLspType
                    INTEGER,
                hwMplsLspStatisticsIngressLspCount
                    Unsigned32,
                hwMplsLspStatisticsTransitLspCount
                    Unsigned32,
                hwMplsLspStatisticsEgressLspCount
                    Unsigned32,
                hwMplsLspStatisticsTotalLspCount
                    Unsigned32
             }

        hwMplsLspStatisticsLspType OBJECT-TYPE
            SYNTAX INTEGER
                {
                staticLsp(1),
                staticCrLsp(2),
                ldpLsp(3),
                rsvpCrLsp(4),
                bgpLsp(5),
                asbrLsp(6),
                bgpIpv6Lsp(7),
                l3vpnIpv6Lsp(8)
                }
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the LSP type.
                Options:                                                      
                1. staticLsp(1)   -indicates the static LSP.    
                2. staticCrLsp(2) -indicates the static CR-LSP.  
                3. ldpLsp(3)      -indicates the LDP LSP.      
                4. rsvpCrLsp(4)   -indicates the RSVP LSP.     
                5. bgpLsp(5)      -indicates the BGP LSP.       
                6. asbrLsp(6)     -indicates the ASBR LSP.     
                7. bgpIpv6Lsp(7)  -indicates the BGP IPv6 LSP.  
                8. l3vpnIpv6Lsp(8)-indicates the L3VPN IPv6 LSP.
                "
            ::= { hwMplsLspStatisticsEntry 1 }
        
        hwMplsLspStatisticsIngressLspCount OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the number of ingress LSPs of a specified type."
            ::= { hwMplsLspStatisticsEntry 2 }
        
        hwMplsLspStatisticsTransitLspCount OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the number of transit LSPs of a specified type."
            ::= { hwMplsLspStatisticsEntry 3 }
        
        hwMplsLspStatisticsEgressLspCount OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the number of egress LSPs of a specified type."
            ::= { hwMplsLspStatisticsEntry 4 }
        
        hwMplsLspStatisticsTotalLspCount OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the total number of the ingress LSPs, transit LSPs and egress LSP of specified types."
            ::= { hwMplsLspStatisticsEntry 5 }
        
-- 1.3.6.1.4.1.2011.5.25.121.4.2
        hwMplsTrafficStatisticsStaticLspTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwMplsTrafficStatisticsStaticLspEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the traffic statistics of a LSP.                                        
                 The indexes of this table is hwMplsTrafficStatisticsStaticLspName."
        ::= { hwMplsLspStatistics 2 }
        
--  1.3.6.1.4.1.2011.5.25.121.4.2.1
        hwMplsTrafficStatisticsStaticLspEntry OBJECT-TYPE
            SYNTAX HwMplsTrafficStatisticsStaticLspEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the traffic statistics of a LSP. The indexes of this entry is 
                hwMplsTrafficStatisticsStaticLspName."
            INDEX { hwMplsTrafficStatisticsStaticLspName }
            ::= { hwMplsTrafficStatisticsStaticLspTable 1 }

        HwMplsTrafficStatisticsStaticLspEntry ::=
            SEQUENCE { 
                hwMplsTrafficStatisticsStaticLspName
                    SnmpAdminString,
                hwMplsTrafficStatisticsStaticLspForwardInBytes
                    Counter64,
                hwMplsTrafficStatisticsStaticLspForwardInPackets
                    Counter64,
                hwMplsTrafficStatisticsStaticLspForwardOutBytes
                    Counter64,
                hwMplsTrafficStatisticsStaticLspForwardOutPackets
                    Counter64,
                hwMplsTrafficStatisticsStaticLspBackwardInBytes
                    Counter64,
                hwMplsTrafficStatisticsStaticLspBackwardInPackets
                    Counter64,
                hwMplsTrafficStatisticsStaticLspBackwardOutBytes
                    Counter64,
                hwMplsTrafficStatisticsStaticLspBackwardOutPackets
                    Counter64
             }

--   1.3.6.1.4.1.2011.5.25.121.4.2.1.1
        hwMplsTrafficStatisticsStaticLspName OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the name of the static LSP or CR-LSP. 
                The name is appointed when the static LSP or CR-LSP 
                is created."
            ::= { hwMplsTrafficStatisticsStaticLspEntry 1 }
        
--   1.3.6.1.4.1.2011.5.25.121.4.2.1.2
        hwMplsTrafficStatisticsStaticLspForwardInBytes OBJECT-TYPE
            SYNTAX Counter64
            UNITS "bytes"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "An estimate of the forward of bistatic LSP's current incoming traffic statistics
                in units of bytes.
                For a sub-layer which has no concept of
                traffic statistics, this object should be zero.
                Unit: bytes"
            ::= { hwMplsTrafficStatisticsStaticLspEntry 2 }
            
--   1.3.6.1.4.1.2011.5.25.121.4.2.1.3
        hwMplsTrafficStatisticsStaticLspForwardInPackets OBJECT-TYPE
            SYNTAX Counter64
            UNITS "packets"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "An estimate of the forward of bistatic LSP's current incoming traffic statistics
                in units of packets.
                For a sub-layer which has no concept of
                traffic statistics, this object should be zero.
                Unit: packets"
            ::= { hwMplsTrafficStatisticsStaticLspEntry 3 }

--   1.3.6.1.4.1.2011.5.25.121.4.2.1.4
        hwMplsTrafficStatisticsStaticLspForwardOutBytes OBJECT-TYPE
            SYNTAX Counter64
            UNITS "bytes"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "An estimate of the forward of bistatic LSP's current outgoing traffic statistics
                in units of bytes.
                For a sub-layer which has no concept of
                traffic statistics, this object should be zero.
                Unit: bytes"
            ::= { hwMplsTrafficStatisticsStaticLspEntry 4 }
            
--   1.3.6.1.4.1.2011.5.25.121.4.2.1.5
        hwMplsTrafficStatisticsStaticLspForwardOutPackets OBJECT-TYPE
            SYNTAX Counter64
            UNITS "packets"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "An estimate of the forward of bistatic LSP's current outgoing traffic statistics
                in units of packets.
                For a sub-layer which has no concept of
                traffic statistics, this object should be zero.
                Unit: packets"
            ::= { hwMplsTrafficStatisticsStaticLspEntry 5 }

--   1.3.6.1.4.1.2011.5.25.121.4.2.1.6
        hwMplsTrafficStatisticsStaticLspBackwardInBytes OBJECT-TYPE
            SYNTAX Counter64
            UNITS "bytes"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "An estimate of the backward of bistatic LSP's current incoming traffic statistics
                in units of bytes.
                For a sub-layer which has no concept of
                traffic statistics, this object should be zero.
                Unit: bytes"
            ::= { hwMplsTrafficStatisticsStaticLspEntry 6 }
            
--   1.3.6.1.4.1.2011.5.25.121.4.2.1.7
        hwMplsTrafficStatisticsStaticLspBackwardInPackets OBJECT-TYPE
            SYNTAX Counter64
            UNITS "packets"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "An estimate of the backward of bistatic LSP's current incoming traffic statistics
                in units of packets.
                For a sub-layer which has no concept of
                traffic statistics, this object should be zero.
                Unit: packets"
            ::= { hwMplsTrafficStatisticsStaticLspEntry 7 }

--   1.3.6.1.4.1.2011.5.25.121.4.2.1.8
        hwMplsTrafficStatisticsStaticLspBackwardOutBytes OBJECT-TYPE
            SYNTAX Counter64
            UNITS "bytes"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "An estimate of the backward of bistatic LSP's current outgoing traffic statistics
                in units of bytes.
                For a sub-layer which has no concept of
                traffic statistics, this object should be zero.
                Unit: bytes"
            ::= { hwMplsTrafficStatisticsStaticLspEntry 8 }
            
--   1.3.6.1.4.1.2011.5.25.121.4.2.1.9
        hwMplsTrafficStatisticsStaticLspBackwardOutPackets OBJECT-TYPE
            SYNTAX Counter64
            UNITS "packets"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "An estimate of the backward of bistatic LSP's current outgoing traffic statistics
                in units of packets.
                For a sub-layer which has no concept of
                traffic statistics, this object should be zero.
                Unit: packets"
            ::= { hwMplsTrafficStatisticsStaticLspEntry 9 }
        
        hwMplsExtendConformance OBJECT IDENTIFIER ::= { hwMplsExtendMib 6 }
        
        hwMplsExtendGroups OBJECT IDENTIFIER ::= { hwMplsExtendConformance 1 }
        
        hwMplsTunnelGroup OBJECT-GROUP
            OBJECTS { hwTunnelFrrRouteDBInnerLabel, hwTunnelFrrRouteDBBypassIfIndex, hwTunnelFrrARHopProtActual, hwTunnelFrrARHopProtDesired, hwTunnelFrrBypassProtIfIndex, 
                hwStaticLspOwner, hwMplsTunnelClassType, hwMplsTunnelSessionAttr, hwMplsTunnelFrrARHopTableIndex, hwMplsTunnelName, 
                hwMplsTunnelIfIndex, hwMplsTunnelPreBandwidth, hwMplsTunnelNextBandwidth, hwMplsTunnelFrrSwitchover, hwMplsTunnelFrrBandwidth, 
                hwMplsTunnelOperStatus, hwMplsTunnelAdminStatus, hwMplsTunnelBandwidth, hwMplsTeVpnMaxBandwidth, hwMplsTeVpnAllocatedBandwidth, 
                hwMplsTunnelFrrHoldingPrio, hwMplsTunnelFrrSetupPrio, hwMplsTunnelFrrBypassTableIndex, hwMplsTunnelLspType,hwMplsTunnelInterfaceName, hwMplsTunnelSignalProto, hwMplsTunnelType }
            STATUS current
            DESCRIPTION 
                "Indicate the atrributes of the tunnel."
            ::= { hwMplsExtendGroups 1 }
        
        hwStaticLspGroup OBJECT-GROUP
            OBJECTS { hwStaticLspName, hwStaticLspStatus, hwStaticLspTnlToken, hwStaticLspInIfIndex, hwStaticLspInIfName, hwStaticLspDownReason }
            STATUS current
            DESCRIPTION 
                "Indicate the atrributes of the static lsp."
            ::= { hwMplsExtendGroups 2 }
        
        hwMplsDsTeGroup OBJECT-GROUP
            OBJECTS { hwMplsTunnelCt0Bandwidth, hwMplsTunnelCt1Bandwidth, hwMplsTunnelCt2Bandwidth, hwMplsTunnelCt3Bandwidth, hwMplsTunnelCt4Bandwidth, 
                hwMplsTunnelCt5Bandwidth, hwMplsTunnelCt6Bandwidth, hwMplsTunnelCt7Bandwidth, hwStaticLspClassType, hwStaticLspBandwidth, 
                hwMplsTeClassClassType, hwMplsTeClassPriority, hwMplsTeClassDescription, hwMplsGlobalBcModel, hwMplsGlobalWorkMode, 
                hwMplsIfBc7Bandwidth, hwMplsIfBc6Bandwidth, hwMplsIfBc5Bandwidth, hwMplsIfBc4Bandwidth, hwMplsIfBc3Bandwidth, 
                hwMplsIfBc2Bandwidth, hwMplsIfBc1Bandwidth, hwMplsIfBc0Bandwidth, hwMplsIfMaxResvBandwidth }
            STATUS current
            DESCRIPTION 
                "Indicate the atrributes about DS-TE."
            ::= { hwMplsExtendGroups 3 }
        
        hwMplsLspStatisticsGroup OBJECT-GROUP
            OBJECTS { hwMplsLspStatisticsIngressLspCount, hwMplsLspStatisticsTransitLspCount, hwMplsLspStatisticsEgressLspCount, hwMplsLspStatisticsTotalLspCount }
            STATUS current
            DESCRIPTION 
                "Indicate LSP statistics."
            ::= { hwMplsExtendGroups 4 }

        hwMplsObsoleteGroup OBJECT-GROUP
        OBJECTS { hwMplsTunnelIfName, hwMplsTunnelFrrConfigOper }
        STATUS obsolete
        DESCRIPTION 
           "Indicate the OBSOLETE objects of MPLS."
        ::= { hwMplsExtendGroups 5 }

     hwMplsTrapGroup OBJECT-GROUP
        OBJECTS { hwMplsTunnelDownReason, hwMplsTunnelDownLSRID, hwMplsTunnelDownIfIpAddrType, hwMplsTunnelDownIfIpAddr }
        STATUS current
        DESCRIPTION 
           "For mpls trap object."
        ::= { hwMplsExtendGroups 6 }
        
        
        hwMplsRingGroup OBJECT-GROUP
        OBJECTS { hwMplsRingNodeID, hwMplsRingName, hwMplsRingDirection, hwMplsRingSwitchReason }
        STATUS current
        DESCRIPTION 
           "For mpls ring trap object."
        ::= { hwMplsExtendGroups 7 }

        hwMplsGlobalGroup OBJECT-GROUP
        OBJECTS { hwMplsDynamicLabelTotalCount, hwMplsDynamicLabelCurrentCount, hwMplsDynamicLabelThresholdUpperLimit, hwMplsDynamicLabelThresholdLowerLimit }
        STATUS current
        DESCRIPTION 
           "For mpls global object."
        ::= { hwMplsExtendGroups 8 }

        hwMplsLspGroup OBJECT-GROUP
        OBJECTS { hwMplsLspCurrentCount, hwMplsLspTotalCount, hwMplsLspProtocol, hwMplsLspThreshold }
        STATUS current
        DESCRIPTION 
           "For mpls lsp object."
        ::= { hwMplsExtendGroups 9 }

        hwMplsLspTrafficStatisticGroup OBJECT-GROUP
        OBJECTS { hwMplsTrafficStatisticsStaticLspForwardInBytes, hwMplsTrafficStatisticsStaticLspForwardInPackets,
            hwMplsTrafficStatisticsStaticLspForwardOutBytes, hwMplsTrafficStatisticsStaticLspForwardOutPackets, 
            hwMplsTrafficStatisticsStaticLspBackwardInBytes, hwMplsTrafficStatisticsStaticLspBackwardInPackets,
            hwMplsTrafficStatisticsStaticLspBackwardOutBytes, hwMplsTrafficStatisticsStaticLspBackwardOutPackets }
        STATUS current
        DESCRIPTION 
            "Indicate the traffic statistic of the LSP."
        ::= { hwMplsExtendGroups 10 }

        hwMplsResourceGroup OBJECT-GROUP
        OBJECTS { hwMplsResourceType, hwMplsResourceCurrentCount, hwMplsResourceThreshold, hwMplsResourceTotalCount }
        STATUS current
        DESCRIPTION 
           "For mpls resource object."
        ::= { hwMplsExtendGroups 11 }

        hwMplsExtendCompliances OBJECT IDENTIFIER ::= { hwMplsExtendConformance 2 }

        
        hwExtendTrapGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwMplsTeFrrProtAval, hwMplsTeFrrProtNotAval, hwMplsStaticLspUp, hwMplsStaticLspDown, hwMplsStaticCRLspUp, 
                hwMplsStaticCRLspDown, hwMplsTeFrrSwitch, hwMplsTeFrrResume, hwMplsTunnelHSBSwitch, hwMplsTunnelHSBResume, 
                hwMplsTunnelOBSwitch, hwMplsTunnelOBResume, hwMplsTunnelChangeBw, hwMplsTunnelTpOamLossSD, hwMplsOamSDRecovery, 
                hwMplsOamLoss, hwMplsOamLossRecovery, hwMplsOamAis, hwMplsOamAisRecovery, hwMplsOamRdi, hwMplsOamRdiRecovery, 
                hwMplsOamMeg, hwMplsOamMegRecovery, hwMplsOamMep, hwMplsOamMepRecovery, hwMplsOamSF, hwMplsOamSFRecovery, 
                hwMplsOamPeriod, hwMplsOamPeriodRecovery, hwMplsOamLck, hwMplsOamLckRecovery, hwMplsOamExcess, hwMplsOamExcessRecovery, 
                hwMplsOamMisMatch, hwMplsOamMisMatchRecovery, hwMplsOamMisMerge, hwMplsOamMisMergeRecovery, hwMplsOamUnknown, hwMplsOamUnknownRecovery, 
                hwMplsOamBDI, hwMplsOamBDIRecovery, hwMplsOamFail, hwMplsOamFailRecovery, 
                hwMplsTunnelPrimaryUp, hwMplsTunnelPrimaryDown, hwMplsTunnelHotstandbyUp, hwMplsTunnelHotstandbyDown,
                hwMplsTunnelOrdinaryUp, hwMplsTunnelOrdinaryDown, hwMplsTunnelBesteffortUp, hwMplsTunnelBesteffortDown, hwMplsTeAutoTunnelDownClear, hwMplsTeAutoTunnelPrimaryDownClear,
                hwMplsTunnelBBSwitch, hwMplsTunnelBBResume, hwMplsExtTunnelDown, hwMplsExtTunnelDownClear, hwMplsOamLocalLock, hwMplsOamLocalLockRecovery, hwMplsRingWestOamLoss, hwMplsRingWestOamLossClear, hwMplsRingEastOamLoss,
                hwMplsRingEastOamLossClear, hwMplsRingWestOamRDI, hwMplsRingWestOamRDIClear, hwMplsRingEastOamRDI, hwMplsRingEastOamRDIClear, hwMplsRingWestOamUnexpectedMEG, 
                hwMplsRingWestOamUnexpectedMEGClear, hwMplsRingEastOamUnexpectedMEG, hwMplsRingEastOamUnexpectedMEGClear, hwMplsRingWestOamUnexpectedPeriod, hwMplsRingWestOamUnexpectedPeriodClear,
                hwMplsRingEastOamUnexpectedPeriod, hwMplsRingEastOamUnexpectedPeriodClear, hwMplsRingWestOamExcess, hwMplsRingWestOamExcessClear, hwMplsRingEastOamExcess,
                hwMplsRingEastOamExcessClear, hwMplsRingWestOamSD, hwMplsRingWestOamSDClear, hwMplsRingEastOamSD, hwMplsRingEastOamSDClear, hwMplsRingWestOamSF, hwMplsRingWestOamSFClear,
                hwMplsRingEastOamSF, hwMplsRingEastOamSFClear, hwMplsRingWestAPSSwitch, hwMplsRingWestAPSResume, hwMplsRingEastAPSSwitch, hwMplsRingEastAPSResume,
                hwMplsRingWestAPSSwitchFail, hwMplsRingWestAPSSwitchFailClear, hwMplsRingEastAPSSwitchFail, hwMplsRingEastAPSSwitchFailClear, hwMplsRingSwitch, hwMplsRingResume,
                hwMplsRingWestAPSLost, hwMplsRingWestAPSLostClear, hwMplsRingEastAPSLost, hwMplsRingEastAPSLostClear, hwMplsRingWestAPSMismatch, hwMplsRingWestAPSMismatchClear,
                hwMplsRingEastAPSMismatch, hwMplsRingEastAPSMismatchClear,hwMplsRingWestOamUnexpectedMEP, hwMplsRingWestOamUnexpectedMEPClear, hwMplsRingEastOamUnexpectedMEP, hwMplsRingEastOamUnexpectedMEPClear, hwMplsTunnelDelete,
                hwMplsLspTotalCountExceed, hwMplsLspThresholdExceed, hwMplsLspTotalCountExceedClear, hwMplsLspThresholdExceedClear, hwMplsDynamicLabelThresholdExceed,
                hwMplsDynamicLabelThresholdExceedClear, hwMplsDynamicLabelTotalCountExceed, hwMplsDynamicLabelTotalCountExceedClear,
                hwMplsResourceThresholdExceed, hwMplsResourceThresholdExceedClear, hwMplsResourceTotalCountExceed, hwMplsResourceTotalCountExceedClear,
                hwMplsLspLoopBack, hwMplsLspLoopBackClear, hwMplsTunnelCommitLost, hwMplsTunnelCommitLostClear, hwMplsTunnelHotstandbySwitch, hwMplsTunnelHotstandbyResume, hwMplsTunnelBfdPathMismatch, hwMplsTunnelBfdPathMismatchClear,
                hwMplsTeLspBfdDown, hwMplsTeLspBfdDownClear, hwMplsTunnelDelegationReturn, hwMplsTunnelDelegationReturnClear 
            }
            STATUS current
            DESCRIPTION 
                "Indicate the traps."
            ::= { hwMplsExtendCompliances 1 }

        hwObsoleteTrapGroup NOTIFICATION-GROUP
        NOTIFICATIONS { hwMplsTunnelFrrConfigChange, hwMplsTunnelUp, hwMplsTunnelDown, hwMplsRingSwitch, hwMplsRingResume }
        STATUS obsolete
        DESCRIPTION 
             "Indicate the Obsolete traps."
        ::= { hwMplsExtendCompliances 2 }
          
        hwMplsModuleCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION
                "hwMplsModuleCompliance"
            MODULE HUAWEI-MPLS-EXTEND-MIB
                MANDATORY-GROUPS { hwStaticLspGroup, hwMplsTunnelGroup, hwMplsDsTeGroup, hwMplsRingGroup }
                ::= { hwMplsExtendCompliances 3 }
    
       -- 1.3.6.1.4.1.2011.5.25.121.7
        hwMplsRingMib OBJECT IDENTIFIER ::= { hwMplsExtendMib 7 }
        
        -- 1.3.6.1.4.1.2011.5.25.121.7.1
        hwMplsRingTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwMplsRingEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
                "Indicates the table information of the MPLS ring."
            ::= { hwMplsRingMib 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.121.7.1.1
        hwMplsRingEntry OBJECT-TYPE
            SYNTAX HwMplsRingEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the table information of the MPLS ring."
            INDEX {hwMplsRingID}
            ::= { hwMplsRingTable 1 }

        
        HwMplsRingEntry ::=
            SEQUENCE { 
                hwMplsRingID
                    Unsigned32,
                hwMplsRingNodeID
                    Unsigned32,
                hwMplsRingName
                    OCTET STRING,
                hwMplsRingDirection
                    OCTET STRING,
                hwMplsRingSwitchReason
                    OCTET STRING
             }
             
        -- 1.3.6.1.4.1.2011.5.25.121.7.1.1.1
        hwMplsRingID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the ID of the MPLS ring. "
            ::= { hwMplsRingEntry 1 }
            
        -- 1.3.6.1.4.1.2011.5.25.121.7.1.1.2
        hwMplsRingNodeID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the ID of the current Node on the MPLS ring."
            ::= { hwMplsRingEntry 2 }
            
        hwMplsRingName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the name of MPLS ring."
            ::= { hwMplsRingEntry 3 }
            
        hwMplsRingDirection OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the direction of the MPLS ring."
            ::= { hwMplsRingEntry 4 }
        
        hwMplsRingSwitchReason OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the switch reason of the MPLS ring."
            ::= { hwMplsRingEntry 5 }
        
        
        
        -- 1.3.6.1.4.1.2011.5.25.121.7.2
        hwMplsRingTrap OBJECT IDENTIFIER ::= { hwMplsRingMib 2 }
        
         -- 1.3.6.1.4.1.2011.5.25.121.7.2.1
        hwMplsRingSwitch NOTIFICATION-TYPE
            OBJECTS { hwMplsRingNodeID, hwMplsRingName, hwMplsRingDirection, hwMplsRingSwitchReason}
            STATUS obsolete
            DESCRIPTION 
                "
                The notification indicates that the MPLS ring switched.
                "
            ::= { hwMplsRingTrap 1 }
            
         -- 1.3.6.1.4.1.2011.5.25.121.7.2.2    
       hwMplsRingResume NOTIFICATION-TYPE
            OBJECTS { hwMplsRingNodeID, hwMplsRingName, hwMplsRingDirection }
            STATUS obsolete
            DESCRIPTION 
                "
                The notification indicates that the MPLS ring resumed.
                "
            ::= { hwMplsRingTrap 2 }

       
       -- 1.3.6.1.4.1.2011.5.25.121.7.2.3    
       hwMplsRingWestOamLoss NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that no expected CV/FFD packet is received for three consecutive cycles in the west of the MPLS ring.
                "
            ::= { hwMplsRingTrap 3 }
       
       -- 1.3.6.1.4.1.2011.5.25.121.7.2.4    
       hwMplsRingWestOamLossClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingWestOamLoss alarm was cleared.
                "
            ::= { hwMplsRingTrap 4 }
            
       -- 1.3.6.1.4.1.2011.5.25.121.7.2.5    
       hwMplsRingEastOamLoss NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that no expected CV/FFD packet is received for three consecutive cycles in the east of the MPLS ring.
                "
            ::= { hwMplsRingTrap 5 }
       
       -- 1.3.6.1.4.1.2011.5.25.121.7.2.6    
       hwMplsRingEastOamLossClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingEastOamLoss alarm was cleared.
                "
            ::= { hwMplsRingTrap 6 }
            
       -- 1.3.6.1.4.1.2011.5.25.121.7.2.7    
       hwMplsRingWestOamRDI NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that RDI packets are received in the west of the MPLS ring, indicating that a fault occurs on the forward ring.
                "
            ::= { hwMplsRingTrap 7 }
            
       -- 1.3.6.1.4.1.2011.5.25.121.7.2.8    
       hwMplsRingWestOamRDIClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingWestOamRDI alarm was cleared.
                "
            ::= { hwMplsRingTrap 8 }
            
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.9    
       hwMplsRingEastOamRDI NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that RDI packets are received in the east of the MPLS ring, indicating that a fault occurs on the forward ring.
                "
            ::= { hwMplsRingTrap 9 }
            
       -- 1.3.6.1.4.1.2011.5.25.121.7.2.10    
       hwMplsRingEastOamRDIClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingEastOamRDI alarm was cleared.
                "
            ::= { hwMplsRingTrap 10 }
            
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.11    
      hwMplsRingWestOamUnexpectedMEG NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that a CCM frame carrying a correct MEG level but incorrect MEG ID is received in the west of the MPLS ring.
                "
            ::= { hwMplsRingTrap 11 }
            
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.12    
      hwMplsRingWestOamUnexpectedMEGClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingWestOamUnexpectedMEG alarm was cleared.
                "
            ::= { hwMplsRingTrap 12 }  
                
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.13    
      hwMplsRingEastOamUnexpectedMEG NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that a CCM frame carrying a correct MEG level but incorrect MEG ID is received in the east of the MPLS ring.
                "
            ::= { hwMplsRingTrap 13 }
            
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.14    
      hwMplsRingEastOamUnexpectedMEGClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingEastOamUnexpectedMEG alarm was cleared.
                "
            ::= { hwMplsRingTrap 14 } 
                   
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.15    
      hwMplsRingWestOamUnexpectedPeriod NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that a CCM frame carrying a correct MEG level, MEG ID, 
                and MEP ID but incorrect period value is received in the west MEP of the MPLS ring.
                "
            ::= { hwMplsRingTrap 15 }
            
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.16    
      hwMplsRingWestOamUnexpectedPeriodClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingWestOamUnexpectedPeriod alarm was cleared.
                "
            ::= { hwMplsRingTrap 16 }
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.17    
      hwMplsRingEastOamUnexpectedPeriod NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that a CCM frame carrying a correct MEG level, MEG ID, 
                and MEP ID but incorrect period value is received in the east MEP of the MPLS ring.
                "
            ::= { hwMplsRingTrap 17 }
            
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.18    
      hwMplsRingEastOamUnexpectedPeriodClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingEastOamUnexpectedPeriod alarm was cleared.
                "
            ::= { hwMplsRingTrap 18 }
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.19    
     hwMplsRingWestOamExcess NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that five or more CV/FFD packets are correctly received 
                within three consecutive cycles in the west of the MPLS ring.
                "
            ::= { hwMplsRingTrap 19 }
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.20    
     hwMplsRingWestOamExcessClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingWestOamExcess alarm was cleared.
                "
            ::= { hwMplsRingTrap 20 } 
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.21    
     hwMplsRingEastOamExcess NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that five or more CV/FFD packets are correctly received 
                within three consecutive cycles in the east of the MPLS ring.
                "
            ::= { hwMplsRingTrap 21 }
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.22    
     hwMplsRingEastOamExcessClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingEastOamExcess alarm was cleared.
                "
            ::= { hwMplsRingTrap 22 }  
                  
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.23    
     hwMplsRingWestOamSD NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the number of packets for connectivity check received 
                in the west of the MPLS ring is smaller than the SD threshold.
                "
            ::= { hwMplsRingTrap 23 }
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.24    
     hwMplsRingWestOamSDClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingWestOamSD alarm was cleared.
                "
            ::= { hwMplsRingTrap 24 } 
     
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.25    
     hwMplsRingEastOamSD NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the number of packets for connectivity check received 
                in the east of the MPLS ring is smaller than the SD threshold.
                "
            ::= { hwMplsRingTrap 25 }
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.26    
     hwMplsRingEastOamSDClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingEastOamSD alarm was cleared.
                "
            ::= { hwMplsRingTrap 26 }     
     
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.27    
     hwMplsRingWestOamSF NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the number of packets for connectivity check received in 
                the west of the MPLS ring is smaller than the SF threshold.
                "
            ::= { hwMplsRingTrap 27 }
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.28    
     hwMplsRingWestOamSFClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingWestOamSF alarm was cleared.
                "
            ::= { hwMplsRingTrap 28 }
            
    -- 1.3.6.1.4.1.2011.5.25.121.7.2.29    
     hwMplsRingEastOamSF NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the number of packets for connectivity check received in 
                the east of the MPLS ring is smaller than the SF threshold.
                "
            ::= { hwMplsRingTrap 29 }
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.30    
     hwMplsRingEastOamSFClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingEastOamSF alarm was cleared.
                "
            ::= { hwMplsRingTrap 30 }
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.31    
     hwMplsRingWestAPSSwitch NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that APS switching occurs in the west of the MPLS ring.
                "
            ::= { hwMplsRingTrap 31 } 
        
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.32    
     hwMplsRingWestAPSResume NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that APS switches back in the west of the MPLS ring.
                "
            ::= { hwMplsRingTrap 32 } 
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.33    
     hwMplsRingEastAPSSwitch NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that APS switching occurs in the east of the MPLS ring.
                "
            ::= { hwMplsRingTrap 33 }
             
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.34    
     hwMplsRingEastAPSResume NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that APS switches back in the east of the MPLS ring.
                "
            ::= { hwMplsRingTrap 34 } 
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.35    
     hwMplsRingWestAPSSwitchFail NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the remote APS switching fails in the west of the MPLS ring.
                "
            ::= { hwMplsRingTrap 35 } 
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.36    
     hwMplsRingWestAPSSwitchFailClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingWestAPSSwitchFail alarm was cleared.
                "
            ::= { hwMplsRingTrap 36 } 
     
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.37    
     hwMplsRingEastAPSSwitchFail NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the remote APS switching fails in the east of the MPLS ring.
                "
            ::= { hwMplsRingTrap 37 } 
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.38    
     hwMplsRingEastAPSSwitchFailClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingEastAPSSwitchFail alarm was cleared.
                "
            ::= { hwMplsRingTrap 38 }  
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.39    
     hwMplsRingWestAPSLost NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that APS packets are missing in the west of the MPLS ring.
                "
            ::= { hwMplsRingTrap 39 }  
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.40    
     hwMplsRingWestAPSLostClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingWestAPSLost alarm was cleared.
                "
            ::= { hwMplsRingTrap 40 } 
            
    -- 1.3.6.1.4.1.2011.5.25.121.7.2.41    
     hwMplsRingEastAPSLost NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that APS packets are missing in the east of the MPLS ring.
                "
            ::= { hwMplsRingTrap 41 }  
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.42    
     hwMplsRingEastAPSLostClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingEastAPSLost alarm was cleared.
                "
            ::= { hwMplsRingTrap 42 }  
            
    -- 1.3.6.1.4.1.2011.5.25.121.7.2.43    
     hwMplsRingWestAPSMismatch NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the source ID carried by APS packets received in the west 
                is different from the peer source ID configured for the west state machine on the MPLS ring.
                "
            ::= { hwMplsRingTrap 43 }  
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.44    
     hwMplsRingWestAPSMismatchClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingWestAPSMismatch alarm was cleared.
                "
            ::= { hwMplsRingTrap 44 } 
            
    -- 1.3.6.1.4.1.2011.5.25.121.7.2.45    
     hwMplsRingEastAPSMismatch NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the source ID carried by APS packets received in the east 
                is different from the peer source ID configured for the east state machine on the MPLS ring.
                "
            ::= { hwMplsRingTrap 45 }  
            
     -- 1.3.6.1.4.1.2011.5.25.121.7.2.46    
     hwMplsRingEastAPSMismatchClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingEastAPSMismatch alarm was cleared.
                "
            ::= { hwMplsRingTrap 46 }                                                                                         
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.47    
      hwMplsRingWestOamUnexpectedMEP NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that a CCM frame carrying a correct MEG level and correct MEG ID but not the expected MEP ID is received in the west of the MPLS ring.
                "
            ::= { hwMplsRingTrap 47 }
            
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.48    
      hwMplsRingWestOamUnexpectedMEPClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingWestOamUnexpectedMEP alarm was cleared.
                "
            ::= { hwMplsRingTrap 48 }  
                
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.49    
      hwMplsRingEastOamUnexpectedMEP NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that a CCM frame carrying a correct MEG level and correct MEG ID but not the expected MEP ID is received in the east of the MPLS ring.
                "
            ::= { hwMplsRingTrap 49 }
            
      -- 1.3.6.1.4.1.2011.5.25.121.7.2.50   
      hwMplsRingEastOamUnexpectedMEPClear NOTIFICATION-TYPE
            OBJECTS { hwMplsRingName }
            STATUS current
            DESCRIPTION 
                "
                The notification indicates that the hwMplsRingEastOamUnexpectedMEP alarm was cleared.
                "
            ::= { hwMplsRingTrap 50 } 
                   

    END

--
-- HUAWEI-MPLS-EXTEND-MIB.mib
--