
-- ==================================================================
-- Copyright (C) 2007 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description: HUAWEI LI Management MIB  HWAWEI-LI-MIB
-- Reference:
-- Version:     V1.0
-- History:
--              V1.0 s49159, 2007-06-10, publish
-- ==================================================================

    HUAWEI-LI-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            hwDatacomm            
                FROM HUAWEI-MIB            
            InetAddress, InetPortNumber, InetAddressType, InetAddressPrefixLength            
                FROM INET-ADDRESS-MIB            
            OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP            
                FROM SNMPv2-CONF            
            Integer32, Unsigned32, BITS, OBJECT-TYPE, MODULE-IDENTITY, 
            NOTIFICATION-TYPE            
                FROM SNMPv2-SMI            
            DateAndTime, MacAddress, RowStatus, TEXTUAL-CONVENTION                        
                FROM SNMPv2-TC;
    
        hwLiMib MODULE-IDENTITY 
            LAST-UPDATED "200706270000Z"        
            ORGANIZATION 
                "hw Technologies co.,Ltd."
            CONTACT-INFO 
                " R&D Meaning, huawei Technologies co.,Ltd.
                Http://www.huawei.com                                       
                E-mail:support@huawei.com "
            DESCRIPTION 
                "This module manages huawei's Lawful interception feature."
            REVISION "200706270000Z"        
            DESCRIPTION 
                "Initial version of this MIB module."
            ::= { hwDatacomm 131 }

        
    
--
-- Textual conventions
--
    
        HWLiDscp ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                "An integer that is in the range of the DiffServ codepoint
                values."
            SYNTAX Integer32 (0..63)

    
--
-- Node definitions
--
    
    
        hwLiMibNotifs OBJECT IDENTIFIER ::= { hwLiMib 1 }

        
    
        hwLiMibActive NOTIFICATION-TYPE
            STATUS current
            DESCRIPTION 
                "This notification is sent when an intercepting router or switch is first 
                capable of intercepting a packet corresponding to a configured data stream. "
            ::= { hwLiMibNotifs 1 }

    
        hwLiX3HeartBeatAlarm NOTIFICATION-TYPE
            OBJECTS { hwLiGatewayX3Address }
            STATUS current
            DESCRIPTION 
                "This notification is sent when an LIG is lost connection to the device 
                which  intercepting packet corresponding to a configured data stream. "
            ::= { hwLiMibNotifs 2 } 
        
    
        hwLiX3HeartBeatRecover NOTIFICATION-TYPE   
            OBJECTS { hwLiGatewayX3Address }
            STATUS current
            DESCRIPTION 
                "This notification is sent when an LIG is recover connection to the device 
                which intercepting packet corresponding to a configured data stream. "
            ::= { hwLiMibNotifs 3 }

    
        hwLiMibObjects OBJECT IDENTIFIER ::= { hwLiMib 2 }

        

        hwLiAgentObjects OBJECT IDENTIFIER ::= { hwLiMibObjects 1 }

        

        hwLiAgentTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The time of the LI agent.Read-only."
            ::= { hwLiAgentObjects 1 }

        

        hwLiAgentEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enabled(1),
                disabled(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The status of the  LI agent.Read-only."
            ::= { hwLiAgentObjects 2 }

        

        hwLiAgentX2IpAddress OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The IP address of the X2 interface in LI agent.Just can be read by server 
                and can be set in command line."
            ::= { hwLiAgentObjects 3 }


        hwLiAgentX2Port OBJECT-TYPE
            SYNTAX InetPortNumber
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Port of the X2 interface in LI agent.Just can be read by server 
                and can be set in command line."
            ::= { hwLiAgentObjects 4 }


        hwLiAgentX3IpAddress OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The IP address of the X3 interface in LI agent.Just can be read by server 
                and can be set in command line."
            ::= { hwLiAgentObjects 5 }


        hwLiAgentX3Port OBJECT-TYPE
            SYNTAX InetPortNumber
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Port of the X3 interface in LI agent.Just can be read by server 
                and can be set in command line."
            ::= { hwLiAgentObjects 6 }

        

        hwLiGatewayGroup OBJECT IDENTIFIER ::= { hwLiMibObjects 3 }

        
    
        hwLiGatewayNewIndex OBJECT-TYPE
            SYNTAX Integer32 (0 | 1..10)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object contains a value which may be used as an index
                value for a new HwLiGatewayEntry. This is to reduce 
                the probability of errors during creation of new hwLiGatewayTable 
                entries.0 means no free resource."
            ::= { hwLiGatewayGroup 1 }


        hwLiGatewayTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwLiGatewayEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table lists the LI Gateway Devices with which the
                intercepting device communicates.
                
                This table is written by the LI Gateway Device, and is always
                volatile. This is because intercepts may disappear during a
                restart of the intercepting equipment.
                
                Entries are added to this table via hwLiGatewayStatus in
                accordance with the RowStatus convention."
            ::= { hwLiGatewayGroup 2 }


        hwLiGatewayEntry OBJECT-TYPE
            SYNTAX HwLiGatewayEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry describes a single session maintained with an
                application on a LI Gateway Device."
            INDEX { hwLiGatewayIndex }
            ::= { hwLiGatewayTable 1 }

        
        HwLiGatewayEntry ::=
            SEQUENCE { 
                hwLiGatewayIndex
                    Integer32,
                hwLiGatewayAddressType
                    InetAddressType,
                hwLiGatewayX2Protocol
                    INTEGER,
                hwLiGatewayX2Address
                    InetAddress,
                hwLiGatewayX2Port
                    InetPortNumber,
                hwLiGatewayX3Protocol
                    INTEGER,
                hwLiGatewayX3Address
                    InetAddress,
                hwLiGatewayX3Port
                    InetPortNumber,
                hwLiGatewayX3HeartBeatTimer
                    Integer32,
                hwLiGatewayX3NoResponseNum
                    Integer32,
                hwLiGatewayX3OperateStatus
                    INTEGER,
                hwLiGatewayX3Dscp
                    HWLiDscp,
                hwLiGatewayRowStatus
                    RowStatus,
                hwLiGatewayX3AddressType
                    InetAddressType,                
                hwLiGatewayX2AddressType
                    InetAddressType                
             }


        hwLiGatewayIndex OBJECT-TYPE
            SYNTAX Integer32 (1..10)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The index of the LIG itself."
            ::= { hwLiGatewayEntry 1 }


        hwLiGatewayAddressType OBJECT-TYPE
            SYNTAX InetAddressType
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The type of address in LIG"
            DEFVAL { ipv4 }
            ::= { hwLiGatewayEntry 2 }


        hwLiGatewayX2Protocol OBJECT-TYPE
            SYNTAX INTEGER
                {
                udp(1),
                tcp(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The protocol used in transferring intercepted data to the
                Gateway Device. "
            DEFVAL { tcp }
            ::= { hwLiGatewayEntry 3 }

        

        hwLiGatewayX2Address OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The IP Address of the Gateway Device's network interface
                to which to direct IRI."
            ::= { hwLiGatewayEntry 4 }

        

        hwLiGatewayX2Port OBJECT-TYPE
            SYNTAX InetPortNumber
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The port number on the Gateway Device's network interface
                to which to direct IRI."
            ::= { hwLiGatewayEntry 5 }

        

        hwLiGatewayX3Protocol OBJECT-TYPE
            SYNTAX INTEGER
                {
                udp(1),
                tcp(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The protocol used in transferring intercepted data to the
                Gateway Device. "
            DEFVAL { udp }
            ::= { hwLiGatewayEntry 6 }


        hwLiGatewayX3Address OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The IP Address of the Gateway Device's network interface
                to which to direct CC."
            ::= { hwLiGatewayEntry 7 }

        

        hwLiGatewayX3Port OBJECT-TYPE
            SYNTAX InetPortNumber
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The port number on the Gateway Device's network interface
                to which to direct intercepted traffic."
            ::= { hwLiGatewayEntry 8 }

        

        hwLiGatewayX3HeartBeatTimer OBJECT-TYPE
            SYNTAX Integer32 (0..255)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The timer for sending HeartBeat to LIG,In seconds"
            DEFVAL { 5 }
            ::= { hwLiGatewayEntry 9 }

        

        hwLiGatewayX3NoResponseNum OBJECT-TYPE
            SYNTAX Integer32 (2..16)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The times of heartbeats that allowed to missed from LIG"
            DEFVAL { 3 }
            ::= { hwLiGatewayEntry 10 }

        

        hwLiGatewayX3OperateStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                normal(1),
                noHeartBeat(2),
                linkdown(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The operate status of X3 interface"
            ::= { hwLiGatewayEntry 11 }

        

        hwLiGatewayX3Dscp OBJECT-TYPE
            SYNTAX HWLiDscp
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The Differentiated Services Code Point the intercepting
                device applies to the IP packets encapsulating the
                intercepted traffic."
            DEFVAL { 0 }
            ::= { hwLiGatewayEntry 12 }

        

        hwLiGatewayRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The status of this conceptual row. This object is used to
                manage creation, modification and deletion of rows in this
                table.
                "
            ::= { hwLiGatewayEntry 14 }


        hwLiGatewayX3AddressType OBJECT-TYPE
            SYNTAX InetAddressType
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The type of address in LIG"
            DEFVAL { ipv4 }
            ::= { hwLiGatewayEntry 15 }

    
        hwLiGatewayX2AddressType OBJECT-TYPE
            SYNTAX InetAddressType
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The type of address in LIG"
            DEFVAL { ipv4 }
            ::= { hwLiGatewayEntry 16 }
    
    

        hwLiGatewayCapabilities OBJECT-TYPE
            SYNTAX BITS
                {
                ipv4SrcInterface(0),
                ipv6SrcInterface(1),
                udp(2),
                tcp(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object displays the device capabilities with respect to
                certain fields in Gateway Device table. This may be dependent
                on hardware capabilities, software capabilities.
                The following values may be supported:
                    ipv4SrcInterface:  SNMP ifIndex Value may be used to select
                                       the interface (denoted by
                                       hwLiGatewaySrcInterface) on the
                                       intercepting device from which to
                                       transmit intercepted data to an IPv4
                                       address Gateway Device.
                
                
                    ipv6SrcInterface:  SNMP ifIndex Value may be used to select
                                       the interface (denoted by
                                       hwLiGatewaySrcInterface) on the
                                       intercepting device from which to
                                       transmit intercepted data to an IPv6
                                       address Gateway Device.
                
                
                    udp:               UDP may be used as transport protocol
                                       (denoted by hwLiGatewayTransport) in
                                       transferring intercepted data to the
                                       Gateway Device.
                
                
                    tcp:               TCP may be used as transport protocol
                                       (denoted by hwLiGatewayTransport) in
                                       transferring intercepted data to the
                                       Gateway Device."
            ::= { hwLiGatewayGroup 3 }

        

        hwLiStreamGroup OBJECT IDENTIFIER ::= { hwLiMibObjects 4 }

        
    
        hwLiStreamTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwLiStreamEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The Intercept Stream Table lists the IPv4 and IPv6 streams
                to be intercepted.  The same data stream must be used by
                one LIG.
                
                The first index indicates which LIG the
                intercepted traffic will be diverted to. The second index
                permits multiple classifiers to be used together, such as
                having an IP address as source or destination."
            ::= { hwLiStreamGroup 2 }


        hwLiStreamEntry OBJECT-TYPE
            SYNTAX HwLiStreamEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A stream entry indicates a single data stream to be
                intercepted to a Mediation Device. Many selected data
                streams may go to the same application interface, and many
                application interfaces are supported."
            INDEX { hwLiGatewayIndex, hwLiStreamIndex }
            ::= { hwLiStreamTable 1 }

        
        HwLiStreamEntry ::=
            SEQUENCE { 
                hwLiStreamIndex
                    Integer32,
                hwLiStreamLiId
                    Unsigned32,
                hwLiStreamActivationType
                    INTEGER,
                hwLiStreamSessionId
                    Integer32,
                hwLiStreamTargetIdType
                    INTEGER,
                hwLiStreamSrcMacAddress
                    MacAddress,
                hwLiStreamDstMacAddress
                    MacAddress,
                hwLiStreamSrcIpAddress
                    InetAddress,
                hwLiStreamSrcIpLength
                    InetAddressPrefixLength,
                hwLiStreamDstIpAddress
                    InetAddress,
                hwLiStreamDstIpLength
                    InetAddressPrefixLength,
                hwLiStreamProtocol
                    Integer32,                
                hwLiStreamSrcPort
                    InetPortNumber,                                
                hwLiStreamDstPort
                    InetPortNumber,                
                hwLiStreamIfIndex
                    Integer32,
                hwLiStreamUserName
                    OCTET STRING, 
                hwLiStreamRowStatus
                    RowStatus,
                hwLiStreamSrcIpAddressType
                    InetAddressType,
                hwLiStreamDstIpAddressType
                    InetAddressType,
                hwLiStreamSrcVpnName
                    OCTET STRING,
                  hwLiStreamDstVpnName 
                      OCTET STRING,
                hwLiStreamL2tpIfIndex
                    Integer32,
                hwLiStreamL2tpVlanId
                    Integer32,
                hwLiStreamAcctSessionId
                    OCTET STRING    
             }


        hwLiStreamIndex OBJECT-TYPE
            SYNTAX Integer32 (1..8192)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The index of the stream itself."
            ::= { hwLiStreamEntry 1 }

        

        hwLiStreamLiId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The ID indicate a independency stream in a LIG ."
            ::= { hwLiStreamEntry 2 }

        

        hwLiStreamActivationType OBJECT-TYPE
            SYNTAX INTEGER
                {
                iri(1),
                cc(2),
                both(3)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Intercepted IRI or CC or BOTH."
            DEFVAL { cc }
            ::= { hwLiStreamEntry 3 }

        
    
        hwLiStreamSessionId OBJECT-TYPE
            SYNTAX Integer32 (0..2147483647)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The index of the stream itself.0 means no session ID will be specified"
            DEFVAL { 0 }
            ::= { hwLiStreamEntry 4 }

        

        hwLiStreamTargetIdType OBJECT-TYPE
            SYNTAX INTEGER
                {
                oneDirection(1),
                biDirection(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Target ID type specifies the type of packets. 
                1 means one direction traffic is intercept, 
                2 means bidirectional traffic is intercept. 
                
                for bidirectional interception,  if the source IP or destination IP 
                in a packet is equal with the configured hwLiStreamSrcIpAddress£¬
                If other condition is satisfied then the packet is intercepted.
                
                for one-directional interception,  if the sourceIP and DestinationIP 
                in a packet is equal with the configured hwLiStreamSrcIpAddress and 
                hwLiStreamDstIPAddress£¬If other condition is satisfied then the 
                packet is intercepted"
            DEFVAL { biDirection }
            ::= { hwLiStreamEntry 5 }

        

        hwLiStreamSrcMacAddress OBJECT-TYPE
            SYNTAX MacAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Source Mac address of the packets which will be intercepted.0000-0000-0000 means no MAC address will be specified"
            ::= { hwLiStreamEntry 7 }

        

        hwLiStreamDstMacAddress OBJECT-TYPE
            SYNTAX MacAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Destination Mac address of the packets which will be intercepted."
            ::= { hwLiStreamEntry 8 }

        

        hwLiStreamSrcIpAddress OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The Source Address used in packet selection. This address will
                be of the type specified in hwLiStreamIpAddrType.0.0.0.0 means no IP address will be specified"
            DEFVAL { '00000000'H }
            ::= { hwLiStreamEntry 9 }

        

        hwLiStreamSrcIpLength OBJECT-TYPE
            SYNTAX InetAddressPrefixLength
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The length of the Source Prefix. A value of 32 causes all
                addresses to match. This prefix length will be consistent with
                the type specified in hwLiStreamIpAddrType."
            DEFVAL { 32 }
            ::= { hwLiStreamEntry 10 }

        
    
        hwLiStreamDstIpAddress OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The Destination address or prefix used in packet selection.
                This address will be of the type specified in
                hwLiStreamIpAddrType.0.0.0.0 means no IP address will be specified"
            DEFVAL { '00000000'H }                
            ::= { hwLiStreamEntry 11 }

        
        hwLiStreamDstIpLength OBJECT-TYPE
            SYNTAX InetAddressPrefixLength
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The length of the Destination Prefix. A value of 32 causes
                all addresses to match.  This prefix length will be consistent
                with the type specified in hwLiStreamIpAddrType."
            DEFVAL { 32 }
            ::= { hwLiStreamEntry 12 }

        
    
        hwLiStreamProtocol OBJECT-TYPE
            SYNTAX Integer32 (0..255)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Protocol type of the packets which will be intercepted.0 means no Protocol type will be specified"
            DEFVAL { 0 }                
            ::= { hwLiStreamEntry 13 }
        
    
        hwLiStreamSrcPort OBJECT-TYPE
            SYNTAX InetPortNumber
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The fourth layer source port.0 means no Port will be specified"
            DEFVAL { 0 }                
            ::= { hwLiStreamEntry 14 }            
            
    
        hwLiStreamDstPort OBJECT-TYPE
            SYNTAX InetPortNumber
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The fourth layer Destination port.0 means no Port will be specified"
            DEFVAL { 0 }                
            ::= { hwLiStreamEntry 15 }

        
    
        hwLiStreamIfIndex OBJECT-TYPE
            SYNTAX Integer32 (0..2147483647)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The interface switch carrying the intercepted taffic.0 means no interface will be specified"
            DEFVAL { 0 }                
            ::= { hwLiStreamEntry 16 }

        
    
        hwLiStreamUserName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The username whose traffic will be intercepted.zero-length means no user will be specified"
            ::= { hwLiStreamEntry 17 }
        
  
        hwLiStreamRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The status of this conceptual row. This object is used to
                manage creation, modification and deletion of rows in this
                table."
            ::= { hwLiStreamEntry 18 }
        

        hwLiStreamSrcIpAddressType OBJECT-TYPE
            SYNTAX InetAddressType
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The source IP address of the interception stream" 
            DEFVAL { ipv4 }            
            ::= { hwLiStreamEntry 19 } 
        
  
        hwLiStreamDstIpAddressType OBJECT-TYPE
            SYNTAX InetAddressType
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The destination IP address of the interception stream"  
            DEFVAL { ipv4 }            
            ::= { hwLiStreamEntry 20 }  


        hwLiStreamSrcVpnName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The source VPN instance name whose traffic will be intercepted.zero-length means no VPN will be specified"
            ::= { hwLiStreamEntry 21 }

         

        hwLiStreamDstVpnName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The destination VPN instance name whose traffic will be intercepted. zero-length means no VPN will be specified"
            ::= { hwLiStreamEntry 22 }
        

        hwLiStreamL2tpIfIndex OBJECT-TYPE
            SYNTAX  Integer32 (0..2147483647)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The L2TP ifindex of intercepting stream.0 means no l2tpIfindex will be specified"        
            DEFVAL { 0 }    
            ::= { hwLiStreamEntry 23 }
 
        hwLiStreamL2tpVlanId OBJECT-TYPE
            SYNTAX  Integer32 (0..2147483647)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The L2TP VLAN ID of intercepting stream.0 means no Vlan will be specified"     
            DEFVAL { 0 }
            ::= { hwLiStreamEntry 24 }
    
        hwLiStreamAcctSessionId OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The accounting session ID of intercepting stream.zero-length means no accouting session ID will be specified"
            ::= { hwLiStreamEntry 25 }
            
        hwLiMibConform OBJECT IDENTIFIER ::= { hwLiMib 3 }

        
    
        hwLiMibCompliances OBJECT IDENTIFIER ::= { hwLiMibConform 2 }


        hwLiMibCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION 
                "Description."
            MODULE -- this module
                MANDATORY-GROUPS { hwLiGatewayComplianceGroup, hwLiStreamComplianceGroup, hwLiNotificationGroup, hwLiGatewayCpbComplianceGroup }
            ::= { hwLiMibCompliances 1 }

        
    
        hwLiMibGroups OBJECT IDENTIFIER ::= { hwLiMibConform 3 }

        
    
        hwLiAgentComplianceGroup OBJECT-GROUP
            OBJECTS { hwLiAgentTime, hwLiAgentEnable, hwLiAgentX2IpAddress, hwLiAgentX2Port, hwLiAgentX3IpAddress, 
                hwLiAgentX3Port }
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwLiMibGroups 1 }

        
    
        hwLiGatewayComplianceGroup OBJECT-GROUP
            OBJECTS { hwLiGatewayNewIndex, hwLiGatewayAddressType, hwLiGatewayX2Protocol, hwLiGatewayX2Address, hwLiGatewayX2Port, 
                hwLiGatewayX3Protocol, hwLiGatewayX3Address, hwLiGatewayX3Port, hwLiGatewayX3HeartBeatTimer, hwLiGatewayX3NoResponseNum, 
                hwLiGatewayX3OperateStatus, hwLiGatewayX3Dscp, hwLiGatewayRowStatus,hwLiGatewayX3AddressType,hwLiGatewayX2AddressType }
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwLiMibGroups 2 }

        
    
        hwLiStreamComplianceGroup OBJECT-GROUP
            OBJECTS { hwLiStreamLiId, hwLiStreamActivationType, hwLiStreamSessionId, hwLiStreamTargetIdType,  
                hwLiStreamProtocol, hwLiStreamSrcPort,hwLiStreamDstPort,hwLiStreamSrcMacAddress, hwLiStreamDstMacAddress, hwLiStreamSrcIpAddress, hwLiStreamSrcIpLength, 
                hwLiStreamDstIpAddress, hwLiStreamDstIpLength, hwLiStreamIfIndex, hwLiStreamUserName, hwLiStreamRowStatus, 
                hwLiStreamSrcIpAddressType,hwLiStreamDstIpAddressType,hwLiStreamSrcVpnName,hwLiStreamDstVpnName,
                hwLiStreamL2tpIfIndex,hwLiStreamL2tpVlanId,hwLiStreamAcctSessionId }
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwLiMibGroups 3 }

        
    
        hwLiNotificationGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwLiMibActive, hwLiX3HeartBeatAlarm, hwLiX3HeartBeatRecover}
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwLiMibGroups 4 }

        
    
        hwLiGatewayCpbComplianceGroup OBJECT-GROUP
            OBJECTS { hwLiGatewayCapabilities }
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwLiMibGroups 5 }

        
    
    END



