--==================================================================
-- Copyright (C) 2015 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description: HUAWEI DATASYNC MIB
-- Reference:
-- Version: V2.02
-- History:
-- <author>,  <date>,  <contents>
-- fengchong   2009-03-17
-- ==================================================================

-- ==================================================================
-- 
-- Variables and types are imported
--
-- ==================================================================

    HUAWEI-DATASYNC-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            hwDatacomm          
                FROM HUAWEI-MIB         
            OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP         
                FROM SNMPv2-CONF            
            TimeTicks, Integer32, Gauge32, OBJECT-TYPE, MODULE-IDENTITY, 
            NOTIFICATION-TYPE           
                FROM SNMPv2-SMI         
            DisplayString, RowStatus, TEXTUAL-CONVENTION           
                FROM SNMPv2-TC;
    
        hwDataSync MODULE-IDENTITY 
            LAST-UPDATED "201507161349Z"        
            ORGANIZATION 
                "Huawei Technologies Co.,Ltd."
            CONTACT-INFO 
                "Huawei Industrial Base
                  Bantian, Longgang
                   Shenzhen 518129
                   People's Republic of China
                   Website: http://www.huawei.com
                   Email: support@huawei.com
                "
              DESCRIPTION 
                "Modified hwCfgChgTerminalID."
                        REVISION "201507161349Z"         
            DESCRIPTION 
                "Add hwCfgLastSaveFailNotify ."
                        REVISION "201409041710Z"               
            DESCRIPTION 
                "The MIB module for Data sync between host and netmanager."
                        REVISION "200903171027Z"        
            DESCRIPTION 
                "The initial revision of this MIB module ."
            ::= { hwDatacomm 191 }

        DateAndTime ::= TEXTUAL-CONVENTION
            DISPLAY-HINT "2d-1d-1d,1d:1d:1d.1d,1a1d:1d"
            STATUS       current
            DESCRIPTION
            "A date-time specification.

            field  octets  contents                  range
            -----  ------  --------                  -----
              1      1-2   year*                     0..65536
              2       3    month                     1..12
              3       4    day                       1..31
              4       5    hour                      0..23
              5       6    minutes                   0..59
              6       7    seconds                   0..60
                           (use 60 for leap-second)
              7       8    deci-seconds              0..9
              8       9    direction from UTC        '+' / '-'
              9      10    hours from UTC*           0..13
             10      11    minutes from UTC          0..59

            * Notes:
            - the value of year is in network-byte order
            - daylight saving time in New Zealand is +13

            For example, Tuesday May 26, 1992 at 1:30:15 PM EDT would be
            displayed as:

                             1992-5-26,13:30:15.0,-4:0
            Note that if only local time is known, then timezone
            information (fields 8-10) is not present."
            SYNTAX       OCTET STRING (SIZE (8 | 11))
--
-- Node definitions
--
    
--  ==================================================================
-- 
-- ======================= definition begin =========================
-- 
-- ==================================================================  
        hwDataSyncScalarObjects OBJECT IDENTIFIER ::= { hwDataSync 1 }
        hwDataSyncTableObjects OBJECT IDENTIFIER ::= { hwDataSync 2 }
        hwDataSyncNotifications OBJECT IDENTIFIER ::= { hwDataSync 3 }
        hwDataSyncConformance OBJECT IDENTIFIER ::= { hwDataSync 4 }
        
        hwCurrentCfgChgSeqID OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the ID of the current configuration change. 
                The value ranges from 0 to 65535. After the ID of the configuration change reaches
                the maximum value, the value of the ID starts from 1 again. 
                After the device is restarted, the value of the ID becomes 0."
            ::= { hwDataSyncScalarObjects 1 }
            
        hwCfgChgSeqIDReveralCount OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the cycle count of the index of configuration change table."
            ::= { hwDataSyncScalarObjects 2 }            
         
         hwCfgChgTableMaxItem OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the maximum number of entries in hwCfgChgTable. "
            ::= { hwDataSyncScalarObjects 3 }   
            
            
        hwCfgBaselineTime OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..20))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Specifies the time of system confiuration was baseline."
            ::= { hwDataSyncScalarObjects 4 }
  
        hwDataSyncGroups OBJECT IDENTIFIER ::= { hwDataSyncConformance 1 }
      
        hwDataSyncScalarObjectsGroup OBJECT-GROUP
            OBJECTS { hwCurrentCfgChgSeqID, hwCfgChgSeqIDReveralCount, hwCfgChgTableMaxItem, hwCfgBaselineTime}
            STATUS current
            DESCRIPTION 
                "A collection of objects on DataSync ScalarObjects Information."
            ::= { hwDataSyncGroups 1 }          
        
        hwCfgChgNotifyGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwCfgChgNotify}
            STATUS current
            DESCRIPTION 
                "A collection of objects on Configuration Change Information."
            ::= { hwDataSyncGroups 2 }        

        hwDataSyncNotifyGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwCfgLastSaveFailNotify }
            STATUS current
            DESCRIPTION 
                "A collection of objects on synchronization Configuration Notify Information."
            ::= { hwDataSyncGroups 3 }            
                  
        hwDataSyncCompliances OBJECT IDENTIFIER ::= { hwDataSyncConformance 2 }
       
        hwDataSyncCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION 
                "The compliance statement for 
                entities that support the huawei DataSync MIB."
            MODULE      -- this module
            ::= { hwDataSyncCompliances 1 }     
	    
        hwCfgChgTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwCfgChgEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is used to record configuration changes. 
                In this table, you can find the configuration change based on the specific index."
            ::= { hwDataSyncTableObjects 1 }


        hwCfgChgEntry OBJECT-TYPE
            SYNTAX HwCfgChgEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Entry of hwCfgChgTable."
            INDEX { hwCfgChgSeqID }
            ::= { hwCfgChgTable 1 }

        
        HwCfgChgEntry::=
            SEQUENCE { 
                hwCfgChgSeqID
                    Integer32,
                hwCfgChgTime
                    DateAndTime,
                hwCfgChgTerminalType
                    INTEGER,
                hwCfgChgTerminalID
                    Integer32,
                hwCfgChgType
                    INTEGER,
                hwCfgChgViewName
                    OCTET STRING,
                hwCfgChgCmdID
                    Integer32,
                hwCfgChgDetailInfo
                    OCTET STRING
             }


        hwCfgChgSeqID OBJECT-TYPE
            SYNTAX Integer32 (0..65535)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the configuration change ID. 
                When configuration is changed, the sequence id will plus 1."
            ::= { hwCfgChgEntry 1 }
        
        hwCfgChgTime OBJECT-TYPE
            SYNTAX DateAndTime 
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the configuration change time."
            ::= { hwCfgChgEntry 2 }

        hwCfgChgTerminalType OBJECT-TYPE
            SYNTAX INTEGER {snmp(1),telnet(2),netconf(3)} 
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the type of the terminal."
            ::= { hwCfgChgEntry 3 }
         
        hwCfgChgTerminalID OBJECT-TYPE
            SYNTAX Integer32 (0..2147483647) 
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the terminal ID."
            ::= { hwCfgChgEntry 4 }           
 
        hwCfgChgType OBJECT-TYPE
            SYNTAX INTEGER {create(1),modify(2),delete(3)}
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the configuration change type."
            ::= { hwCfgChgEntry 5 }  
            
        hwCfgChgViewName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the name of the view in which the configuration change occurs.
                For the command operation, the object is the name of the view in which the command is run.
                For the SNMP operation, the object is the OID of the MIB table or the scalar object."
            ::= { hwCfgChgEntry 6 }  
            

        hwCfgChgCmdID OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the ID of the configuration change command.
                For the SNMP operation, the value is 0."
            ::= { hwCfgChgEntry 7 }  
        
        hwCfgChgDetailInfo OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates detailed configuration change information.
                For the command operation, the object is the command line.
                For the SNMP operation, the object is the index of the MIB table.
                When there are multiple indexes, the format of index1.index2.index3 is adopted."
            ::= { hwCfgChgEntry 8 }     
            
        hwCollectTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwCollectEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is used to enable the NMS to send the collecting script to the device to trigger the collection, 
                and then monitor the collection status."
            ::= { hwDataSyncTableObjects 2 }

        hwCollectEntry OBJECT-TYPE
            SYNTAX HwCollectEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Entry of hwCollectTable."
            INDEX { hwCollectIndex }
            ::= { hwCollectTable 1 }        
        
        HwCollectEntry ::=
            SEQUENCE { 
                    hwCollectIndex
                        Integer32,
                    hwCollectNetManageId
                        Integer32,
                    hwCollectOperation
                        INTEGER,
                    hwCollectInScriptFile
                        OCTET STRING,
                    hwCollectInResultFile
                        OCTET STRING,
                    hwCollectState
                        INTEGER,
                    hwCollectRowStatus
                        RowStatus
                     }  

        hwCollectIndex OBJECT-TYPE
            SYNTAX Integer32 
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The value of this object identifies the collection index."
            ::= { hwCollectEntry 1 }    

        hwCollectNetManageId OBJECT-TYPE
            SYNTAX Integer32 
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The value of this object identifies the NMS ID."
            ::= { hwCollectEntry 2 }               

        hwCollectOperation OBJECT-TYPE
            SYNTAX INTEGER {begin(1),stop(2)}
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the instruction for the collection operation.
                Default value is stop." 
            ::= { hwCollectEntry 3 } 
            
        hwCollectInScriptFile OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..255))
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the name of the script file. T
                he length of the file name ranges from 1 character to 255 characters."  
            ::= { hwCollectEntry 4 } 
            
        hwCollectInResultFile OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..255))
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the name of the result file. 
                The length of the file name ranges from 1 character to 255 characters."
            ::= { hwCollectEntry 5 } 
              

        hwCollectState OBJECT-TYPE
            SYNTAX INTEGER {idle(1),collecting(2)}
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the collection status."
            ::= { hwCollectEntry 6 } 
 
         hwCollectRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the row status."
            ::= { hwCollectEntry 7 }     
        
        hwCfgChgNotify NOTIFICATION-TYPE
        OBJECTS {hwCurrentCfgChgSeqID, hwCfgChgSeqIDReveralCount, hwCfgChgTableMaxItem, hwCfgBaselineTime}
        STATUS current
        DESCRIPTION 
            "This trap is generated when a configuration change occurs 
            on the device within a specified period."
        ::= { hwDataSyncNotifications 1 }      
        
        hwCfgLastSaveFailNotify NOTIFICATION-TYPE
        STATUS current
        DESCRIPTION 
            "The last save operation failed, please check the configuration."
        ::= { hwDataSyncNotifications 2 } 

                    
    END

--
-- HUAWEI-BULKSTAT-MIB.mib
--