--
-- HUAWEI-PERFMGMT-MIB.my
-- Friday, March 19, 2010 at 10:45:33
--

--    ==================================================================
-- Copyright (C) 2017 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description: HUAWEI PERFMGMT MIB
-- Reference:
-- Version: V4.14
-- History:  V4.08  huqing, 2015-09-21,Modify nodes 
-- created 2014-05-05
-- ==================================================================

    HUAWEI-PERFMGMT-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS                    
            hwDatacomm            
                FROM HUAWEI-MIB            
            OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP            
                FROM SNMPv2-CONF            
            Integer32, Unsigned32, OBJECT-TYPE, MODULE-IDENTITY, OBJECT-IDENTITY, NOTIFICATION-TYPE, IpAddress
                FROM SNMPv2-SMI            
            RowStatus, TimeStamp, DateAndTime            
                FROM SNMPv2-TC 
            InetAddressType, InetAddress  
                FROM INET-ADDRESS-MIB;    
    
--  June 07, 2009 at 16:33 GMT
-- February 27, 2009 at 11:41 GMT
        -- 1.3.6.1.4.1.2011.5.25.190
        hwPerfMgmt MODULE-IDENTITY 
            LAST-UPDATED "201708210958Z"        --Aug 21, 2017 at 09:58GMT
            ORGANIZATION 
                  "Huawei Technologies Co.,Ltd."
            CONTACT-INFO 
                  "Huawei Industrial Base
                    Bantian, Longgang
                     Shenzhen 518129
                     People's Republic of China
                     Website: http://www.huawei.com
                     Email: support@huawei.com
                   "
            DESCRIPTION 
                "V4.13  add MIB nodes ." 

           REVISION "201708210958Z"        --Aug 21, 2017 at 09:58GMT
          
           DESCRIPTION 
                "V4.14  modify description." 

                
            REVISION "201708172119Z"        --Aug 17, 2017 at 15:30GMT

            DESCRIPTION 
                "V4.12  add MIB nodes ." 
                
            REVISION "201708092119Z"        --Aug 9, 2017 at 21:19GMT

            DESCRIPTION 
                "V4.11  delete MIB nodes ." 
                
            REVISION "201601291434Z"        --Jur 19, 2016 at 14:34GMT
            
            DESCRIPTION 
                "V4.10  add MIB nodes ." 
                
            REVISION "201601191434Z"        --Jur 19, 2016 at 14:34GMT
                        
            DESCRIPTION 
                "V4.09  modify MIB nodes hwPMMeasureExceed ." 
                
            REVISION "201510161434Z"        --Oct 16, 2015 at 14:34GMT

            DESCRIPTION 
                "The MIB module for performance management."  
                
           REVISION "201509211434Z"        --Sep 21, 2015 at 14:34GMT

            DESCRIPTION 
                "V4.08  add MIB nodes." 
                
            REVISION "201502071434Z"        --Feb 7, 2015 at 14:34GMT
            DESCRIPTION 
                "V4.07  modify MIB nodes  hwPMReSetCurrentDataIndicatorID, hwPMReSetCurrentDataInstanceName,hwPMReSetCurrentDataInstanceType for mistakes in format." 

            REVISION "201502061434Z"        --Feb 6, 2015 at 14:34GMT
            DESCRIPTION 
                "V4.06  delete MIB nodes  hwPMReSetCurrentDataIndicatorID, hwPMReSetCurrentDataInstanceName,hwPMReSetCurrentDataInstanceType from group as they are undefined or unaccessible."    

            REVISION "201405051631Z"        --May 5, 2014 at 16:31GMT
            DESCRIPTION 
                "V4.05  modify MIB nodes."    
        
            REVISION "201403132119Z"        -- Oct 14, 2013 at 16:55GMT
            DESCRIPTION 
                "V4.04  modify MIB nodes."    
            REVISION "201310141655Z"        -- Oct 14, 2013 at 16:55GMT
            DESCRIPTION 
                "V4.03  modify MIB nodes."        
            REVISION "201309261000Z"        -- Sep 26, 2013 at 10:00GMT
            DESCRIPTION 
                "V4.02  Add hwPMServerVPNType to support VPN."                    
            REVISION "201305201512Z"        -- July 19, 2013 at 15:39GMT
            DESCRIPTION 
                "V4.00,  modify MIB nodes." 
            REVISION "201305201512Z"        -- May 20, 2013 at 15:12 GMT
            DESCRIPTION 
                "V3.00,  add MIB nodes."  
            REVISION "201305201512Z"        -- May 20, 2013 at 15:12 GMT
            DESCRIPTION 
                "V3.00,  modify for this MIB module."    
            REVISION "201103160000Z"        
            DESCRIPTION 
                "V1.01  modify for mib index."
            REVISION "200902271141Z"        -- February 27, 2009 at 11:41 GMT
            DESCRIPTION 
                "V1.00, The initial revision of this MIB module."       
          
            ::= { hwDatacomm 190 }

        
    
    
--
-- Node definitions
--
        hwPMStatisticsMIBInstances OBJECT IDENTIFIER ::= { hwPerfMgmt 1 }
        
        hwPMStatisticsEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Enable or disable the statistics data function."
            DEFVAL { disable }
            ::= { hwPMStatisticsMIBInstances 1 }
        
        hwPMStatisticsMaxFilesPerTask OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The maximum number of files reserved for each statistics task."
            ::= { hwPMStatisticsMIBInstances 2 }
        
        hwPMStatisticsMaxTasks OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The maximum number of statistics tasks allowed to be created."
            ::= { hwPMStatisticsMIBInstances 3 }
        
        hwPMStatisticsCurrentTasks OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The current number of statistics tasks configured."
            ::= { hwPMStatisticsMIBInstances 4 }
        
        hwPMStatisticsTaskTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMStatisticsTaskEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The statistics task table, providing create/modify/delete operations.
                To create a task, you need to create a related record in this table, and add instance nodes in the hwPMTaskInstanceTable.
                If you delete a task, the related instances in the hwPMTaskInstanceTable will be deleted."
            ::= { hwPMStatisticsMIBInstances 5 }
        
        hwPMStatisticsTaskEntry OBJECT-TYPE
            SYNTAX HwPMStatisticsTaskEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry of hwStatisticsTaskTable."
            INDEX { hwPMStatisticsTaskName }
            ::= { hwPMStatisticsTaskTable 1 }
        
        HwPMStatisticsTaskEntry ::=
            SEQUENCE { 
                hwPMStatisticsTaskName
                    OCTET STRING,
                hwPMStatisticsTaskFileFormat
                    INTEGER,
                hwPMStatisticsRecordFileEnable
                  INTEGER,
                hwPMStatisticsThresholdEnable
                  INTEGER,
                hwPMStatisticsTaskPeriod
                    INTEGER,
                hwPMStatisticsTaskTransferPeriod
                    Integer32,
                hwPMStatisticsTaskCurrentFileIndex
                    Unsigned32,
                hwPMStatisticsTaskRowStatus
                    RowStatus,
                hwPMStatisticsTaskSampleInterval
                    INTEGER,
                hwPMStatisticsUploadAutoName
                    OCTET STRING,
                hwPMStatisticsTaskType
                	INTEGER,
                hwPMStatisticsHighPrecisionPeriod
                	Unsigned32,
                hwPMStatisticsSampleLevel
                	INTEGER
             }

        hwPMStatisticsTaskName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..31))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the name of a statistics task."
            ::= { hwPMStatisticsTaskEntry 1 }
        
        hwPMStatisticsTaskFileFormat OBJECT-TYPE
            SYNTAX INTEGER
                {
                hwPMtxtv1(1),
                hwPMbinv1(2),
                hwPM3Gppxmlv1(3)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The statistics task file format, only text(1) can be supported now."
            DEFVAL { hwPMtxtv1 }
            ::= { hwPMStatisticsTaskEntry 2 }
        
        
        hwPMStatisticsRecordFileEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Enable or disable the record file function. "
            DEFVAL { enable }
            ::= { hwPMStatisticsTaskEntry 3 }
            
        hwPMStatisticsThresholdEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Enable or disable the threshold function. "
            DEFVAL { disable }
            ::= { hwPMStatisticsTaskEntry 4 }    
            
        hwPMStatisticsTaskPeriod OBJECT-TYPE
            SYNTAX INTEGER
                {
                five(5),
                ten(10),
                fifteen(15),
                thirty(30),
                sixty(60),
                twentyfourhours(1440),
                invalid(0)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The interval of statistics task, in minutes."
            DEFVAL { fifteen }
            ::= { hwPMStatisticsTaskEntry 5 }
        
        hwPMStatisticsTaskTransferPeriod OBJECT-TYPE
            SYNTAX Integer32 (1..60)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the interval for generating performance data files. The value is an integer multiple of the statistics period. If a short statistics collection period (non-24 hour), the value ranges from 1 to 16.
For a long period, the value ranges from 1 to 3."
            DEFVAL { 4 }
            ::= { hwPMStatisticsTaskEntry 6 }
        
        hwPMStatisticsTaskCurrentFileIndex OBJECT-TYPE
            SYNTAX Unsigned32 (0..4)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The current file index of statistics task."
            DEFVAL { 0 }
            ::= { hwPMStatisticsTaskEntry 7 }
            
            hwPMStatisticsTaskRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The row status."
            ::= { hwPMStatisticsTaskEntry 16 }
            
        hwPMStatisticsTaskSampleInterval OBJECT-TYPE
            SYNTAX INTEGER
                {
                one(1),
                two(2),
                three(3),
                five(5),
                ten(10),
                fifteen(15),
                thirty(30),
                sixty(60)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The interval of task sampling, in minutes."
            DEFVAL { 3 }
            ::= { hwPMStatisticsTaskEntry 17 }            
        hwPMStatisticsUploadAutoName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..31))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The object refers to the mib node hwPMFileUploadRequestName,which enables the device to automatically 
                and periodically send statistics files to the server."
            ::= { hwPMStatisticsTaskEntry 18 }
                      
        hwPMStatisticsTaskType OBJECT-TYPE  
           SYNTAX INTEGER
                {
                pmStatistics(3),
                pmSdh(6),
                monHistory(7),
                monStatistics(8),
                sdhShort(10)                
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The type of statistics task."
            DEFVAL { pm-statistics }
            ::= { hwPMStatisticsTaskEntry 19 }    
           
       	hwPMStatisticsHighPrecisionPeriod OBJECT-TYPE
            SYNTAX Unsigned32 (5..86400)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The interval of statistics task, in seconds. if taskType is sdhShort , It must be multiple of 5 seconds and less or equal to 900 seconds, else It must be multiple of 30 seconds."
            DEFVAL { 900 }
            ::= { hwPMStatisticsTaskEntry 20 }
 
       hwPMStatisticsSampleLevel OBJECT-TYPE  
           SYNTAX INTEGER
                {
                default(0),
                second(1)              
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The sample level of statistics task."
            DEFVAL { minute }
            ::= { hwPMStatisticsTaskEntry 21 }    
                 
        hwPMStatisticsTaskInstanceTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMStatisticsTaskInstanceEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The statistics task instance table."
            ::= { hwPMStatisticsMIBInstances 6 }
        
        hwPMStatisticsTaskInstanceEntry OBJECT-TYPE
            SYNTAX HwPMStatisticsTaskInstanceEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry of hwStatisticsTaskInstanceTable."
            INDEX { hwPMStatisticsTaskName, hwPMStatisticsTaskInstanceType, hwPMStatisticsTaskInstanceName }
            ::= { hwPMStatisticsTaskInstanceTable 1 }
        
        HwPMStatisticsTaskInstanceEntry ::=
            SEQUENCE { 
                hwPMStatisticsTaskInstanceType
                    Unsigned32,
                hwPMStatisticsTaskInstanceName
                    OCTET STRING,
                hwPMStatisticsTaskInstanceRowStatus
                    RowStatus
             }

        hwPMStatisticsTaskInstanceType OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The instance type of statistics task."
            ::= { hwPMStatisticsTaskInstanceEntry 1 }
        
        hwPMStatisticsTaskInstanceName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..255))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The instance name of statistics task."
            ::= { hwPMStatisticsTaskInstanceEntry 2 }
        
        hwPMStatisticsTaskInstanceRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The row status."
            ::= { hwPMStatisticsTaskInstanceEntry 3 }
        
        hwPMStatisticsTaskIndicatorTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMStatisticsTaskIndicatorEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The statistics task indicator table."
            ::= { hwPMStatisticsMIBInstances 7 }
        
        hwPMStatisticsTaskIndicatorEntry OBJECT-TYPE
            SYNTAX HwPMStatisticsTaskIndicatorEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry of hwStatisticsTaskIndicatorTable."
            INDEX { hwPMStatisticsTaskName, hwPMStatisticsTaskInstanceType, hwPMStatisticsTaskIndicator }
            ::= { hwPMStatisticsTaskIndicatorTable 1 }
        
        HwPMStatisticsTaskIndicatorEntry ::=
            SEQUENCE { 
                hwPMStatisticsTaskIndicator
                    Unsigned32,
                hwPMStatisticsTaskIndicatorRowStatus
                    RowStatus
             }

        hwPMStatisticsTaskIndicator OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The statistics task indicator."
            ::= { hwPMStatisticsTaskIndicatorEntry 1 }
        
        hwPMStatisticsTaskIndicatorRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The row status."
            ::= { hwPMStatisticsTaskIndicatorEntry 2 }
        
        hwPMStatisticsTaskThresholdRuleTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMStatisticsTaskThresholdRuleEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The table is threshold management rule table, which is used to configure threshold rules for the indexes of the object type to be associated with the threshold template. "
            ::= { hwPMStatisticsMIBInstances 8 }
        
        hwPMStatisticsTaskThresholdRuleEntry OBJECT-TYPE
            SYNTAX HwPMStatisticsTaskThresholdRuleEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry of hwStatisticsTaskThresholdRuleTable."
            INDEX { hwPMStatisticsTaskName, hwPMStatisticsTaskInstanceType, hwPMStatisticsTaskIndicator, hwPMStatisticsTaskThresholdType}
            ::= { hwPMStatisticsTaskThresholdRuleTable 1 }
        
        HwPMStatisticsTaskThresholdRuleEntry ::=
            SEQUENCE { 
              hwPMStatisticsTaskThresholdType
                  INTEGER,
                hwPMStatisticsTaskThresholdHighTriggerValue
                    Unsigned32,
                hwPMStatisticsTaskThresholdLowTriggerValue
                    Unsigned32,
                hwPMStatisticsTaskThresholdHighClearedValue
                    Unsigned32,
                hwPMStatisticsTaskThresholdLowClearedValue
                    Unsigned32,
                hwPMStatisticsTaskThresholdRuleRowStatus
                    RowStatus
             }
    
        
        hwPMStatisticsTaskThresholdType OBJECT-TYPE
            SYNTAX INTEGER
                {
                hightrigger(1),
                lowtrigger(2)
                }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The threshold type of the threshold rule."
            ::= { hwPMStatisticsTaskThresholdRuleEntry 1 }
        
        hwPMStatisticsTaskThresholdHighTriggerValue OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The high 32 bit of threshold alarm trigger value. "
            ::= { hwPMStatisticsTaskThresholdRuleEntry 2 }
        
        hwPMStatisticsTaskThresholdLowTriggerValue OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The low 32 bit of threshold alarm trigger value . "
            ::= { hwPMStatisticsTaskThresholdRuleEntry 3 }
        
        hwPMStatisticsTaskThresholdHighClearedValue OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The high 32 bit of threshold alarm clear value. "
            ::= { hwPMStatisticsTaskThresholdRuleEntry 4 }
        
        hwPMStatisticsTaskThresholdLowClearedValue OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The low 32 bit of threshold alarm clear value. "
            ::= { hwPMStatisticsTaskThresholdRuleEntry 5 }
        
        hwPMStatisticsTaskThresholdRuleRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The row status of the threshold rule."
            ::= { hwPMStatisticsTaskThresholdRuleEntry 50 }
        
    
        
        hwPMStatisticsTaskThresholdEvent OBJECT-IDENTITY
            STATUS current
            DESCRIPTION
                "Definition point for performance threshold notifications."
            ::= { hwPMStatisticsMIBInstances 9 }
                
        hwPMStatisticsTaskThresholdTriggerAlarm NOTIFICATION-TYPE
            OBJECTS { hwPMStatisticsTaskName, hwPMStatisticsTaskPeriod, hwPMStatisticsTaskInstanceName, hwPMStatisticsTaskIndicator, 
            hwPMStatisticsTaskThresholdType, hwPMStatisticsTaskThresholdHighTriggerValue, hwPMStatisticsTaskThresholdLowTriggerValue,
            hwPMStatisticsTaskIndicateHighValue, hwPMStatisticsTaskIndicateLowValue}
            STATUS current
            DESCRIPTION
                "This object indicates the threshold triggering alarm object."
            ::= { hwPMStatisticsTaskThresholdEvent 1 }

        
        hwPMStatisticsTaskThresholdClearAlarm NOTIFICATION-TYPE
            OBJECTS {hwPMStatisticsTaskName, hwPMStatisticsTaskPeriod, hwPMStatisticsTaskInstanceName, hwPMStatisticsTaskIndicator, 
            hwPMStatisticsTaskThresholdType, hwPMStatisticsTaskThresholdHighClearedValue, hwPMStatisticsTaskThresholdLowClearedValue,
            hwPMStatisticsTaskIndicateHighValue, hwPMStatisticsTaskIndicateLowValue}
            STATUS current
            DESCRIPTION
                "This object indicates the threshold clear object. "
            ::= { hwPMStatisticsTaskThresholdEvent 2 } 

        hwPMCSESEvent NOTIFICATION-TYPE
            OBJECTS {hwPMEventStartTime, hwPMEventDuration, hwPMStatisticsInstanceTypeName, hwPMInstanceType, 
            hwPMInstanceName, hwPMIndicator, hwPMStatisticsIndicatorName}
            STATUS current
            DESCRIPTION
                "The SNMP trap that is generated when CSES measure
                entry crosses its falling or rising threshold  generates
                an event that is configured for sending SNMP
                traps."
            ::= { hwPMStatisticsTaskThresholdEvent 3 }

        hwPMUATEvent NOTIFICATION-TYPE
            OBJECTS {hwPMEventStartTime, hwPMEventEndTime, hwPMEventState, hwPMStatisticsInstanceTypeName, hwPMInstanceType, 
            hwPMInstanceName, hwPMIndicator, hwPMStatisticsIndicatorName}
            STATUS current
            DESCRIPTION
                "The SNMP trap that is generated when UAT measure
                entry crosses its falling or rising threshold  generates
                an event that is configured for sending SNMP
                traps."
            ::= { hwPMStatisticsTaskThresholdEvent 4 }
            
        hwPMStatisticsTaskIndicateLowValue OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "This object indicates the lower 32 bits of the current alarm value. "
            ::= { hwPMStatisticsMIBInstances 10 }  
               
        hwPMStatisticsTaskIndicateHighValue OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "This object indicates the higher 32 bits of the current alarm value. "
            ::= { hwPMStatisticsMIBInstances 11 }

    
        hwPMStatisticsTaskFileTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMStatisticsTaskFileEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is used to query information about statistic tasks' performance data files."
            ::= { hwPMStatisticsMIBInstances 12 }
      
        
        hwPMStatisticsTaskFileEntry OBJECT-TYPE
            SYNTAX HwPMStatisticsTaskFileEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry of hwStatisticsTaskFileTable."
            INDEX { hwPMStatisticsTaskName, hwPMStatisticsTaskFileIndex }
            ::= { hwPMStatisticsTaskFileTable 1 }
        
        HwPMStatisticsTaskFileEntry ::=
            SEQUENCE { 
                hwPMStatisticsTaskFileIndex
                    Unsigned32,
                hwPMStatisticsTaskFileName
                    OCTET STRING    
                     }

        hwPMStatisticsTaskFileIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The statistics task file index."
            ::= { hwPMStatisticsTaskFileEntry 1 }
        
        hwPMStatisticsTaskFileName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The statistics task file name."
            ::= { hwPMStatisticsTaskFileEntry 2 }
            
        hwPMStatisticsTraps OBJECT-IDENTITY
            STATUS current
            DESCRIPTION
                "Definition point for measure exceed notifications."
            ::= { hwPMStatisticsMIBInstances 13}

        hwPMEventStartTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The CSES event  starttime value. "
            ::= { hwPMStatisticsMIBInstances 14 }

        hwPMEventEndTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The CSES event endtime value. "
            ::= { hwPMStatisticsMIBInstances 15 }

        hwPMEventDuration OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The CSES event duration value. "
            ::= { hwPMStatisticsMIBInstances 16 }
        
        hwPMEventState OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The UAT event state. "
            ::= { hwPMStatisticsMIBInstances 17 }

         hwPMIndicator  OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The indicator ID."
            ::= { hwPMStatisticsMIBInstances 18 }
            
        hwPMInstanceType  OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The instance type ID."
            ::= { hwPMStatisticsMIBInstances 19 }
        
        hwPMStatisticsInstanceTypeName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The statistics instance type name."
            ::= { hwPMStatisticsMIBInstances 20 }
             
        hwPMInstanceName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The instance name."
            ::= { hwPMStatisticsMIBInstances 21 }
                               
         hwPMStatisticsIndicatorName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The statistics indicator name."
            ::= { hwPMStatisticsMIBInstances 22 }
          
        hwPMMeasureExceed NOTIFICATION-TYPE
            STATUS current
            DESCRIPTION
                "The number of statistical indexes has reached the upper limit."
            ::= { hwPMStatisticsTraps 1 }
        
        hwPMFileUploadMgmtInstances OBJECT IDENTIFIER ::= { hwPerfMgmt 2 }
        
        hwPMServerTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMServerEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "After the performance statistics file is generated, the file is transmitted to the performance management server. The table is used to create a performance management server."
            ::= { hwPMFileUploadMgmtInstances 1 }
        
        hwPMServerEntry OBJECT-TYPE
            SYNTAX HwPMServerEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
            "The entry of hwPMServerTable."
            INDEX { hwPMServerName }
            ::= { hwPMServerTable 1 }        
 
        HwPMServerEntry ::=
            SEQUENCE { 
                hwPMServerName
                    OCTET STRING,  
                hwPMServerSrcAddrType
                   InetAddressType,  
                hwPMServerSrcAddr
                    InetAddress,
                hwPMServerVpnName
                    OCTET STRING, 
                hwPMServerHostAddrType
                   InetAddressType, 
                hwPMServerHostAddr
                    InetAddress,
                hwPMServerPort
                    Integer32,
                hwPMServerUserName
                    OCTET STRING,
                hwPMServerPassword
                    OCTET STRING,
                hwPMServerSrcIfName
                    OCTET STRING, 
                hwPMServerRetryTimes
                    Unsigned32,
                hwPMServerDestPath
                   OCTET STRING,
                hwPMServerTransferProtocol
                    INTEGER,
                hwPMServerRowStatus
                    RowStatus,
                hwPMServerVpnType
                    INTEGER
            }

        hwPMServerName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..31))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
            "The server name."
            ::= { hwPMServerEntry 1 }

        hwPMServerSrcAddrType OBJECT-TYPE
             SYNTAX InetAddressType
             MAX-ACCESS read-only
             STATUS current 
              DESCRIPTION
            "Server source ip-address type."    
            DEFVAL { ipv4 }
            ::= { hwPMServerEntry 2 }   
            

            
        hwPMServerSrcAddr OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
            "The server source ip-address, reservation node, don't support now."
            ::= { hwPMServerEntry 3 }

        
        hwPMServerVpnName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..31))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
            "The server VPN name."
            ::= { hwPMServerEntry 4 }

        hwPMServerHostAddrType OBJECT-TYPE
         SYNTAX InetAddressType
             MAX-ACCESS read-create
             STATUS current 
              DESCRIPTION
            "Server host ip-address type."   
            DEFVAL { ipv4 }
            ::= { hwPMServerEntry 5 }  
            

        hwPMServerHostAddr OBJECT-TYPE
            SYNTAX InetAddress
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
            "The server host ip-address."
            ::= { hwPMServerEntry 6 }  

        
        hwPMServerPort OBJECT-TYPE
            SYNTAX Integer32 (1..65535)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION 
            "The server port." 
            ::= { hwPMServerEntry 7 }

        
        hwPMServerUserName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..255))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
            "The server user name."
            ::= { hwPMServerEntry 8 }

        
        hwPMServerPassword OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..128))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
            "This object indicates the password for logging in to the PM server."
            ::= { hwPMServerEntry 9 }

        hwPMServerSrcIfName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..48))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
            "The server source interface name, reservation node, don't support now."
            ::= { hwPMServerEntry 10 }

        hwPMServerRetryTimes OBJECT-TYPE
            SYNTAX Unsigned32 (1..3)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
            "The erver retry times."
            DEFVAL { 3 }
            ::= { hwPMServerEntry 11 }

        hwPMServerDestPath OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..63))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The server destination path." 
            ::= { hwPMServerEntry 12 }
            
        hwPMServerTransferProtocol OBJECT-TYPE
            SYNTAX INTEGER
                {
                ftp(1),
                tftp(2), 
                sftp(3)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
            "The server transfer protocol"
            ::= { hwPMServerEntry 13 }
                
        hwPMServerRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
            "The row status."
            ::= { hwPMServerEntry 14 }       
       
        hwPMServerVpnType OBJECT-TYPE
            SYNTAX INTEGER
                {
                none(0),
                managevpn(1),
                vpninstance(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
            "The server VPN type."
            ::= { hwPMServerEntry 15 }
            
        hwPMFileUploadCfgTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMFileUploadCfgEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The PM file upload config table."
            ::= { hwPMFileUploadMgmtInstances 2 }
            
            hwPMFileUploadCfgEntry OBJECT-TYPE
            SYNTAX HwPMFileUploadCfgEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The Entry of hwPMFileUploadCfgTable."
            INDEX { hwPMFileUploadRequestName }
            ::= { hwPMFileUploadCfgTable 1 }
        
        HwPMFileUploadCfgEntry  ::=
            SEQUENCE { 
                hwPMFileUploadRequestName
                    OCTET STRING,
                hwPMFileUploadServerName
                    OCTET STRING,
                hwPMFileUploadCfgRowStatus
                    RowStatus
             }    
             
     hwPMFileUploadRequestName OBJECT-TYPE
             SYNTAX OCTET STRING (SIZE (1..31))
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
               "The Upload Request name."
           ::= { hwPMFileUploadCfgEntry 1 }
        
         hwPMFileUploadServerName OBJECT-TYPE
             SYNTAX OCTET STRING (SIZE (1..31))
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                 "The file upload server name."
             ::= { hwPMFileUploadCfgEntry 2 }
            
        hwPMFileUploadCfgRowStatus OBJECT-TYPE
             SYNTAX RowStatus
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                 "File upload request config row status."
             ::= { hwPMFileUploadCfgEntry 3 }
                   
      hwPMFileUploadMgmtTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMFileUploadMgmtEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is a file upload management table and is used to create file upload requests."
            ::= { hwPMFileUploadMgmtInstances 3 }

        hwPMFileUploadMgmtEntry OBJECT-TYPE
            SYNTAX HwPMFileUploadMgmtEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Entry of hwPMFileUploadMgmtTable."
            INDEX { hwPMFileUploadRequestName }
            ::= { hwPMFileUploadMgmtTable 1 }
        
        HwPMFileUploadMgmtEntry ::=
            SEQUENCE { 
                hwPMFileUploadFileList
                    OCTET STRING,
                hwPMFileUploadStatus
                    INTEGER             
                    }
                
        hwPMFileUploadFileList OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..543))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the performance statistics file transfer list."
            ::= { hwPMFileUploadMgmtEntry 3 }
        
        hwPMFileUploadStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                init(1),
                running(2),
                success(3),
                fileOpenFail(4),
                unreachableServerIp(5),
                linkFailed(6),
                authenticateFailed(7),
                fileReadFailed(8),
                fileWriteFailed(9),
                failed(10)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The file upload status. 
                init(1): FTP has not been starting to upload file.
                running(2): FTP is running. If you set this node as running, the FTP will be started.                
                success(3): FTP completed successfully.                                                              
                fileOpenFail(4): FTP failed. The cause is file open failure.                                         
                unreachableServerIp(5): FTP failed. The cause is that the IP address of the server is not reachable. 
                linkFailed(6): FTP failed. The cause is connecting to server failed.                                 
                authenticateFailed(7): FTP failed. The cause is authenticating failed.For FTP mode only.             
                fileReadFailed(8): FTP failed. The cause is reading file failed.                                     
                fileWriteFailed(9): FTP failed. The cause is writing file failed.
                failed(10):FTP failed, General error."
            ::= { hwPMFileUploadMgmtEntry 4 }
                            
            
        hwPMDataInstances OBJECT IDENTIFIER ::= { hwPerfMgmt 4 }
        
        hwPMHistoryDataTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMHistoryDataEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is the historical performance data table and is used to provide historical data query function."
            ::= { hwPMDataInstances 1 }
        
        hwPMHistoryDataEntry OBJECT-TYPE
            SYNTAX HwPMHistoryDataEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry of performance statistic history data table."
            INDEX { hwPMStatisticsTaskName, hwPMHistoryDataInstanceType, hwPMHistoryDataInstanceName, hwPMHistoryDataIndicatorID, hwPMHistoryDataIntervalIndex
                 }
            ::= { hwPMHistoryDataTable 1 }
        
        HwPMHistoryDataEntry ::=
            SEQUENCE { 
                hwPMHistoryDataInstanceType
                    Unsigned32,
                hwPMHistoryDataInstanceName
                    OCTET STRING,
                hwPMHistoryDataIndicatorID
                    Unsigned32,
                hwPMHistoryDataIntervalIndex
                    Integer32,
                hwPMHistoryDataHighValue
                    Unsigned32,
                hwPMHistoryDataLowValue
                    Unsigned32,
                hwPMHistoryDataValidFlag
                    INTEGER,
                hwPMHistoryDateAndTime
                    DateAndTime
             }

        hwPMHistoryDataInstanceType OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The instance type of history data."
            ::= { hwPMHistoryDataEntry 1 }
        
        hwPMHistoryDataInstanceName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The instance name of history data."
            ::= { hwPMHistoryDataEntry 2 }
        
        hwPMHistoryDataIndicatorID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The indicator ID of history data."
            ::= { hwPMHistoryDataEntry 3 }
        
        hwPMHistoryDataIntervalIndex OBJECT-TYPE
            SYNTAX Integer32 (1..16)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The interval index of history data."
            ::= { hwPMHistoryDataEntry 4 }
        
        hwPMHistoryDataHighValue OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The high 32 bit of history data value."
            ::= { hwPMHistoryDataEntry 5 }
        
        hwPMHistoryDataLowValue OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The low 32 bit of history data value."
            ::= { hwPMHistoryDataEntry 6 }
        
        hwPMHistoryDataValidFlag OBJECT-TYPE
            SYNTAX INTEGER
                {  
                init(1),
                valid(2),
                incredible(3),
                measureNotConfigured(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The valid flag of history data."
            ::= { hwPMHistoryDataEntry 7 }
        
        hwPMHistoryDateAndTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The date and time of history data."
            ::= { hwPMHistoryDataEntry 8 }
        
        hwPMCurrentDataTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMCurrentDataEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is the current performance data table and is used to provide the query function of the statistical data and the current data reset function."
            ::= { hwPMDataInstances 2 }
        
        hwPMCurrentDataEntry OBJECT-TYPE
            SYNTAX HwPMCurrentDataEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Entry of performance statistic current data table."
            INDEX { hwPMStatisticsTaskName, hwPMCurrentDataInstanceType, hwPMCurrentDataInstanceName, hwPMCurrentDataIndicatorID }
            ::= { hwPMCurrentDataTable 1 }
        
        HwPMCurrentDataEntry ::=
            SEQUENCE { 
                hwPMCurrentDataInstanceType
                    Unsigned32,
                hwPMCurrentDataInstanceName
                    OCTET STRING,
                hwPMCurrentDataIndicatorID
                    Unsigned32,
                hwPMCurrentDataHighValue
                    Unsigned32,
                hwPMCurrentDataLowValue
                    Unsigned32,
                hwPMCurrentDataValidFlag
                    INTEGER,
                hwPMCurrentDateAndTime
                    DateAndTime
             }

        hwPMCurrentDataInstanceType OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The instance type of current data."
            ::= { hwPMCurrentDataEntry 1 }
        
        hwPMCurrentDataInstanceName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The instance name of current data."
            ::= { hwPMCurrentDataEntry 2 }
        
        hwPMCurrentDataIndicatorID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The indicator ID of current data."
            ::= { hwPMCurrentDataEntry 3 }
        
        hwPMCurrentDataHighValue OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The high 32 bit of current data value."
            ::= { hwPMCurrentDataEntry 5 }
        
        hwPMCurrentDataLowValue OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The low 32 bit of current data value."
            ::= { hwPMCurrentDataEntry 6 }
        
        hwPMCurrentDataValidFlag OBJECT-TYPE
            SYNTAX INTEGER
                {
                init(1),
                valid(2),
                incredible(3),
                measureNotConfigured(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The valid flag of current data."
            ::= { hwPMCurrentDataEntry 7 } 
            
        hwPMCurrentDateAndTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The date and time of current data."
            ::= { hwPMCurrentDataEntry 8 }
            
               hwPMResetCurrentDataTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMResetCurrentDataEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Performance statistic current data table." 
            ::= { hwPMDataInstances 3 }
        
        hwPMResetCurrentDataEntry OBJECT-TYPE
            SYNTAX HwPMResetCurrentDataEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Entry of reset performance statistic current data table."
            INDEX { hwPMStatisticsTaskName, hwPMResetCurrentDataInstanceType }
            ::= { hwPMResetCurrentDataTable 1 }
        
        HwPMResetCurrentDataEntry ::=
            SEQUENCE { 
                hwPMResetCurrentDataInstanceType
                    Unsigned32,
                hwPMResetCurrentDataInstanceName
                    OCTET STRING,
                hwPMResetCurrentDataIndicatorID
                    Unsigned32
             }

        hwPMResetCurrentDataInstanceType OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The instance type of current data."
            ::= { hwPMResetCurrentDataEntry 1 }
        
        hwPMResetCurrentDataInstanceName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The instance name of current data."
            ::= { hwPMResetCurrentDataEntry 2 }
        
        hwPMResetCurrentDataIndicatorID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The indicator ID of current data."
            ::= { hwPMResetCurrentDataEntry 3 }
        
        hwPMGlobalInstances OBJECT IDENTIFIER ::= { hwPerfMgmt 5 }
        
        hwPMIntervalTypeTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMIntervalTypeEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is of the period type and is used to provide the performance measurement period attribute query function."
            ::= { hwPMGlobalInstances 1 }
        
        hwPMIntervalTypeEntry OBJECT-TYPE
            SYNTAX HwPMIntervalTypeEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry of hwPMIntervalTypeTable."
            INDEX { hwPMIntervalType }
            ::= { hwPMIntervalTypeTable 1 }
        
        HwPMIntervalTypeEntry ::=
            SEQUENCE { 
                hwPMIntervalType
                    Unsigned32,
                hwPMIntervalTypeName
                    OCTET STRING,
                hwPMIntervalTypeInterval
                    INTEGER,
                hwPMIntervalTypeHistorynum
                    Unsigned32,
                hwPMIntervalTypeDelayRange
                    Unsigned32,
                hwPMIntervalTypeSampleInterval
                    Unsigned32
             }

        hwPMIntervalType OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The interval type ID."
            ::= { hwPMIntervalTypeEntry 1 }
        
        hwPMIntervalTypeName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The interval type name."
            ::= { hwPMIntervalTypeEntry 2 }
        
        hwPMIntervalTypeInterval OBJECT-TYPE
            SYNTAX INTEGER
                {
                five(5),
                ten(10),
                fifteen(15),
                thirty(30),
                sixty(60),
                twentyfourhours(1440)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the length of the performance measurement period, in minutes."
            ::= { hwPMIntervalTypeEntry 3 }
        
        hwPMIntervalTypeHistorynum OBJECT-TYPE
            SYNTAX Unsigned32 (0..16)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The history number of save data per interval type."
            ::= { hwPMIntervalTypeEntry 4 }
        
        hwPMIntervalTypeDelayRange OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The range of delay time per interval type."
            ::= { hwPMIntervalTypeEntry 5 }
        
        hwPMIntervalTypeSampleInterval OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "second"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The default sample interval per interval type."
            ::= { hwPMIntervalTypeEntry 6 }
        
        hwPMInstanceTypeTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMInstanceTypeEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is used to provide the function of querying the performance statistics instance type."
            ::= { hwPMGlobalInstances 2 }
        
        hwPMInstanceTypeEntry OBJECT-TYPE
            SYNTAX HwPMInstanceTypeEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry of hwPMInstanceTypeTable."
            INDEX { hwPMInstanceTypeID }
            ::= { hwPMInstanceTypeTable 1 }
        
        HwPMInstanceTypeEntry ::=
            SEQUENCE { 
                hwPMInstanceTypeID
                    Unsigned32,
                hwPMInstanceTypeName
                    OCTET STRING
             }

        hwPMInstanceTypeID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The instance type ID."
            ::= { hwPMInstanceTypeEntry 1 }
        
        hwPMInstanceTypeName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The instance type name."
            ::= { hwPMInstanceTypeEntry 2 }
        
        hwPMIndicatorTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPMIndicatorEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is used to provide the function of querying performance counters."
            ::= { hwPMGlobalInstances 3 }
        
        hwPMIndicatorEntry OBJECT-TYPE
            SYNTAX HwPMIndicatorEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry of hwPMIndicatorTable."
            INDEX { hwPMIndicatorID }
            ::= { hwPMIndicatorTable 1 }
        
        HwPMIndicatorEntry ::=
            SEQUENCE { 
                hwPMIndicatorID
                    Unsigned32,
                hwPMIndicatorName
                    OCTET STRING,
                hwPMIndicatorType
                    INTEGER,
                hwPMIndicatorCounterType
                    INTEGER
             }

        hwPMIndicatorID OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The indicator ID."
            ::= { hwPMIndicatorEntry 1 }
        
        hwPMIndicatorName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The indicator name."
            ::= { hwPMIndicatorEntry 2 }
        
        hwPMIndicatorType OBJECT-TYPE
            SYNTAX INTEGER
                {
                increase(1),
                measure(2),
                max(3),
                min(4),
                avg(5),
                es(6),
                delta(7)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The indicator type."
            ::= { hwPMIndicatorEntry 3 }
        
        hwPMIndicatorCounterType OBJECT-TYPE
            SYNTAX INTEGER
                {
                counter32(1),
                counter64(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The indicator counter type."
            ::= { hwPMIndicatorEntry 4 }
                        
        hwPMConformance OBJECT IDENTIFIER ::= { hwPerfMgmt 6 }
        
        hwPMCompliances OBJECT IDENTIFIER ::= { hwPMConformance 1 }
        
        hwPMCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION
                "The performance management compliance."
            MODULE -- this module
                MANDATORY-GROUPS { hwPMMIBGroup, hwPMTaskGroup, hwPMTaskInstanceGroup, hwPMTaskThresholdGroup, hwPMFileUploadGroup, hwPMTaskFileGroup, hwPMDataInstanceGroup,
                hwPMIntervalTypeGroup, hwPMInstanceTypeGroup, hwPMIndicatorGroup, hwPMNotificationGroup }
            ::= { hwPMCompliances 1 }
        
        hwPMGroup OBJECT IDENTIFIER ::= { hwPMConformance 2 }
        
        hwPMMIBGroup OBJECT-GROUP
            OBJECTS { hwPMStatisticsEnable, hwPMStatisticsMaxFilesPerTask, hwPMStatisticsMaxTasks, hwPMStatisticsCurrentTasks }
            STATUS current
            DESCRIPTION
                "The performance management group."
            ::= { hwPMGroup 1 }
        
        hwPMTaskGroup OBJECT-GROUP
            OBJECTS { hwPMStatisticsTaskName, hwPMStatisticsTaskFileFormat, hwPMStatisticsRecordFileEnable, hwPMStatisticsThresholdEnable, hwPMStatisticsTaskPeriod, hwPMStatisticsTaskTransferPeriod,  
                hwPMStatisticsTaskRowStatus, hwPMStatisticsTaskSampleInterval, hwPMStatisticsTaskIndicator, hwPMStatisticsTaskIndicatorRowStatus, hwPMStatisticsTaskCurrentFileIndex, hwPMStatisticsUploadAutoName}
            STATUS current
            DESCRIPTION
                "The performance management statistics task group."
            ::= { hwPMGroup 2 }
        
        hwPMTaskInstanceGroup OBJECT-GROUP
            OBJECTS { hwPMStatisticsTaskInstanceType, hwPMStatisticsTaskInstanceName, hwPMStatisticsTaskInstanceRowStatus }
            STATUS current
            DESCRIPTION
                "The performance management statistics task instances group."
            ::= { hwPMGroup 3 }
        hwPMTaskThresholdGroup OBJECT-GROUP
            OBJECTS { hwPMStatisticsTaskThresholdType,hwPMStatisticsTaskThresholdHighTriggerValue,hwPMStatisticsTaskThresholdLowTriggerValue, 
            hwPMStatisticsTaskThresholdHighClearedValue,hwPMStatisticsTaskThresholdLowClearedValue,hwPMStatisticsTaskThresholdRuleRowStatus,hwPMStatisticsTaskIndicateLowValue,
            hwPMStatisticsTaskIndicateHighValue, hwPMStatisticsTaskThresholdRuleRowStatus }
            STATUS current
            DESCRIPTION
                "The performance management statistics task threshold group."
            ::= { hwPMGroup 4 }
            
        hwPMTaskFileGroup OBJECT-GROUP
            OBJECTS { hwPMStatisticsTaskFileIndex, hwPMStatisticsTaskFileName }
            STATUS current
            DESCRIPTION
                "The performance management statistics task file group."
            ::= { hwPMGroup 5 }
        
        hwPMFileUploadGroup OBJECT-GROUP
            OBJECTS { hwPMFileUploadRequestName, hwPMFileUploadServerName, hwPMFileUploadFileList, hwPMFileUploadStatus, hwPMFileUploadCfgRowStatus, 
                hwPMServerName, hwPMServerSrcAddrType,hwPMServerSrcAddr, hwPMServerVpnName, hwPMServerHostAddr,hwPMServerHostAddrType, hwPMServerPort, 
                hwPMServerUserName, hwPMServerPassword, hwPMServerSrcIfName, hwPMServerRetryTimes, 
                hwPMServerTransferProtocol, hwPMServerDestPath, hwPMServerRowStatus, hwPMServerVpnType }
            STATUS current
            DESCRIPTION
                "The performance management statistics file upload group."
            ::= { hwPMGroup 6 }
        
        hwPMDataInstanceGroup OBJECT-GROUP
            OBJECTS {hwPMHistoryDataHighValue, 
                hwPMHistoryDataLowValue, hwPMHistoryDataValidFlag, hwPMHistoryDateAndTime, 
                hwPMCurrentDataHighValue, hwPMCurrentDataLowValue, hwPMCurrentDataValidFlag, hwPMCurrentDateAndTime ,hwPMResetCurrentDataIndicatorID,hwPMResetCurrentDataInstanceName,hwPMResetCurrentDataInstanceType}
            STATUS current
            DESCRIPTION
                "The performance management data group."
            ::= { hwPMGroup 7 }
        
        hwPMIntervalTypeGroup OBJECT-GROUP
            OBJECTS { hwPMIntervalTypeName, hwPMIntervalTypeInterval, hwPMIntervalTypeHistorynum, hwPMIntervalTypeDelayRange, 
                hwPMIntervalTypeSampleInterval }
            STATUS current
            DESCRIPTION
                "The performance management interval type group."
            ::= { hwPMGroup 8 }
        
        hwPMInstanceTypeGroup OBJECT-GROUP
            OBJECTS { hwPMInstanceTypeName }
            STATUS current
            DESCRIPTION
                "The performance management instance type group."
            ::= { hwPMGroup 9 }
        
        hwPMIndicatorGroup OBJECT-GROUP
            OBJECTS { hwPMIndicatorName, hwPMIndicatorType, hwPMIndicatorCounterType}
            STATUS current
            DESCRIPTION
                "The performance management indicator group."
            ::= { hwPMGroup 10 }
            
        hwPMNotificationGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwPMStatisticsTaskThresholdTriggerAlarm, hwPMStatisticsTaskThresholdClearAlarm ,hwPMCSESEvent, hwPMUATEvent}
            STATUS current
            DESCRIPTION 
                "The notification group."
            ::= { hwPMGroup 11 }
    
    END

--
-- HUAWEI-PERFMGMT-MIB.my
--