--==================================================================
-- Copyright (C) 2017 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description: HUAWEI Layer Two VLAN MIB
-- Reference:
-- Version: V2.09
-- History:
-- ==================================================================
-- ==================================================================
-- 
-- Varibles and types be imported
--
-- ==================================================================
HUAWEI-L2VLAN-MIB DEFINITIONS ::= BEGIN
IMPORTS
    
    RowStatus,MacAddress,TEXTUAL-CONVENTION
        FROM SNMPv2-TC

    MODULE-IDENTITY, OBJECT-TYPE, Integer32, OBJECT-IDENTITY, TimeTicks, 
    NOTIFICATION-TYPE, Counter64, IpAddress, Gauge32
        FROM SNMPv2-SMI  
        
    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
        FROM SNMPv2-CONF
                
    hwDatacomm
        FROM HUAWEI-MIB
        
    VlanId, PortList, VlanIndex, VlanIdOrNone
        FROM Q-BRIDGE-MIB
    
    ifIndex,InterfaceIndex
        FROM IF-MIB        
    
    EnabledStatus
        FROM P-BRIDGE-MIB
        
    hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType
        FROM HUAWEI-BASE-TRAP-MIB;    
        
    hwL2Mgmt OBJECT IDENTIFIER ::= { hwDatacomm 42 }
    
    hwL2Vlan MODULE-IDENTITY
            LAST-UPDATED "201708170000Z"                
    ORGANIZATION 
            "Huawei Technologies Co.,Ltd."
    CONTACT-INFO 
            "Huawei Industrial Base
              Bantian, Longgang
               Shenzhen 518129
               People's Republic of China
               Website: http://www.huawei.com
               Email: support@huawei.com
             "
   DESCRIPTION
            "add a mib node hwL2QinQVlanInnerRemark."
   
   REVISION
            "201708170000Z"
   DESCRIPTION
            "Modify the description of the nodes"
   REVISION
            "201706220000Z"
   DESCRIPTION
            "The L2Vlan MIB module is defined to manage several layer two function of Huawei Technologies co.,Ltd."
   REVISION
            "201609180000Z"
   DESCRIPTION
            "Add hwL2VlanMultiVoiceVlanPortTag0Enable."            
   REVISION
            "201409170000Z"
   DESCRIPTION
            "Modify the disable value of the hwL2VlanSmartMacLearn."
   REVISION
            "201408140000Z"
   DESCRIPTION
            "Add traps hwMuxVlanGroupCountExceedThreshold, hwMuxVlanGroupCountExceedThresholdResume, hwVlantransCountExceedThreshold and hwVlantransCountExceedThresholdResume. Add hwPrincipalVlanID, hwMuxVlanUpperThreshold, hwMuxVlanLowerThreshold, hwVlantransIfIndex, hwVlantransUpperThreshold and hwVlantransLowerThreshold for traps."
   REVISION	
             "201312191000Z"
   DESCRIPTION
            "Add hwL2VlanVoiceVlanPortModifyPriorityMode and hwL2VlanMultiVoiceVlanPortUntagEnable"  
   REVISION	
             "201307291000Z"
   DESCRIPTION
            "Add hwVcmpGroup for hwVcmpDeviceMac."
   REVISION	
             "201307021400Z"
   DESCRIPTION
            "Add vcmp traps :hwVcmpServerMacConflict and hwVcmpRevisionConflict."
   REVISION
            "201303250000Z"
   DESCRIPTION
            "add a mib node hwL2QinQIsolateTable."

            ::= { hwL2Mgmt 3 }
    
-- ==================================================================
--
-- ======================= definition begin =========================
--
-- ==================================================================
           
hwL2VlanMngObjects OBJECT IDENTIFIER ::= { hwL2Vlan 1 }
    
-- =============================================================
-- groups in the hwL2Vlan MIB
-- =============================================================
hwL2VlanBase          OBJECT IDENTIFIER ::= { hwL2VlanMngObjects 1 }
hwL2VlanApply         OBJECT IDENTIFIER ::= { hwL2VlanMngObjects 2 }
hwL2VlanStatistics     OBJECT IDENTIFIER ::= { hwL2VlanMngObjects 3 }


    hwL2VlanMIBTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanMIBEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "This table shows the VLAN status information. It describes information about a VLAN, such as the type, interface list, and current status of the VLAN."
        ::= { hwL2VlanBase  1 }


    hwL2VlanMIBEntry OBJECT-TYPE
        SYNTAX HwL2VlanMIBEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Entries of vlan MIB table."
        INDEX   { hwL2VlanIndex }
        ::= { hwL2VlanMIBTable 1}

    HwL2VlanMIBEntry ::=
    SEQUENCE {
        hwL2VlanIndex    VlanId   ,
        hwL2VlanDescr     OCTET STRING ,
        hwL2VlanPortList    PortList   ,
        hwL2VlanType     INTEGER ,
        hwL2VlanUnknownUnicastProcessing   INTEGER  , 
        hwL2VlanIfIndex    Integer32,
        hwL2VlanMacLearn EnabledStatus  ,
        hwL2VlanMulticast EnabledStatus,
        hwL2VlanAdminStatus EnabledStatus, 
        hwL2VlanStatisStatus EnabledStatus, 
        hwL2VlanCreateStatus     INTEGER ,
        hwL2VlanRowStatus    RowStatus ,
        hwL2VlanBcast    EnabledStatus,
        hwL2VlanUnknownMulticastProcessing  INTEGER,
        hwL2VlanProperty    INTEGER,
        hwL2VlanAgingTime   Integer32,
        hwL2VlanName   OCTET STRING,
        hwL2VlanSmartMacLearn EnabledStatus,
        hwL2VlanServiceName   OCTET STRING,
        hwL2VlanManagementVlan EnabledStatus,
        hwL2VlanDynamicVlan EnabledStatus
        }

    hwL2VlanIndex OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The vlan-id or other identifier referring to this vlan."
        ::= { hwL2VlanMIBEntry 1 }


    hwL2VlanDescr  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (0..80))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Description of the vlan."
        ::= { hwL2VlanMIBEntry 2 }


    hwL2VlanPortList OBJECT-TYPE
        SYNTAX  PortList    
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The set of Ports which belong to the vlan."
        ::= { hwL2VlanMIBEntry 3 }

    hwL2VlanType  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        superVlan (1),
        commonVlan (2),  
        subVlan (3),
        muxVlan (4),
        muxSubVlan (5),
        protocolTransVlan (6)
        }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The value of this object identifies the type of a VLAN.Change the value from '2' to '1' indicates that the common-vlan is configured into super-vlan; 
		   Change the value from '1' to '2' indicates that the super-vlan is canceled; Change the value from '2' to '4' indicates that the common-vlan is configured into mux-vlan; 
		   Change the value from '4' to '2' indicates that the mux-vlan is canceled; Change the value from '2' to '6' indicates that the common-vlan is configured into protocol-transparent-vlan; 
		   Change the value from '6' to '2' indicates that the protocol-transparent-vlan is canceled; Note that the switch between other pairs is forbidden."
        ::= { hwL2VlanMIBEntry 4 }


    hwL2VlanUnknownUnicastProcessing OBJECT-TYPE
        SYNTAX  INTEGER
        {
        broadcast (1),
        discard (2)
        }
        MAX-ACCESS read-create  
        STATUS current
        DESCRIPTION 
           "The value of this object identifies whether the unknown unicast packet is broadcasted."
        ::= { hwL2VlanMIBEntry 5 }


    hwL2VlanIfIndex OBJECT-TYPE
        SYNTAX  Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION " Whether vlan interface is configured on vlan. If vlan interface is configured,
                      the value of the node is InterfaceIndex, else the value is -1. "
        ::= { hwL2VlanMIBEntry 6 }


    hwL2VlanMacLearn OBJECT-TYPE   
        SYNTAX  EnabledStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The value of this object identifies whether the VLAN multicast function is enabled.The value enabled(1) indicates vlan Multicasting is allowed; disable(2) indicates it's closed. The default value is disable(2)."
        ::= { hwL2VlanMIBEntry 7 }
 
        
    hwL2VlanMulticast  OBJECT-TYPE
        SYNTAX  EnabledStatus      
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The value enabled(1) indicates vlan Multicasting is allowed; disable(2) indicates it's closed. The default value is disable(2)."
        ::= { hwL2VlanMIBEntry 8 }
             
    hwL2VlanAdminStatus  OBJECT-TYPE
        SYNTAX  EnabledStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The value of this object identifies whether a VLAN is shut down.Value disable(2) indicates shutdown the vlan; enabled(1) indicates open the vlan."
        DEFVAL  {1}
        ::= { hwL2VlanMIBEntry 9 }
        
        
    hwL2VlanStatisStatus  OBJECT-TYPE
        SYNTAX  EnabledStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The value of this object identifies whether the VLAN statistics function is enabled.The value enabled(1) indicates Statistics onvlan are allowed; disable(2) indicates aren't. The default value is disable(2)."
        DEFVAL  {2}
        ::= { hwL2VlanMIBEntry 10 }
        
    hwL2VlanCreateStatus  OBJECT-TYPE
        SYNTAX  INTEGER
                     {
        other (1),
        static (2),  
        dynamic (3)
        }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The status indicates how the vlan is created,
           static configured by management or created dynamicly by GVRP."
        ::= { hwL2VlanMIBEntry 11 }
        
    hwL2VlanRowStatus  OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The value of this object identifies the row status recorded by the VLAN."
        ::= { hwL2VlanMIBEntry 12 } 
        
    hwL2VlanBcast OBJECT-TYPE
        SYNTAX  EnabledStatus
        MAX-ACCESS read-create  
        STATUS current
        DESCRIPTION 
           "Whether to broadcast the broadcast packets when ports receive it.
           enabled(1) indicates broadcast the packets,disable(2) indicates it'll discard 
           the broadcast packet. Default value is enabled(1)."
        ::= { hwL2VlanMIBEntry 13 }  
        
    hwL2VlanUnknownMulticastProcessing OBJECT-TYPE
        SYNTAX  INTEGER
        {
        broadcast (1),
        discard (2)
        }
        MAX-ACCESS read-create  
        STATUS current
        DESCRIPTION 
           "Whether to broadcast the unknown multicast packets when ports receive it.
           broadcast(1) indicates broadcast the packet, discard(2) indicates it'll discard 
           the unknow multicast packet. Default value is broadcast(1)."
        ::= { hwL2VlanMIBEntry 14 }   
        
    hwL2VlanProperty OBJECT-TYPE
        SYNTAX  INTEGER
        {
            default(1),
            backboneVlan(2),
            mutilcastVlan(3),
            userVlan(4)
        }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The value of this object identifies the type of a VLAN."
        ::= { hwL2VlanMIBEntry 15 }    
        
    hwL2VlanAgingTime OBJECT-TYPE
        SYNTAX  Integer32(60..1000000 | 0 | -1)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The aging time of MAC entry that associated with the vlan.'0' means  
                     will be never aged,'-1' means aging-time is not configured to the vlan."
        ::= { hwL2VlanMIBEntry 16 }   

    
    hwL2VlanName OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (0..31))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Name of the vlan."
        ::= { hwL2VlanMIBEntry 17 }   
    
    hwL2VlanSmartMacLearn OBJECT-TYPE   
        SYNTAX  EnabledStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The value indicates whether the MAC address learning is opened, when the number of the port which is up state and belonging to the vlan is below and equal to two. The value enabled(1) indicates learning is not allowed, when the number of the port which is up state and belonging to the vlan is below and equal to two.
           Just the common vlan and Sub-vlan have the attribute. Default value is disable(2)."
        ::= { hwL2VlanMIBEntry 18 }

    hwL2VlanServiceName  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (0..100))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Service name of the vlan."
        ::= { hwL2VlanMIBEntry 19 }

    hwL2VlanManagementVlan  OBJECT-TYPE
        SYNTAX  EnabledStatus
        MAX-ACCESS read-create 
        STATUS current
        DESCRIPTION 
           "This object indicates whether the VLAN is a management VLAN:
            enable: 1 
            disable: 2
          "
        ::= { hwL2VlanMIBEntry 20 } 

    hwL2VlanDynamicVlan  OBJECT-TYPE
        SYNTAX  EnabledStatus
        MAX-ACCESS read-only  
        STATUS current
        DESCRIPTION 
           "This object indicates whether the VLAN is a dynamic VLAN:
            enable: 1 
            disable: 2
           "
        ::= { hwL2VlanMIBEntry 21 } 



    hwL2VlanStackingTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanStackingEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "This is the table to configure the double tags for the incoming packets of the VLAN stacking interface. It describes the function to encapsulate the incoming packets of a VLAN stacking interface with the double tags."
        ::= { hwL2VlanApply  1 }

    hwL2VlanStackingEntry  OBJECT-TYPE
        SYNTAX HwL2VlanStackingEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "QinQ-port configuration table."
        INDEX   { hwL2VlanStackingPortIndex, hwL2VlanStackingInsideVlanId }
        ::= { hwL2VlanStackingTable 1}

    HwL2VlanStackingEntry  ::=
    SEQUENCE {
        hwL2VlanStackingPortIndex            Integer32,
        hwL2VlanStackingInsideVlanId         VlanId,
        hwL2VlanStackingOutsideVlanListLow    OCTET STRING,
        hwL2VlanStackingOutsideVlanListHigh    OCTET STRING,
        hwL2VlanStackingRowStatus   RowStatus
        }


    hwL2VlanStackingPortIndex  OBJECT-TYPE
        SYNTAX  Integer32(1..65535) 
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Index number of QinQ-port."
        ::= { hwL2VlanStackingEntry 1 }
    
    
    hwL2VlanStackingInsideVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Inside vlan-id of QinQ-port, use it as the Index."
        ::= { hwL2VlanStackingEntry 2 }


    hwL2VlanStackingOutsideVlanListLow  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "This object indicates the low 2048 bits of the VLAN list, specifying the outer VLAN tag of incoming packets on the QinQ interface. Each bit corresponds to a VLAN ID."
        ::= { hwL2VlanStackingEntry 3 }
    
    hwL2VlanStackingOutsideVlanListHigh  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "This object indicates the high 2048 bits of the VLAN list, specifying the outer VLAN tag of incoming packets on the QinQ interface. Each bit corresponds to a VLAN ID."
        ::= { hwL2VlanStackingEntry 4 }

    hwL2VlanStackingRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION   
           "The value of this object identifies the row status of the double VLAN tag configuration table of the VLAN stacking interface."
        ::= { hwL2VlanStackingEntry 5 }
        
        
    hwL2VlanMappingTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanMappingEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "This is the table to configure the VLAN swapping on the VLAN mapping interface. It describes the mapping relationship in the VLAN substitution on the VLAN mapping interface."
        ::= { hwL2VlanApply  2 }


    hwL2VlanMappingEntry  OBJECT-TYPE
        SYNTAX HwL2VlanMappingEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "QinQ-port configuration table."
        INDEX   { hwL2VlanMappingPortIndex, hwL2VlanMappingInsideVlanId }
        ::= { hwL2VlanMappingTable 1}

    HwL2VlanMappingEntry  ::=
    SEQUENCE {
        hwL2VlanMappingPortIndex            Integer32,
        hwL2VlanMappingInsideVlanId         VlanId,
        hwL2VlanMappingOutsideVlanListLow    OCTET STRING,
        hwL2VlanMappingOutsideVlanListHigh    OCTET STRING,
        hwL2VlanMappingRowStatus   RowStatus
        }


    hwL2VlanMappingPortIndex  OBJECT-TYPE
        SYNTAX  Integer32(1..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "This object indicates the index of an interface where VLAN mapping is configured."
        ::= { hwL2VlanMappingEntry 1 }
    
    
    hwL2VlanMappingInsideVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The value of this object identifies the VLAN ID. This object describes the VLAN ID after the replacement."
        ::= { hwL2VlanMappingEntry 2 }


    hwL2VlanMappingOutsideVlanListLow  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "This object indicates the low 2048 bits of the VLAN list. This object specifies the VLAN list to be replaced. Each bit corresponds to a VLAN."
        ::= { hwL2VlanMappingEntry 3 }
    
    hwL2VlanMappingOutsideVlanListHigh  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "This object indicates the high 2048 bits of the VLAN list. This object specifies the VLAN list to be replaced. Each bit corresponds to a VLAN."
        ::= { hwL2VlanMappingEntry 4 }

    hwL2VlanMappingRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The value of this object identifies the row status of the modify replacement table of the VLAN mapping interface."
        ::= { hwL2VlanMappingEntry 5 }      
          
          
    hwSuperVlanTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwSuperVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The table contains configuration and control information for the super vlan."
        ::= { hwL2VlanApply 3 }
        
    hwSuperVlanEntry OBJECT-TYPE
        SYNTAX HwSuperVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Entries of the super vlan table."
        INDEX { hwSuperVlanId }
        ::= { hwSuperVlanTable 1 }
        
    HwSuperVlanEntry ::=
    SEQUENCE { 
        hwSuperVlanId    VlanId,
        hwSubVlanListLow OCTET STRING,
        hwSubVlanListHigh OCTET STRING        
             }

    hwSuperVlanId OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS not-accessible
        STATUS current
    DESCRIPTION 
       "The super vlan-id."
        ::= { hwSuperVlanEntry 1 }
    
    hwSubVlanListLow OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (256))
        MAX-ACCESS read-write
        STATUS current
    DESCRIPTION    
       "The lowest possible value of the sub vlan list on the supervlan."
        ::= { hwSuperVlanEntry 2 }
    
    hwSubVlanListHigh OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (256))
        MAX-ACCESS read-write
        STATUS current
    DESCRIPTION    
       "The highest possible value of the sub vlan list on the supervlan."
        ::= { hwSuperVlanEntry 3 }    
            
    
    hwL2InterfIsolateTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2InterfIsolateEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table contains configuration and control information for interfaces isolate."
        ::= { hwL2VlanApply  4 }

    hwL2InterfIsolateEntry OBJECT-TYPE
        SYNTAX HwL2InterfIsolateEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Secondary vlan lists of Isolate-vlans."
        INDEX   { hwL2InterfIsolateVlanId }
        ::= { hwL2InterfIsolateTable 1}
        
    HwL2InterfIsolateEntry    ::=
        SEQUENCE 
        {
        hwL2InterfIsolateVlanId  VlanId   ,
        hwL2InterfIsolateInterflistLow   OCTET STRING,
        hwL2InterfIsolateInterflistHigh  OCTET STRING
        }
        
    hwL2InterfIsolateVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "vlan-id. The vlan into which interf-isolate is configured."
        ::= { hwL2InterfIsolateEntry 1 }

    hwL2InterfIsolateInterflistLow  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (65))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION 
           "The lowest possible value of Interface list on the vlan."
        ::= { hwL2InterfIsolateEntry 2 }

    hwL2InterfIsolateInterflistHigh  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (65))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION 
           "The highest possible value of Interface list on the vlan."
        ::= { hwL2InterfIsolateEntry 3 }
        
    hwL2IsolatemappingTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2IsolatemappingEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table contains mapping information between isolated ports."
        ::= { hwL2VlanApply  5 }

    hwL2IsolatemappingEntry OBJECT-TYPE
        SYNTAX HwL2IsolatemappingEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           " "
        INDEX   { hwL2IsolatemappingPortNum }
        ::= { hwL2IsolatemappingTable 1}
        
    HwL2IsolatemappingEntry    ::=
        SEQUENCE 
        {
        hwL2IsolatemappingPortNum    Integer32,
        hwL2IsolateInterflistLow   OCTET STRING,
        hwL2IsolateInterflistHigh  OCTET STRING
        }
        
    hwL2IsolatemappingPortNum  OBJECT-TYPE
        SYNTAX  Integer32(0..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Port number."
        ::= { hwL2IsolatemappingEntry 1 }

    hwL2IsolateInterflistLow  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (256))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION 
           "The lowest possible value of Interface list."
        ::= { hwL2IsolatemappingEntry 2 }

    hwL2IsolateInterflistHigh  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (256))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION 
           "The highest possible value of Interface."
        ::= { hwL2IsolatemappingEntry 3 }
  
    hwL2VlanStackingExtTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanStackingExtEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           " "
        ::= { hwL2VlanApply  6 }

    hwL2VlanStackingExtEntry  OBJECT-TYPE
        SYNTAX HwL2VlanStackingExtEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           " "
        INDEX   { hwL2VlanStackingExtPortIndex, hwL2VlanStackingExtVlanId,hwL2VlanStackingExtAction, hwL2VlanStackingExtDirection}
        ::= { hwL2VlanStackingExtTable 1}

    HwL2VlanStackingExtEntry  ::=
    SEQUENCE {
        hwL2VlanStackingExtPortIndex             InterfaceIndex,
        hwL2VlanStackingExtVlanId                VlanIdOrNone,
        hwL2VlanStackingExtAction                INTEGER,
        hwL2VlanStackingExtDirection             INTEGER,
        hwL2VlanStackingExtVlanListLow           OCTET STRING,
        hwL2VlanStackingExtVlanListHigh          OCTET STRING,
        hwL2VlanStackingExtRowStatus             RowStatus,
        hwL2VlanStackingExtPriorityMode          INTEGER,
        hwL2VlanStackingExtVlan8021p             Integer32
        }


    hwL2VlanStackingExtPortIndex  OBJECT-TYPE
        SYNTAX  InterfaceIndex 
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Configured QinQ-Port Index."
        ::= { hwL2VlanStackingExtEntry 1 }
    
    
    hwL2VlanStackingExtVlanId  OBJECT-TYPE
        SYNTAX  VlanIdOrNone
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "This vlan-id need be poped or pushed in interface."
        ::= { hwL2VlanStackingExtEntry 2 }
        
     
    hwL2VlanStackingExtAction    OBJECT-TYPE         
        SYNTAX  INTEGER
        {
        pop   (1),
        push  (2)
        }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The packet will be poped or pushed."
        ::= { hwL2VlanStackingExtEntry 3}
        
    hwL2VlanStackingExtDirection    OBJECT-TYPE         
        SYNTAX  INTEGER
        {
        inside   (1),
        outside  (2)
        }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The direction which the packet need be poped or pushed.
           That is, the packet is receviced or transitted."
        ::= { hwL2VlanStackingExtEntry 4}
        
   hwL2VlanStackingExtVlanListLow  OBJECT-TYPE
    SYNTAX OCTET STRING (SIZE (256))
    MAX-ACCESS read-create
    STATUS current
        DESCRIPTION 
           "If hwL2VlanStackingBothAction is pop, the packet
           which has hwL2VlanStackingBothPopOrPushVlanId will  
           be taken tag away. If hwL2VlanStackingBothAction is push, the packet
           will be added tag which is hwL2VlanStackingBothPopOrPushVlanId."
        ::= { hwL2VlanStackingExtEntry 5 }
        
   hwL2VlanStackingExtVlanListHigh  OBJECT-TYPE
    SYNTAX OCTET STRING (SIZE (256))
    MAX-ACCESS read-create
    STATUS current
        DESCRIPTION 
           "If hwL2VlanStackingBothAction is pop, the packet
           which has hwL2VlanStackingBothPopOrPushVlanId will  
           be taken tag away. If hwL2VlanStackingBothAction is push, the packet
           will be added tag which is hwL2VlanStackingBothPopOrPushVlanId."
        ::= { hwL2VlanStackingExtEntry 6 }         
      

    hwL2VlanStackingExtRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "This table can be created."
        ::= { hwL2VlanStackingExtEntry 7 }
        
    hwL2VlanStackingExtPriorityMode OBJECT-TYPE
        SYNTAX  INTEGER
        {
        priorityInherit  (1),
        remark8021p   (2)
        }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The priority mode of outer VLAN, the priority can be appointed or 
           inherit from inner VLAN's priority."
        DEFVAL  {priorityInherit}
        ::= { hwL2VlanStackingExtEntry 8 }
        
    hwL2VlanStackingExtVlan8021p OBJECT-TYPE
        SYNTAX Integer32(0..7)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The 8021p of outer VLAN ID after pushing, it's an optional field,
           its default value is 0."
        DEFVAL  {0}
        ::= { hwL2VlanStackingExtEntry 9 }
      
        
     hwL2VlanQinQTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanQinQEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table contains global view configuration information for Flexible QinQ."
        ::= { hwL2VlanApply  7 }
        
    hwL2VlanQinQEntry  OBJECT-TYPE
        SYNTAX HwL2VlanQinQEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Flexible QinQ configuration Entry."
        INDEX   { hwL2VlanQinQIndex,hwL2VlanQinQDirection }
        ::= { hwL2VlanQinQTable 1}
        
    HwL2VlanQinQEntry  ::=
    SEQUENCE {
        hwL2VlanQinQIndex            Integer32 ,
        hwL2VlanQinQDirection        INTEGER ,
        hwL2VlanQinQOutSideVlanId    VlanId ,
        hwL2VlanSysQinQRowStatus     RowStatus
        }
        
    hwL2VlanQinQIndex  OBJECT-TYPE
        SYNTAX  Integer32(0..31) 
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Index number of Flexible QinQ."
        ::= { hwL2VlanQinQEntry 1 }
        
    hwL2VlanQinQDirection  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        inbound   (1),
        outbound  (2)
        }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Inbound or outbound direction for VPN instance."
        ::= { hwL2VlanQinQEntry 2 }
      
    hwL2VlanQinQOutSideVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Outside vlan-id for ISP."
        ::= { hwL2VlanQinQEntry 3 }
        
    hwL2VlanSysQinQRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The table contains interface view configuration information for Flexible QinQ."
        ::= { hwL2VlanQinQEntry 4 }
        
     hwL2VlanInterfaceQinQTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanInterfaceQinQEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Interface view Flexible QinQ configuration table."
        ::= { hwL2VlanApply  8 }
        
    hwL2VlanInterfaceQinQEntry  OBJECT-TYPE
        SYNTAX HwL2VlanInterfaceQinQEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Interface view Flexible QinQ configuration entry."
        INDEX   { hwL2VlanQinQInterfaceIndex,hwL2VlanQinQIndex,hwL2VlanQinQCVlanId,hwL2VlanQinQDirection }
        ::= { hwL2VlanInterfaceQinQTable 1}
        
    HwL2VlanInterfaceQinQEntry  ::=
    SEQUENCE {
        hwL2VlanQinQInterfaceIndex     InterfaceIndex ,
        hwL2VlanQinQCVlanId            VlanId ,
        hwL2VlanQinQSVlanId            VlanId ,
        hwL2VlanQinQAction             INTEGER ,
        hwL2VlanQinQNewCVlanId         VlanId ,
        hwL2VlanInterfaceQinQRowStatus        RowStatus
        }
        
    hwL2VlanQinQInterfaceIndex  OBJECT-TYPE
        SYNTAX  InterfaceIndex 
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Interface index."
        ::= { hwL2VlanInterfaceQinQEntry 1 }
        
    hwL2VlanQinQCVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Client vlan-id."
        ::= { hwL2VlanInterfaceQinQEntry 2 } 
        
    hwL2VlanQinQSVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Internet service provide vlan-id"
        ::= { hwL2VlanInterfaceQinQEntry 3 }
        
    hwL2VlanQinQAction  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        push   (1),
        nop    (2)
        }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Action push or nop."
        ::= { hwL2VlanInterfaceQinQEntry 4 }
        
    hwL2VlanQinQNewCVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Replaced of new client vlan-id."
        ::= { hwL2VlanInterfaceQinQEntry 5 }
        
    hwL2VlanInterfaceQinQRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "This table can be created."
        ::= { hwL2VlanInterfaceQinQEntry 6 }
        

    hwL2DVlanMappingTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2DVlanMappingEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table contains double Vlan-Mapping."
        ::= { hwL2VlanApply  9 }

    hwL2DVlanMappingEntry  OBJECT-TYPE
        SYNTAX HwL2DVlanMappingEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table contains double Vlan-Mapping entry."
        INDEX   {hwL2DVlanMappingInterfaceIndex,hwL2DVlanMappingExternalVlanId, hwL2DVlanMappingInternalVlanId,hwL2DVlanMappingDirection}
        ::= { hwL2DVlanMappingTable 1}

    HwL2DVlanMappingEntry  ::=
    SEQUENCE {
        hwL2DVlanMappingInterfaceIndex      InterfaceIndex ,
        hwL2DVlanMappingExternalVlanId      VlanId ,
        hwL2DVlanMappingInternalVlanId      VlanId ,
        hwL2DVlanMappingDirection           INTEGER ,
        hwL2DVlanMappingMapExternalVlanId   VlanId ,
        hwL2DVlanMappingMapInternalVlanId   VlanId,
        hwL2DVlanMappingAction              INTEGER ,
        hwL2DVlanMappingRowStatus           RowStatus
        }

    hwL2DVlanMappingInterfaceIndex  OBJECT-TYPE
        SYNTAX  InterfaceIndex 
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Interface Index."
        ::= { hwL2DVlanMappingEntry 1 }
        
    hwL2DVlanMappingExternalVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Service vlan-id."
        ::= { hwL2DVlanMappingEntry 2 } 
 
    hwL2DVlanMappingInternalVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Client vlan-id."
        ::= { hwL2DVlanMappingEntry 3 }

        
    hwL2DVlanMappingDirection  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        inbound (1),
        outbound (2)
        }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Direction inbound and outbound."
        ::= { hwL2DVlanMappingEntry 4 }  

    hwL2DVlanMappingMapExternalVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Replaced of new service vlan-id."
        ::= { hwL2DVlanMappingEntry 5 }
        
    hwL2DVlanMappingMapInternalVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Replaced of new client vlan-id."
        ::= { hwL2DVlanMappingEntry 6 }
    
    hwL2DVlanMappingAction  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        swap   (1),
        popExternalVlan (2),
        drop   (3)
        }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Action drop, pop-externalvlan and swap."
        ::= { hwL2DVlanMappingEntry 7 }
        
    hwL2DVlanMappingRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Operation status."
        ::= { hwL2DVlanMappingEntry 8 }
        
        
    hwL2VlanMappingExtTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanMappingExtEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Configuration table."
        ::= { hwL2VlanApply  10 }


    hwL2VlanMappingExtEntry  OBJECT-TYPE
        SYNTAX HwL2VlanMappingExtEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table contains Vlan-Mapping entry."
        INDEX   { hwL2VlanMappingExtPortIndex,hwL2VlanMappingExtDirection, hwL2VlanMappingExtVlanId }
        ::= { hwL2VlanMappingExtTable 1}

    HwL2VlanMappingExtEntry  ::=
    SEQUENCE {
        hwL2VlanMappingExtPortIndex        Integer32,        
        hwL2VlanMappingExtDirection        INTEGER, 
        hwL2VlanMappingExtVlanId           VlanId,
        hwL2VlanMappingExtVlanListLow      OCTET STRING,
        hwL2VlanMappingExtVlanListHigh     OCTET STRING,
        hwL2VlanMappingExtRowStatus        RowStatus,
        hwL2VlanMappingExtPriorityMode     INTEGER,
        hwL2VlanMappingExtVlan8021p        Integer32
        }


    hwL2VlanMappingExtPortIndex  OBJECT-TYPE
        SYNTAX  Integer32(1..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Port Index."
        ::= { hwL2VlanMappingExtEntry 1 }
    
    hwL2VlanMappingExtDirection  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        inbound   (1),
        outbound  (2)
        }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Direction inbound and outbound."
        ::= { hwL2VlanMappingExtEntry 2 }

    
    hwL2VlanMappingExtVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The outside vlan-id."
        ::= { hwL2VlanMappingExtEntry 3 }


    hwL2VlanMappingExtVlanListLow  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The possible value of the inside vlan list."
        ::= { hwL2VlanMappingExtEntry 4 }
    
    hwL2VlanMappingExtVlanListHigh  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The possible value of the inside vlan list."
        ::= { hwL2VlanMappingExtEntry 5 }

    hwL2VlanMappingExtRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "This table can be created."
        ::= { hwL2VlanMappingExtEntry 6 } 
        
    hwL2VlanMappingExtPriorityMode OBJECT-TYPE
        SYNTAX  INTEGER
        {
        priorityInherit  (1),
        remark8021p   (2)
        }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The priority mode of outside VLAN after mapping, the priority 
           can be appointed or inherit from inner VLAN's priority."
        DEFVAL  {priorityInherit  }
        ::= { hwL2VlanMappingExtEntry 7 }
        
    hwL2VlanMappingExtVlan8021p OBJECT-TYPE
        SYNTAX Integer32(0..7)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The priority of outside VLAN after mapping, its default value is 0."
        DEFVAL  {0}
        ::= { hwL2VlanMappingExtEntry 8 }
      
       
    hwL2VlanStackingAdvTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanStackingAdvEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The table of advanced vlan stacking."
        ::= { hwL2VlanApply 11 }
    
    hwL2VlanStackingAdvEntry OBJECT-TYPE
        SYNTAX HwL2VlanStackingAdvEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The entry of advanced vlan stacking table."
        INDEX {hwL2VlanStackingAdvPortIndex,hwL2VlanStackingAdvOutside8021p,
        hwL2VlanStackingAdvStackVlanId,hwL2VlanStackingAdvStack8021p,hwL2VlanStackingAdvMapVlanId}
        ::= { hwL2VlanStackingAdvTable 1 }
    
    HwL2VlanStackingAdvEntry ::=
        SEQUENCE { 
                     hwL2VlanStackingAdvPortIndex 
                         Integer32, 
                     hwL2VlanStackingAdvOutside8021p    
                         Integer32,                     
                     hwL2VlanStackingAdvStackVlanId    
                         VlanId, 
                     hwL2VlanStackingAdvStack8021p 
                         Integer32,
                     hwL2VlanStackingAdvMapVlanId 
                         VlanIdOrNone,
                     hwL2VlanStackingAdvOutsideVlanListLow 
                         OCTET STRING,
                     hwL2VlanStackingAdvOutsideVlanListHigh 
                         OCTET STRING,
                     hwL2VlanStackingAdvRowStatus 
                         RowStatus
                  }
    hwL2VlanStackingAdvPortIndex OBJECT-TYPE
        SYNTAX Integer32 (1..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The Index of L2-Switch Interface."
        ::= { hwL2VlanStackingAdvEntry 1 }
                
    hwL2VlanStackingAdvOutside8021p OBJECT-TYPE
        SYNTAX Integer32(0..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The 8021p value of vlan before stacked operation."
        ::= { hwL2VlanStackingAdvEntry 2 }    
        
    hwL2VlanStackingAdvStackVlanId OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The outer vlan-id after stacked operation."
        ::= { hwL2VlanStackingAdvEntry 3 } 
         
    hwL2VlanStackingAdvStack8021p OBJECT-TYPE
        SYNTAX Integer32(0..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The 8021p of outer vlan-id after stacked, it's an optional 
           field, if it is not selected, its value is 8."
        ::= { hwL2VlanStackingAdvEntry 4 }
        
    hwL2VlanStackingAdvMapVlanId OBJECT-TYPE
        SYNTAX VlanIdOrNone
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The possible value of the inner vlan after mapped operation."
        ::= { hwL2VlanStackingAdvEntry 5 } 

    hwL2VlanStackingAdvOutsideVlanListLow OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The possible value of the CE-Vlan low list."
        ::= { hwL2VlanStackingAdvEntry 6 }

    hwL2VlanStackingAdvOutsideVlanListHigh OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The possible value of the CE-Vlan high list."
        ::= { hwL2VlanStackingAdvEntry 7 }  
        
    hwL2VlanStackingAdvRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "This table can be created."
        ::= { hwL2VlanStackingAdvEntry 8 }

    hwL2VlanMappingAdvTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanMappingAdvEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The table of advanced vlan mapping."
        ::= { hwL2VlanApply 12 }

    hwL2VlanMappingAdvEntry OBJECT-TYPE
        SYNTAX HwL2VlanMappingAdvEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The entry of advanced vlan mapping table."
        INDEX {hwL2VlanMappingAdvPortIndex,hwL2VlanMappingAdvOutsideVlan8021p,
        hwL2VlanMappingAdvMapVlanId,hwL2VlanMappingAdvMapVlan8021p}
        ::= { hwL2VlanMappingAdvTable 1 }
    
    HwL2VlanMappingAdvEntry ::=
        SEQUENCE { 
                hwL2VlanMappingAdvPortIndex 
                    Integer32,  
                hwL2VlanMappingAdvOutsideVlan8021p 
                    Integer32,
                hwL2VlanMappingAdvMapVlanId 
                    VlanId,    
                hwL2VlanMappingAdvMapVlan8021p 
                    Integer32,
                hwL2VlanMappingAdvOutsideVlanListLow 
                    OCTET STRING,
                hwL2VlanMappingAdvOutsideVlanListHigh 
                    OCTET STRING,                            
                hwL2VlanMappingAdvRowStatus 
                    RowStatus
                 }
                 
    hwL2VlanMappingAdvPortIndex OBJECT-TYPE
        SYNTAX Integer32 (1..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            " The index of L2-Switch port. "
        ::= { hwL2VlanMappingAdvEntry 1 } 
        
    hwL2VlanMappingAdvOutsideVlan8021p OBJECT-TYPE
        SYNTAX Integer32(0..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            " The possible value  of the CE-Vlan's 802.1p."
        ::= { hwL2VlanMappingAdvEntry 2 }
            
    hwL2VlanMappingAdvMapVlanId OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The mapped vlan-id, using it as the index."
        ::= { hwL2VlanMappingAdvEntry 3 } 
    
    hwL2VlanMappingAdvMapVlan8021p OBJECT-TYPE
        SYNTAX Integer32(0..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The 8021p of outer vlan-id after mapped, it's an optional 
           field, if it is not selected, its value is 8."
        ::= { hwL2VlanMappingAdvEntry 4 }    
    
    hwL2VlanMappingAdvOutsideVlanListLow OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            " The possible value of the CE-Vlan low list "
        ::= { hwL2VlanMappingAdvEntry 5 }
    
    hwL2VlanMappingAdvOutsideVlanListHigh OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            " The possible value of the CE-Vlan high list."
        ::= { hwL2VlanMappingAdvEntry 6 }    
    
    hwL2VlanMappingAdvRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            " This table can be created."
        ::= { hwL2VlanMappingAdvEntry 7 }    
        
    
    hwL2VlanSwitchTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanSwitchEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table to config the vlan switch."
        ::= { hwL2VlanApply 13 }

        
    hwL2VlanSwitchEntry OBJECT-TYPE
    SYNTAX HwL2VlanSwitchEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION 
       "The entry of the vlan switch table."
    INDEX { hwL2VlanSwitchIfIndex, hwL2VlanSwitchOuterVlanId, hwL2VlanSwitchInnerVlanId }
    ::= { hwL2VlanSwitchTable 1 }

    HwL2VlanSwitchEntry ::=
    SEQUENCE { 
        hwL2VlanSwitchIfIndex
            InterfaceIndex,
        hwL2VlanSwitchOuterVlanId
            VlanIdOrNone,
        hwL2VlanSwitchInnerVlanId
            VlanIdOrNone,
        hwL2VlanSwitchMode
            INTEGER,
        hwL2VlanSwitchOuterSwitchVlanId
            VlanIdOrNone,
        hwL2VlanSwitchInnerSwitchVlanId
            VlanIdOrNone,
        hwL2VlanSwitch8021pRemark
            Integer32,
        hwL2VlanSwitchOutIfIndex
            InterfaceIndex,
        hwL2VlanSwitchMtu
            Integer32,
        hwL2VlanSwitchMtuDiscardPkts
            Counter64,
        hwL2VlanSwitchMtuDiscardBytes
            Counter64,                  
        hwL2VlanSwitchMtuResetFlag
            EnabledStatus,
        hwL2VlanSwitchMtuEnableFlag 
            EnabledStatus,                         
        hwL2VlanSwitchRowStatus
            RowStatus
     }

    hwL2VlanSwitchIfIndex OBJECT-TYPE
        SYNTAX InterfaceIndex
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The interface index."
        ::= { hwL2VlanSwitchEntry 1 }

    hwL2VlanSwitchOuterVlanId OBJECT-TYPE
        SYNTAX VlanIdOrNone
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The ID of the outer vlan tag(customer's tag)."
        ::= { hwL2VlanSwitchEntry 2 }

    hwL2VlanSwitchInnerVlanId OBJECT-TYPE
        SYNTAX VlanIdOrNone
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The ID of the inner vlan tag."
        ::= { hwL2VlanSwitchEntry 3 }    

    hwL2VlanSwitchMode OBJECT-TYPE
        SYNTAX INTEGER
            {
                zeroToOne(1),
                zeroToTwo(2),
                oneToZero(3),
                oneToOne(4),
                oneToTwo(5),
                twoToZero(6),
                twoToOne(7),
                twoToTwo(8)
            }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The Mode of switch vlan operation, including the following case: 
           0 to 1, 0 to 2, 1 to 0, 1 to 1, 1 to 2, 2 to 0, 2 to 1, 2 to 2."
        ::= { hwL2VlanSwitchEntry 4 }

    hwL2VlanSwitchOuterSwitchVlanId OBJECT-TYPE
        SYNTAX VlanIdOrNone
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The outer vlan-id after switched."
        ::= { hwL2VlanSwitchEntry 5 }

    hwL2VlanSwitchInnerSwitchVlanId OBJECT-TYPE
        SYNTAX VlanIdOrNone
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The inner vlan-id after switched. 0 indicates it's not used."
        ::= { hwL2VlanSwitchEntry 6 }

    hwL2VlanSwitch8021pRemark OBJECT-TYPE
        SYNTAX Integer32(0..8)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The 8021p of outer vlan-id after switched, it's an optional 
           field, if it is not selected, its value is 8."
        ::= { hwL2VlanSwitchEntry 7 }

    hwL2VlanSwitchOutIfIndex OBJECT-TYPE
        SYNTAX InterfaceIndex
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The out interface index."
        ::= { hwL2VlanSwitchEntry 8 }

    hwL2VlanSwitchMtu OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The value of mtu."
        ::= { hwL2VlanSwitchEntry 9 }

    hwL2VlanSwitchMtuDiscardPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The number of discard packets."
        ::= { hwL2VlanSwitchEntry 10 }

    hwL2VlanSwitchMtuDiscardBytes OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The number of discard bytes."
        ::= { hwL2VlanSwitchEntry 11 }

    hwL2VlanSwitchMtuResetFlag  OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION 
           "The flag of reset the discard statistics."
        ::= { hwL2VlanSwitchEntry 12 }

    hwL2VlanSwitchMtuEnableFlag  OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION 
           "The flag of enable the discard statistics."
        ::= { hwL2VlanSwitchEntry 13 }


    hwL2VlanSwitchRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Used for controlling the creation and deletion of this
           row. All writable objects in this row may be modified at any time.
           If a Network Management Application attempts to delete a conceptual
           row by setting this object to 'destroy' and there are one or more entries
           in hwL2VlanSwitchTable pointing to the row, the agent MUST also
           destroy the corresponding entries in hwL2VlanSwitchTable."
        ::= { hwL2VlanSwitchEntry 14 }

    hwL2VlanQinqVlanTransEnaTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanQinqVlanTransEnaEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The table of QinQ VLAN translation enable."
        ::= { hwL2VlanApply 14 }

    hwL2VlanQinqVlanTransEnaEntry OBJECT-TYPE
        SYNTAX HwL2VlanQinqVlanTransEnaEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The entry of QinQ VLAN translation enable."
        INDEX {hwL2VlanQinqVlanTransEnaPortIndex}
        ::= { hwL2VlanQinqVlanTransEnaTable 1 }
    
    HwL2VlanQinqVlanTransEnaEntry ::=
        SEQUENCE { 
                hwL2VlanQinqVlanTransEnaPortIndex
                    Integer32,  
                hwL2VlanQinqVlanTransEna 
                    EnabledStatus,
                hwL2VlanQinqVlanTransEnaRowStatus
                    RowStatus
                 }
                 
    hwL2VlanQinqVlanTransEnaPortIndex OBJECT-TYPE
        SYNTAX Integer32 (1..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            " The index of L2-Switch port. "
        ::= { hwL2VlanQinqVlanTransEnaEntry 1 } 
        
    hwL2VlanQinqVlanTransEna OBJECT-TYPE
        SYNTAX  EnabledStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Enable QinQ VLAN translation."
        DEFVAL  {2}
        ::= { hwL2VlanQinqVlanTransEnaEntry 2 }                 
        
    hwL2VlanQinqVlanTransEnaRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "This table can be created."
        ::= { hwL2VlanQinqVlanTransEnaEntry 3 } 
         
    hwL2VlanQinqVlanTransMissDropTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanQinqVlanTransMissDropEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The table of QinQ VLAN translation miss drop."
        ::= { hwL2VlanApply 15 }

    hwL2VlanQinqVlanTransMissDropEntry OBJECT-TYPE
        SYNTAX HwL2VlanQinqVlanTransMissDropEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The entry of QinQ VLAN translation miss drop."
        INDEX {hwL2VlanQinqVlanTransMissDropPortIndex}
        ::= { hwL2VlanQinqVlanTransMissDropTable 1 }
    
    HwL2VlanQinqVlanTransMissDropEntry ::=
        SEQUENCE { 
                hwL2VlanQinqVlanTransMissDropPortIndex
                    Integer32,  
                hwL2VlanQinqVlanTransMissDrop 
                    INTEGER,
                hwL2VlanQinqVlanTransMissDropRowStatus
                    RowStatus                    
                 }
                 
    hwL2VlanQinqVlanTransMissDropPortIndex OBJECT-TYPE
        SYNTAX Integer32 (1..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            " The index of L2-Switch port. "
        ::= { hwL2VlanQinqVlanTransMissDropEntry 1 } 
        
    hwL2VlanQinqVlanTransMissDrop OBJECT-TYPE
        SYNTAX  INTEGER
                {
                    noDrop(1),  
                    drop(2)      
                }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Packets are dropped when a VLAN translation miss occurs."
        DEFVAL  {noDrop}
        ::= { hwL2VlanQinqVlanTransMissDropEntry 2 }
        
     hwL2VlanQinqVlanTransMissDropRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "This table can be created."
        ::= { hwL2VlanQinqVlanTransMissDropEntry 3 }        
             
    hwL2VlanViewMappingTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanViewMappingEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table of vlan-mapping at the VLAN view."
        ::= { hwL2VlanApply 16 }

    hwL2VlanViewMappingEntry  OBJECT-TYPE
        SYNTAX HwL2VlanViewMappingEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table contains vlan-mapping at the VLAN view entry."
        INDEX   { hwL2VlanViewMappingVlanId,hwL2VlanViewMappingDirection }
        ::= { hwL2VlanViewMappingTable 1}

    HwL2VlanViewMappingEntry  ::=
    SEQUENCE {
        hwL2VlanViewMappingVlanId           VlanId,
        hwL2VlanViewMappingDirection        INTEGER, 
        hwL2VlanViewMappingMapVlanId        VlanId,
        hwL2VlanViewMappingPriorityMode     INTEGER,
        hwL2VlanViewMappingVlan8021p        Integer32,
        hwL2VlanViewMappingRowStatus        RowStatus
        }
    
    hwL2VlanViewMappingVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The VLAN ID before mapping, using it as the index."
        ::= { hwL2VlanViewMappingEntry 1 }

    hwL2VlanViewMappingDirection  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        inbound   (1),
        outbound  (2),
        both      (3)
        }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Direction inbound and outbound."
        ::= { hwL2VlanViewMappingEntry 2 }   

    hwL2VlanViewMappingMapVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The VLAN ID after mapping."
        ::= { hwL2VlanViewMappingEntry 3 }    
       
    hwL2VlanViewMappingPriorityMode OBJECT-TYPE
        SYNTAX  INTEGER
        {
        priorityInherit  (1),
        remark8021p   (2)
        }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The priority mode: the priority can be remarked or inherit: 
            1: priority inherit
            2: remark 8021p "
        DEFVAL  {priorityInherit}
        ::= { hwL2VlanViewMappingEntry 4 }
        
    hwL2VlanViewMappingVlan8021p OBJECT-TYPE
        SYNTAX Integer32(0..7)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The priority after mapping, its default value is 0."
        DEFVAL  {0}
        ::= { hwL2VlanViewMappingEntry 5 }   
        
    hwL2VlanViewMappingRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Operation status."
        ::= { hwL2VlanViewMappingEntry 6 } 
       
    hwL2VlanStackingMaskTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanStackingMaskEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table of VLAN-stacking with Mask."
        ::= { hwL2VlanApply  17 }

    hwL2VlanStackingMaskEntry  OBJECT-TYPE
        SYNTAX HwL2VlanStackingMaskEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The entry of the table of VLAN-stacking with Mask. "
        INDEX {
                  hwL2VlanStackingMaskPortIndex, 
                  hwL2VlanStackingMaskStackVlanId, 
                  hwL2VlanStackingMaskStack8021p, 
                  hwL2VlanStackingMaskAction, 
                  hwL2VlanStackingMaskDirection
              }
        ::= { hwL2VlanStackingMaskTable 1}

    HwL2VlanStackingMaskEntry  ::=
    SEQUENCE {
        hwL2VlanStackingMaskPortIndex             InterfaceIndex,
        hwL2VlanStackingMaskStackVlanId           VlanIdOrNone,
        hwL2VlanStackingMaskStack8021p            Integer32,
        hwL2VlanStackingMaskAction                INTEGER,
        hwL2VlanStackingMaskDirection             INTEGER,
        hwL2VlanStackingMaskVlanListLow           OCTET STRING,
        hwL2VlanStackingMaskVlanListHigh          OCTET STRING,
        hwL2VlanStackingMaskRowStatus             RowStatus
        }

    hwL2VlanStackingMaskPortIndex  OBJECT-TYPE
        SYNTAX  InterfaceIndex 
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The index of L2-Switch interface."
        ::= { hwL2VlanStackingMaskEntry 1 }
    
    
    hwL2VlanStackingMaskStackVlanId  OBJECT-TYPE
        SYNTAX  VlanIdOrNone
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The outer VLAN-ID after stacking operation."
        ::= { hwL2VlanStackingMaskEntry 2 }
       
    hwL2VlanStackingMaskStack8021p OBJECT-TYPE
        SYNTAX Integer32(0..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The 8021p of outer VLAN-ID after stacking, it's an optional field, 
           if it is not selected, its value is 8, means inherit the 8021p from inner tag."
        ::= { hwL2VlanStackingMaskEntry 3 }    
     
    hwL2VlanStackingMaskAction  OBJECT-TYPE         
        SYNTAX  INTEGER
        {
        pop   (1),
        push  (2)
        }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The packet will be poped or pushed."
        ::= { hwL2VlanStackingMaskEntry 4}
        
    hwL2VlanStackingMaskDirection    OBJECT-TYPE         
        SYNTAX  INTEGER
        {
        inside   (1),
        outside  (2),
        both     (3)
        }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The direction which the packet need be poped or pushed, 
           that is ,the packet is receviced or transitted"
        ::= { hwL2VlanStackingMaskEntry 5}
        
   hwL2VlanStackingMaskVlanListLow  OBJECT-TYPE
    SYNTAX OCTET STRING (SIZE (256))
    MAX-ACCESS read-create
    STATUS current
        DESCRIPTION 
           "The possible value of the CE-VLAN low list."
        ::= { hwL2VlanStackingMaskEntry 6 }
        
   hwL2VlanStackingMaskVlanListHigh  OBJECT-TYPE
    SYNTAX OCTET STRING (SIZE (256))
    MAX-ACCESS read-create
    STATUS current
        DESCRIPTION 
           "The possible value of the CE-VLAN high list."
        ::= { hwL2VlanStackingMaskEntry 7 }         

    hwL2VlanStackingMaskRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Operation status."
        ::= { hwL2VlanStackingMaskEntry 8 }
                    
   hwL2VlanIpSubnetVlanTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanIpSubnetVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table of VLAN assignment based on ip subnet."
        ::= { hwL2VlanApply  18 }

    hwL2VlanIpSubnetVlanEntry  OBJECT-TYPE
        SYNTAX HwL2VlanIpSubnetVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The entry of the table of VLAN assignment based on ip subnet. "
        INDEX {
                  hwL2VlanIpSubnetVlanVlanId,
                  hwL2VlanIpSubnetVlanIpSubnetIndex
              }
        ::= { hwL2VlanIpSubnetVlanTable 1 }

    HwL2VlanIpSubnetVlanEntry  ::=
    SEQUENCE {
        hwL2VlanIpSubnetVlanVlanId               VlanId,
        hwL2VlanIpSubnetVlanIpSubnetIndex        Integer32,
        hwL2VlanIpSubnetVlanIpAddress            IpAddress,
        hwL2VlanIpSubnetVlanIpSubnetMask         IpAddress,
        hwL2VlanIpSubnetVlanPriority             Integer32, 
        hwL2VlanIpSubnetVlanRowStatus            RowStatus
        }

    hwL2VlanIpSubnetVlanVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The VLAN-ID after VLAN assignment based on ip subnet."
        ::= { hwL2VlanIpSubnetVlanEntry 1 }
       
    hwL2VlanIpSubnetVlanIpSubnetIndex OBJECT-TYPE
        SYNTAX Integer32(1..12)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The index of ip subnet on this vlan, ranging from integer 1 to 12."
        ::= { hwL2VlanIpSubnetVlanEntry 2 }    
     
    hwL2VlanIpSubnetVlanIpAddress  OBJECT-TYPE         
        SYNTAX IpAddress
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The IpAddress based on vlan."
        ::= { hwL2VlanIpSubnetVlanEntry 3}
        
    hwL2VlanIpSubnetVlanIpSubnetMask  OBJECT-TYPE         
        SYNTAX IpAddress
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The IpAddress or Ip subnet mask."
        ::= { hwL2VlanIpSubnetVlanEntry 4}
       
   hwL2VlanIpSubnetVlanPriority OBJECT-TYPE
        SYNTAX Integer32(0..7)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The priority after vlan assignment based on ip subnet, its default value is 0."
        DEFVAL  {0}
        ::= { hwL2VlanIpSubnetVlanEntry 5 }      

    hwL2VlanIpSubnetVlanRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Operation status."
        ::= { hwL2VlanIpSubnetVlanEntry 6 }

 hwL2VlanMacVlanTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanMacVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table of VLAN assignment based on MAC."
        ::= { hwL2VlanApply  19 }

    hwL2VlanMacVlanEntry  OBJECT-TYPE
        SYNTAX HwL2VlanMacVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The entry of the table of VLAN assignment based on MAC. "
        INDEX {
                  hwL2VlanMacVlanVlanId
              }
        ::= { hwL2VlanMacVlanTable 1 }

    HwL2VlanMacVlanEntry  ::=
    SEQUENCE {
        hwL2VlanMacVlanVlanId               VlanId,        
        hwL2VlanMacVlanMac                  MacAddress, 
        hwL2VlanMacVlanVlanPriority         Integer32,
        hwL2VlanMacVlanMacRowStatus         RowStatus
        }

        
    hwL2VlanMacVlanVlanId  OBJECT-TYPE         
        SYNTAX VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "mac-vlan."
        ::= { hwL2VlanMacVlanEntry 1}
        
    hwL2VlanMacVlanMac  OBJECT-TYPE
        SYNTAX  MacAddress
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The VLAN-ID after VLAN assignment based on mac."
        ::= { hwL2VlanMacVlanEntry 2}  
     
    hwL2VlanMacVlanVlanPriority OBJECT-TYPE
        SYNTAX Integer32(0..7)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The priority after vlan assignment based on mac, its default value is 0."
        DEFVAL  {0}
        ::= { hwL2VlanMacVlanEntry 3 }      

    hwL2VlanMacVlanMacRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Operation status."
        ::= { hwL2VlanMacVlanEntry 4 }

    hwL2VlanProtocolVlanTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanProtocolVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table of VLAN assignment based on protocol."
        ::= { hwL2VlanApply  20 }

    hwL2VlanProtocolVlanEntry  OBJECT-TYPE
        SYNTAX HwL2VlanProtocolVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The entry of the table of VLAN assignment based on protocol. "
        INDEX {
                  hwL2VlanProtocolVlanVlanId,
                  hwL2VlanProtocolVlanProtocolIndex 
              }
        ::= { hwL2VlanProtocolVlanTable 1 }

    HwL2VlanProtocolVlanEntry  ::=
    SEQUENCE {
        hwL2VlanProtocolVlanVlanId               VlanId,
        hwL2VlanProtocolVlanProtocolIndex        Integer32,
        hwL2VlanProtocolVlanProtocolType         Integer32,
        hwL2VlanProtocolVlanEncapType            INTEGER,        
        hwL2VlanProtocolVlanRowStatus            RowStatus
        }

    hwL2VlanProtocolVlanVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The VLAN-ID after VLAN assignment based on protocol."
        ::= { hwL2VlanProtocolVlanEntry 1 }
       
    hwL2VlanProtocolVlanProtocolIndex OBJECT-TYPE
        SYNTAX Integer32(1..16)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The index of protocol on vlan, ranging from integer 1 to 16"
        ::= { hwL2VlanProtocolVlanEntry 2 }    
     
    hwL2VlanProtocolVlanProtocolType  OBJECT-TYPE         
        SYNTAX Integer32
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Protocol type."
        ::= { hwL2VlanProtocolVlanEntry 3}        

    hwL2VlanProtocolVlanEncapType  OBJECT-TYPE
        SYNTAX  INTEGER
        {
            etherii(1),  
            snap(2),    
            llc(3)  
        }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Encap type, include ETHERII,SNAP,LLC."
        ::= { hwL2VlanProtocolVlanEntry 4 }

   
    hwL2VlanProtocolVlanRowStatus  OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Operation status."
        ::= { hwL2VlanProtocolVlanEntry 5 }


                  
   hwL2VlanPolicyVlanTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanPolicyVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table of VLAN assignment based on strategy."
        ::= { hwL2VlanApply  21 }

    hwL2VlanPolicyVlanEntry  OBJECT-TYPE
        SYNTAX HwL2VlanPolicyVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The entry of the table of VLAN assignment based on strategy. "
        INDEX {
                  hwL2VlanPolicyVlanVlanId
              }
        ::= { hwL2VlanPolicyVlanTable 1 }

    HwL2VlanPolicyVlanEntry  ::=
    SEQUENCE {
        hwL2VlanPolicyVlanMac                  MacAddress,
        hwL2VlanPolicyVlanIp                   IpAddress,
        hwL2VlanPolicyVlanPort                 Integer32, 
        hwL2VlanPolicyVlanVlanId               VlanId,
        hwL2VlanPolicyVlanVlanPriority         Integer32, 
        hwL2VlanPolicyVlanRowStatus            RowStatus
        }
            
    hwL2VlanPolicyVlanMac  OBJECT-TYPE         
        SYNTAX MacAddress
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Support MAC+IP and MAC+IP+PORT."
        ::= { hwL2VlanPolicyVlanEntry 1}
        
    hwL2VlanPolicyVlanIp  OBJECT-TYPE         
        SYNTAX IpAddress
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Support MAC+IP and MAC+IP+PORT."
        ::= { hwL2VlanPolicyVlanEntry 2}
       
    hwL2VlanPolicyVlanPort OBJECT-TYPE
        SYNTAX Integer32(0..7)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Support MAC+IP+PORT."
        DEFVAL  {0}
        ::= { hwL2VlanPolicyVlanEntry 3 }      
 
    hwL2VlanPolicyVlanVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The VLAN-ID after VLAN assignment based on policy."
        ::= { hwL2VlanPolicyVlanEntry 4 }

    hwL2VlanPolicyVlanVlanPriority  OBJECT-TYPE
        SYNTAX  Integer32
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The VLAN-ID after VLAN assignment based on policy."
        ::= { hwL2VlanPolicyVlanEntry 5 }

    hwL2VlanPolicyVlanRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Operation status."
        ::= { hwL2VlanPolicyVlanEntry 6 }
        

    hwL2VlanVoiceVlanEnabledVlanId  OBJECT-TYPE
        SYNTAX  Integer32(0..4294967295)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "Indicates the global voice VLAN ID. Global voice VLAN is enabled if the value  ranges from 1 to 4094; global voice VLAN is disabled if the value is 0."
        ::= { hwL2VlanApply 22 }

    hwL2VlanVoiceVlanAgingTime  OBJECT-TYPE
        SYNTAX  Integer32(5..43200)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "Voice vlan aging time(in minute). The default value is 1440."
        ::= { hwL2VlanApply  23 }

   hwL2VlanVoiceVlanSecurityMode  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        security (1),
        normal (2)
        }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "Voice vlan security mode status."
        ::= { hwL2VlanApply 24 }
        
   hwL2VlanVoiceVlanPortTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF HwL2VlanVoiceVlanPortEntry
        MAX-ACCESS not-accessible
        STATUS   current
        DESCRIPTION " A list of voice vlan mode entries."
        ::= { hwL2VlanApply  25  }

   hwL2VlanVoiceVlanPortEntry OBJECT-TYPE
        SYNTAX  HwL2VlanVoiceVlanPortEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION " An entry containing voice vlan mode information,
            which is applicable to a voice vlan enabled interface."
        INDEX   { hwL2VlanVoiceVlanPortIndex }        
        ::= { hwL2VlanVoiceVlanPortTable 1}

   HwL2VlanVoiceVlanPortEntry ::=
        SEQUENCE {
         hwL2VlanVoiceVlanPortIndex    Integer32,
         hwL2VlanVoiceVlanPortEnable   EnabledStatus,
         hwL2VlanVoiceVlanPortMode     INTEGER,
         hwL2VlanVoiceVlanPortLegacy   EnabledStatus,
         hwL2VlanVoiceVlanPortSecurityMode   INTEGER,
         hwL2VlanVoiceVlanPortModifyPriorityMode  INTEGER
         }

   hwL2VlanVoiceVlanPortIndex OBJECT-TYPE
        SYNTAX  Integer32(1..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The port index on which voice vlan is enabled."
    ::= { hwL2VlanVoiceVlanPortEntry 1 }

   hwL2VlanVoiceVlanPortEnable OBJECT-TYPE
        SYNTAX  EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "Voice VLAN enable status at port ."
        ::= { hwL2VlanVoiceVlanPortEntry 2 }  
        
   hwL2VlanVoiceVlanPortMode OBJECT-TYPE
        SYNTAX  INTEGER
            {
            auto (1),
            manual (2)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "Voice VLAN configuration mode status, 1 for auto, 2 for manual."
        ::= { hwL2VlanVoiceVlanPortEntry 3 } 
         
   hwL2VlanVoiceVlanPortLegacy OBJECT-TYPE
        SYNTAX  EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "This flag is enabled. It indicates that the interworking with other vendors' equipment is enabled."
        ::= { hwL2VlanVoiceVlanPortEntry 4}  
           
   hwL2VlanVoiceVlanPortSecurityMode OBJECT-TYPE
        SYNTAX  INTEGER  
         {
         security (1),
         normal (2)
         }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "Voice VLAN configuration security mode status, 1 for security, 2 for normal."
        ::= { hwL2VlanVoiceVlanPortEntry 5}   

   hwL2VlanVoiceVlanPortModifyPriorityMode OBJECT-TYPE
        SYNTAX  INTEGER  
         {
         modifyPriByVlan (1),
         modifyPriByOui (2)
         }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "The value of this object identifies the priority of voice packets to be forwarded , 1 for modifyPriByVlan, 2 for modifyPriByOui."
        ::= { hwL2VlanVoiceVlanPortEntry 6}  
                 
    hwL2VlanVoiceVlanOuiTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF HwL2VlanVoiceVlanOuiEntry
        MAX-ACCESS not-accessible
        STATUS   current
        DESCRIPTION " A table containing the MAC address which can be identified by voice vlan. "
        ::= { hwL2VlanApply  26 }


    hwL2VlanVoiceVlanOuiEntry OBJECT-TYPE
        SYNTAX  HwL2VlanVoiceVlanOuiEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION " An entry containing the information of MAC address which can be identified by voice vlan."
        INDEX   { hwL2VlanVoiceVlanOuiAddress, hwL2VlanVoiceVlanOuiMask }        
        ::= { hwL2VlanVoiceVlanOuiTable 1}

    HwL2VlanVoiceVlanOuiEntry    ::=
        SEQUENCE {
        hwL2VlanVoiceVlanOuiAddress    MacAddress  ,
        hwL2VlanVoiceVlanOuiMask    MacAddress  ,
        hwL2VlanVoiceVlanOuiDescription    OCTET STRING  ,
        hwL2VlanVoiceVlanOuiRowStatus      RowStatus
        }

    hwL2VlanVoiceVlanOuiAddress OBJECT-TYPE
        SYNTAX  MacAddress  
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "MAC address can be identified by Voice VLAN."
        ::= { hwL2VlanVoiceVlanOuiEntry 1 }

    hwL2VlanVoiceVlanOuiMask OBJECT-TYPE
        SYNTAX  MacAddress  
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The mask of MAC address."
        ::= { hwL2VlanVoiceVlanOuiEntry 2 }

    hwL2VlanVoiceVlanOuiDescription OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(0..80))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The description of OUI."
        ::= { hwL2VlanVoiceVlanOuiEntry 3 }

    hwL2VlanVoiceVlanOuiRowStatus OBJECT-TYPE
        SYNTAX  RowStatus  
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "Operation status. "
        ::= { hwL2VlanVoiceVlanOuiEntry 4 }

    hwL2VlanMappingMultiTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanMappingMultiEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Configuration table."
        ::= { hwL2VlanApply  27 }


    hwL2VlanMappingMultiEntry  OBJECT-TYPE
        SYNTAX HwL2VlanMappingMultiEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table contains Vlan-Mapping entry."
        INDEX   {hwL2VlanMappingMultiPortIndex,hwL2VlanMappingMultiDirection, 
                  hwL2VlanMappingMultiVlanId,hwL2VlanMappingMultiVlan8021p}
        ::= { hwL2VlanMappingMultiTable 1}

    HwL2VlanMappingMultiEntry  ::=
    SEQUENCE {
        hwL2VlanMappingMultiPortIndex        Integer32,        
        hwL2VlanMappingMultiDirection        INTEGER, 
        hwL2VlanMappingMultiVlanId           VlanId,
        hwL2VlanMappingMultiVlan8021p        Integer32,        
        hwL2VlanMappingMultiVlanListLow      OCTET STRING,
        hwL2VlanMappingMultiVlanListHigh     OCTET STRING,
        hwL2VlanMappingMultiRowStatus        RowStatus     
        }


    hwL2VlanMappingMultiPortIndex  OBJECT-TYPE
        SYNTAX  Integer32(1..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Port Index."
        ::= { hwL2VlanMappingMultiEntry 1 }
    
    hwL2VlanMappingMultiDirection  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        inbound   (1),
        outbound  (2),
        both      (3)
        }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Direction inbound and outbound."
        ::= { hwL2VlanMappingMultiEntry 2 }

    hwL2VlanMappingMultiVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The outside vlan-id."
        ::= { hwL2VlanMappingMultiEntry 3 }
        
    hwL2VlanMappingMultiVlan8021p OBJECT-TYPE
        SYNTAX Integer32(0..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The priority of outside VLAN after mapping,8 means priority-inherit."
        ::= { hwL2VlanMappingMultiEntry 4 }


    hwL2VlanMappingMultiVlanListLow  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The possible value of the inside vlan list."
        ::= { hwL2VlanMappingMultiEntry 5 }
    
    hwL2VlanMappingMultiVlanListHigh  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The possible value of the inside vlan list."
        ::= { hwL2VlanMappingMultiEntry 6 }

    hwL2VlanMappingMultiRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "This table can be created."
        ::= { hwL2VlanMappingMultiEntry 7 }           
    
    hwL2VlanMacVlanNewTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanMacVlanNewEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table of VLAN assignment based on MAC."
        ::= { hwL2VlanApply  28 }

    hwL2VlanMacVlanNewEntry  OBJECT-TYPE
        SYNTAX HwL2VlanMacVlanNewEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The entry of the table of VLAN assignment based on MAC. "
        INDEX {                  
                  hwL2VlanMacVlanNewMac
              }
        ::= { hwL2VlanMacVlanNewTable 1 }

    HwL2VlanMacVlanNewEntry  ::=
    SEQUENCE {
        hwL2VlanMacVlanNewMac                  MacAddress, 
        hwL2VlanMacVlanNewVlanId               VlanId,        
        hwL2VlanMacVlanNewVlanPriority         Integer32,
        hwL2VlanMacVlanNewMacRowStatus         RowStatus
        }

    hwL2VlanMacVlanNewMac  OBJECT-TYPE
        SYNTAX  MacAddress
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The VLAN-ID after VLAN assignment based on MAC."
        ::= { hwL2VlanMacVlanNewEntry 1}  
        
    hwL2VlanMacVlanNewVlanId  OBJECT-TYPE         
        SYNTAX VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "MAC-VLAN VLAN ID."
        ::= { hwL2VlanMacVlanNewEntry 2}
           
    hwL2VlanMacVlanNewVlanPriority OBJECT-TYPE
        SYNTAX Integer32(0..7)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The priority after VLAN assignment based on MAC, its default value is 0."
        DEFVAL  {0}
        ::= { hwL2VlanMacVlanNewEntry 3 }      

    hwL2VlanMacVlanNewMacRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Operation status."
        ::= { hwL2VlanMacVlanNewEntry 4 }

    hwL2VlanProtocolVlanNewTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanProtocolVlanNewEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table of VLAN assignment based on protocol."
        ::= { hwL2VlanApply  29 }

    hwL2VlanProtocolVlanNewEntry  OBJECT-TYPE
        SYNTAX HwL2VlanProtocolVlanNewEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The entry of the table of VLAN assignment based on protocol. "
        INDEX {
                  hwL2VlanProtocolVlanNewVlanId,
                  hwL2VlanProtocolVlanNewProtocolIndex 
              }
        ::= { hwL2VlanProtocolVlanNewTable 1 }

    HwL2VlanProtocolVlanNewEntry  ::=
    SEQUENCE {
        hwL2VlanProtocolVlanNewVlanId               VlanId,
        hwL2VlanProtocolVlanNewProtocolIndex        Integer32,
        hwL2VlanProtocolVlanNewProtocolType         INTEGER,
        hwL2VlanProtocolVlanNewProtocolTypeValue    OCTET STRING,        
        hwL2VlanProtocolVlanNewRowStatus            RowStatus
        }

    hwL2VlanProtocolVlanNewVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The VLAN-ID after VLAN assignment based on protocol."
        ::= { hwL2VlanProtocolVlanNewEntry 1 }
       
    hwL2VlanProtocolVlanNewProtocolIndex OBJECT-TYPE
        SYNTAX Integer32(0..15)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The index of protocol on vlan, ranging from integer 1 to 16"
        ::= { hwL2VlanProtocolVlanNewEntry 2 }    
     
    hwL2VlanProtocolVlanNewProtocolType  OBJECT-TYPE         
        SYNTAX  INTEGER
        {
            at(1),  
            ipv4(2),    
            ipv6(3),
            ipxEthernetii (4),
            ipxLlc(5),
            ipxRaw(6),
            ipxSnap(7),
            modeEthernetii(8),
            modeLlc(9),
            modeSnap (10)              
        }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Protocol type."
        ::= { hwL2VlanProtocolVlanNewEntry 3}        

    hwL2VlanProtocolVlanNewProtocolTypeValue  OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE(2))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The value of the configured protocol type.
           
           The relationship among hwL2VlanProtocolVlanNewProtocolType and hwL2VlanProtocolVlanNewProtocolTypeValue is as follows.
     
     |============================================================================================|
     | hwL2VlanProtocol-|                  | hwL2VlanProtocolVlanNewProtocolTypeValue             |
     | VlanProtocolType | ProtocolSubType  |                                                      |
     |============================================================================================|
     | ipv4             | notused          | Zero length string                                   |
     |============================================================================================|
     | ipv6             | notused          | Zero length string                                   |
     |============================================================================================|
     | at               | notused          | Zero length string                                   |
     |============================================================================================|
     | ipx              | ethernetii       | Zero length string                                   |
     |                  | llc              |                                                      |
     |                  | raw              |                                                      |
     |                  | snap             |                                                      |
     |============================================================================================|
     | mode-ethernetii  | etype            | hex string like '600', which means 0x0600.           |
     |                  |                  | The range is [0x600..0xffff]                         |
     |============================================================================================|
     | mode-llc         | etype            | the sequence of different parts is as follows.       |
     |                  |                  | [dsap value;ssap value]                              |
     |                  |                  | Both range is [0x00..0xff]                           |
     |                  |                  |                                                      |
     |                  |                  | For example. Suppose value of dsap and ssap are 0x09 |
     |                  |                  | and 0x0a, the value is '090a'                        |
     |============================================================================================|
        | mode-snap        | etype            | hex string like '600', which means 0x0600.           |
     |                  |                  | The range is [0x600..0xffff]                         |
     |============================================================================================|
        "
        ::= { hwL2VlanProtocolVlanNewEntry 4 }

   
    hwL2VlanProtocolVlanNewRowStatus  OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Operation status."
        ::= { hwL2VlanProtocolVlanNewEntry 5 }
                  
   hwL2VlanPolicyVlanNewTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanPolicyVlanNewEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table of VLAN assignment based on strategy."
        ::= { hwL2VlanApply  30 }

    hwL2VlanPolicyVlanNewEntry  OBJECT-TYPE
        SYNTAX HwL2VlanPolicyVlanNewEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The entry of the table of VLAN assignment based on strategy. "
        INDEX {
                  hwL2VlanPolicyVlanNewVlanId,
                  hwL2VlanPolicyVlanNewMac,
                  hwL2VlanPolicyVlanNewIp,
                  hwL2VlanPolicyVlanNewPort
              }
        ::= { hwL2VlanPolicyVlanNewTable 1 }

    HwL2VlanPolicyVlanNewEntry  ::=
    SEQUENCE {
        hwL2VlanPolicyVlanNewMac                  MacAddress,
        hwL2VlanPolicyVlanNewIp                   IpAddress,
        hwL2VlanPolicyVlanNewPort                 Integer32, 
        hwL2VlanPolicyVlanNewVlanId               VlanId,
        hwL2VlanPolicyVlanNewVlanPriority         Integer32, 
        hwL2VlanPolicyVlanNewRowStatus            RowStatus
        }
            
    hwL2VlanPolicyVlanNewMac  OBJECT-TYPE         
        SYNTAX MacAddress
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Support MAC+IP and MAC+IP+PORT."
        ::= { hwL2VlanPolicyVlanNewEntry 1}
        
    hwL2VlanPolicyVlanNewIp  OBJECT-TYPE         
        SYNTAX IpAddress
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Support MAC+IP and MAC+IP+PORT."
        ::= { hwL2VlanPolicyVlanNewEntry 2}
       
    hwL2VlanPolicyVlanNewPort OBJECT-TYPE
        SYNTAX Integer32 
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Support MAC+IP+PORT."
        ::= { hwL2VlanPolicyVlanNewEntry 3 }      
 
    hwL2VlanPolicyVlanNewVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The VLAN-ID after VLAN assignment based on policy."
        ::= { hwL2VlanPolicyVlanNewEntry 4 }

    hwL2VlanPolicyVlanNewVlanPriority  OBJECT-TYPE
        SYNTAX  Integer32(0..7)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The Priority after VLAN assignment based on policy."
        ::= { hwL2VlanPolicyVlanNewEntry 5 }

    hwL2VlanPolicyVlanNewRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Operation status."
        ::= { hwL2VlanPolicyVlanNewEntry 6 }
        
        
    hwL2VlanProtocolVlanPortNewTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanProtocolVlanPortNewEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "
            Protocol-based VLAN port information table.

            hwL2VlanProtocolVlanPortNewVlanId refers to hwL2VlanProtocolVlanNewVlanId
            in hwL2VlanProtocolVlanNewTable.

            hwL2VlanProtocolVlanPortNewProtocolId refers to hwL2VlanProtocolVlanNewProtocolIndex
            in hwL2VlanProtocolVlanNewTable. So if the value of hwL2VlanProtocolVlanPortNewVlanId
            and hwL2VlanProtocolVlanPortNewProtocolId have no corresponding entry in
            hwL2VlanProtocolVlanNewTable, set operation for this table will fail.
            "
        ::= { hwL2VlanApply 31 }

    hwL2VlanProtocolVlanPortNewEntry OBJECT-TYPE
        SYNTAX HwL2VlanProtocolVlanPortNewEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "
            Protocol-based VLAN port information entry.
            "
        INDEX { hwL2VlanProtocolVlanPortNewIndex, hwL2VlanProtocolVlanPortNewVlanId,
                hwL2VlanProtocolVlanPortNewProtocolIndex }
        ::= { hwL2VlanProtocolVlanPortNewTable 1 }

    HwL2VlanProtocolVlanPortNewEntry ::=
        SEQUENCE {
            hwL2VlanProtocolVlanPortNewIndex
                Integer32,
            hwL2VlanProtocolVlanPortNewVlanId
                VlanId,
            hwL2VlanProtocolVlanPortNewProtocolIndex
                Integer32,
            hwL2VlanProtocolVlanPortNewPriority
                Integer32,
            hwL2VlanProtocolVlanPortNewRowStatus
                RowStatus
         }

    hwL2VlanProtocolVlanPortNewIndex OBJECT-TYPE
        SYNTAX  Integer32(1..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "
            The maximum number is the total number of the ports supported by device.
            "
        ::= { hwL2VlanProtocolVlanPortNewEntry 1 }

    hwL2VlanProtocolVlanPortNewVlanId OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The protocol-based VLAN ID."
        ::= { hwL2VlanProtocolVlanPortNewEntry 2 }

    hwL2VlanProtocolVlanPortNewProtocolIndex OBJECT-TYPE
        SYNTAX Integer32(0..15)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The protocol index."
        ::= { hwL2VlanProtocolVlanPortNewEntry 3 }

    hwL2VlanProtocolVlanPortNewPriority OBJECT-TYPE
        SYNTAX Integer32(0..7)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The protocol-based VLAN priority."
        ::= { hwL2VlanProtocolVlanPortNewEntry 4 }

    hwL2VlanProtocolVlanPortNewRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The row status of this table."
        ::= { hwL2VlanProtocolVlanPortNewEntry 5}   
        
    hwL2VlanMultiVoiceVlanPortTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF HwL2VlanMultiVoiceVlanPortEntry
        MAX-ACCESS not-accessible
        STATUS   current
        DESCRIPTION "Voice VLAN is enabled on the port."
        ::= { hwL2VlanApply  32 }

    hwL2VlanMultiVoiceVlanPortEntry OBJECT-TYPE
        SYNTAX  HwL2VlanMultiVoiceVlanPortEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION " An entry containing voice VLAN mode information,
            which is applicable to a voice VLAN enabled interface."
        INDEX   { hwL2VlanMultiVoiceVlanIfIndex }        
        ::= { hwL2VlanMultiVoiceVlanPortTable 1}

    HwL2VlanMultiVoiceVlanPortEntry ::=
        SEQUENCE {
         hwL2VlanMultiVoiceVlanIfIndex         InterfaceIndex,
         hwL2VlanMultiVoiceVlanPortVLanId        VlanId,
         hwL2VlanMultiVoiceVlanPortUntagEnable   INTEGER,
         hwL2VlanMultiVoiceVlanPortTag0Enable   INTEGER,
         hwL2VlanMultiVoiceVlanPortRowStatus     RowStatus 
         }
               
    hwL2VlanMultiVoiceVlanIfIndex OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The interface index on which voice VLAN is enabled."
        ::= { hwL2VlanMultiVoiceVlanPortEntry 1 }

    hwL2VlanMultiVoiceVlanPortVLanId OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The VLAN ID of voice VLAN on port ."
        ::= { hwL2VlanMultiVoiceVlanPortEntry 2 }   

   hwL2VlanMultiVoiceVlanPortUntagEnable OBJECT-TYPE
        SYNTAX  INTEGER  
         {
         enabled (1),
         disabled (2)
         }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "The value of this object identifies whether untagged voice packets can be forwarded in voice VLAN, 1 for enabled, 2 for disabled."
        ::= { hwL2VlanMultiVoiceVlanPortEntry 3}   

   hwL2VlanMultiVoiceVlanPortTag0Enable OBJECT-TYPE
        SYNTAX  INTEGER  
         {
         enabled (1),
         disabled (2)
         }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "The value of this object identifies whether tag0 voice packets can be forwarded in voice VLAN, 1 for enabled, 2 for disabled."
        ::= { hwL2VlanMultiVoiceVlanPortEntry 4}  
                
    hwL2VlanMultiVoiceVlanPortRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The row status of this table."
        ::= { hwL2VlanMultiVoiceVlanPortEntry 51 }     

        
    hwL2VlanSwitchExtTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanSwitchExtEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The table to config the vlan switch."
        ::= { hwL2VlanApply 33 }
    
    
    hwL2VlanSwitchExtEntry OBJECT-TYPE
        SYNTAX HwL2VlanSwitchExtEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The entry of the vlan switch table."
        INDEX { hwL2VlanSwitchExtName }
        ::= { hwL2VlanSwitchExtTable 1 }
    
    
    HwL2VlanSwitchExtEntry ::=
        SEQUENCE { 
            hwL2VlanSwitchExtName
                OCTET STRING,
            hwL2VlanSwitchExtSrcIfIndex
                InterfaceIndex,
            hwL2VlanSwitchExtOuterVlanId
                Integer32,
            hwL2VlanSwitchExtVlanListLow
                OCTET STRING,
            hwL2VlanSwitchExtVlanListHigh
                OCTET STRING,
            hwL2VlanSwitchExtDstIfIndex
                InterfaceIndex,
            hwL2VlanSwitchExtVlanXlateAction
                INTEGER,
            hwL2VlanSwitchExtDstVlan
                Integer32,
            hwL2VlanSwitchExtDstInnerVlan
                Integer32,
            hwL2VlanSwitchExtRemark
                Integer32,
            hwL2VlanSwitchExtRemarkReverse
                Integer32,
            hwL2VlanSwitchExtLinkStatus
                INTEGER,
            hwL2VlanSwitchExtRowStatus
                RowStatus
         }
    
    hwL2VlanSwitchExtName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..32))
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The vlan switch name."
        ::= { hwL2VlanSwitchExtEntry 1 }
    
    
    hwL2VlanSwitchExtSrcIfIndex OBJECT-TYPE
        SYNTAX InterfaceIndex
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The index of source interface."
        ::= { hwL2VlanSwitchExtEntry 2 }
    
    
    hwL2VlanSwitchExtOuterVlanId OBJECT-TYPE
        SYNTAX Integer32 (0..4094)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The outer vlan."
        ::= { hwL2VlanSwitchExtEntry 3 }
    
    
    hwL2VlanSwitchExtVlanListLow OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The possible value of the inside vlan list."
        ::= { hwL2VlanSwitchExtEntry 4 }
    
    
    hwL2VlanSwitchExtVlanListHigh OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (256))
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The possible value of the inside vlan list."
        ::= { hwL2VlanSwitchExtEntry 5 }
    
    
    hwL2VlanSwitchExtDstIfIndex OBJECT-TYPE
        SYNTAX InterfaceIndex
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The index of destination interface."
        ::= { hwL2VlanSwitchExtEntry 6 }
    
    
    hwL2VlanSwitchExtVlanXlateAction OBJECT-TYPE
        SYNTAX INTEGER
            {
            unchange(1),
            switch(2),
            push(3)
            }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The action type of vlan:
            1 : unchange vlan,
            2 : switch vlan,
            3 : push vlan."
        ::= { hwL2VlanSwitchExtEntry 7 }
    
    
    hwL2VlanSwitchExtDstVlan OBJECT-TYPE
        SYNTAX Integer32 (0..4094)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The outer vlan of destination."
        ::= { hwL2VlanSwitchExtEntry 8 }
    
    
    hwL2VlanSwitchExtDstInnerVlan OBJECT-TYPE
        SYNTAX Integer32 (0..4094)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The inner vlan of destination."
        ::= { hwL2VlanSwitchExtEntry 9 }
    
    
    hwL2VlanSwitchExtRemark OBJECT-TYPE
        SYNTAX Integer32 (0..8)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The remark 8021p value."
        ::= { hwL2VlanSwitchExtEntry 10 }
    
    
    hwL2VlanSwitchExtRemarkReverse OBJECT-TYPE
        SYNTAX Integer32 (0..8)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The reverse remark 8021p value."
        ::= { hwL2VlanSwitchExtEntry 11 }
    
    
    hwL2VlanSwitchExtLinkStatus OBJECT-TYPE
        SYNTAX INTEGER
            {
            up(1),
            down(2)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The link status of vlan switch."
        ::= { hwL2VlanSwitchExtEntry 12 }
    
    
    hwL2VlanSwitchExtRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The row status."
        ::= { hwL2VlanSwitchExtEntry 51 }

    hwL2VlanPrecedence  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        macvlan (1),
        ipsubnetvlan (2)
        }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "Determine whether to select the MAC-based VLAN or subnet-based VLAN,
                      1:MAC VLAN(default);  2:IPSUBNET VLAN."
        ::= { hwL2VlanApply 34 }

    hwL2VlanXlateTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF HwL2VlanXlateEntry
        MAX-ACCESS not-accessible
        STATUS   current
        DESCRIPTION "VLAN mapping configuration table."
        ::= { hwL2VlanApply  35 }

    hwL2VlanXlateEntry OBJECT-TYPE
        SYNTAX  HwL2VlanXlateEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The entry in the VLAN mapping configuration table."
        INDEX   { 
                  hwL2VlanXlateInterfaceIndex,
                  hwL2VlanXlateVlanIdBegin,
                  hwL2VlanXlateOuterVlanId,
                  hwL2VlanXlateVlan8021p,
                  hwL2VlanXlateDirection 
                }        
        ::= { hwL2VlanXlateTable 1}

    HwL2VlanXlateEntry ::=
        SEQUENCE {
                    hwL2VlanXlateInterfaceIndex   InterfaceIndex,
                    hwL2VlanXlateVlanIdBegin      VlanId,
                    hwL2VlanXlateVlanIdEnd        VlanIdOrNone,
                    hwL2VlanXlateOuterVlanId      VlanIdOrNone,
                    hwL2VlanXlateVlan8021p        Integer32,
                    hwL2VlanXlateDirection        INTEGER,
                    hwL2VlanXlateAction           INTEGER,
                    hwL2VlanXlateToVlanId         VlanIdOrNone,
                    hwL2VlanXlateToinnerVlanId    VlanIdOrNone,
                    hwL2VlanXlateremark           Integer32,
                    hwL2VlanXlateRowStatus        RowStatus
         }
               
    hwL2VlanXlateInterfaceIndex OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The index of the interface."
        ::= { hwL2VlanXlateEntry 1 }

    hwL2VlanXlateVlanIdBegin OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION " The ID of the first VLAN (VLAN ID in the inner VLAN tag if there are double VLAN tags) 
                    at the user side."
        ::= { hwL2VlanXlateEntry 2 }   
        
    hwL2VlanXlateVlanIdEnd OBJECT-TYPE
        SYNTAX  VlanIdOrNone
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The ID of the end VLAN (VLAN ID in the inner VLAN tag if there are double VLAN tags)
                     at the user side."
        ::= { hwL2VlanXlateEntry 3 }    
        
    hwL2VlanXlateOuterVlanId OBJECT-TYPE
        SYNTAX  VlanIdOrNone
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The value of outer VLAN for packets with double tags in customer side. 
                     For one-tag-packet, it's 0."
        ::= { hwL2VlanXlateEntry 4 }    
        
    hwL2VlanXlateVlan8021p OBJECT-TYPE
        SYNTAX  Integer32(0..8 | 65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "This object indicates the 802.1p priority in the VLAN tag to be mapped to."
        ::= { hwL2VlanXlateEntry 5 }        
        
    hwL2VlanXlateDirection  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        inbound   (1),
        outbound  (2),
        both      (3)
        }
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Direction inbound or outbound or both."
        ::= { hwL2VlanXlateEntry 6 }        
        
    hwL2VlanXlateAction  OBJECT-TYPE
        SYNTAX  INTEGER
        {
        map    (1),
        stack  (2),
        pop    (3)
        }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The packet will be mapped or stacked or poped."
        ::= { hwL2VlanXlateEntry 7 }  
                                     
    hwL2VlanXlateToVlanId  OBJECT-TYPE
        SYNTAX  VlanIdOrNone
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The ID of the outer VLAN at the network side. 
        If this VLAN is not in use, the ID is 0."
        ::= { hwL2VlanXlateEntry 8 }       
        
    hwL2VlanXlateToinnerVlanId  OBJECT-TYPE
        SYNTAX  VlanIdOrNone
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The value of inner VLAN in network side. It's 0 when it is not used."
        ::= { hwL2VlanXlateEntry 9 }                  
             
     hwL2VlanXlateremark  OBJECT-TYPE
        SYNTAX  Integer32
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The priority of outer VLAN in network side."
        ::= { hwL2VlanXlateEntry 10 } 
        
     hwL2VlanXlateRowStatus  OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "Operation status."
        ::= { hwL2VlanXlateEntry 51 }      
        
    hwL2QinQVlanTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2QinQVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The table of QinQ-VLAN configuration."
        ::= { hwL2VlanApply 36 }

    hwL2QinQVlanEntry OBJECT-TYPE
        SYNTAX HwL2QinQVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The entry of QinQ-VLAN table."
        INDEX { 
                hwL2QinQVlanIfIndex, 
                hwL2QinQVlanIdBegin, 
                hwL2QinQVlanIdEnd, 
                hwL2QinQVlanInnerVlanIdBegin, 
                hwL2QinQVlanInnerVlanIdEnd, 
                hwL2QinQVlan8021pBegin, 
                hwL2QinQVlan8021pEnd, 
                hwL2QinQVlanEtherType 
        }
        ::= { hwL2QinQVlanTable 1 }   
        
    HwL2QinQVlanEntry ::=
        SEQUENCE { 
            hwL2QinQVlanIfIndex
                InterfaceIndex,
            hwL2QinQVlanIdBegin
                VlanId,
            hwL2QinQVlanIdEnd
                VlanId,
            hwL2QinQVlanInnerVlanIdBegin
                VlanIdOrNone,
            hwL2QinQVlanInnerVlanIdEnd
                VlanIdOrNone,
            hwL2QinQVlan8021pBegin
                Integer32,
            hwL2QinQVlan8021pEnd
                Integer32,
            hwL2QinQVlanEtherType
                Integer32,
            hwL2QinQVlanMode
                INTEGER,
            hwL2QinQVlanChangedVlanId
                VlanId,
            hwL2QinQVlanChangedInnerVlanId
                VlanIdOrNone,
            hwL2QinQVlanRemark
                Integer32,
            hwL2QinQVlanMapStackVlanId
                VlanIdOrNone,
            hwL2QinQVlanRowStatus
                RowStatus,
            hwL2QinQVlanInnerRemark
                Integer32
        }

    hwL2QinQVlanIfIndex OBJECT-TYPE
        SYNTAX InterfaceIndex
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The index number of QinQ-VLAN port."
        ::= { hwL2QinQVlanEntry 1 }

    hwL2QinQVlanIdBegin OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The begin VLAN ID of outside."
        ::= { hwL2QinQVlanEntry 2 }

    hwL2QinQVlanIdEnd OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The end VLAN ID of outside."
        ::= { hwL2QinQVlanEntry 3 }

    hwL2QinQVlanInnerVlanIdBegin OBJECT-TYPE
        SYNTAX VlanIdOrNone
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The begin VLAN ID of inside."
        ::= { hwL2QinQVlanEntry 4 }

    hwL2QinQVlanInnerVlanIdEnd OBJECT-TYPE
        SYNTAX VlanIdOrNone
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The end VLAN ID of inside."
        ::= { hwL2QinQVlanEntry 5 }

    hwL2QinQVlan8021pBegin OBJECT-TYPE
        SYNTAX Integer32(0..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The begin number of 8021p."   
        ::= { hwL2QinQVlanEntry 6 }         

    hwL2QinQVlan8021pEnd OBJECT-TYPE
        SYNTAX Integer32(0..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The end number of 8021p." 
        ::= { hwL2QinQVlanEntry 7 } 

    hwL2QinQVlanEtherType OBJECT-TYPE
        SYNTAX Integer32(0..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The value of Ethernet Type."
        ::= { hwL2QinQVlanEntry 8 }        

    hwL2QinQVlanMode OBJECT-TYPE
        SYNTAX INTEGER
        {
            stacking(1),
            mapping(2),
            cosstacking(3),
            cosmapping(4),
            mapping2to1(5),
            mapping2to2(6) 
        }
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The mode of QinQ-VLAN configuration."
        ::= { hwL2QinQVlanEntry 9 }

    hwL2QinQVlanChangedVlanId OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The changed VLAN ID of outside."
        ::= { hwL2QinQVlanEntry 10 }

    hwL2QinQVlanChangedInnerVlanId OBJECT-TYPE
        SYNTAX VlanIdOrNone
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The changed VLAN ID of inside."
        ::= { hwL2QinQVlanEntry 11 }

    hwL2QinQVlanRemark OBJECT-TYPE
        SYNTAX Integer32(0..8)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The remark number of outside 8021p.If the value is 8, the priority in
                     the outer tag is not changed."
        ::= { hwL2QinQVlanEntry 12 } 
        
    hwL2QinQVlanMapStackVlanId OBJECT-TYPE
        SYNTAX VlanIdOrNone
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The map VLAN ID for inside after stacking action."
        ::= { hwL2QinQVlanEntry 13 }

    hwL2QinQVlanRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "This table can read, create and delete."
        ::= { hwL2QinQVlanEntry 14 }   
    
    hwL2QinQVlanInnerRemark OBJECT-TYPE
        SYNTAX Integer32(0..8)
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The remark number of the changed VLAN for inside.
                     If the value is 8, the priority in tag is not changed."   
        ::= { hwL2QinQVlanEntry 15 }

    hwL2UntagAddDTagTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2UntagAddDTagEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The table of untagged VLAN add double tagged VLAN configuration."
        ::= { hwL2VlanApply 37 }

    hwL2UntagAddDTagEntry OBJECT-TYPE
        SYNTAX HwL2UntagAddDTagEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The entry of untagged VLAN add double tagged VLAN table."
        INDEX { hwL2UntagAddDTagPortIndex }
        ::= { hwL2UntagAddDTagTable 1 }   
        
    HwL2UntagAddDTagEntry ::=
        SEQUENCE { 
            hwL2UntagAddDTagPortIndex
                Integer32,
            hwL2UntagAddDTagOuterVlanId
                VlanId,
            hwL2UntagAddDTagInnerVlanId
                VlanId,
            hwL2UntagAddDTagRowStatus
                RowStatus
        }

    hwL2UntagAddDTagPortIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "The port index number of interface."
        ::= { hwL2UntagAddDTagEntry 1 }

    hwL2UntagAddDTagOuterVlanId OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The outer VLAN ID."
        ::= { hwL2UntagAddDTagEntry 2 }

    hwL2UntagAddDTagInnerVlanId OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "The inner VLAN ID."
        ::= { hwL2UntagAddDTagEntry 3 }

    hwL2UntagAddDTagRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION "This table can read, create and delete."
        ::= { hwL2UntagAddDTagEntry 4 } 

    hwL2VlanVoiceVlan8021p  OBJECT-TYPE
        SYNTAX  Integer32(0..7)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "It indicates the IEEE 802.1Q priority of the voice VLAN and the 
                     default value is 6."
        ::= { hwL2VlanApply 38 }  
        
    hwL2VlanVoiceVlanDscp  OBJECT-TYPE
        SYNTAX  Integer32(0..63)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "It indicates the Differentiated Services CodePoint priority of 
                     the voice VLAN and the default value is 0x2e."
        ::= { hwL2VlanApply 39 }      
                                  
    hwL2QinQIsolateTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2QinQIsolateEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Configuration table."
        ::= { hwL2VlanApply  40 }

    hwL2QinQIsolateEntry  OBJECT-TYPE
        SYNTAX HwL2QinQIsolateEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "QinQ-VLAN isolate port configuration table."
        INDEX   { hwL2QinQIsolatePortIndex, hwL2QinQIsolateVlanId, hwL2QinQIsolatePeVlanId }
        ::= { hwL2QinQIsolateTable 1}

    HwL2QinQIsolateEntry  ::=
    SEQUENCE {
        hwL2QinQIsolatePortIndex        Integer32,
        hwL2QinQIsolateVlanId         VlanId,
        hwL2QinQIsolatePeVlanId         VlanIdOrNone,
        hwL2QinQIsolateCeVlanListLow    OCTET STRING,
        hwL2QinQIsolateCeVlanListHigh   OCTET STRING,
        hwL2QinQTagType                 INTEGER
        }

    hwL2QinQIsolatePortIndex  OBJECT-TYPE
        SYNTAX  Integer32(1..65535)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Index number of QinQ-port isolate port, use it as the Index."
        ::= { hwL2QinQIsolateEntry 1 }

    hwL2QinQIsolateVlanId  OBJECT-TYPE
        SYNTAX  VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The global vlan identifier that is associated with the QinQ-port, use it as the Index."
        ::= { hwL2QinQIsolateEntry 2 }
                
    hwL2QinQIsolatePeVlanId  OBJECT-TYPE
        SYNTAX  VlanIdOrNone
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Outside vlan-id of QinQ-port ,use it as the Index."
        ::= { hwL2QinQIsolateEntry 3 }

    hwL2QinQIsolateCeVlanListLow  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(256))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION 
           "The possible value of the CE vlan-id list."
        ::= { hwL2QinQIsolateEntry 4 }
    
    hwL2QinQIsolateCeVlanListHigh  OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(256))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION 
           "The possible value of the CE vlan-id list."
        ::= { hwL2QinQIsolateEntry 5 }    
        
    hwL2QinQTagType OBJECT-TYPE
        SYNTAX INTEGER
        {
            dot1q(1),
            qinq(2)
        }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION "The mode of QinQ-VLAN configuration."
        ::= { hwL2QinQIsolateEntry 6 }            
                            
   hwL2IfStatVlanCfgTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2IfStatVlanCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The table contains statistics enable configuration for the port and vlan."
        ::= { hwL2VlanStatistics 1 }
    
    
    hwL2IfStatVlanCfgEntry OBJECT-TYPE
        SYNTAX HwL2IfStatVlanCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Entries of vlan and port statistics enable table."
        INDEX { hwL2IfStatVlanCfgPortIndex,hwL2IfStatVlanCfgVlanId }
        ::= { hwL2IfStatVlanCfgTable 1 }
        
    HwL2IfStatVlanCfgEntry ::=
        SEQUENCE { 
                    hwL2IfStatVlanCfgPortIndex   
                        Integer32,
                    hwL2IfStatVlanCfgVlanId 
                        VlanId,
                    hwL2IfStatVlanCfgEnableFlag
                        EnabledStatus,
                    hwL2IfStatVlanCfgRowStatus 
                        RowStatus
                }
    
    hwL2IfStatVlanCfgPortIndex OBJECT-TYPE
        SYNTAX Integer32 (1..512)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The virtual index of L2 Interface."
        ::= { hwL2IfStatVlanCfgEntry 1 }
        
    
    hwL2IfStatVlanCfgVlanId  OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The vlan-id of packets'tag that's received or sent out from the port."
        ::= { hwL2IfStatVlanCfgEntry 2 }
        
    
    hwL2IfStatVlanCfgEnableFlag  OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The flag of enable the statistic function based on vlan 
           in the interface."
        ::= { hwL2IfStatVlanCfgEntry 11 }
    
    
    hwL2IfStatVlanCfgRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Used for controlling the creation and deletion of this
           row. All writable objects in this row may be modified at any time.
           If a Network Management Application attempts to delete a conceptual
           row by setting this object to 'destroy' and there are one or more entries
           in hwL2IfStatVlanCfgTable pointing to the row, the agent MUST also
           destroy the corresponding entries in hwL2IfStatVlanCfgTable."
        ::= { hwL2IfStatVlanCfgEntry 12 }
        

    hwL2IfStat8021pCfgTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2IfStat8021pCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The table contains statistics enable for the port and 8021p."
        ::= { hwL2VlanStatistics 2 }
        

    hwL2IfStat8021pCfgEntry OBJECT-TYPE
        SYNTAX HwL2IfStat8021pCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Entries of port and 8021p statistics enable table."
        INDEX { hwL2IfStat8021pCfgPortIndex,hwL2IfStat8021pCfg8021p }
        ::= { hwL2IfStat8021pCfgTable 1 }
        
    HwL2IfStat8021pCfgEntry ::=
        SEQUENCE { 
                    hwL2IfStat8021pCfgPortIndex   
                        Integer32,
                    hwL2IfStat8021pCfg8021p 
                        Integer32,
                    hwL2IfStat8021pCfgEnableFlag
                        EnabledStatus,
                    hwL2IfStat8021pCfgRowStatus 
                        RowStatus
                }

    hwL2IfStat8021pCfgPortIndex OBJECT-TYPE
        SYNTAX Integer32 (1..512)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The virtual index of L2 Interface."
        ::= { hwL2IfStat8021pCfgEntry 1 }

    hwL2IfStat8021pCfg8021p  OBJECT-TYPE
        SYNTAX     Integer32 (0..7)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The 8021p of packet's tag that's received or sent from the port."
        ::= { hwL2IfStat8021pCfgEntry 2 }

    hwL2IfStat8021pCfgEnableFlag  OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            " The flag of enable the static function based on 8021p 
            in the interface."
        ::= { hwL2IfStat8021pCfgEntry 11 }

    hwL2IfStat8021pCfgRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Used for controlling the creation and deletion of this
           row. All writable objects in this row may be modified at any time.
           If a Network Management Application attempts to delete a conceptual
           row by setting this object to 'destroy' and there are one or more entries
           in hwL2IfStat8021pCfgTable pointing to the row, the agent MUST also
           destroy the corresponding entries in hwL2IfStat8021pCfgTable."
        ::= { hwL2IfStat8021pCfgEntry 12 }
        
    hwL2IfStat8021pAndVlanCfgTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2IfStat8021pAndVlanCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table contains statistics enable for the port, vlan and 8021p."
        ::= { hwL2VlanStatistics 3 }

    hwL2IfStat8021pAndVlanCfgEntry OBJECT-TYPE
        SYNTAX HwL2IfStat8021pAndVlanCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Entries of port, 8021p and vlan statistics enable table."
        INDEX { hwL2IfStat8021pAndVlanCfgPortIndex,hwL2IfStat8021pAndVlanCfgVlanId,
                hwL2IfStat8021pAndVlanCfg8021p }
        ::= { hwL2IfStat8021pAndVlanCfgTable 1 }
        
    HwL2IfStat8021pAndVlanCfgEntry ::=
        SEQUENCE { 
                    hwL2IfStat8021pAndVlanCfgPortIndex   
                        Integer32,
                    hwL2IfStat8021pAndVlanCfgVlanId
                        VlanId,
                    hwL2IfStat8021pAndVlanCfg8021p 
                        Integer32,                    
                    hwL2IfStat8021pAndVlanCfgEnableFlag
                        EnabledStatus,
                    hwL2IfStat8021pAndVlanCfgRowStatus 
                        RowStatus
                }

    hwL2IfStat8021pAndVlanCfgPortIndex OBJECT-TYPE
        SYNTAX Integer32 (1..512)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The virtual index of L2 Interface."
        ::= { hwL2IfStat8021pAndVlanCfgEntry 1 }

    

    hwL2IfStat8021pAndVlanCfgVlanId  OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The vlan-id of packet's tag that's received or sent out from the port."
        ::= { hwL2IfStat8021pAndVlanCfgEntry 2 }
        
        
    hwL2IfStat8021pAndVlanCfg8021p  OBJECT-TYPE
        SYNTAX     Integer32 (0..7)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The 8021p value of packet's tag that's received or sent from the port."
        ::= { hwL2IfStat8021pAndVlanCfgEntry 3 }


    hwL2IfStat8021pAndVlanCfgEnableFlag  OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "The Flag of enable the static function based on vlan-id and 8021p
           in the interface."
        ::= { hwL2IfStat8021pAndVlanCfgEntry 11 }

    hwL2IfStat8021pAndVlanCfgRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION 
           "Used for controlling the creation and deletion of this
           row. All writable objects in this row may be modified at any time.
           If a Network Management Application attempts to delete a conceptual
           row by setting this object to 'destroy' and there are one or more entries
           in hwL2IfStat8021pAndVlanCfgTable pointing to the row, the agent MUST also
           destroy the corresponding entries in hwL2IfStat8021pAndVlanCfgTable."
        ::= { hwL2IfStat8021pAndVlanCfgEntry 12 }
    
    hwL2VlanStatTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2VlanStatEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table lists the statistics about packets in a VLAN, including the number of packets and bytes sent and received by the VLAN."
        ::= { hwL2VlanStatistics 4 }

    hwL2VlanStatEntry OBJECT-TYPE
        SYNTAX HwL2VlanStatEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Entries of vlan statistics table."
        INDEX { hwL2VlanStatVlanId }
        ::= { hwL2VlanStatTable 1 }
    
    HwL2VlanStatEntry ::=
        SEQUENCE { 
            hwL2VlanStatVlanId 
                VlanId,
            hwL2VlanStatInTotalPkts
                Counter64,
            hwL2VlanStatInTotalBytes 
                Counter64,
            hwL2VlanStatOutTotalPkts
                Counter64,
            hwL2VlanStatOutTotalBytes
                Counter64,
            hwL2VlanStatUnknownUcastDiscardPkts
                Counter64,         
            hwL2VlanStatUnknownMcastDiscardPkts
                Counter64, 
            hwL2VlanStatBcastDiscardPkts 
                Counter64,
            hwL2VlanStatInUcastPkts
                Counter64,
            hwL2VlanStatInUcastBytes
                Counter64,
            hwL2VlanStatOutUcastPkts
                Counter64,
            hwL2VlanStatOutUcastBytes
                Counter64,
            hwL2VlanStatInMcastPkts
                Counter64,
            hwL2VlanStatInMcastBytes
                Counter64,
            hwL2VlanStatOutMcastPkts
                Counter64,
            hwL2VlanStatOutMcastBytes
                Counter64,
            hwL2VlanStatInBcastPkts
                Counter64,
            hwL2VlanStatInBcastBytes
                Counter64,
            hwL2VlanStatOutBcastPkts
                Counter64,
            hwL2VlanStatOutBcastBytes
                Counter64,
            hwL2VlanStatResetFlag
                EnabledStatus
         }

    
    hwL2VlanStatVlanId  OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The vlan-id."
        ::= { hwL2VlanStatEntry 1 }
        
        
    hwL2VlanStatInTotalPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The number of received packets."
        ::= { hwL2VlanStatEntry 2 }
    
    
    hwL2VlanStatInTotalBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The byte number of received packets."
        ::= { hwL2VlanStatEntry 3 }
        
    
    hwL2VlanStatOutTotalPkts  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION  
           "The number of sent packets."
        ::= { hwL2VlanStatEntry 4 }
        
    
    hwL2VlanStatOutTotalBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The byte number of sent packets."
        ::= { hwL2VlanStatEntry 5 }
    
    
    hwL2VlanStatUnknownUcastDiscardPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The number of aborted unknown unicast packets."
        ::= { hwL2VlanStatEntry 6 }     
        
    
    hwL2VlanStatUnknownMcastDiscardPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The number of aborted unknown multicast packets."
        ::= { hwL2VlanStatEntry 7 }   
    
    
    hwL2VlanStatBcastDiscardPkts  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The number of aborted broadcast packets."
        ::= { hwL2VlanStatEntry 8 }

        
    hwL2VlanStatInUcastPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of received unicast packets."
        ::= { hwL2VlanStatEntry 9 } 
        
        
    hwL2VlanStatInUcastBytes OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of received unicast packets' bytes."
        ::= { hwL2VlanStatEntry 10 } 
        
        
    hwL2VlanStatOutUcastPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of sent unicast packets."
        ::= { hwL2VlanStatEntry 11 }
        
        
    hwL2VlanStatOutUcastBytes OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of sent unicast packets' bytes."
        ::= { hwL2VlanStatEntry 12 }
        
        
    hwL2VlanStatInMcastPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of received multicast packets."
        ::= { hwL2VlanStatEntry 13 }
        
        
    hwL2VlanStatInMcastBytes OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of received multicast packets' bytes."
        ::= { hwL2VlanStatEntry 14 }
        
        
    hwL2VlanStatOutMcastPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of sent multicast packets."
        ::= { hwL2VlanStatEntry 15 }
        
        
    hwL2VlanStatOutMcastBytes OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of sent multicast packets' bytes."
        ::= { hwL2VlanStatEntry 16 }
        
        
    hwL2VlanStatInBcastPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of received broadcast packets."
        ::= { hwL2VlanStatEntry 17 }
        
        
    hwL2VlanStatInBcastBytes OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of received broadcast packets' bytes."
        ::= { hwL2VlanStatEntry 18 }
        
        
    hwL2VlanStatOutBcastPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of sent broadcast packets."
        ::= { hwL2VlanStatEntry 19 }
        
        
    hwL2VlanStatOutBcastBytes OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of sent broadcast packets."
        ::= { hwL2VlanStatEntry 20 }
        
    
    hwL2VlanStatResetFlag  OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION 
           "The flag of reset."
        ::= { hwL2VlanStatEntry 21 }
        
    
    hwL2IfStatVlanTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2IfStatVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table contains statistics information for the port and vlan."
        ::= { hwL2VlanStatistics 5 }
    
    
    hwL2IfStatVlanEntry OBJECT-TYPE
        SYNTAX HwL2IfStatVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Entries of vlan and port statistics table."
        INDEX { hwL2IfStatVlanPortIndex,hwL2IfStatVlanId }
        ::= { hwL2IfStatVlanTable 1 }
    
    HwL2IfStatVlanEntry ::=
        SEQUENCE { 
            hwL2IfStatVlanPortIndex   
                Integer32,
            hwL2IfStatVlanId 
                VlanId,
            hwL2IfStatVlanInTotalPkts
                Counter64,
            hwL2IfStatVlanInTotalBytes 
                Counter64,
            hwL2IfStatVlanOutTotalPkts
                Counter64,
            hwL2IfStatVlanOutTotalBytes 
                Counter64,
            hwL2IfStatVlanInPktsRate
                Gauge32,
            hwL2IfStatVlanInBytesRate
                Gauge32,
            hwL2IfStatVlanOutPktsRate
                Gauge32,
            hwL2IfStatVlanOutBytesRate
                Gauge32,
            hwL2IfStatVlanInUcastPkts
                Counter64, 
            hwL2IfStatVlanInUcastBytes
                Counter64,
            hwL2IfStatVlanOutUcastPkts
                Counter64,   
            hwL2IfStatVlanOutUcastBytes
                Counter64,
            hwL2IfStatVlanInMcastPkts
                Counter64, 
            hwL2IfStatVlanInMcastBytes
                Counter64,
            hwL2IfStatVlanOutMcastPkts
                Counter64, 
            hwL2IfStatVlanOutMcastBytes
                Counter64,
            hwL2IfStatVlanInBcastPkts
                Counter64, 
            hwL2IfStatVlanInBcastBytes
                Counter64,
            hwL2IfStatVlanOutBcastPkts
                Counter64,  
            hwL2IfStatVlanOutBcastBytes
                Counter64,
            hwL2IfStatVlanResetFlag
                EnabledStatus            
         }

    hwL2IfStatVlanPortIndex OBJECT-TYPE
        SYNTAX Integer32 (1..512)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The virtual Index of L2 Interface."
        ::= { hwL2IfStatVlanEntry 1 }
        
    
    hwL2IfStatVlanId  OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The vlan-id of packets'tag that's received or sent out from the port."
        ::= { hwL2IfStatVlanEntry 2 }
    
    
    hwL2IfStatVlanInTotalPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The number of received packets."
        ::= { hwL2IfStatVlanEntry 3 }
    
    
    hwL2IfStatVlanInTotalBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " The bytes of received packets. "
        ::= { hwL2IfStatVlanEntry 4 }
    
    
    hwL2IfStatVlanOutTotalPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of sent packets."
        ::= { hwL2IfStatVlanEntry 5 }
    
    
    hwL2IfStatVlanOutTotalBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The bytes of sent packets."
        ::= { hwL2IfStatVlanEntry 6 }
        
    
    hwL2IfStatVlanInPktsRate  OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " The rate of received packets."
        ::= { hwL2IfStatVlanEntry 7 }
        
    
    hwL2IfStatVlanInBytesRate  OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The rate of received bytes."
        ::= { hwL2IfStatVlanEntry 8 }
        
    
    hwL2IfStatVlanOutPktsRate  OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The rate of sent packet."
        ::= { hwL2IfStatVlanEntry 9 }
        
    
    hwL2IfStatVlanOutBytesRate  OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The rate of sent bytes."
        ::= { hwL2IfStatVlanEntry 10 }
        
    
    hwL2IfStatVlanInUcastPkts  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " The number of unicast packets received."
        ::= { hwL2IfStatVlanEntry 11 }
         
    
    hwL2IfStatVlanInUcastBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " The number of unicast bytes received."
        ::= { hwL2IfStatVlanEntry 12 }
        
    
    hwL2IfStatVlanOutUcastPkts  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The packet number of unicast packets sent."
        ::= { hwL2IfStatVlanEntry 13 } 
        
    
    hwL2IfStatVlanOutUcastBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of unicast bytes sent."
        ::= { hwL2IfStatVlanEntry 14 }

        
    
    hwL2IfStatVlanInMcastPkts  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " The number of multicast packets received."
        ::= { hwL2IfStatVlanEntry 15 } 
        
    
    hwL2IfStatVlanInMcastBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " The number of multicast bytes received."
        ::= { hwL2IfStatVlanEntry 16 }
        
    
    hwL2IfStatVlanOutMcastPkts  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of multicast packets sent."
        ::= { hwL2IfStatVlanEntry 17 }   
        
    
    hwL2IfStatVlanOutMcastBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of multicast bytes sent."
        ::= { hwL2IfStatVlanEntry 18 }
        
    
    hwL2IfStatVlanInBcastPkts  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " The number of broadcast packets received."
        ::= { hwL2IfStatVlanEntry 19 }  
        
    
    hwL2IfStatVlanInBcastBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " The number of broadcast bytes received. "
        ::= { hwL2IfStatVlanEntry 20 }    
        
    
    hwL2IfStatVlanOutBcastPkts  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of broadcast packets sent."
        ::= { hwL2IfStatVlanEntry 21 }  
        
    
    hwL2IfStatVlanOutBcastBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of broadcast bytes sent."
        ::= { hwL2IfStatVlanEntry 22 }    
        
    
    hwL2IfStatVlanResetFlag  OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            " The flag of reset the statistic counter. "
        ::= { hwL2IfStatVlanEntry 23 }
        
    
    hwL2IfStat8021pTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2IfStat8021pEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The table contains statistics information for the port and 8021p."
        ::= { hwL2VlanStatistics 6 }
    
    
    hwL2IfStat8021pEntry OBJECT-TYPE
        SYNTAX HwL2IfStat8021pEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Entries of port and 8021p statistics table."
        INDEX { hwL2IfStat8021pPortIndex,hwL2IfStat8021p }
        ::= { hwL2IfStat8021pTable 1 }
    
    HwL2IfStat8021pEntry ::=
        SEQUENCE { 
            hwL2IfStat8021pPortIndex 
                Integer32,
            hwL2IfStat8021p
                Integer32,
            hwL2IfStat8021pInTotalPkts
                Counter64,
            hwL2IfStat8021pInTotalBytes 
                Counter64,
            hwL2IfStat8021pOutTotalPkts
                Counter64,
            hwL2IfStat8021pOutTotalBytes 
                Counter64,
            hwL2IfStat8021pInPktsRate
                Gauge32,
            hwL2IfStat8021pInBytsRate
                Gauge32,
            hwL2IfStat8021pOutPktsRate
                Gauge32,
            hwL2IfStat8021pOutBytesRate
                Gauge32,
            hwL2IfStat8021pResetFlag
                EnabledStatus
         }

    
    hwL2IfStat8021pPortIndex  OBJECT-TYPE
        SYNTAX Integer32 (1..512)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The virtual index of L2 Interface."
        ::= { hwL2IfStat8021pEntry 1 }
    
    
    hwL2IfStat8021p OBJECT-TYPE
        SYNTAX Integer32 (0..7)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The priority of the packet's tag."
        ::= { hwL2IfStat8021pEntry 2 }
    
    
    hwL2IfStat8021pInTotalPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The number of received packets."
        ::= { hwL2IfStat8021pEntry 3 }
    
    
    hwL2IfStat8021pInTotalBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " The bytes of received packets. "
        ::= { hwL2IfStat8021pEntry 4 }
    
    
    hwL2IfStat8021pOutTotalPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The number of sent packets."
        ::= { hwL2IfStat8021pEntry 5 }
    
    
    hwL2IfStat8021pOutTotalBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The bytes of sent packets."
        ::= { hwL2IfStat8021pEntry 6 }
        
    
    hwL2IfStat8021pInPktsRate  OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " The rate of received packets. "
        ::= { hwL2IfStat8021pEntry 7 }
        
    
    hwL2IfStat8021pInBytsRate  OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The rate of received bytes."
        ::= { hwL2IfStat8021pEntry 8 }
        
    
    hwL2IfStat8021pOutPktsRate  OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The rate of the sent packets."
        ::= { hwL2IfStat8021pEntry 9 }
        
    
    hwL2IfStat8021pOutBytesRate  OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
           "The rate of sent bytes."
        ::= { hwL2IfStat8021pEntry 10 }
        
    
    hwL2IfStat8021pResetFlag  OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            " The flag of reset the statistic counter."
        ::= { hwL2IfStat8021pEntry 11 }

    
    hwL2IfStat8021pAndVlanTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwL2IfStat8021pAndVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "The table contains statistics information for the port ,8021p and vlan-id."
        ::= { hwL2VlanStatistics 7 }
    
    
    hwL2IfStat8021pAndVlanEntry OBJECT-TYPE
        SYNTAX HwL2IfStat8021pAndVlanEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Entries of port statistics table based on 8021p and vlan-id fields."
        INDEX { hwL2IfStat8021pAndVlanPortIndex,hwL2IfStat8021pAndVlanVlanId,hwL2IfStat8021pAndVlan8021p }
        ::= { hwL2IfStat8021pAndVlanTable 1 }
    
    HwL2IfStat8021pAndVlanEntry ::=
        SEQUENCE { 
            hwL2IfStat8021pAndVlanPortIndex 
                Integer32,
            hwL2IfStat8021pAndVlanVlanId
                VlanId,
            hwL2IfStat8021pAndVlan8021p
                Integer32,    
            hwL2IfStat8021pAndVlanInTotalPkts
                Counter64,
            hwL2IfStat8021pAndVlanInTotalBytes 
                Counter64,
            hwL2IfStat8021pAndVlanInPktsRate
                Gauge32,
            hwL2IfStat8021pAndVlanInBytsRate
                Gauge32,
            hwL2IfStat8021pAndVlanResetFlag
                EnabledStatus
         }

    
    hwL2IfStat8021pAndVlanPortIndex  OBJECT-TYPE
        SYNTAX Integer32 (1..512)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The virtual Index of L2 Interface."
        ::= { hwL2IfStat8021pAndVlanEntry 1 }
    
    
    hwL2IfStat8021pAndVlanVlanId OBJECT-TYPE
        SYNTAX VlanId
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
           "Vlan-id."
        ::= { hwL2IfStat8021pAndVlanEntry 2 }
    
    
    hwL2IfStat8021pAndVlan8021p OBJECT-TYPE
        SYNTAX Integer32 (0..7)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The priority in the 8021p packets'tag."
        ::= { hwL2IfStat8021pAndVlanEntry 3 }
        
    
    hwL2IfStat8021pAndVlanInTotalPkts OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The number of received packets."
        ::= { hwL2IfStat8021pAndVlanEntry 4 }
    
    
    hwL2IfStat8021pAndVlanInTotalBytes  OBJECT-TYPE
        SYNTAX Counter64
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The bytes of received packets."
        ::= { hwL2IfStat8021pAndVlanEntry 5 }
        
    
    hwL2IfStat8021pAndVlanInPktsRate  OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The rate of received packets. "
        ::= { hwL2IfStat8021pAndVlanEntry 6 }
        
    
    hwL2IfStat8021pAndVlanInBytsRate  OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " The rate of received bytes. "
        ::= { hwL2IfStat8021pAndVlanEntry 7 }
            
    
    hwL2IfStat8021pAndVlanResetFlag  OBJECT-TYPE
        SYNTAX EnabledStatus
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            " The flag of reset statistic counters."
        ::= { hwL2IfStat8021pAndVlanEntry 8 }

    hwL2VlanSwitchPSTable OBJECT-TYPE
    SYNTAX SEQUENCE OF HwL2VlanSwitchPSEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION 
       "The table to config the vlan switch by Port+SVlan index."
    ::= { hwL2VlanStatistics 8 }

    hwL2VlanSwitchPSEntry OBJECT-TYPE
    SYNTAX HwL2VlanSwitchPSEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION 
       "The entry of the vlan switch IfIndex+SVlan table."
    INDEX { hwL2VlanSwitchPSIfIndex, hwL2VlanSwitchPSSVlanId, hwL2VlanSwitchPSCVlanId }
    ::= { hwL2VlanSwitchPSTable 1 }

    HwL2VlanSwitchPSEntry ::=
    SEQUENCE { 
        hwL2VlanSwitchPSIfIndex
            InterfaceIndex,           
        hwL2VlanSwitchPSSVlanId
            Integer32,
        hwL2VlanSwitchPSCVlanId
            Integer32,
           hwL2VlanSwitchPSInputPkts
                  Counter64,
           hwL2VlanSwitchPSInputBytes
                  Counter64,      
        hwL2VlanSwitchPSOutputPkts
               Counter64,
        hwL2VlanSwitchPSOutputBytes
               Counter64,     
           hwL2VlanSwitchPSResetFlag
                     EnabledStatus,
        hwL2VlanSwitchPSEnableFlag 
               EnabledStatus                     
     }

     hwL2VlanSwitchPSIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The interface index."
    ::= { hwL2VlanSwitchPSEntry 1 }

     hwL2VlanSwitchPSSVlanId OBJECT-TYPE
    SYNTAX Integer32(1..4094)
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Vlan-id."
    ::= { hwL2VlanSwitchPSEntry 2 }

     hwL2VlanSwitchPSCVlanId OBJECT-TYPE
    SYNTAX Integer32(0..4096)
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "CVlan-id."
    ::= { hwL2VlanSwitchPSEntry 3 }

     hwL2VlanSwitchPSInputPkts OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The number of inbound discard packets."
    ::= { hwL2VlanSwitchPSEntry 4 }

     hwL2VlanSwitchPSInputBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The number of inbound discard bytes."
    ::= { hwL2VlanSwitchPSEntry 5 }

     hwL2VlanSwitchPSOutputPkts OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The number of outbound discard packets."
    ::= { hwL2VlanSwitchPSEntry 6 }

     hwL2VlanSwitchPSOutputBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The number of outbound discard bytes."
    ::= { hwL2VlanSwitchPSEntry 7 }

     hwL2VlanSwitchPSResetFlag  OBJECT-TYPE
    SYNTAX EnabledStatus
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION 
       "The flag of reset statistics."
    ::= { hwL2VlanSwitchPSEntry 8 }

     hwL2VlanSwitchPSEnableFlag  OBJECT-TYPE
    SYNTAX EnabledStatus
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION 
       "The flag of enable statistics."
    ::= { hwL2VlanSwitchPSEntry 9 }

   
    
    hwL2VlanTraps OBJECT IDENTIFIER ::= { hwL2VlanMngObjects 4 }

    
    hwL2VlanUnkownPacketAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, hwL2VlanStatUnknownUcastDiscardPkts, hwL2VlanStatUnknownMcastDiscardPkts, hwL2VlanStatBcastDiscardPkts}
            STATUS current
            DESCRIPTION 
               "Warning of unkown Packets in vlan."
            ::= { hwL2VlanTraps 1 }
    hwVcmpServerMacConflict NOTIFICATION-TYPE
            OBJECTS { hwVcmpDeviceMac}
            STATUS current
            DESCRIPTION 
               "More than one server exists in the VCMP domain."
            ::= { hwL2VlanTraps 2 }

    hwVcmpRevisionConflict NOTIFICATION-TYPE
            OBJECTS { hwVcmpDeviceMac}
            STATUS current
            DESCRIPTION 
               " A server received a VCMP packet with a higher revision number."
            ::= { hwL2VlanTraps 3 }

    hwMuxVlanGroupCountExceedThreshold NOTIFICATION-TYPE
            OBJECTS { hwPrincipalVlanID, hwMuxVlanUpperThreshold}
            STATUS current
            DESCRIPTION 
               "The number of the group VLANs in the principal VLAN exceeded the upper threshold."
            ::= { hwL2VlanTraps 4 }

    hwMuxVlanGroupCountExceedThresholdResume NOTIFICATION-TYPE
            OBJECTS { hwPrincipalVlanID, hwMuxVlanLowerThreshold}
            STATUS current
            DESCRIPTION 
               "The number of the group VLANs in the principal VLAN fell below the lower threshold."
            ::= { hwL2VlanTraps 5 }
            
    hwVlantransCountExceedThreshold NOTIFICATION-TYPE
            OBJECTS { hwVlantransIfIndex, hwVlantransUpperThreshold}
            STATUS current
            DESCRIPTION 
               "The number of VLAN mapping or VLAN stacking configurations on the interface exceeded the upper threshold."
            ::= { hwL2VlanTraps 6 }
            
    hwVlantransCountExceedThresholdResume NOTIFICATION-TYPE
            OBJECTS { hwVlantransIfIndex, hwVlantransLowerThreshold}
            STATUS current
            DESCRIPTION 
               "The number of the VLAN mapping and VLAN stacking configurations on the interface fell below the threshold."
            ::= { hwL2VlanTraps 7 }
	
     hwL2VlanTrapObjects OBJECT IDENTIFIER ::= { hwL2VlanMngObjects 5 }
     hwVcmpDeviceMac OBJECT-TYPE
            SYNTAX MacAddress
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "MAC address of a device running VCMP"
            ::= { hwL2VlanTrapObjects 1 }
            
     hwPrincipalVlanID OBJECT-TYPE
            SYNTAX Integer32 (1..4094)
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Principal VLAN ID of a MUX VLAN."
            ::= { hwL2VlanTrapObjects 2 }
            
     hwMuxVlanUpperThreshold OBJECT-TYPE
            SYNTAX Integer32 (1..128)
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Upper threshold for the number of group VLANs in a principal VLAN."
            ::= { hwL2VlanTrapObjects 3 }
            
     hwMuxVlanLowerThreshold OBJECT-TYPE
            SYNTAX Integer32 (1..128)
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Lower threshold for the number of group VLANs in a principal VLAN."
            ::= { hwL2VlanTrapObjects 4 }
            
     hwVlantransIfIndex OBJECT-TYPE
            SYNTAX Integer32 (1..2147483647)
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Index of the interface that has vlan mapping or vlan stacking configured."
            ::= { hwL2VlanTrapObjects 5 }
            
     hwVlantransUpperThreshold OBJECT-TYPE
            SYNTAX Integer32 (0..2147483647)
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Upper threshold for the number of vlan mapping and vlan stacking configurations on the interface."
            ::= { hwL2VlanTrapObjects 6 }
            
     hwVlantransLowerThreshold OBJECT-TYPE
            SYNTAX Integer32 (0..2147483647)
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Lower threshold for the number of vlan mapping and vlan stacking configurations on the interface."
            ::= { hwL2VlanTrapObjects 7 }

-- ============================================================
-- IEEE 802.1Q MIB - Conformance Information
-- ============================================================
hwL2vlanConformance OBJECT IDENTIFIER ::= { hwL2Vlan 2 }

hwL2vlanGroups OBJECT IDENTIFIER ::= { hwL2vlanConformance 1 }

hwL2vlanCompliances OBJECT IDENTIFIER  ::= { hwL2vlanConformance 2 }                               
-- ============================================================
-- units of conformance
-- ============================================================

hwL2VlanMIBTableGroup OBJECT-GROUP
    OBJECTS {
        hwL2VlanDescr    ,
        hwL2VlanPortList   ,
        hwL2VlanType    ,
        hwL2VlanUnknownUnicastProcessing   ,
        hwL2VlanIfIndex   ,
        hwL2VlanMacLearn ,
        hwL2VlanCreateStatus   ,
        hwL2VlanMulticast ,
        hwL2VlanAdminStatus ,
        hwL2VlanStatisStatus ,
        hwL2VlanRowStatus ,
        hwL2VlanBcast ,
        hwL2VlanUnknownMulticastProcessing ,
        hwL2VlanProperty ,
        hwL2VlanAgingTime,
        hwL2VlanName,
        hwL2VlanSmartMacLearn,
        hwL2VlanServiceName,
        hwL2VlanManagementVlan,
        hwL2VlanDynamicVlan
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing device level control
        and status information for the Virtual LAN bridge
        services."
    ::= { hwL2vlanGroups 1 }

hwL2vlanStackingGroup OBJECT-GROUP
     OBJECTS {
        hwL2VlanStackingOutsideVlanListLow  , 
        hwL2VlanStackingOutsideVlanListHigh ,
        hwL2VlanStackingRowStatus       
             }
     STATUS      current
     DESCRIPTION
        "A collection of objects providing l2vlan stacking service."
     ::= { hwL2vlanGroups 2 }
        
hwL2vlanMappingGroup OBJECT-GROUP
     OBJECTS {
        hwL2VlanMappingOutsideVlanListLow  , 
        hwL2VlanMappingOutsideVlanListHigh  ,
        hwL2VlanMappingRowStatus        
             }
     STATUS      current
     DESCRIPTION
        "A collection of objects providing l2vlan mapping service."
     ::= { hwL2vlanGroups 3 }
        
hwSupervlanGroup OBJECT-GROUP
     OBJECTS {
            hwSubVlanListLow ,
        hwSubVlanListHigh 
             }
     STATUS      current
     DESCRIPTION
        "A collection of objects providing supervlan  service."
     ::= { hwL2vlanGroups 4 }
        
hwL2InterfIsolateGroup OBJECT-GROUP
      OBJECTS {
        hwL2InterfIsolateInterflistLow  , 
        hwL2InterfIsolateInterflistHigh  
               }
      STATUS     current
      DESCRIPTION
         "A collection of objects provding l2interfisolate service. "  
      ::= { hwL2vlanGroups 5 }
      
hwL2IsolatemappingGroup  OBJECT-GROUP
       OBJECTS {
        hwL2IsolateInterflistLow    ,
        hwL2IsolateInterflistHigh  
               }
      STATUS     current
      DESCRIPTION
         "A collection of objects provding enhanced l2isolate service. "  
      ::= { hwL2vlanGroups 6 }

 hwL2VlanStackingExtGroup OBJECT-GROUP
     OBJECTS {
        hwL2VlanStackingExtVlanListLow   ,
        hwL2VlanStackingExtVlanListHigh  ,
        hwL2VlanStackingExtPriorityMode,
        hwL2VlanStackingExtVlan8021p,
        hwL2VlanStackingExtRowStatus        
             }
     STATUS      current
     DESCRIPTION
        "A collection of objects providing flexible QinQ  service."
     ::= { hwL2vlanGroups 7 }  
hwL2vlanQinQGroup OBJECT-GROUP
     OBJECTS {
        hwL2VlanQinQOutSideVlanId  ,
        hwL2VlanSysQinQRowStatus              
             }
     STATUS      current
     DESCRIPTION
        "A collection of objects providing l2vlan QinQ service."
     ::= { hwL2vlanGroups 8 }

hwL2vlanQinQInterfaceGroup OBJECT-GROUP
     OBJECTS {
        hwL2VlanQinQSVlanId            ,
        hwL2VlanQinQAction             ,
        hwL2VlanQinQNewCVlanId         ,        
        hwL2VlanInterfaceQinQRowStatus             
             }
     STATUS      current
     DESCRIPTION
        "A collection of objects providing l2vlan QinQ service."
     ::= { hwL2vlanGroups 9}  
 
    
 hwL2DVlanMappingGroup OBJECT-GROUP
     OBJECTS {
        hwL2DVlanMappingMapExternalVlanId   ,
        hwL2DVlanMappingMapInternalVlanId   ,
        hwL2DVlanMappingAction ,
        hwL2DVlanMappingRowStatus            
             }
     STATUS      current
     DESCRIPTION
        "A collection of objects providing double Vlan-Mapping service."
     ::= { hwL2vlanGroups 10 } 
     
 hwL2VlanStackingAdvGroup OBJECT-GROUP
     OBJECTS {
                 hwL2VlanStackingAdvOutsideVlanListLow,
                 hwL2VlanStackingAdvOutsideVlanListHigh,
                 hwL2VlanStackingAdvRowStatus
            
             }
     STATUS      current
     DESCRIPTION 
        "A collection of objects vlan Stacking 8021p."
     ::= { hwL2vlanGroups 11 } 
 hwL2VlanMappingAdvGroup OBJECT-GROUP
     OBJECTS {                                                            
                hwL2VlanMappingAdvOutsideVlanListLow ,          
                hwL2VlanMappingAdvOutsideVlanListHigh ,                               
                hwL2VlanMappingAdvRowStatus                                          
             }                                             
     STATUS      current                                   
     DESCRIPTION 
        "A collection of objects Vlan-Mapping 8021p."
     ::= { hwL2vlanGroups 12 }  
     
    hwL2VlanSwitchGroup OBJECT-GROUP
       OBJECTS {
                hwL2VlanSwitchMode,
                hwL2VlanSwitchOuterSwitchVlanId,
                hwL2VlanSwitchInnerSwitchVlanId,
                hwL2VlanSwitch8021pRemark,
                hwL2VlanSwitchOutIfIndex,
                   hwL2VlanSwitchMtu,
                   hwL2VlanSwitchMtuDiscardPkts,
                   hwL2VlanSwitchMtuDiscardBytes,                  
                   hwL2VlanSwitchMtuResetFlag,
                   hwL2VlanSwitchMtuEnableFlag,                         
                hwL2VlanSwitchRowStatus      
               }
       STATUS current
       DESCRIPTION
          "A collection of hwL2VlanSwitchTable objects."
       ::= { hwL2vlanGroups 13 }  
 
 hwL2IfStatVlanCfgGroup OBJECT-GROUP
        OBJECTS {    
                hwL2IfStatVlanCfgEnableFlag,
                hwL2IfStatVlanCfgRowStatus
                }                                             
        STATUS      current                                   
     DESCRIPTION 
        "A collection of objects enable the vlan statistic funtion in the port."
     ::= { hwL2vlanGroups 14 }
     
    hwL2IfStat8021pCfgGroup OBJECT-GROUP
        OBJECTS {    
                hwL2IfStat8021pCfgEnableFlag,
                hwL2IfStat8021pCfgRowStatus
                }                                             
        STATUS      current                                   
        DESCRIPTION                                           
        "A collection of objects enable the 8021p statistic funtion in the port."
        ::= { hwL2vlanGroups 15 }
     
    hwL2IfStat8021pAndVlanCfgGroup OBJECT-GROUP
        OBJECTS {    
                hwL2IfStat8021pAndVlanCfgEnableFlag,
                hwL2IfStat8021pAndVlanCfgRowStatus
                }                                             
         STATUS      current                                   
         DESCRIPTION 
            "A collection of objects enable the 8021p and vlan statistic funtion in the port."
        ::= { hwL2vlanGroups 16 }

 hwL2VlanStatGroup OBJECT-GROUP
     OBJECTS {
        hwL2VlanStatInTotalPkts,
        hwL2VlanStatInTotalBytes ,
        hwL2VlanStatOutTotalPkts,
        hwL2VlanStatOutTotalBytes,
        hwL2VlanStatUnknownUcastDiscardPkts,
        hwL2VlanStatUnknownMcastDiscardPkts,
        hwL2VlanStatBcastDiscardPkts ,
        hwL2VlanStatInUcastPkts,
        hwL2VlanStatInUcastBytes,
        hwL2VlanStatOutUcastPkts,
        hwL2VlanStatOutUcastBytes,
        hwL2VlanStatInMcastPkts,
        hwL2VlanStatInMcastBytes,
        hwL2VlanStatOutMcastPkts,
        hwL2VlanStatOutMcastBytes,
        hwL2VlanStatInBcastPkts,
        hwL2VlanStatInBcastBytes,
        hwL2VlanStatOutBcastPkts,
        hwL2VlanStatOutBcastBytes,
        hwL2VlanStatResetFlag
             }                                             
     STATUS      current                                   
     DESCRIPTION 
        "A collection of objects vlan statistic in the port."
     ::= { hwL2vlanGroups 17 }  
     
 hwL2IfStatVlanGroup OBJECT-GROUP
     OBJECTS {
        hwL2IfStatVlanInTotalPkts,
        hwL2IfStatVlanInTotalBytes ,
        hwL2IfStatVlanOutTotalPkts,
        hwL2IfStatVlanOutTotalBytes ,
        hwL2IfStatVlanInPktsRate,
        hwL2IfStatVlanInBytesRate,
        hwL2IfStatVlanOutPktsRate,
        hwL2IfStatVlanOutBytesRate,
        hwL2IfStatVlanInUcastPkts,
        hwL2IfStatVlanInUcastBytes,
        hwL2IfStatVlanOutUcastPkts,
        hwL2IfStatVlanOutUcastBytes,
        hwL2IfStatVlanInMcastPkts,
        hwL2IfStatVlanInMcastBytes,
        hwL2IfStatVlanOutMcastPkts,
        hwL2IfStatVlanOutMcastBytes,
        hwL2IfStatVlanInBcastPkts,
        hwL2IfStatVlanInBcastBytes,
        hwL2IfStatVlanOutBcastPkts,
        hwL2IfStatVlanOutBcastBytes,
        hwL2IfStatVlanResetFlag
        }                                             
     STATUS      current                                   
     DESCRIPTION 
        "A collection of objects vlan statistic in the port."
     ::= { hwL2vlanGroups 18 }
     
 hwL2IfStat8021pGroup OBJECT-GROUP
     OBJECTS {
        hwL2IfStat8021pInTotalPkts,
        hwL2IfStat8021pInTotalBytes ,
        hwL2IfStat8021pOutTotalPkts,
        hwL2IfStat8021pOutTotalBytes ,
        hwL2IfStat8021pInPktsRate,
        hwL2IfStat8021pInBytsRate,
        hwL2IfStat8021pOutPktsRate,
        hwL2IfStat8021pOutBytesRate,
        hwL2IfStat8021pResetFlag                               
             }                                             
     STATUS      current                                   
     DESCRIPTION                                           
        "A collection of objects  8021p statistic in the port."
     ::= { hwL2vlanGroups 19 }   

  hwL2IfStat8021pAndVlanGroup OBJECT-GROUP
     OBJECTS {    
        hwL2IfStat8021pAndVlanInTotalPkts,
        hwL2IfStat8021pAndVlanInTotalBytes ,
        hwL2IfStat8021pAndVlanInPktsRate,
        hwL2IfStat8021pAndVlanInBytsRate,
        hwL2IfStat8021pAndVlanResetFlag                
             }                                             
     STATUS      current                                   
     DESCRIPTION 
        "A collection of objects vlan and 8021p statistic in the port."
     ::= { hwL2vlanGroups 20 }
     
  hwL2VlanMappingExtGroup OBJECT-GROUP
     OBJECTS {    
        hwL2VlanMappingExtVlanListLow,
        hwL2VlanMappingExtVlanListHigh,
        hwL2VlanMappingExtRowStatus,  
        hwL2VlanMappingExtPriorityMode,
        hwL2VlanMappingExtVlan8021p     
             }                                             
     STATUS      current                                   
     DESCRIPTION 
        "A collection of objects VLAN Mapping in the port."
     ::= { hwL2vlanGroups 21 }       
     
  hwL2VlanQinqVlanTransEnaGroup OBJECT-GROUP
     OBJECTS {    
        hwL2VlanQinqVlanTransEna,
        hwL2VlanQinqVlanTransEnaRowStatus
             }                                             
     STATUS      current                                   
     DESCRIPTION 
        "A collection of objects QinQ VLAN translation enable in the port."
     ::= { hwL2vlanGroups 22 }   
     
  hwL2VlanQinqVlanTransMissDropGroup OBJECT-GROUP
     OBJECTS {    
        hwL2VlanQinqVlanTransMissDrop,
        hwL2VlanQinqVlanTransMissDropRowStatus
             }                                             
     STATUS      current                                   
     DESCRIPTION 
        "A collection of objects QinQ VLAN translation miss drop in the port."
     ::= { hwL2vlanGroups 23 } 
     
  hwL2VlanViewMappingGroup OBJECT-GROUP
     OBJECTS {    
        hwL2VlanViewMappingMapVlanId, 
        hwL2VlanViewMappingPriorityMode,
        hwL2VlanViewMappingVlan8021p,
        hwL2VlanViewMappingRowStatus 
             }                                             
     STATUS      current                                   
     DESCRIPTION 
        "A collection of objects VLAN Mapping at the VLAN view."
     ::= { hwL2vlanGroups 24 } 
     
      hwL2VlanStackingMaskGroup OBJECT-GROUP
     OBJECTS {
                hwL2VlanStackingMaskVlanListLow,
                hwL2VlanStackingMaskVlanListHigh,
                hwL2VlanStackingMaskRowStatus        
             }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanStackingMaskTable objects."
     ::= { hwL2vlanGroups 25 }  
     
      hwL2VlanIpSubnetVlanGroup OBJECT-GROUP
     OBJECTS {  
                hwL2VlanIpSubnetVlanIpAddress,
                hwL2VlanIpSubnetVlanIpSubnetMask,
                hwL2VlanIpSubnetVlanPriority,
                hwL2VlanIpSubnetVlanRowStatus 
             }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanIpSubnetVlanTable objects."
     ::= { hwL2vlanGroups 26 }

    hwL2VlanMacVlanGroup OBJECT-GROUP
     OBJECTS {  
                hwL2VlanMacVlanVlanId,
                hwL2VlanMacVlanMac,                
                hwL2VlanMacVlanVlanPriority,
                hwL2VlanMacVlanMacRowStatus    
             }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanMacVlanTable objects."
     ::= { hwL2vlanGroups 27 }

      hwL2VlanProtocolVlanGroup OBJECT-GROUP
     OBJECTS {  
                hwL2VlanProtocolVlanProtocolType, 
                hwL2VlanProtocolVlanEncapType,
                hwL2VlanProtocolVlanRowStatus                    
             }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanProtocolVlanTable objects."
     ::= { hwL2vlanGroups 28 }

      hwL2VlanPolicyVlanGroup OBJECT-GROUP
     OBJECTS {  
                hwL2VlanPolicyVlanVlanId, 
                hwL2VlanPolicyVlanVlanPriority,
                hwL2VlanPolicyVlanMac,
                hwL2VlanPolicyVlanIp,
                hwL2VlanPolicyVlanPort,
                hwL2VlanPolicyVlanRowStatus                                                
             }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanPolicyVlanTable objects."
     ::= { hwL2vlanGroups 29 }

      hwL2VlanVoiceVlanGroup OBJECT-GROUP
     OBJECTS {  
                hwL2VlanVoiceVlanEnabledVlanId ,
                hwL2VlanVoiceVlanAgingTime,
                hwL2VlanVoiceVlanSecurityMode,    
                hwL2VlanVoiceVlanPortEnable,
                hwL2VlanVoiceVlanPortMode, 
                hwL2VlanVoiceVlanPortLegacy, 
                hwL2VlanVoiceVlanPortSecurityMode,
                hwL2VlanVoiceVlanPortModifyPriorityMode,
                hwL2VlanVoiceVlanOuiDescription,
                hwL2VlanVoiceVlanOuiRowStatus,
                hwL2VlanVoiceVlan8021p,
                hwL2VlanVoiceVlanDscp
    }
     STATUS current
     DESCRIPTION
        "A collection of Voice VLAN related objects."
     ::= { hwL2vlanGroups 30 }
     
      hwL2VlanMappingMultiGroup OBJECT-GROUP
     OBJECTS {
                hwL2VlanMappingMultiVlanListLow,
                hwL2VlanMappingMultiVlanListHigh,
                hwL2VlanMappingMultiRowStatus        
             }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanMappingMultiTable objects."
     ::= { hwL2vlanGroups 31 }     
     
  hwL2VlanSwitchPSGroup OBJECT-GROUP
     OBJECTS {
             hwL2VlanSwitchPSInputPkts,
             hwL2VlanSwitchPSInputBytes,      
             hwL2VlanSwitchPSOutputPkts,
             hwL2VlanSwitchPSOutputBytes,     
             hwL2VlanSwitchPSResetFlag,
             hwL2VlanSwitchPSEnableFlag 
             }
     STATUS current
     DESCRIPTION
        "A collection of vlan statistic in the port."
     ::= { hwL2vlanGroups 32 } 
    hwL2VlanMacVlanNewGroup OBJECT-GROUP
     OBJECTS {  
                hwL2VlanMacVlanNewVlanId,                
                hwL2VlanMacVlanNewVlanPriority,
                hwL2VlanMacVlanNewMacRowStatus    
             }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanMacVlanNewTable objects."
     ::= { hwL2vlanGroups 33 }

      hwL2VlanProtocolVlanNewGroup OBJECT-GROUP
     OBJECTS {  
                hwL2VlanProtocolVlanNewProtocolType, 
                hwL2VlanProtocolVlanNewProtocolTypeValue,
                hwL2VlanProtocolVlanNewRowStatus                    
             }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanProtocolVlanNewTable objects."
     ::= { hwL2vlanGroups 34 }

      hwL2VlanPolicyVlanNewGroup OBJECT-GROUP
     OBJECTS {  
                hwL2VlanPolicyVlanNewVlanPriority,
                hwL2VlanPolicyVlanNewRowStatus                                                
             }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanPolicyVlanNewTable objects."
     ::= { hwL2vlanGroups 35 }
     
   hwL2VlanProtocolVlanPortNewGroup OBJECT-GROUP
     OBJECTS {
             hwL2VlanProtocolVlanPortNewPriority ,
             hwL2VlanProtocolVlanPortNewRowStatus }
     STATUS current
     DESCRIPTION
        "A group of protocol vlan port."
     ::= { hwL2vlanGroups 36 }
  hwL2VlanMultiVoiceVlanPortGroup OBJECT-GROUP
    OBJECTS {
              hwL2VlanMultiVoiceVlanPortVLanId,
              hwL2VlanMultiVoiceVlanPortUntagEnable,
              hwL2VlanMultiVoiceVlanPortTag0Enable,
              hwL2VlanMultiVoiceVlanPortRowStatus }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanMultiVoiceVlanPortTable objects."
     ::= { hwL2vlanGroups 37 }  
  hwL2VlanPrecedenceGroup OBJECT-GROUP
    OBJECTS {
                hwL2VlanPrecedence
        }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanPrecedence object."
     ::= { hwL2vlanGroups 38 }  

    hwL2VlanXlateGroup OBJECT-GROUP
    OBJECTS {
              hwL2VlanXlateVlanIdEnd,
              hwL2VlanXlateAction,
              hwL2VlanXlateToVlanId,
              hwL2VlanXlateToinnerVlanId,
              hwL2VlanXlateremark,
              hwL2VlanXlateRowStatus
 
              }
     STATUS current
     DESCRIPTION
        "A collection of hwL2VlanXlateGroup object."
     ::= { hwL2vlanGroups 39 }  
             
     hwL2VlanSwitchExtGroup OBJECT-GROUP
     OBJECTS { hwL2VlanSwitchExtSrcIfIndex, hwL2VlanSwitchExtDstIfIndex, hwL2VlanSwitchExtDstInnerVlan, hwL2VlanSwitchExtRowStatus, 
        hwL2VlanSwitchExtLinkStatus, hwL2VlanSwitchExtVlanXlateAction, hwL2VlanSwitchExtDstVlan, hwL2VlanSwitchExtRemark, hwL2VlanSwitchExtRemarkReverse, 
        hwL2VlanSwitchExtOuterVlanId, hwL2VlanSwitchExtVlanListLow, hwL2VlanSwitchExtVlanListHigh }
     STATUS current
     DESCRIPTION 
     "A group of vlan switch extent table."
     ::= { hwL2vlanGroups 40 }
     
     hwL2QinQVlanGroup OBJECT-GROUP
     OBJECTS { 
        hwL2QinQVlanMode,
        hwL2QinQVlanChangedVlanId,
        hwL2QinQVlanChangedInnerVlanId,
        hwL2QinQVlanRemark,
        hwL2QinQVlanMapStackVlanId,
        hwL2QinQVlanRowStatus,
        hwL2QinQVlanInnerRemark
     }
     STATUS current
     DESCRIPTION 
     "A group of QinQ-VLAN table."
     ::= { hwL2vlanGroups 41 }   

     hwL2UntagAddDTagGroup OBJECT-GROUP
     OBJECTS { 
        hwL2UntagAddDTagOuterVlanId,
        hwL2UntagAddDTagInnerVlanId,
        hwL2UntagAddDTagRowStatus
     }
     STATUS current
     DESCRIPTION 
     "A group of untagged VLAN add double tagged VLAN table."
     ::= { hwL2vlanGroups 42 }

     hwVcmpGroup OBJECT-GROUP
     OBJECTS { 
       hwVcmpDeviceMac
     }
     STATUS current
     DESCRIPTION 
     "A collection of VCMP objects."
     ::= { hwL2vlanGroups 43 }

     hwL2VlanTrapsGroups OBJECT IDENTIFIER ::= { hwL2vlanConformance 3 }
  
     hwL2VlanTrapsGroup NOTIFICATION-GROUP
            NOTIFICATIONS 
                    {
                        hwL2VlanUnkownPacketAlarm,
                        hwVcmpServerMacConflict,
                        hwVcmpRevisionConflict,
                        hwMuxVlanGroupCountExceedThreshold,
                        hwMuxVlanGroupCountExceedThresholdResume,
                        hwVlantransCountExceedThreshold,
                        hwVlantransCountExceedThresholdResume
                    }
            STATUS current
            DESCRIPTION 
                "The Group of L2VLAN Trap."
            ::= { hwL2VlanTrapsGroups 1 } 
                                                                      
-- ============================================================
-- compliance statements
-- ============================================================

hwL2vlanCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
        "The compliance statement for device support of Virtual
        LAN services."

    MODULE
        MANDATORY-GROUPS {
            hwL2VlanMIBTableGroup,
            hwSupervlanGroup 
        }


     GROUP      hwL2vlanStackingGroup
        DESCRIPTION
            "This group is optional ."

     GROUP      hwL2vlanMappingGroup
        DESCRIPTION
            "This group is optional ."

     GROUP      hwL2InterfIsolateGroup
        DESCRIPTION
            "This group is optional ."
            
     GROUP      hwL2IsolatemappingGroup
        DESCRIPTION
            "This group is optional ."
     GROUP      hwL2vlanQinQGroup
        DESCRIPTION
            "This group is optional ."
     
     GROUP      hwL2vlanQinQInterfaceGroup
        DESCRIPTION
            "This group is optional ."  
                                            
     GROUP      hwL2DVlanMappingGroup
        DESCRIPTION
            "This group is optional ."     
    GROUP      hwL2VlanStackingAdvGroup
        DESCRIPTION
            "This group is optional ."   
    GROUP      hwL2VlanMappingAdvGroup
        DESCRIPTION
            "This group is optional ."   
    GROUP      hwL2VlanSwitchGroup
        DESCRIPTION
            "This group is optional ."
     ::= { hwL2vlanCompliances 1 }
            
END 