--  ===================================================================
-- Copyright (C) 2017 by HUAWEI TECHNOLOGIES. All rights reserved.
-- Description:
-- Reference:
-- Version: V2.41
-- ===================================================================

	HUAWEI-SECURITY-MIB DEFINITIONS ::= BEGIN
 
		IMPORTS
			hwDatacomm			
				FROM HUAWEI-MIB			
			EnabledStatus			
				FROM P-BRIDGE-MIB			
			OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP			
				FROM SNMPv2-CONF			
			Integer32, Unsigned32, IpAddress, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE			
				FROM SNMPv2-SMI			
			DisplayString, DateAndTime			
				FROM SNMPv2-TC;
	
	
		hwSecurityMIB MODULE-IDENTITY 
			LAST-UPDATED "201708181014Z"             -- Aug 18, 2017 at 10:14 GMT
			ORGANIZATION 
				"Huawei Technologies Co.,Ltd."
			CONTACT-INFO 
				"Huawei Industrial Base
				Bantian, Longgang
				 Shenzhen 518129
				 People's Republic of China
				 Website: http://www.huawei.com
				 Email: support@huawei.com"
			DESCRIPTION
				"Add hwDapDeviceIP,hwDapMibAuthRequest for DAP"
            REVISION "201708181014Z"		-- Aug 18, 2017 at 10:14 GMT
			DESCRIPTION
				"Add node for  hwL3LoopDetectAlarm and hwL3LoopDetectAlarmResume"
                                                                REVISION "201708171517Z"		-- Aug 17, 2017 at 15:17 GMT
		                     DESCRIPTION 
				"Modify description of hwBaseSecurityMaDiscardedRateResume "
			REVISION "201707201540Z"		-- July 20, 2017 at 15:40 GMT
			DESCRIPTION 
				"Add hwCpcarAutoPortDefendAlarm for cpcar"
			REVISION "201704081440Z"		-- April 08, 2017 at 14:40 GMT
                                                                DESCRIPTION 
				"Add hwCpcarAutoPortDefendAlarmResume for cpcar"
			REVISION "201704081440Z"		-- April 08, 2017 at 14:40 GMT			
			DESCRIPTION  
                                                                                     "Add hwStrackUserAbnormal for security trap"       
                                                                REVISION "201701251558Z"        -- January 25, 2017 at 15:58 GMT 
			DESCRIPTION 
				"Add hwCpcarDropPacketAlarmResume for cpcar"
			REVISION "201503241012Z"		-- March 24, 2015 at 10:12 GMT
			DESCRIPTION
				"CP-CAR Add hwAppliApperProtocolDescirption hwTcpIpDefendProtocolDescirption"
			REVISION "201404041301Z"		-- April 04, 2014 at 13:01 GMT
			DESCRIPTION
				"SOC modify SeqNo"
			REVISION "201303061443Z"		-- March 06, 2013 at 14:43 GMT
			DESCRIPTION
				"SOC add IPv6"
			REVISION "201304081653Z"		-- April 08, 2013 at 16:53 GMT
			DESCRIPTION
				"Add ipprotocol(19) for hwMaDefendProtocol ."
			REVISION "201304171111Z"		-- April 17, 2013 at 11:11 GMT
			DESCRIPTION
				"Add the VB object hwBaseSecurityStormControlInterfaceVlanID for hwBaseSecurityStormControlInterface and hwBaseSecurityStormControlInterfaceResume"
			REVISION "201305201404Z"		-- May 20, 2013 at 14:04 GMT
			DESCRIPTION
				"Add telnetv6Server(64),telnetv6Client(65),tftpv6Client(66),icmpv6(67),dnsv6(68),pimv6(69),sshv6Server(70),ospfv3(71),bgpv6(72),ftpv6Client(73),ftpv6Server(74) for hwAppliApperProtocol"
			REVISION "201306051756Z"		-- June 05, 2013 at 17:56 GMT
			DESCRIPTION
				"Add the indispensable fields, e.g. chassisid and slotid for hwBaseSecurityUrpfDiscardedRateRising, hwBaseSecurityUrpfDiscardedRateResume, hwBaseSecurityTcpIpAttackDiscardedRateRising, 
				hwBaseSecurityTcpIpAttackDiscardedRateResume, hwBaseSecurityMaDiscardedRateRising, hwBaseSecurityMaDiscardedRateResume, hwBaseSecurityApplicationApperceiveDiscardedRateRising and hwBaseSecurityApplicationApperceiveDiscardedRateResume"
			REVISION "201310181123Z"		-- October 18, 2013 at 11:23 GMT
			DESCRIPTION
				"Add webAuthServer(36) for hwAppliApperProtocol"
			REVISION "201310241529Z"		-- October 24, 2013 at 15:29 GMT
			DESCRIPTION
				"Add hwArpsLearnStrictCheck"
			REVISION "201409182020Z"		-- September 18, 2014 at 20:20 GMT
			DESCRIPTION
				"MIB file for NETSEC."
			REVISION "201409182020Z"		-- September 18, 2014 at 20:20 GMT
			DESCRIPTION
				"MIB file fo APP alarm and MADEFEND."
			REVISION "201503241012Z"		-- March 24, 2015 at 10:12 GMT
			DESCRIPTION
				"Add hwDapPortChange,hwDapMibPortChange for DAP"
			REVISION "201504071102Z"		-- April 07, 2015 at 11:02 GMT
			DESCRIPTION
				"Add hwBaseSecurityTtlExpiredLoop"
			REVISION "201505262023Z"		-- May 26, 2015 at 20:23 GMT
			DESCRIPTION
				"Add hwBaseArpVlanCarTrap"
			REVISION "201509291648Z"		-- September 29, 2015 at 16:48 GMT
			DESCRIPTION
				"Add hwCfgApTrapObject hwCfgApTrap hwCfgApTrapFailAlarm for Virtual-Access"
			REVISION "201510141420Z"		-- October 14, 2015 at 14:20 GMT
			DESCRIPTION
				"Add hwAntiAttack hwAntiAttackObjectGroup hwBaseSecurityAntiAttackRateRising hwBaseSecurityAntiAttackRateResume for DFNS(LDM)"
			REVISION "201511161411Z"		-- November 16, 2015 at 14:11 GMT
			DESCRIPTION
				"Add hwCpcarDropPacketAlarm for cpcar"
			REVISION "201601221125Z"		-- January 22, 2016 at 11:25 GMT
			DESCRIPTION
				"Add hwMACsecFailNotify for MACsec"
			REVISION "201604200924Z"		-- April 20, 2016 at 09:24 GMT
			DESCRIPTION
				"Add node for  hwBaseArpVlanCarTrap and hwBaseArpVlanCarResumeTrap"
			REVISION "201605110919Z"		-- May 11, 2016 at 09:19 GMT
			DESCRIPTION
				"Add hwStrackPortAtk for Auto-port-defend"
			REVISION "201605201144Z"		-- May 20, 2016 at 11:44 GMT
			DESCRIPTION
				"The private mib file includes the general extent 
				information of the device.hwDatacomm(165).hwSecurityMIB."
			REVISION "201606171050Z"		-- June 17, 2016 at 10:50 GMT
			DESCRIPTION
				"Add node for  hwBaseArpVlanCarEnhanceTrap and hwBaseArpVlanCarEnhanceResumeTrap"
			REVISION "201610102112Z"		-- October 10, 2016 at 21:12 GMT
			DESCRIPTION
				"Add node for  hwMplsTrapObject and hwMplsTrap. Add hwTeSourceInterfaceCheckTable hwTeSourceInterfaceCheckEntry.Add hwTeSourceInterfaceCheckAlarm   "
			REVISION "201611041650Z"		-- November 04, 2016 at 16:50 GMT
			DESCRIPTION
				"Modify the Max-access of node hwMacFilterIfIndex, hwMacFilterIfIndex , hwMacFilterMacAddr  "
			REVISION "201612241650Z"		-- December 24, 2016 at 16:50 GMT
			DESCRIPTION
				"Add node hwArpSourceMacSpeedLimitALarm for hwArpsTrap"
			::= { hwDatacomm 165 }
		
	
	
--
-- Node definitions
--
	
		-- 1.3.6.1.4.1.2011.5.25.165.1
		hwBaseSecurityMIBObjects OBJECT IDENTIFIER ::= { hwSecurityMIB 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.2
		hwLocalUrpf OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.2.1
		hwLocalUrpfTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwLocalUrpfEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				" The table lists the information about local URPF Packets. "
			::= { hwLocalUrpf 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.2.1.1
		hwLocalUrpfEntry OBJECT-TYPE
			SYNTAX HwLocalUrpfEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				" The table lists the information about local URPF protection."
			INDEX { hwLocalUrpfChassisId, hwLocalUrpfSlotId }
			::= { hwLocalUrpfTable 1 }
		
		HwLocalUrpfEntry ::=
			SEQUENCE { 
				hwLocalUrpfChassisId
					INTEGER,
				hwLocalUrpfSlotId
					Integer32,
				hwLocalUrpfCurrentRateLow
					Integer32,
				hwLocalUrpfCurrentRateHigh
					Integer32,
				hwLocalUrpfNotifyEnabledStatus
					EnabledStatus,
				hwLocalUrpfRateThreshold
					Integer32,
				hwLocalUrpfRateInterval
					Integer32
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.2.1.1.1
		hwLocalUrpfChassisId OBJECT-TYPE
			SYNTAX INTEGER
				{
				clc1(1),
				clc2(2),
				clc3(3),
				clc4(4),
				clc5(5),
				clc6(6),
				clc7(7),
				clc8(8)
				}
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Data index of local URPF,the chassis ID indicates the slot on which chassis is configured with URPF."
			::= { hwLocalUrpfEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.2.1.1.2
		hwLocalUrpfSlotId OBJECT-TYPE
			SYNTAX Integer32 (1..16)
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Data index of local URPF,the slot configured with URPF."
			::= { hwLocalUrpfEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.2.1.1.11
		hwLocalUrpfCurrentRateLow OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The lower 32 bits discard number during the interval of local URPF.unit(packet)."
			::= { hwLocalUrpfEntry 11 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.2.1.1.12
		hwLocalUrpfCurrentRateHigh OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The upper 32 bits discard number during the interval of local URPF.unit(packet)."
			::= { hwLocalUrpfEntry 12 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.2.1.1.13
		hwLocalUrpfNotifyEnabledStatus OBJECT-TYPE
			SYNTAX EnabledStatus
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The alarm state of local URPF."
			::= { hwLocalUrpfEntry 13 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.2.1.1.14
		hwLocalUrpfRateThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Local URPF's discard threshold during the configured interval.unit(packet)."
			::= { hwLocalUrpfEntry 14 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.2.1.1.15
		hwLocalUrpfRateInterval OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The detection interval of the local URPF.unit(s). "
			::= { hwLocalUrpfEntry 15 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.3
		hwTcpIpDefend OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.3.1
		hwTcpIpDefendTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwTcpIpDefendEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about TCPIP protection."
			::= { hwTcpIpDefend 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.3.1.1
		hwTcpIpDefendEntry OBJECT-TYPE
			SYNTAX HwTcpIpDefendEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about TCPIP protection."
			INDEX { hwTcpIpDefendChassisId, hwTcpIpDefendSlotId, hwTcpIpDefendType }
			::= { hwTcpIpDefendTable 1 }
		
		HwTcpIpDefendEntry ::=
			SEQUENCE { 
				hwTcpIpDefendChassisId
					INTEGER,
				hwTcpIpDefendSlotId
					Integer32,
				hwTcpIpDefendType
					INTEGER,
				hwTcpIpDefendCurrentRateLow
					Integer32,
				hwTcpIpDefendCurrentRateHigh
					Integer32,
				hwTcpIpDefendNotifyEnabledStatus
					EnabledStatus,
				hwTcpIpDefendRateThreshold
					Integer32,
				hwTcpIpDefendRateInterval
					Integer32,
				hwTcpIpDefendProtocolDescirption
					OCTET STRING
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.3.1.1.1
		hwTcpIpDefendChassisId OBJECT-TYPE
			SYNTAX INTEGER
				{
				clc1(1),
				clc2(2),
				clc3(3),
				clc4(4),
				clc5(5),
				clc6(6),
				clc7(7),
				clc8(8)
				}
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Data index of TCPIP protection,the chassis ID indicates the slot on which chassis is configured with TCPIP protection."
			::= { hwTcpIpDefendEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.3.1.1.2
		hwTcpIpDefendSlotId OBJECT-TYPE
			SYNTAX Integer32 (1..16)
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Data index of TCPIP protection,the slot configured with TCPIP protection."
			::= { hwTcpIpDefendEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.3.1.1.3
		hwTcpIpDefendType OBJECT-TYPE
			SYNTAX INTEGER
				{
				abnormalPacket(1),
				udpPacket(2),
				tcpSyn(3),
				ipFragmentation(4)
				}
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Data index of TCPIP protection,the type of TCPIP protection."
			::= { hwTcpIpDefendEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.3.1.1.11
		hwTcpIpDefendCurrentRateLow OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The lower 32 bits discard number during the interval of TCPIP protection.unit(packet)."
			::= { hwTcpIpDefendEntry 11 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.3.1.1.12
		hwTcpIpDefendCurrentRateHigh OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The upper 32 bits discard number during the interval of TCPIP protection.unit(packet)."
			::= { hwTcpIpDefendEntry 12 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.3.1.1.13
		hwTcpIpDefendNotifyEnabledStatus OBJECT-TYPE
			SYNTAX EnabledStatus
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The alarm state of TCPIP protection."
			::= { hwTcpIpDefendEntry 13 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.3.1.1.14
		hwTcpIpDefendRateThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"TCPIP protection's discard threshold during the configured interval.unit(packet)."
			::= { hwTcpIpDefendEntry 14 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.3.1.1.15
		hwTcpIpDefendRateInterval OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The detection interval of TCPIP protection.unit(s)."
			::= { hwTcpIpDefendEntry 15 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.3.1.1.16
		hwTcpIpDefendProtocolDescirption OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The descirption of Protocol."
			::= { hwTcpIpDefendEntry 16 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.4
		hwMaDefend OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.4.1
		hwMaDefendTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwMaDefendEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about management and application protection."
			::= { hwMaDefend 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.4.1.1
		hwMaDefendEntry OBJECT-TYPE
			SYNTAX HwMaDefendEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about management and application protection."
			INDEX { hwMaDefendChassisId, hwMaDefendSlotId, hwMaDefendProtocol }
			::= { hwMaDefendTable 1 }
		
		HwMaDefendEntry ::=
			SEQUENCE { 
				hwMaDefendChassisId
					INTEGER,
				hwMaDefendSlotId
					Integer32,
				hwMaDefendProtocol
					INTEGER,
				hwMaDefendCurrentRateLow
					Integer32,
				hwMaDefendCurrentRateHigh
					Integer32,
				hwMaDefendNotifyEnabledStatus
					EnabledStatus,
				hwMaDefendRateThreshold
					Integer32,
				hwMaDefendRateInterval
					Integer32
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.4.1.1.1
		hwMaDefendChassisId OBJECT-TYPE
			SYNTAX INTEGER
				{
				clc1(1),
				clc2(2),
				clc3(3),
				clc4(4),
				clc5(5),
				clc6(6),
				clc7(7),
				clc8(8)
				}
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Data index of management and application protection,the chassis ID indicates the slot on which chassis is configured with management and application protection."
			::= { hwMaDefendEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.4.1.1.2
		hwMaDefendSlotId OBJECT-TYPE
			SYNTAX Integer32 (1..16)
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Data index of management and application protection,the slots configured with management and application protection."
			::= { hwMaDefendEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.4.1.1.3
		hwMaDefendProtocol OBJECT-TYPE
			SYNTAX INTEGER
				{
				ftp(1),
				ssh(2),
				snmp(3),
				telnet(4),
				tftp(5),
				bgp(6),
				ldp(7),
				rsvp(8),
				ospf(9),
				rip(10),
				isis(11),
				pim(12),
				ntp(13),
				lspping(14),
				dhcpc(15),
				dhcpr(16),
				tcp(17),
				udp(18),
				ipprotocol(19)
				}
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Data index of management and application protection,the protocols configured in management and application protection."
			::= { hwMaDefendEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.4.1.1.11
		hwMaDefendCurrentRateLow OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The lower 32 bits discard number during the interval of management and application protection.unit(packet)."
			::= { hwMaDefendEntry 11 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.4.1.1.12
		hwMaDefendCurrentRateHigh OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The upper 32 bits discard number during the interval of management and application protection.unit(packet)."
			::= { hwMaDefendEntry 12 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.4.1.1.13
		hwMaDefendNotifyEnabledStatus OBJECT-TYPE
			SYNTAX EnabledStatus
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The alarm state of management and application protection."
			::= { hwMaDefendEntry 13 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.4.1.1.14
		hwMaDefendRateThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The discard threshold of management and application protection during the configured interval.unit(packet)."
			::= { hwMaDefendEntry 14 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.4.1.1.15
		hwMaDefendRateInterval OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The detection interval of management and application protection. unit(s)."
			::= { hwMaDefendEntry 15 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.5
		hwApplicationApperceive OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.5.1
		hwApplicationApperceiveTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwApplicationApperceiveEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about Application-Apperceive protection."
			::= { hwApplicationApperceive 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.5.1.1
		hwApplicationApperceiveEntry OBJECT-TYPE
			SYNTAX HwApplicationApperceiveEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about Application-Apperceive protection."
			INDEX { hwAppliApperChassisId, hwAppliApperSlotId, hwAppliApperProtocol }
			::= { hwApplicationApperceiveTable 1 }
		
		HwApplicationApperceiveEntry ::=
			SEQUENCE { 
				hwAppliApperChassisId
					INTEGER,
				hwAppliApperSlotId
					Integer32,
				hwAppliApperProtocol
					INTEGER,
				hwAppliApperCurrentRateLow
					Integer32,
				hwAppliApperCurrentRateHigh
					Integer32,
				hwAppliApperNotifyEnabledStatus
					EnabledStatus,
				hwAppliApperRateThreshold
					Integer32,
				hwAppliApperRateInterval
					Integer32,
				hwAppliApperProtocolDescirption
					OCTET STRING
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.5.1.1.1
		hwAppliApperChassisId OBJECT-TYPE
			SYNTAX INTEGER
				{
				clc1(1),
				clc2(2),
				clc3(3),
				clc4(4),
				clc5(5),
				clc6(6),
				clc7(7),
				clc8(8)
				}
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Data index of Application-Apperceive protection,the chassis ID indicates the slot on which chassis is configured with Application-Apperceive protection."
			::= { hwApplicationApperceiveEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.5.1.1.2
		hwAppliApperSlotId OBJECT-TYPE
			SYNTAX Integer32 (1..16)
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Data index of Application-Apperceive protection,the slots configured with Application-Apperceive protection."
			::= { hwApplicationApperceiveEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.5.1.1.3
		hwAppliApperProtocol OBJECT-TYPE
			SYNTAX INTEGER
				{
				ftpServer(1),
				sshServer(2),
				snmp(3),
				telnetServer(4),
				tftp(5),
				bgp(6),
				ldp(7),
				rsvp(8),
				ospf(9),
				rip(10),
				isis(11),
				sftpSever(12),
				icmp(13),
				msdp(14),
				pim(15),
				ipv4Arp(16),
				bpdu(17),
				dhcp(18),
				lacp(19),
				ntp(20),
				radius(21),
				hwTacacs(22),
				lspPing(23),
				igmp(24),
				vgmp(25),
				rrpp(26),
				vrrp(27),
				bfd(28),
				mplsOam(29),
				eth8021ag(30),
				ftpClient(31),
				telnetClient(32),
				sshClient(33),
				sftpClient(34),
				dnsClient(35),
				webAuthServer(36),
				telnetv6Server(64),
				telnetv6Client(65),
				tftpv6Client(66),
				icmpv6(67),
				dnsv6(68),
				pimv6(69),
				sshv6Server(70),
				ospfv3(71),
				bgpv6(72),
				ftpv6Client(73),
				ftpv6Server(74)
				}
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Data index of Application-Apperceive protection,the protocol configured in Application-Apperceive protection."
			::= { hwApplicationApperceiveEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.5.1.1.11
		hwAppliApperCurrentRateLow OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The lower 32 bits discard number during the interval of Application-Apperceive protection.unit(packet)."
			::= { hwApplicationApperceiveEntry 11 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.5.1.1.12
		hwAppliApperCurrentRateHigh OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The upper 32 bits discard number during the interval of Application-Apperceive protection.unit(packet)."
			::= { hwApplicationApperceiveEntry 12 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.5.1.1.13
		hwAppliApperNotifyEnabledStatus OBJECT-TYPE
			SYNTAX EnabledStatus
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The alarm state of Application-Apperceive protection."
			::= { hwApplicationApperceiveEntry 13 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.5.1.1.14
		hwAppliApperRateThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The discard threshold of Application-Apperceive protection during the configured interval.unit(packet)."
			::= { hwApplicationApperceiveEntry 14 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.5.1.1.15
		hwAppliApperRateInterval OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The detect interval of Application-Apperceive protection. unit(s)."
			::= { hwApplicationApperceiveEntry 15 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.5.1.1.16
		hwAppliApperProtocolDescirption OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The descirption of Protocol."
			::= { hwApplicationApperceiveEntry 16 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.6
		hwDefdPortVlan OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 6 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.6.1
		hwDefdPortVlanTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwDefdPortVlanEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				" The table lists the information about defend port vlan packet. "
			::= { hwDefdPortVlan 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.6.1.1
		hwDefdPortVlanEntry OBJECT-TYPE
			SYNTAX HwDefdPortVlanEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about defend port vlan ."
			INDEX { hwDefdPortVlanIfIndex }
			::= { hwDefdPortVlanTable 1 }
		
		HwDefdPortVlanEntry ::=
			SEQUENCE { 
				hwDefdPortVlanIfIndex
					Integer32,
				hwDefdPortVlanIfName
					OCTET STRING,
				hwDefdPortVlanId
					Integer32,
				hwDefdPortVlanCheckProtocol
					OCTET STRING
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.6.1.1.1
		hwDefdPortVlanIfIndex OBJECT-TYPE
			SYNTAX Integer32 (1..2147483647)
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Interface Index, equal to ifIndex."
			::= { hwDefdPortVlanEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.6.1.1.2
		hwDefdPortVlanIfName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (1..256))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The name of the interface."
			::= { hwDefdPortVlanEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.6.1.1.3
		hwDefdPortVlanId OBJECT-TYPE
			SYNTAX Integer32 (0..4096)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The Data index of defend port vlan."
			::= { hwDefdPortVlanEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.6.1.1.4
		hwDefdPortVlanCheckProtocol OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (1..100))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Check protocol name."
			::= { hwDefdPortVlanEntry 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7
		hwSocAttackTrapObject OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 7 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1
		hwSocAttackInfoTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwSocAttackInfoEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				" The table lists the information about Security Operation Center. "
			::= { hwSocAttackTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1.1
		hwSocAttackInfoEntry OBJECT-TYPE
			SYNTAX HwSocAttackInfoEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about Securty Operation Center detected one attack."
			INDEX { hwSocAttackSeqNo }
			::= { hwSocAttackInfoTable 1 }
		
		HwSocAttackInfoEntry ::=
			SEQUENCE { 
				hwSocAttackSeqNo
					Integer32,
				hwSocAttackPossib
					OCTET STRING,
				hwSocAttackReason
					OCTET STRING,
				hwSocAttackIfName
					OCTET STRING,
				hwSocAttackSubIfName
					OCTET STRING,
				hwSocAttackVlanIndex
					OCTET STRING,
				hwSocAttackUserQinQIndex
					OCTET STRING,
				hwSocAttackMacAddr
					OCTET STRING,
				hwSocAttackIPAddr
					OCTET STRING,
				hwSocAttackIPv6Addr
					OCTET STRING
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1.1.1
		hwSocAttackSeqNo OBJECT-TYPE
			SYNTAX Integer32 (1..16777215)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The sequence number of attack infomation."
			::= { hwSocAttackInfoEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1.1.2
		hwSocAttackPossib OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..32))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The prabability of the attack ."
			::= { hwSocAttackInfoEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1.1.3
		hwSocAttackReason OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..63))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The reason of the attack ."
			::= { hwSocAttackInfoEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1.1.4
		hwSocAttackIfName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..63))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The interface of the attack"
			::= { hwSocAttackInfoEntry 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1.1.5
		hwSocAttackSubIfName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..256))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The sub-interface of the attack"
			::= { hwSocAttackInfoEntry 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1.1.6
		hwSocAttackVlanIndex OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..32))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The vlan of the attack"
			::= { hwSocAttackInfoEntry 6 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1.1.7
		hwSocAttackUserQinQIndex OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..64))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The UserQinQ of the attack"
			::= { hwSocAttackInfoEntry 7 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1.1.8
		hwSocAttackMacAddr OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..128))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The MAC of the attack"
			::= { hwSocAttackInfoEntry 8 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1.1.9
		hwSocAttackIPAddr OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..128))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The IP of the attack"
			::= { hwSocAttackInfoEntry 9 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.7.1.1.10
		hwSocAttackIPv6Addr OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..128))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The IPv6 of the attack"
			::= { hwSocAttackInfoEntry 10 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11
		hwBaseSecurityNotifications OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 11 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.1
		hwBaseSecurityUrpfDiscardedRateRising NOTIFICATION-TYPE
			OBJECTS { hwLocalUrpfCurrentRateLow, hwLocalUrpfCurrentRateHigh, hwLocalUrpfRateThreshold, hwLocalUrpfChassisId, hwLocalUrpfSlotId
				 }
			STATUS current
			DESCRIPTION 
				" The discard packets exceed the threshold of local URPF protection."
			::= { hwBaseSecurityNotifications 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.2
		hwBaseSecurityUrpfDiscardedRateResume NOTIFICATION-TYPE
			OBJECTS { hwLocalUrpfCurrentRateLow, hwLocalUrpfCurrentRateHigh, hwLocalUrpfRateThreshold, hwLocalUrpfChassisId, hwLocalUrpfSlotId
				 }
			STATUS current
			DESCRIPTION 
				" The alarm of local URPF is resumed."
			::= { hwBaseSecurityNotifications 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.3
		hwBaseSecurityTcpIpAttackDiscardedRateRising NOTIFICATION-TYPE
			OBJECTS { hwTcpIpDefendCurrentRateLow, hwTcpIpDefendCurrentRateHigh, hwTcpIpDefendRateThreshold, hwTcpIpDefendRateInterval, hwTcpIpDefendChassisId, 
				hwTcpIpDefendSlotId, hwTcpIpDefendType, hwTcpIpDefendProtocolDescirption }
			STATUS current
			DESCRIPTION 
				" The discard packets exceed the threshold of TCPIP protection. "
			::= { hwBaseSecurityNotifications 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.4
		hwBaseSecurityTcpIpAttackDiscardedRateResume NOTIFICATION-TYPE
			OBJECTS { hwTcpIpDefendCurrentRateLow, hwTcpIpDefendCurrentRateHigh, hwTcpIpDefendRateThreshold, hwTcpIpDefendRateInterval, hwTcpIpDefendChassisId, 
				hwTcpIpDefendSlotId, hwTcpIpDefendType, hwTcpIpDefendProtocolDescirption }
			STATUS current
			DESCRIPTION 
				" The alarm of TCPIP protection is resumed. "
			::= { hwBaseSecurityNotifications 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.5
		hwBaseSecurityMaDiscardedRateRising NOTIFICATION-TYPE
			OBJECTS { hwMaDefendCurrentRateLow, hwMaDefendCurrentRateHigh, hwMaDefendRateThreshold, hwMaDefendRateInterval, hwMaDefendChassisId, 
				hwMaDefendSlotId, hwMaDefendProtocol }
			STATUS current
			DESCRIPTION 
				" The discard packets exceed the threshold of management and application protection."
			::= { hwBaseSecurityNotifications 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.6
		hwBaseSecurityMaDiscardedRateResume NOTIFICATION-TYPE
			OBJECTS { hwMaDefendCurrentRateLow, hwMaDefendCurrentRateHigh, hwMaDefendRateThreshold, hwMaDefendRateInterval, hwMaDefendChassisId, 
				hwMaDefendSlotId, hwMaDefendProtocol }
			STATUS current
			DESCRIPTION 
				" The rate at which the management and service plane protection drops invalid packets falls below the threshold. "
			::= { hwBaseSecurityNotifications 6 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.7
		hwBaseSecurityApplicationApperceiveDiscardedRateRising NOTIFICATION-TYPE
			OBJECTS { hwAppliApperCurrentRateLow, hwAppliApperCurrentRateHigh, hwAppliApperRateThreshold, hwAppliApperRateInterval, hwAppliApperChassisId, 
				hwAppliApperSlotId, hwAppliApperProtocol, hwAppliApperProtocolDescirption }
			STATUS current
			DESCRIPTION 
				" The discard packets exceed the threshold of Application-Apperceive protection. "
			::= { hwBaseSecurityNotifications 7 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.8
		hwBaseSecurityApplicationApperceiveDiscardedRateResume NOTIFICATION-TYPE
			OBJECTS { hwAppliApperCurrentRateLow, hwAppliApperCurrentRateHigh, hwAppliApperRateThreshold, hwAppliApperRateInterval, hwAppliApperChassisId, 
				hwAppliApperSlotId, hwAppliApperProtocol, hwAppliApperProtocolDescirption }
			STATUS current
			DESCRIPTION 
				"The alarm of Application-Apperceive protection is resumed."
			::= { hwBaseSecurityNotifications 8 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.9
		hwBaseSecurityStormControlInterface NOTIFICATION-TYPE
			OBJECTS { hwBaseSecurityStormControlInterfaceChassisId, hwBaseSecurityStormControlInterfaceSlotId, hwBaseSecurityStormControlInterfaceName, hwBaseSecurityStormControlInterfaceVlanID }
			STATUS current
			DESCRIPTION 
				"The alarm of storm-control detection."
			::= { hwBaseSecurityNotifications 9 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.12
		hwBaseSocAttackTrap NOTIFICATION-TYPE
			OBJECTS { hwSocAttackSeqNo, hwSocAttackPossib, hwSocAttackReason, hwSocAttackIfName, hwSocAttackSubIfName, 
				hwSocAttackVlanIndex, hwSocAttackUserQinQIndex, hwSocAttackMacAddr, hwSocAttackIPAddr, hwSocAttackIPv6Addr
				 }
			STATUS current
			DESCRIPTION 
				"An attack occur on the Network. "
			::= { hwBaseSecurityNotifications 12 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.13
		hwBaseSocAttackResumeTrap NOTIFICATION-TYPE
			OBJECTS { hwSocAttackSeqNo, hwSocAttackPossib, hwSocAttackReason, hwSocAttackIfName, hwSocAttackSubIfName, 
				hwSocAttackVlanIndex, hwSocAttackUserQinQIndex, hwSocAttackMacAddr, hwSocAttackIPAddr, hwSocAttackIPv6Addr
				 }
			STATUS current
			DESCRIPTION 
				"An attack cancels on the Network."
			::= { hwBaseSecurityNotifications 13 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.14
		hwBaseSecurityStormControlInterfaceResume NOTIFICATION-TYPE
			OBJECTS { hwBaseSecurityStormControlInterfaceChassisId, hwBaseSecurityStormControlInterfaceSlotId, hwBaseSecurityStormControlInterfaceName, hwBaseSecurityStormControlInterfaceVlanID }
			STATUS current
			DESCRIPTION 
				"L2 loop detect alarm cleared."
			::= { hwBaseSecurityNotifications 14 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.15
		hwBaseSecurityTtlExpiredLoop NOTIFICATION-TYPE
			OBJECTS { hwTtlExpiredLoopChassisId, hwTtlExpiredLoopSlotId, hwTtlExpiredLoopLastRateLow, hwTtlExpiredLoopLastRateHigh, hwTtlExpiredLoopCurrentRateLow, 
				hwTtlExpiredLoopCurrentRateHigh, hwTtlExpiredLoopRateInterval, hwTtlExpiredLoopRateThreshold }
			STATUS current
			DESCRIPTION 
				"The alarm of ttl-expired loop detection."
			::= { hwBaseSecurityNotifications 15 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.16
		hwBaseSecurityTtlExpiredLoopResume NOTIFICATION-TYPE
			OBJECTS { hwTtlExpiredLoopChassisId, hwTtlExpiredLoopSlotId, hwTtlExpiredLoopLastRateLow, hwTtlExpiredLoopLastRateHigh, hwTtlExpiredLoopCurrentRateLow, 
				hwTtlExpiredLoopCurrentRateHigh, hwTtlExpiredLoopRateInterval, hwTtlExpiredLoopRateThreshold }
			STATUS current
			DESCRIPTION 
				"TTL-Expired loop alarm cleared."
			::= { hwBaseSecurityNotifications 16 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.17
		hwBaseArpVlanCarTrap NOTIFICATION-TYPE
			OBJECTS { hwBaseArpVlanCarLogIfName, hwBaseArpVlanCarPhyIfName, hwBaseArpVlanCarVlanId }
			STATUS current
			DESCRIPTION 
				"ARP VLAN CAR took effect on an interface, which may be because a loop occurred on the interface."
			::= { hwBaseSecurityNotifications 17 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.18
		hwBaseArpVlanCarResumeTrap NOTIFICATION-TYPE
			OBJECTS { hwBaseArpVlanCarLogIfName, hwBaseArpVlanCarPhyIfName, hwBaseArpVlanCarVlanId }
			STATUS current
			DESCRIPTION 
				"ARP VLAN CAR become ineffective on an interface."
			::= { hwBaseSecurityNotifications 18 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.19
		hwBaseSecurityAntiAttackRateRising NOTIFICATION-TYPE
			OBJECTS { hwAntiAttackType, hwAntiAttackRateThreshold, hwAntiAttackCurrentRate }
			STATUS current
			DESCRIPTION 
				" The rate of packets exceed the threshold of anti-attack alarm. "
			::= { hwBaseSecurityNotifications 19 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.20
		hwBaseSecurityAntiAttackRateResume NOTIFICATION-TYPE
			OBJECTS { hwAntiAttackType, hwAntiAttackRateThreshold, hwAntiAttackCurrentRate }
			STATUS current
			DESCRIPTION 
				" The alarm of anti-attack alarm is resumed. "
			::= { hwBaseSecurityNotifications 20 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.21
		hwBaseArpVlanCarEnhanceTrap NOTIFICATION-TYPE
			OBJECTS { hwBaseArpVlanCarEnhanceLogIfName, hwBaseArpVlanCarEnhancePhyIfName, hwBaseArpVlanCarEnhancePeVlanId, hwBaseArpVlanCarEnhanceCeVlanId, hwBaseArpVlanCarEnhanceSampleRate
				 }
			STATUS current
			DESCRIPTION 
				"ARP VLAN CAR became effective on an interface, which may be because a loop occurred on the interface."
			::= { hwBaseSecurityNotifications 21 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.22
		hwBaseArpVlanCarEnhanceResumeTrap NOTIFICATION-TYPE
			OBJECTS { hwBaseArpVlanCarEnhanceLogIfName, hwBaseArpVlanCarEnhancePhyIfName, hwBaseArpVlanCarEnhancePeVlanId, hwBaseArpVlanCarEnhanceCeVlanId, hwBaseArpVlanCarEnhanceSampleRate
				 }
			STATUS current
			DESCRIPTION 
				"ARP VLAN CAR became ineffective on an interface."
			::= { hwBaseSecurityNotifications 22 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.11.23
		hwL3LoopDetectAlarm NOTIFICATION-TYPE
			OBJECTS { hwL3LoopDetectChassisID, hwL3LoopDetectSlotID, hwL3LoopDetectIPAddr
				 }
			STATUS current
			DESCRIPTION 
				"The alarm of l3 loop detect."
			::= { hwBaseSecurityNotifications 23 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.11.24
		hwL3LoopDetectAlarmResume NOTIFICATION-TYPE
			OBJECTS { hwL3LoopDetectChassisID, hwL3LoopDetectSlotID, hwL3LoopDetectIPAddr
				 }
			STATUS current
			DESCRIPTION 
				"L3 loop detect alarm cleared."
			::= { hwBaseSecurityNotifications 24 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.12
		hwMacFilter OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 12 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.12.1
		hwMacFilterModeTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwMacFilterModeEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about mac-filter statistics."
			::= { hwMacFilter 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.12.1.1
		hwMacFilterModeEntry OBJECT-TYPE
			SYNTAX HwMacFilterModeEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about mac-filter statistics."
			INDEX { hwMacFilterIfIndex }
			::= { hwMacFilterModeTable 1 }
		
		HwMacFilterModeEntry ::=
			SEQUENCE { 
				hwMacFilterIfIndex
					Integer32,
				hwMacFilterInterface
					DisplayString,
				hwMacFilterEnableMode
					INTEGER,
				hwMacFilterMatchNum
					Integer32
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.12.1.1.1
		hwMacFilterIfIndex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Mac-filter interface index."
			::= { hwMacFilterModeEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.12.1.1.2
		hwMacFilterInterface OBJECT-TYPE
			SYNTAX DisplayString (SIZE (1..128))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Mac-filter interface name."
			::= { hwMacFilterModeEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.12.1.1.3
		hwMacFilterEnableMode OBJECT-TYPE
			SYNTAX INTEGER
				{
				none(0),
				whitelist(1),
				balcklist(2)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Mac-filter enable mode."
			::= { hwMacFilterModeEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.12.1.1.4
		hwMacFilterMatchNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Mac-filter if-match number."
			::= { hwMacFilterModeEntry 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.12.2
		hwMacFilterMacAddrTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwMacFilterMacAddrEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about mac-filter if-match mac-address."
			::= { hwMacFilter 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.12.2.1
		hwMacFilterMacAddrEntry OBJECT-TYPE
			SYNTAX HwMacFilterMacAddrEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about mac-filter if-match mac-address."
			INDEX { hwMacFilterIfindex, hwMacFilterMacAddr }
			::= { hwMacFilterMacAddrTable 1 }
		
		HwMacFilterMacAddrEntry ::=
			SEQUENCE { 
				hwMacFilterIfindex
					Integer32,
				hwMacFilterInterfaceBuf
					DisplayString,
				hwMacFilterMacAddr
					DisplayString
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.12.2.1.1
		hwMacFilterIfindex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Mac-filter interface index."
			::= { hwMacFilterMacAddrEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.12.2.1.2
		hwMacFilterInterfaceBuf OBJECT-TYPE
			SYNTAX DisplayString (SIZE (1..128))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Mac-filter interface name."
			::= { hwMacFilterMacAddrEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.12.2.1.3
		hwMacFilterMacAddr OBJECT-TYPE
			SYNTAX DisplayString (SIZE (1..100))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Mac-filter if-match mac-address."
			::= { hwMacFilterMacAddrEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.13
		hwBaseSecurityStormControlInterfaceObjects OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 13 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.13.1
		hwBaseSecurityStormControlInterfaceTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwBaseSecurityStormControlInterfaceEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"A Table about storm-control interface information."
			::= { hwBaseSecurityStormControlInterfaceObjects 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.13.1.1
		hwBaseSecurityStormControlInterfaceEntry OBJECT-TYPE
			SYNTAX HwBaseSecurityStormControlInterfaceEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { hwBaseSecurityStormControlInterfaceChassisId, hwBaseSecurityStormControlInterfaceSlotId }
			::= { hwBaseSecurityStormControlInterfaceTable 1 }
		
		HwBaseSecurityStormControlInterfaceEntry ::=
			SEQUENCE { 
				hwBaseSecurityStormControlInterfaceChassisId
					Integer32,
				hwBaseSecurityStormControlInterfaceSlotId
					Integer32,
				hwBaseSecurityStormControlInterfaceName
					OCTET STRING,
				hwBaseSecurityStormControlInterfaceVlanID
					Integer32
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.13.1.1.1
		hwBaseSecurityStormControlInterfaceChassisId OBJECT-TYPE
			SYNTAX Integer32 (1..128)
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The chassis ID indicates the slot on which chassis is configured with storm control."
			::= { hwBaseSecurityStormControlInterfaceEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.13.1.1.2
		hwBaseSecurityStormControlInterfaceSlotId OBJECT-TYPE
			SYNTAX Integer32 (1..128)
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The slot configured with storm control."
			::= { hwBaseSecurityStormControlInterfaceEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.13.1.1.3
		hwBaseSecurityStormControlInterfaceName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..63))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The interface name."
			::= { hwBaseSecurityStormControlInterfaceEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.13.1.1.4
		hwBaseSecurityStormControlInterfaceVlanID OBJECT-TYPE
			SYNTAX Integer32 (0..4094)
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The VlanID of VlanIF which the interface join in."
			::= { hwBaseSecurityStormControlInterfaceEntry 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.14
		hwBaseArpVlanCarTrapObject OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 14 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.14.1
		hwBaseArpVlanCarInfoTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwBaseArpVlanCarInfoEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"A Table about arp vlan car information."
			::= { hwBaseArpVlanCarTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.14.1.1
		hwBaseArpVlanCarInfoEntry OBJECT-TYPE
			SYNTAX HwBaseArpVlanCarInfoEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { hwBaseArpVlanCarLogIfName, hwBaseArpVlanCarPhyIfName }
			::= { hwBaseArpVlanCarInfoTable 1 }
		
		HwBaseArpVlanCarInfoEntry ::=
			SEQUENCE { 
				hwBaseArpVlanCarLogIfName
					OCTET STRING,
				hwBaseArpVlanCarPhyIfName
					OCTET STRING,
				hwBaseArpVlanCarVlanId
					Integer32
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.14.1.1.1
		hwBaseArpVlanCarLogIfName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The logic interface name."
			::= { hwBaseArpVlanCarInfoEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.14.1.1.2
		hwBaseArpVlanCarPhyIfName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The physical interface name."
			::= { hwBaseArpVlanCarInfoEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.14.1.1.3
		hwBaseArpVlanCarVlanId OBJECT-TYPE
			SYNTAX Integer32 (0..4094)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The VlanId of arp vlan car."
			::= { hwBaseArpVlanCarInfoEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.15
		hwTtlExpiredLoop OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 15 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.15.1
		hwTtlExpiredLoopTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwTtlExpiredLoopEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"A Table about TTL-expired loop information."
			::= { hwTtlExpiredLoop 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.15.1.1
		hwTtlExpiredLoopEntry OBJECT-TYPE
			SYNTAX HwTtlExpiredLoopEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { hwTtlExpiredLoopChassisId, hwTtlExpiredLoopSlotId }
			::= { hwTtlExpiredLoopTable 1 }
		
		HwTtlExpiredLoopEntry ::=
			SEQUENCE { 
				hwTtlExpiredLoopChassisId
					Unsigned32,
				hwTtlExpiredLoopSlotId
					Unsigned32,
				hwTtlExpiredLoopLastRateLow
					Unsigned32,
				hwTtlExpiredLoopLastRateHigh
					Unsigned32,
				hwTtlExpiredLoopCurrentRateLow
					Unsigned32,
				hwTtlExpiredLoopCurrentRateHigh
					Unsigned32,
				hwTtlExpiredLoopRateInterval
					Unsigned32,
				hwTtlExpiredLoopRateThreshold
					Unsigned32
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.15.1.1.1
		hwTtlExpiredLoopChassisId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The chassis ID indicates the chassis ttl-expired loop occur."
			::= { hwTtlExpiredLoopEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.15.1.1.2
		hwTtlExpiredLoopSlotId OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The slot ID indicates the slot ttl-expired loop occur."
			::= { hwTtlExpiredLoopEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.15.1.1.3
		hwTtlExpiredLoopLastRateLow OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The lower 32 bits of last discard bytes."
			::= { hwTtlExpiredLoopEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.15.1.1.4
		hwTtlExpiredLoopLastRateHigh OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The high 32 bits of last discard bytes."
			::= { hwTtlExpiredLoopEntry 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.15.1.1.5
		hwTtlExpiredLoopCurrentRateLow OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The lower 32 bits of current discard bytes."
			::= { hwTtlExpiredLoopEntry 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.15.1.1.6
		hwTtlExpiredLoopCurrentRateHigh OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The high 32 bits of current discard bytes."
			::= { hwTtlExpiredLoopEntry 6 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.15.1.1.7
		hwTtlExpiredLoopRateInterval OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Interval."
			::= { hwTtlExpiredLoopEntry 7 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.15.1.1.8
		hwTtlExpiredLoopRateThreshold OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Threshold."
			::= { hwTtlExpiredLoopEntry 8 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.16
		hwAntiAttack OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 16 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.16.1
		hwAntiAttackTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwAntiAttackEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about anti-attack alarm."
			::= { hwAntiAttack 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.16.1.1
		hwAntiAttackEntry OBJECT-TYPE
			SYNTAX HwAntiAttackEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table list the information about anti-attack alarm."
			INDEX { hwAntiAttackType }
			::= { hwAntiAttackTable 1 }
		
		HwAntiAttackEntry ::=
			SEQUENCE { 
				hwAntiAttackType
					INTEGER,
				hwAntiAttackRateThreshold
					Integer32,
				hwAntiAttackCurrentRate
					Integer32
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.16.1.1.1
		hwAntiAttackType OBJECT-TYPE
			SYNTAX INTEGER
				{
				abnormal(1),
				fragment(2),
				tcpSyn(3),
				udpFlood(4),
				icmpFlood(5)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The data index of anti-attack, attack type configured in anti-attack alarm."
			::= { hwAntiAttackEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.16.1.1.2
		hwAntiAttackRateThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The alarm threshold of anti-attack alarm during the processing of pkt-flooding.unit(bps)."
			::= { hwAntiAttackEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.16.1.1.3
		hwAntiAttackCurrentRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The current rate of anti-attack alarm. unit(bps)."
			::= { hwAntiAttackEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.17
		hwBaseArpVlanCarEnhanceTrapObject OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 17 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.17.1
		hwBaseArpVlanCarEnhanceInfoTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwBaseArpVlanCarEnhanceInfoEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"A Table about arp vlan car information."
			::= { hwBaseArpVlanCarEnhanceTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.17.1.1
		hwBaseArpVlanCarEnhanceInfoEntry OBJECT-TYPE
			SYNTAX HwBaseArpVlanCarEnhanceInfoEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { hwBaseArpVlanCarEnhanceLogIfName, hwBaseArpVlanCarEnhancePhyIfName, hwBaseArpVlanCarEnhancePeVlanId, hwBaseArpVlanCarEnhanceCeVlanId, hwBaseArpVlanCarEnhanceSampleRate
				 }
			::= { hwBaseArpVlanCarEnhanceInfoTable 1 }
		
		HwBaseArpVlanCarEnhanceInfoEntry ::=
			SEQUENCE { 
				hwBaseArpVlanCarEnhanceLogIfName
					OCTET STRING,
				hwBaseArpVlanCarEnhancePhyIfName
					OCTET STRING,
				hwBaseArpVlanCarEnhancePeVlanId
					Integer32,
				hwBaseArpVlanCarEnhanceCeVlanId
					Integer32,
				hwBaseArpVlanCarEnhanceSampleRate
					Integer32
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.17.1.1.1
		hwBaseArpVlanCarEnhanceLogIfName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The logic interface name."
			::= { hwBaseArpVlanCarEnhanceInfoEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.17.1.1.2
		hwBaseArpVlanCarEnhancePhyIfName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The physical interface name."
			::= { hwBaseArpVlanCarEnhanceInfoEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.17.1.1.3
		hwBaseArpVlanCarEnhancePeVlanId OBJECT-TYPE
			SYNTAX Integer32 (0..4094)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The PeVlanId of arp vlan car."
			::= { hwBaseArpVlanCarEnhanceInfoEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.17.1.1.4
		hwBaseArpVlanCarEnhanceCeVlanId OBJECT-TYPE
			SYNTAX Integer32 (0..4094)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The CeVlanId of arp vlan car."
			::= { hwBaseArpVlanCarEnhanceInfoEntry 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.17.1.1.5
		hwBaseArpVlanCarEnhanceSampleRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The sample rate of arp vlan car."
			::= { hwBaseArpVlanCarEnhanceInfoEntry 5 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.18
		hwL3LoopDetectObject OBJECT IDENTIFIER ::= { hwBaseSecurityMIBObjects 18 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.18.1
		hwL3LoopDetectTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwL3LoopDetectEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"A Table about l3 loop detect information."
			::= { hwL3LoopDetectObject 1 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.18.1.1
		hwL3LoopDetectEntry OBJECT-TYPE
			SYNTAX HwL3LoopDetectEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { hwL3LoopDetectChassisID, hwL3LoopDetectSlotID, hwL3LoopDetectIPAddr
				 }
			::= { hwL3LoopDetectTable 1 }
		
		HwL3LoopDetectEntry ::=
			SEQUENCE { 
				hwL3LoopDetectChassisID
					Integer32,
				hwL3LoopDetectSlotID
					Integer32,
				hwL3LoopDetectIPAddr
					OCTET STRING
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.1.18.1.1.1
		hwL3LoopDetectChassisID OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The chassis ID indicates the chassis L3 loop occur."
			::= {hwL3LoopDetectEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.18.1.1.2
		hwL3LoopDetectSlotID OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The slot ID indicates the slot L3 loop occur."
			::= { hwL3LoopDetectEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.1.18.1.1.3
		hwL3LoopDetectIPAddr OBJECT-TYPE
			SYNTAX OCTET STRING 
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"IP address."
			::= { hwL3LoopDetectEntry 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2
		hwMeSecurityMIBObjects OBJECT IDENTIFIER ::= { hwSecurityMIB 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1
		hwSecurityTrapObject OBJECT IDENTIFIER ::= { hwMeSecurityMIBObjects 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1
		hwStrackTrapObject OBJECT IDENTIFIER ::= { hwSecurityTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1.1
		hwStrackTotalPacket OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The total packets of strack during the configured interval.unit(packet)."
			::= { hwStrackTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1.2
		hwStrackEndTime OBJECT-TYPE
			SYNTAX DateAndTime
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of strack."
			::= { hwStrackTrapObject 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1.3
		hwStrackSourceMac OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of strack."
			::= { hwStrackTrapObject 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1.4
		hwStrackPacketPVlan OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of strack."
			::= { hwStrackTrapObject 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1.5
		hwStrackPacketCVlan OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of strack."
			::= { hwStrackTrapObject 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1.6
		hwStrackPacketIfName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of strack."
			::= { hwStrackTrapObject 6 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1.7
		hwStrackSourceIp OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of strack."
			::= { hwStrackTrapObject 7 }
		
--  1.3.6.1.4.1.2011.5.25.165.2.1.1.8
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1.8
		hwStrackSlotid OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwStrackTrapObject 8 }
		
--  1.3.6.1.4.1.2011.5.25.165.2.1.1.9
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1.9
		hwStrackNormalAverage OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwStrackTrapObject 9 }
		
--  1.3.6.1.4.1.2011.5.25.165.2.1.1.10
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1.10
		hwStrackActualRate OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwStrackTrapObject 10 }
		
--  1.3.6.1.4.1.2011.5.25.165.2.1.1.11
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.1.11
		hwStrackPacketType OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwStrackTrapObject 11 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.2
		hwArpsTrapObject OBJECT IDENTIFIER ::= { hwSecurityTrapObject 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.2.1
		hwArpsSourceInterface OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of arp security."
			::= { hwArpsTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.2.2
		hwArpsSourceIp OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"TThe data of arp security."
			::= { hwArpsTrapObject 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.2.3
		hwArpsSourceMac OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of arp security."
			::= { hwArpsTrapObject 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.2.4
		hwArpsPVlan OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of arp security."
			::= { hwArpsTrapObject 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.2.5
		hwArpsCVlan OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of arp security."
			::= { hwArpsTrapObject 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.2.6
		hwArpsPacketDropNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The number of packets discarded by arp inspection .unit(packet)."
			::= { hwArpsTrapObject 6 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.2.7
		hwArpsAlarmThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The alarm threshold of dynamic arp inspection during the configured interval.unit(packet)."
			::= { hwArpsTrapObject 7 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.2.8
		hwArpsBlockTime OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of time which ARP Packet will be blocked. unit(second)."
			::= { hwArpsTrapObject 8 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.3
		hwIpsgTrapObject OBJECT IDENTIFIER ::= { hwSecurityTrapObject 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.3.1
		hwIpsgPacketDropNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of ip source check ."
			::= { hwIpsgTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.3.2
		hwIpsgAlarmThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The alarm threshold of ip source check during the configured interval.unit(packet)."
			::= { hwIpsgTrapObject 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.3.3
		hwIpsgSourceInterface OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of ip souce check."
			::= { hwIpsgTrapObject 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.4
		hwIcmpTrapObject OBJECT IDENTIFIER ::= { hwSecurityTrapObject 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.4.1
		hwIcmpPacketDropNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The number of packets discarded by ip source check .unit(packet)."
			::= { hwIcmpTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.4.2
		hwIcmpAlarmThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The alarm threshold of icmp defend during the configured interval.unit(packet)."
			::= { hwIcmpTrapObject 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.4.3
		hwIcmpSourceInterface OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The data of icmp security."
			::= { hwIcmpTrapObject 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.5
		hwDapTrapObject OBJECT IDENTIFIER ::= { hwSecurityTrapObject 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.5.1
		hwDapPortChange OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The alarm of dap port changed"
			::= { hwDapTrapObject 1 }
			
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.5.2
		hwDapDeviceIP OBJECT-TYPE
			SYNTAX IpAddress
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The IP address of interface bind to DAP service."
			::= { hwDapTrapObject 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.6
		hwCfgApTrapObject OBJECT IDENTIFIER ::= { hwSecurityTrapObject 6 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.6.1
		hwCfgApUserName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..128))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The name of user failed to configure access point."
			::= { hwCfgApTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.6.2
		hwCfgApIPAddress OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..128))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The IP-address of user failed to configure access point."
			::= { hwCfgApTrapObject 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.6.3
		hwCfgApApID OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The ID of access point failed to be configured."
			::= { hwCfgApTrapObject 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.6.4
		hwCfgApOperation OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..128))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The operation of confiuration to access point."
			::= { hwCfgApTrapObject 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.6.5
		hwCfgApReason OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..128))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The reason of failed to configure access point."
			::= { hwCfgApTrapObject 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.7
		hwCpcarTrapObject OBJECT IDENTIFIER ::= { hwSecurityTrapObject 7 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.7.1
		hwCpcarDropPacketSlotStr OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..32))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The slot in which rate of packets to cpu exceeded the cpcar limit."
			::= { hwCpcarTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.7.2
		hwCpcarDropPacketProtocol OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..32))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Rate of packets of the protocol exceeded the cpcar limit."
			::= { hwCpcarTrapObject 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.7.3
		hwCpcarDropPacketCir OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Committed information rate."
			::= { hwCpcarTrapObject 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.7.4
		hwCpcarDropPacketCbs OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Committed burst size of cpcar."
			::= { hwCpcarTrapObject 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.7.5
		hwCpcarDropPacketNum OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..32))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The number of packets discarded by cpcar."
			::= { hwCpcarTrapObject 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.7.6
		hwCpcarAutoDefendIfName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..32))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The interface name of autodefend by cpcar."
			::= { hwCpcarTrapObject 6 }
		
        -- 1.3.6.1.4.1.2011.5.25.165.2.1.7.7
		hwCpcarAutoDefendSlotStr OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..32))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The slot of autodefend by cpcar."
			::= { hwCpcarTrapObject 7 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.7.8
		hwCpcarAutoDefendProtocol OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (0..32))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The protocal of autodefend by cpcar."
			::= { hwCpcarTrapObject 8 }		
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.8
		hwMACsecTrapObject OBJECT IDENTIFIER ::= { hwSecurityTrapObject 8 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.8.1
		hwMACsecIfName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The name of MACsec failed interface."
			::= { hwMACsecTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.8.2
		hwMACsecReason OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Fail reason."
			::= { hwMACsecTrapObject 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.9
		hwStrackPortTrapObject OBJECT IDENTIFIER ::= { hwSecurityTrapObject 9 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.9.1
		hwStrackPortPacketIfName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The name of auto-port-defend interface."
			::= { hwStrackPortTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.9.2
		hwStrackPortPacketType OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Auto-port-defend attack protocol."
			::= { hwStrackPortTrapObject 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.10
		hwMplsTrapObject OBJECT IDENTIFIER ::= { hwSecurityTrapObject 10 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.10.1
		hwTeSourceInterfaceCheckTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwTeSourceInterfaceCheckEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"A table containing the Te Source interface check information for device."
			::= { hwMplsTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.10.1.1
		hwTeSourceInterfaceCheckEntry OBJECT-TYPE
			SYNTAX HwTeSourceInterfaceCheckEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Entries of the TE source interface check table."
			INDEX { hwRpfTeLabel, hwRpfPortName }
			::= { hwTeSourceInterfaceCheckTable 1 }
		
		HwTeSourceInterfaceCheckEntry ::=
			SEQUENCE { 
				hwRpfTeLabel
					Integer32,
				hwRpfPortName
					OCTET STRING
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.2.1.10.1.1.1
		hwRpfTeLabel OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"the te tunnel label"
			::= { hwTeSourceInterfaceCheckEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.1.10.1.1.2
		hwRpfPortName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (1..31))
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The Port Name."
			::= { hwTeSourceInterfaceCheckEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2
		hwSecurityTraps OBJECT IDENTIFIER ::= { hwMeSecurityMIBObjects 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.1
		hwStrackTrap OBJECT IDENTIFIER ::= { hwSecurityTraps 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.1.1
		hwStrackUserInfo NOTIFICATION-TYPE
			OBJECTS { hwStrackPacketIfName, hwStrackSourceMac, hwStrackPacketCVlan, hwStrackPacketPVlan, hwStrackEndTime, 
				hwStrackTotalPacket }
			STATUS current
			DESCRIPTION 
				"The user data of strack."
			::= { hwStrackTrap 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.1.2
		hwStrackIfVlanInfo NOTIFICATION-TYPE
			OBJECTS { hwStrackPacketIfName, hwStrackPacketCVlan, hwStrackPacketPVlan, hwStrackEndTime, hwStrackTotalPacket
				 }
			STATUS current
			DESCRIPTION 
				"The data of strack."
			::= { hwStrackTrap 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.1.3
		hwStrackDenyPacket NOTIFICATION-TYPE
			OBJECTS { hwStrackPacketIfName, hwStrackSourceMac, hwStrackSourceIp, hwStrackPacketCVlan, hwStrackPacketPVlan
				 }
			STATUS current
			DESCRIPTION 
				"The infomation of the packets discarded by strack."
			::= { hwStrackTrap 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.1.4
		hwStrackErrorDown NOTIFICATION-TYPE
			OBJECTS { hwStrackPacketIfName }
			STATUS current
			DESCRIPTION 
				"The interface that is shutdown by strack."
			::= { hwStrackTrap 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.1.5
		hwStrackIpInfo NOTIFICATION-TYPE
			OBJECTS { hwStrackPacketIfName, hwStrackSourceIp, hwStrackPacketCVlan, hwStrackPacketPVlan, hwStrackEndTime, 
				hwStrackTotalPacket }
			STATUS current
			DESCRIPTION 
				"The user data of strack."
			::= { hwStrackTrap 5 }
		
--  1.3.6.1.4.1.2011.5.25.165.2.2.1.6
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.1.6
		hwStrackUserAbnormal NOTIFICATION-TYPE
			OBJECTS { hwStrackSlotid, hwStrackSourceIp, hwStrackPacketType, hwStrackNormalAverage, hwStrackActualRate
				 }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwStrackTrap 6 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2
		hwArpsTrap OBJECT IDENTIFIER ::= { hwSecurityTraps 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.1
		hwArpsGatewayConflict NOTIFICATION-TYPE
			OBJECTS { hwArpsSourceInterface, hwArpsSourceIp, hwArpsSourceMac, hwArpsPVlan, hwArpsCVlan
				 }
			STATUS current
			DESCRIPTION 
				"The gateway conflict alarm is resumed."
			::= { hwArpsTrap 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.2
		hwArpsEntryCheck NOTIFICATION-TYPE
			OBJECTS { hwArpsSourceInterface, hwArpsSourceIp, hwArpsSourceMac, hwArpsPVlan, hwArpsCVlan
				 }
			STATUS current
			DESCRIPTION 
				"The arp talbe chekc alarm is resumed."
			::= { hwArpsTrap 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.3
		hwArpsPacketCheck NOTIFICATION-TYPE
			OBJECTS { hwArpsSourceInterface, hwArpsSourceIp, hwArpsSourceMac, hwArpsPVlan, hwArpsCVlan
				 }
			STATUS current
			DESCRIPTION 
				"The arp packet check alarm is resumed."
			::= { hwArpsTrap 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.4
		hwArpsDaiDropALarm NOTIFICATION-TYPE
			OBJECTS { hwArpsPacketDropNum, hwArpsAlarmThreshold, hwArpsSourceInterface }
			STATUS current
			DESCRIPTION 
				"The DAI alarm is resumed."
			::= { hwArpsTrap 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.5
		hwArpGlobleSpeedLimitALarm NOTIFICATION-TYPE
			OBJECTS { hwArpsAlarmThreshold }
			STATUS current
			DESCRIPTION 
				"The arp rate limit alarm is resumed."
			::= { hwArpsTrap 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.6
		hwArpIfSpeedLimitALarm NOTIFICATION-TYPE
			OBJECTS { hwArpsAlarmThreshold, hwArpsSourceInterface }
			STATUS current
			DESCRIPTION 
				"TThe arp rate limit alarm is resumed."
			::= { hwArpsTrap 6 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.7
		hwArpVlanSpeedLimitALarm NOTIFICATION-TYPE
			OBJECTS { hwArpsAlarmThreshold, hwArpsPVlan }
			STATUS current
			DESCRIPTION 
				"The arp rate limit alarm is resumed."
			::= { hwArpsTrap 7 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.8
		hwArpMissGlobleSpeedLimitALarm NOTIFICATION-TYPE
			OBJECTS { hwArpsAlarmThreshold }
			STATUS current
			DESCRIPTION 
				"The arp miss rate limit alarm is resumed."
			::= { hwArpsTrap 8 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.9
		hwArpMissIfSpeedLimitALarm NOTIFICATION-TYPE
			OBJECTS { hwArpsAlarmThreshold, hwArpsSourceInterface }
			STATUS current
			DESCRIPTION 
				"The arp miss rate limit alarm is resumed."
			::= { hwArpsTrap 9 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.10
		hwArpMissVlanSpeedLimitALarm NOTIFICATION-TYPE
			OBJECTS { hwArpsAlarmThreshold, hwArpsPVlan }
			STATUS current
			DESCRIPTION 
				"The arp miss rate limit alarm is resumed."
			::= { hwArpsTrap 10 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.11
		hwArpSourceIpSpeedLimitALarm NOTIFICATION-TYPE
			OBJECTS { hwArpsSourceIp, hwArpsAlarmThreshold }
			STATUS current
			DESCRIPTION 
				"The alarm of arp speed limit."
			::= { hwArpsTrap 11 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.12
		hwArpMissSourceIpSpeedLimitALarm NOTIFICATION-TYPE
			OBJECTS { hwArpsSourceIp, hwArpsAlarmThreshold }
			STATUS current
			DESCRIPTION 
				"The alarm of arp miss speed limit."
			::= { hwArpsTrap 12 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.13
		hwArpIfRateLimitBlockALarm NOTIFICATION-TYPE
			OBJECTS { hwArpsSourceInterface, hwArpsBlockTime }
			STATUS current
			DESCRIPTION 
				"The arp rate limit block alarm is resumed."
			::= { hwArpsTrap 13 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.14
		hwArpsLearnStrictCheck NOTIFICATION-TYPE
			OBJECTS { hwArpsSourceInterface, hwArpsSourceIp, hwArpsSourceMac, hwArpsPVlan }
			STATUS current
			DESCRIPTION 
				"The alarm of arp learn strict check."
			::= { hwArpsTrap 14 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.2.15
		hwArpSourceMacSpeedLimitALarm NOTIFICATION-TYPE
			OBJECTS { hwArpsSourceMac, hwArpsAlarmThreshold }
			STATUS current
			DESCRIPTION 
				"The alarm of arp speed limit."
			::= { hwArpsTrap 15 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.3
		hwIpsgTrap OBJECT IDENTIFIER ::= { hwSecurityTraps 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.3.1
		hwIpsgDropALarm NOTIFICATION-TYPE
			OBJECTS { hwIpsgPacketDropNum, hwIpsgAlarmThreshold, hwIpsgSourceInterface }
			STATUS current
			DESCRIPTION 
				"The ipsg alarm is resumed."
			::= { hwIpsgTrap 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.4
		hwIcmpTrap OBJECT IDENTIFIER ::= { hwSecurityTraps 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.4.1
		hwIcmpGlobleDropALarm NOTIFICATION-TYPE
			OBJECTS { hwIcmpAlarmThreshold }
			STATUS current
			DESCRIPTION 
				"The icmp rate limit alarm is resumed."
			::= { hwIcmpTrap 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.4.2
		hwIcmpIfDropALarm NOTIFICATION-TYPE
			OBJECTS { hwIcmpAlarmThreshold, hwIcmpSourceInterface }
			STATUS current
			DESCRIPTION 
				"The icmp rate limit alarm is resumed."
			::= { hwIcmpTrap 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.5
		hwDapTrap OBJECT IDENTIFIER ::= { hwSecurityTraps 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.5.1
		hwDapMibPortChange NOTIFICATION-TYPE
			OBJECTS { hwDapPortChange }
			STATUS current
			DESCRIPTION 
				"The dap port is changed."
			::= { hwDapTrap 1 }
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.5.2
		hwDapMibAuthRequest NOTIFICATION-TYPE
			OBJECTS { hwDapDeviceIP }
			STATUS current
			DESCRIPTION 
				"New device request authentication."
			::= { hwDapTrap 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.6
		hwCfgApTrap OBJECT IDENTIFIER ::= { hwSecurityTraps 6 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.6.1
		hwCfgApTrapFailAlarm NOTIFICATION-TYPE
			OBJECTS { hwCfgApUserName, hwCfgApIPAddress, hwCfgApApID, hwCfgApOperation, hwCfgApReason
				 }
			STATUS current
			DESCRIPTION 
				"The operation failed to config access point."
			::= { hwCfgApTrap 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.7
		hwCpcarTrap OBJECT IDENTIFIER ::= { hwSecurityTraps 7 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.7.1
		hwCpcarDropPacketAlarm NOTIFICATION-TYPE
			OBJECTS { hwCpcarDropPacketSlotStr, hwCpcarDropPacketProtocol, hwCpcarDropPacketCir, hwCpcarDropPacketCbs, hwCpcarDropPacketNum
				 }
			STATUS current
			DESCRIPTION 
				"The alarm of cpcar drop packets."
			::= { hwCpcarTrap 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.7.2
		hwCpcarDropPacketAlarmResume NOTIFICATION-TYPE
			OBJECTS { hwCpcarDropPacketSlotStr, hwCpcarDropPacketProtocol, hwCpcarDropPacketCir, hwCpcarDropPacketCbs, hwCpcarDropPacketNum
				 }
			STATUS current
			DESCRIPTION 
				"The resume alarm of cpcar drop packets."
			::= { hwCpcarTrap 2 }
			
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.7.3
		hwCpcarAutoPortDefendAlarm NOTIFICATION-TYPE
			OBJECTS { hwCpcarAutoDefendSlotStr, hwCpcarAutoDefendProtocol, hwCpcarAutoDefendIfName
				 }
			STATUS current
			DESCRIPTION 
				"The alarm of cpcar auto-port-defend."
			::= { hwCpcarTrap 3 }	
		
        -- 1.3.6.1.4.1.2011.5.25.165.2.2.7.4
		hwCpcarAutoPortDefendAlarmResume NOTIFICATION-TYPE
			OBJECTS { hwCpcarAutoDefendSlotStr, hwCpcarAutoDefendProtocol, hwCpcarAutoDefendIfName
				 }
			STATUS current
			DESCRIPTION 
				"The alarm of cpcar auto-port-defend."
			::= { hwCpcarTrap 4 }		
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.8
		hwMACsecTrap OBJECT IDENTIFIER ::= { hwSecurityTraps 8 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.8.1
		hwMACsecFailNotify NOTIFICATION-TYPE
			OBJECTS { hwMACsecIfName, hwMACsecReason }
			STATUS current
			DESCRIPTION 
				"The alarm of MACsec fail."
			::= { hwMACsecTrap 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.9
		hwStrackPortTrap OBJECT IDENTIFIER ::= { hwSecurityTraps 9 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.9.1
		hwStrackPortAtk NOTIFICATION-TYPE
			OBJECTS { hwStrackPortPacketIfName, hwStrackPortPacketType }
			STATUS current
			DESCRIPTION 
				"The alarm of auto-port-defend occurs."
			::= { hwStrackPortTrap 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.10
		hwMplsTrap OBJECT IDENTIFIER ::= { hwSecurityTraps 10 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.2.10.1
		hwTeSourceInterfaceCheckAlarm NOTIFICATION-TYPE
			OBJECTS { hwRpfTeLabel, hwRpfPortName }
			STATUS current
			DESCRIPTION 
				"The packets are discarded because they do not match the TE source interface."
			::= { hwMplsTrap 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.3
		hwTrafficSuppression OBJECT IDENTIFIER ::= { hwMeSecurityMIBObjects 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.3.1
		hwTrafficSuppressionTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwTrafficSuppressionEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				" The table lists the information about the configuration of traffic 
				suppression on an interface. "
			::= { hwTrafficSuppression 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.3.1.1
		hwTrafficSuppressionEntry OBJECT-TYPE
			SYNTAX HwTrafficSuppressionEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				" The table lists the information about traffic suppression protection."
			INDEX { hwTrafficSuppressionIfIndex }
			::= { hwTrafficSuppressionTable 1 }
		
		HwTrafficSuppressionEntry ::=
			SEQUENCE { 
				hwTrafficSuppressionIfIndex
					Integer32,
				hwTrafficSuppressionBcastRatio
					Integer32
			 }

		-- 1.3.6.1.4.1.2011.5.25.165.2.3.1.1.1
		hwTrafficSuppressionIfIndex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"The port index."
			::= { hwTrafficSuppressionEntry 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.2.3.1.1.2
		hwTrafficSuppressionBcastRatio OBJECT-TYPE
			SYNTAX Integer32 (0..100)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				" Broadcast-suppression ratio. Default is 100% . 100% indicates 
				that the broadcast isn't suppressed."
			::= { hwTrafficSuppressionEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11
		hwSecurityConformance OBJECT IDENTIFIER ::= { hwSecurityMIB 11 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.1
		hwSecurityCompliances OBJECT IDENTIFIER ::= { hwSecurityConformance 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.1.1
		hwSecurityCompliance MODULE-COMPLIANCE
			STATUS current
			DESCRIPTION 
				"The compliance statement for systems supporting 
				the HUAWEI-SECURITY-MIB."
			MODULE -- this module
				MANDATORY-GROUPS { hwLocalUrpfObjectGroup, hwTcpIpDefendObjectGroup, hwMaDefendObjectGroup, hwApplicationApperceiveObjectGroup, hwBaseSecurityNotificationsObjectGroup, 
					hwMeSecurityObjectGroup, hwMeSecurityTrapGroup, hwDefdPortVlanObjectGroup, hwSocAttackTrapGroup, hwAntiAttackObjectGroup
					 }
			::= { hwSecurityCompliances 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2
		hwBaseSecurityGroups OBJECT IDENTIFIER ::= { hwSecurityConformance 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2.2
		hwLocalUrpfObjectGroup OBJECT-GROUP
			OBJECTS { hwLocalUrpfCurrentRateLow, hwLocalUrpfCurrentRateHigh, hwLocalUrpfNotifyEnabledStatus, hwLocalUrpfRateThreshold, hwLocalUrpfRateInterval, 
				hwLocalUrpfChassisId, hwLocalUrpfSlotId }
			STATUS current
			DESCRIPTION 
				"The alarm parameter of URPF."
			::= { hwBaseSecurityGroups 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2.3
		hwTcpIpDefendObjectGroup OBJECT-GROUP
			OBJECTS { hwTcpIpDefendCurrentRateLow, hwTcpIpDefendCurrentRateHigh, hwTcpIpDefendNotifyEnabledStatus, hwTcpIpDefendRateThreshold, hwTcpIpDefendRateInterval, 
				hwTcpIpDefendChassisId, hwTcpIpDefendSlotId, hwTcpIpDefendType, hwTcpIpDefendProtocolDescirption }
			STATUS current
			DESCRIPTION 
				"The alarm parameter of TCPIP protection."
			::= { hwBaseSecurityGroups 3 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2.4
		hwMaDefendObjectGroup OBJECT-GROUP
			OBJECTS { hwMaDefendCurrentRateLow, hwMaDefendCurrentRateHigh, hwMaDefendNotifyEnabledStatus, hwMaDefendRateThreshold, hwMaDefendRateInterval, 
				hwMaDefendChassisId, hwMaDefendSlotId, hwMaDefendProtocol }
			STATUS current
			DESCRIPTION 
				"The alarm parameter of management and application protection."
			::= { hwBaseSecurityGroups 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2.5
		hwApplicationApperceiveObjectGroup OBJECT-GROUP
			OBJECTS { hwAppliApperCurrentRateLow, hwAppliApperCurrentRateHigh, hwAppliApperNotifyEnabledStatus, hwAppliApperRateThreshold, hwAppliApperRateInterval, 
				hwAppliApperChassisId, hwAppliApperSlotId, hwAppliApperProtocol, hwAppliApperProtocolDescirption }
			STATUS current
			DESCRIPTION 
				"The alarm parameter of Application-Apperceive protection."
			::= { hwBaseSecurityGroups 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2.6
		hwBaseSecurityNotificationsObjectGroup NOTIFICATION-GROUP
			NOTIFICATIONS { hwBaseSecurityUrpfDiscardedRateRising, hwBaseSecurityUrpfDiscardedRateResume, hwBaseSecurityTcpIpAttackDiscardedRateRising, hwBaseSecurityTcpIpAttackDiscardedRateResume, hwBaseSecurityMaDiscardedRateRising, 
				hwBaseSecurityMaDiscardedRateResume, hwBaseSecurityApplicationApperceiveDiscardedRateRising, hwBaseSecurityApplicationApperceiveDiscardedRateResume, hwBaseSecurityStormControlInterface, hwBaseSocAttackTrap, 
				hwBaseSocAttackResumeTrap, hwBaseSecurityStormControlInterfaceResume, hwBaseSecurityTtlExpiredLoop, hwBaseSecurityTtlExpiredLoopResume, hwBaseArpVlanCarTrap, 
				hwBaseArpVlanCarResumeTrap, hwBaseSecurityAntiAttackRateRising, hwBaseSecurityAntiAttackRateResume, hwBaseArpVlanCarEnhanceTrap, hwBaseArpVlanCarEnhanceResumeTrap, hwL3LoopDetectAlarm, hwL3LoopDetectAlarmResume
				 }
			STATUS current
			DESCRIPTION 
				"Total alarm of protection are resumed."
			::= { hwBaseSecurityGroups 6 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2.7
		hwMeSecurityObjectGroup OBJECT-GROUP
			OBJECTS { hwStrackTotalPacket, hwStrackEndTime, hwStrackSourceMac, hwStrackPacketPVlan, hwStrackPacketCVlan, 
				hwStrackPacketIfName, hwStrackSourceIp, hwArpsSourceInterface, hwArpsSourceIp, hwArpsSourceMac, 
				hwArpsPVlan, hwArpsCVlan, hwArpsPacketDropNum, hwArpsAlarmThreshold, hwArpsBlockTime, 
				hwIpsgPacketDropNum, hwIpsgAlarmThreshold, hwIpsgSourceInterface, hwIcmpPacketDropNum, hwIcmpAlarmThreshold, 
				hwIcmpSourceInterface, hwDapPortChange, hwCfgApUserName, hwCfgApIPAddress, hwCfgApApID, 
				hwCfgApOperation, hwCfgApReason, hwCpcarDropPacketSlotStr, hwCpcarDropPacketProtocol, hwCpcarDropPacketCir, 
				hwCpcarDropPacketCbs, hwCpcarDropPacketNum, hwMACsecIfName, hwMACsecReason, hwStrackPortPacketIfName, 
				hwStrackPortPacketType, hwCpcarAutoDefendIfName, hwCpcarAutoDefendSlotStr, hwCpcarAutoDefendProtocol, hwDapDeviceIP }
			STATUS current
			DESCRIPTION 
				"The alarm parameter of huawei base security group."
			::= { hwBaseSecurityGroups 7 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2.8
		hwMeSecurityTrapGroup NOTIFICATION-GROUP
			NOTIFICATIONS { hwStrackUserInfo, hwStrackIfVlanInfo, hwStrackDenyPacket, hwStrackErrorDown, hwStrackIpInfo, 
				hwArpsGatewayConflict, hwArpsEntryCheck, hwArpsPacketCheck, hwArpsDaiDropALarm, hwArpGlobleSpeedLimitALarm, 
				hwArpIfSpeedLimitALarm, hwArpVlanSpeedLimitALarm, hwArpMissGlobleSpeedLimitALarm, hwArpMissIfSpeedLimitALarm, hwArpMissVlanSpeedLimitALarm, 
				hwArpSourceIpSpeedLimitALarm, hwArpMissSourceIpSpeedLimitALarm, hwArpIfRateLimitBlockALarm, hwArpsLearnStrictCheck, hwArpSourceMacSpeedLimitALarm, 
				hwIpsgDropALarm, hwIcmpGlobleDropALarm, hwIcmpIfDropALarm, hwDapMibPortChange, hwCfgApTrapFailAlarm, 
				hwCpcarDropPacketAlarm, hwMACsecFailNotify, hwStrackPortAtk, hwTeSourceInterfaceCheckAlarm, hwCpcarDropPacketAlarmResume, hwCpcarAutoPortDefendAlarm,
				hwCpcarAutoPortDefendAlarmResume, hwDapMibAuthRequest
				 }
			STATUS current
			DESCRIPTION 
				"Total alarm of protection are resumed."
			::= { hwBaseSecurityGroups 8 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2.9
		hwDefdPortVlanObjectGroup OBJECT-GROUP
			OBJECTS { hwDefdPortVlanIfName, hwDefdPortVlanId, hwDefdPortVlanCheckProtocol }
			STATUS current
			DESCRIPTION 
				"The alarm parameter of l2 ring-route ."
			::= { hwBaseSecurityGroups 9 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2.11
		hwSocAttackTrapGroup OBJECT-GROUP
			OBJECTS { hwSocAttackSeqNo, hwSocAttackPossib, hwSocAttackReason, hwSocAttackIfName, hwSocAttackSubIfName, 
				hwSocAttackVlanIndex, hwSocAttackUserQinQIndex, hwSocAttackMacAddr, hwSocAttackIPAddr, hwSocAttackIPv6Addr
				 }
			STATUS current
			DESCRIPTION 
				"The alarm parameter of Security Operation Center"
			::= { hwBaseSecurityGroups 11 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2.12
		hwAntiAttackObjectGroup OBJECT-GROUP
			OBJECTS { hwAntiAttackType, hwAntiAttackRateThreshold, hwAntiAttackCurrentRate }
			STATUS current
			DESCRIPTION 
				"The alarm parameter of anti-attack alarm."
			::= { hwBaseSecurityGroups 12 }
		
		-- 1.3.6.1.4.1.2011.5.25.165.11.2.13
		hwTeSourceInterfaceCheckGroup OBJECT-GROUP
			OBJECTS { hwRpfTeLabel, hwRpfPortName }
			STATUS current
			DESCRIPTION 
				"A collection of items of te source interface check."
			::= { hwBaseSecurityGroups 13 }
		
	
	END

--
-- HUAWEI-SECURITY-MIB.mib
--