-- =================================================================
-- Copyright (C) 2017 by  HUAWEI TECHNOLOGIES. All rights reserved.
--
-- Description: task mib
-- Reference:   huawei enterprise mib
-- Version:     V2.02
-- History:
--                initial version 2003-07-31
-- =================================================================

HUAWEI-TASK-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        hwDatacomm
            FROM HUAWEI-MIB            
        OBJECT-GROUP, MODULE-COMPLIANCE            
            FROM SNMPv2-CONF            
        Gauge32, OBJECT-TYPE, MODULE-IDENTITY, Integer32
            FROM SNMPv2-SMI            
        DisplayString, TEXTUAL-CONVENTION            
            FROM SNMPv2-TC;

    hwTask MODULE-IDENTITY 
        LAST-UPDATED "201708170000Z"        -- 08 17, 2017 at 00:00 GMT
        ORGANIZATION 
            "Huawei Technologies Co.,Ltd."
        CONTACT-INFO 
            "Huawei Industrial Base
              Bantian, Longgang
               Shenzhen 518129
               People's Republic of China
               Website: http://www.huawei.com
               Email: support@huawei.com
             "
        DESCRIPTION 
            "The MIB module describes active system tasks, including the status 
            and the general information of a task."
	
        REVISION "201708170000Z"        -- 08 17, 2017 at 00:00 GMT
        DESCRIPTION
            "V2.02, Modify hwKeyTaskIndex."
    
        REVISION "201409250000Z"        -- 09 25, 2014 at 00:00 GMT
        DESCRIPTION
            "V2.01, modify hwKeyTaskIndex, hwKeyTaskID and hwKeyTaskName."
  
        REVISION "200307310000Z"        -- 07 31, 2002 at 00:00 GMT
        DESCRIPTION
            "Initial version of this MIB module."
        ::= { hwDatacomm 27 }

    --
    -- Textual conventions
    --

    HwTaskStatusType ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION 
            "The status of the specified task. The parameter have seventeen different value.
            Normally a task may be status of the following:
            Normalready(0): task is ready,
            Block(1): task is blocked,
            Slept(2): task is slept,
            Suspend(4): task is suspended blocked,
            BlockAndSuspend(5): task is suspended blocked,
            SleptAndSuspend(6): task is slept and suspended,
            running(8): task is running,
            Queueblock(17): task is blocked on receiving queue messages,
            QueueblockAndSuspend(21): task is blocked on receiving queue messages and suspended,
            Semaphoreblock(33): task is blocked on taking a semaphore,
            SemaphoreblockAandSuspend(37): task is blocked on taking a semaphore and suspended,
            Eventblock(65): task is blocked on receiving events,
            EventblockAndSuspend(69): task is blocked on receiving events and suspended,
            prioblock(128): task is priblock,
            Preemptready(256): task is preempt ready,
            Writequeueblock(513): task is blocked on sending queue messages,
            WritequeueblockAndSuspend(517): task is blocked on sending queue messages and suspended."
        SYNTAX INTEGER
            {
            normalready(0),
            block(1),
            sleep(2),
            suspend(4),
            blockAndSuspend(5),
            sleptAndSuspend(6),
            running(8),
            queueblock(17),
            queueblockAndSuspend(21),
            semaphoreblock(33),
            semaphoreblockAandSuspend(37),
            eventblock(65),
            eventblockAndSuspend(69),
            prioblock(128),
            preemptready(256),
            writequeueblock(513),
            writequeueblockAndSuspend(517)
            }

    --
    -- Node definitions
    --

    -- 1.3.6.1.4.1.2011.5.109.1
    hwTaskObjects OBJECT IDENTIFIER ::= { hwTask 1 }
    
    --  huawei task Common Table
    -- 1.3.6.1.4.1.2011.5.109.1.1
    hwTaskTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwTaskEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table of generic information on all active 
            tasks on this device."
        ::= { hwTaskObjects 1 }
    
    -- 1.3.6.1.4.1.2011.5.109.1.1.1
    hwTaskEntry OBJECT-TYPE
        SYNTAX HwTaskEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Generic information about active tasks on this 
            device. Entries in this table will change when tasks are 
            created and destroyed on the device."
        INDEX { hwTaskIndex, hwTaskID }
        ::= { hwTaskTable 1 }
    
    HwTaskEntry ::=
        SEQUENCE { 
            hwTaskIndex
                Gauge32,
            hwTaskID
                Gauge32,
            hwTaskName
                DisplayString,
            hwTaskStatus
                HwTaskStatusType,
            hwTaskCpuUsage
                Gauge32,
            hwTaskuSecs
                Gauge32
         }

    -- 1.3.6.1.4.1.2011.5.109.1.1.1.1
    hwTaskIndex OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The object indicates some physical information, such as slot number of VIU 
            or RSU board plugged in. "
        ::= { hwTaskEntry 1 }
    
    -- 1.3.6.1.4.1.2011.5.109.1.1.1.2
    hwTaskID OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This object contains the task ID. "
        ::= { hwTaskEntry 2 }
    
    -- 1.3.6.1.4.1.2011.5.109.1.1.1.3
    hwTaskName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (1..255))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The name associated with this task. If the name is
            longer than 255 characters, it will be truncated to the first
            255 characters."
        ::= { hwTaskEntry 3 }
    
    -- 1.3.6.1.4.1.2011.5.109.1.1.1.4
    hwTaskStatus OBJECT-TYPE
        SYNTAX HwTaskStatusType
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The status of the specified task. The parameter have seventeen different value.
            Normally a task may be status of the following:
            normalready(0): task is ready,  
            block(1): task is blocked,
            slept(2): task is slept,
            suspend(4): task is suspended blocked,
            blockAndSuspend(5): task is suspended blocked,
            sleepAndSuspend(6): task is slept and suspended,
            running(8): task is running,
            queueblock(17): task is blocked on receiving queue messages,
            queueblockAndSuspend(21): task is blocked on receiving queue messages and suspended,
            semaphoreblock(33): task is blocked on taking a semaphore,
            semaphoreblockAandSuspend(37): task is blocked on taking a semaphore and suspended,
            eventblock(65): task is blocked on receiving events,
            eventblockAndSuspend(69): task is blocked on receiving events and suspended,
            prioblock(128): task is priblock,
            preemptready(256): task is preempt ready,
            writequeueblock(513): task is blocked on sending queue messages,
            writequeueblockAndSuspend(517): task is blocked on sending queue messages and suspended."
        ::= { hwTaskEntry 4 }
    
    -- 1.3.6.1.4.1.2011.5.109.1.1.1.5
    hwTaskCpuUsage OBJECT-TYPE
        SYNTAX Gauge32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Cpu usage information of this task(0%-100%).If a task's cpu usage is more than 90, 
            it means that the task is very busy."
        ::= { hwTaskEntry 5 }
    
    -- 1.3.6.1.4.1.2011.5.109.1.1.1.6
    hwTaskuSecs OBJECT-TYPE
        SYNTAX Gauge32
        UNITS "millseconds"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Average elapsed CPU time in millseconds when the task was active."
        ::= { hwTaskEntry 6 }
    
        hwKeyTaskTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwKeyTaskEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A table of generic information on all active 
                tasks on this device."
            ::= { hwTaskObjects 2 }
        
        hwKeyTaskEntry OBJECT-TYPE
            SYNTAX HwKeyTaskEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Generic information about active tasks on this 
                device. Entries in this table will change when tasks are 
                created and destroyed on the device."
            INDEX { hwKeyTaskIndex, hwKeyTaskID }
            ::= { hwKeyTaskTable 1 }
        
        HwKeyTaskEntry ::=
            SEQUENCE { 
                hwKeyTaskIndex
                    Integer32,
                hwKeyTaskID
                    Integer32,
                hwKeyTaskName
                    DisplayString,
                hwKeyTaskCpuUsage
                    Integer32
             }

        hwKeyTaskIndex OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Specifies the slot ID of the task. Currently, the MIB provides information only about the main control board. The value of TaskIndex is 0 in centralized system mode; the value of TaskIndex is the slot ID of the main control board in distributed system mode. "
            ::= { hwKeyTaskEntry 1 }
        
        hwKeyTaskID OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object contains the task ID. "
            ::= { hwKeyTaskEntry 2 }
        
        hwKeyTaskName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..255))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The name associated with this task. If the name is
                longer than 255 characters, it will be truncated to the first
                255 characters."
            ::= { hwKeyTaskEntry 3 }
        
        hwKeyTaskCpuUsage OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Cpu usage information of this task(0%-100%).If a task's cpu usage is more than 90, 
                it means that the task is very busy."
            ::= { hwKeyTaskEntry 4 }
        
    -- 1.3.6.1.4.1.2011.5.109.2
    hwTaskNotifications OBJECT IDENTIFIER ::= { hwTask 2 }
    
    --  (no notifications are currently defined)
    -- conformance information
    -- 1.3.6.1.4.1.2011.5.109.3
    hwTaskConformance OBJECT IDENTIFIER ::= { hwTask 3 }
    
    -- 1.3.6.1.4.1.2011.5.109.3.1
    hwTaskCompliances OBJECT IDENTIFIER ::= { hwTaskConformance 1 }
    
    --  this module
    -- 1.3.6.1.4.1.2011.5.109.3.1.1
    hwTaskCompliance MODULE-COMPLIANCE
        STATUS current
        DESCRIPTION 
            "The compliance statement for entities which implement
            the huawei Task MIB,Write access is not required."
        MODULE -- this module
            MANDATORY-GROUPS { hwTaskGroup }
        ::= { hwTaskCompliances 1 }
    
    -- 1.3.6.1.4.1.2011.5.109.3.2
    hwTaskGroups OBJECT IDENTIFIER ::= { hwTaskConformance 2 }
    
    --  units of conformance
    -- 1.3.6.1.4.1.2011.5.109.3.2.1
    hwTaskGroup OBJECT-GROUP
        OBJECTS { hwTaskName, hwTaskStatus, hwTaskCpuUsage, hwTaskuSecs }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing common task 
            monitoring information. This group is mandatory for 
            all huawei devices."
        ::= { hwTaskGroups 1 }
        hwKeyTaskGroup OBJECT-GROUP
            OBJECTS { hwKeyTaskName, hwKeyTaskCpuUsage }
            STATUS current
            DESCRIPTION 
                "A collection of objects providing common task 
                monitoring information. This group is mandatory for 
                all huawei devices."
            ::= { hwTaskGroups 2 }
    

END