-- ============================================================================
-- Copyright (C) 2015 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- Description:  The mib is used for configuring the information of the SAC.
-- Reference: 
-- Version: V1.01
-- ============================================================================
-- Module definition

	HUAWEI-WLAN-SAC-MIB DEFINITIONS ::= BEGIN

		IMPORTS
			hwWlan
				FROM HUAWEI-WLAN-MIB
			OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP
				FROM SNMPv2-CONF
			IpAddress, Integer32, Unsigned32, Counter64, OBJECT-TYPE,
			MODULE-IDENTITY, NOTIFICATION-TYPE
				FROM SNMPv2-SMI
			MacAddress, RowStatus, DateAndTime
				FROM SNMPv2-TC;
		--1.3.6.1.4.1.2011.6.139.20
		hwWlanSac MODULE-IDENTITY
			LAST-UPDATED "201506190900Z"		-- June 19, 2015 at 09:00 GMT
			ORGANIZATION
				"Huawei Technologies Co.,Ltd."
			CONTACT-INFO
			 "Huawei Industrial Base
				   Bantian, Longgang
				   Shenzhen 518129
				   People's Republic of China
				   Website: http://www.huawei.com
				   Email: support@huawei.com
				  "
                        DESCRIPTION 
				"The MIB module defines the information of the SAC."
	                REVISION "201506190900Z"		-- June 19, 2015 at 09:00 GMT
			DESCRIPTION
				"V1.01, Inital version."
	                REVISION "201502120900Z"		-- February 12, 2015 at 09:00 GMT
			DESCRIPTION
				"V1.00, Inital version."
			::= { hwWlan 20 }

--
--Node definitions
--

		--1.3.6.1.4.1.2011.6.139.20.1
		hwSacObjects OBJECT IDENTIFIER ::= { hwWlanSac 1 }

		--1.3.6.1.4.1.2011.6.139.20.1.1
		hwSACEnableConfig OBJECT IDENTIFIER ::= { hwSacObjects 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.1.1
		hwSACEnableOper OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(1),
				enable(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACEnableConfig 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.1.2
		hwSACEnableRuleLibName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (1..32))
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACEnableConfig 2 }

		--1.3.6.1.4.1.2011.6.139.20.1.2
		hwSACProtocolGroupTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwSACProtocolGroupEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSacObjects 2 }

		--1.3.6.1.4.1.2011.6.139.20.1.2.1
		hwSACProtocolGroupEntry OBJECT-TYPE
			SYNTAX HwSACProtocolGroupEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			INDEX { hwSACProtocolGroupName }
			::= { hwSACProtocolGroupTable 1 }


		HwSACProtocolGroupEntry ::=
			SEQUENCE {				
				hwSACProtocolGroupName
					OCTET STRING,
				hwSACProtocolGroupRowstatus
					RowStatus 
			 }

		 --1.3.6.1.4.1.2011.6.139.20.1.2.1.1
		hwSACProtocolGroupName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (1..35))
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACProtocolGroupEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.2.1.2
		hwSACProtocolGroupRowstatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACProtocolGroupEntry 2 }

		--1.3.6.1.4.1.2011.6.139.20.1.3
		hwSACProGroupProTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwSACProGroupProEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSacObjects 3 }

		--1.3.6.1.4.1.2011.6.139.20.1.3.1
		hwSACProGroupProEntry OBJECT-TYPE
			SYNTAX HwSACProGroupProEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			INDEX { hwSACProtocolGroupName, hwSACProtocolName }
			::= { hwSACProGroupProTable 1 }


		HwSACProGroupProEntry ::=
			SEQUENCE {				
				hwSACProtocolName
					OCTET STRING,
				hwSACProGroupProRowstatus
					RowStatus 
			 }

		 --1.3.6.1.4.1.2011.6.139.20.1.3.1.1
		hwSACProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACProGroupProEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.3.1.2
		hwSACProGroupProRowstatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACProGroupProEntry 2 }

		--1.3.6.1.4.1.2011.6.139.20.1.4
		hwSACVapStatTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwSACVapStatEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSacObjects 4 }

		--1.3.6.1.4.1.2011.6.139.20.1.4.1
		hwSACVapStatEntry OBJECT-TYPE
			SYNTAX HwSACVapStatEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			INDEX { hwSACVapStatApName, hwSACVapStatRadioId, hwSACVapStatSsid, hwSACVapStatProtocolIndex, hwSACVapStatType }
			::= { hwSACVapStatTable 1 }


		HwSACVapStatEntry ::=
			SEQUENCE {				
				hwSACVapStatApName
					OCTET STRING,
				hwSACVapStatRadioId
					Integer32,
				hwSACVapStatSsid
					OCTET STRING,
				hwSACVapStatProtocolIndex
					Integer32,
				hwSACVapStatType
					INTEGER,
				hwSACVapStatProtocolName
					OCTET STRING,
				hwSACVapStatProtocolPktUpNum
					Counter64,
				hwSACVapStatProtocolByteUpNum
					Counter64,
				hwSACVapStatProtocolPktDnNum
					Counter64,
				hwSACVapStatProtocolByteDnNum
					Counter64,
				hwSACVapStatClear
					Integer32,
				hwSACVapStatRowstatus
					RowStatus 
			 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.1
		hwSACVapStatApName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.2
		hwSACVapStatRadioId OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.3
		hwSACVapStatSsid OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.4
		hwSACVapStatProtocolIndex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 4 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.5
		hwSACVapStatType OBJECT-TYPE
			SYNTAX INTEGER
				{
				total(1),
				period(2)
				}
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 5 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.6
		hwSACVapStatProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 6 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.7
		hwSACVapStatProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 7 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.8
		hwSACVapStatProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 8 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.9
		hwSACVapStatProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 9 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.10
		hwSACVapStatProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 10 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.11
		hwSACVapStatClear OBJECT-TYPE
			SYNTAX Integer32 (1)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 11 }

		 --1.3.6.1.4.1.2011.6.139.20.1.4.1.12
		hwSACVapStatRowstatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapStatEntry 12 }

		--1.3.6.1.4.1.2011.6.139.20.1.5
		hwSACUserStatTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwSACUserStatEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSacObjects 5 }

		--1.3.6.1.4.1.2011.6.139.20.1.5.1
		hwSACUserStatEntry OBJECT-TYPE
			SYNTAX HwSACUserStatEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			INDEX { hwSACUserStatUserMac, hwSACUserStatProtocolIndex, hwSACUserStatType }
			::= { hwSACUserStatTable 1 }


		HwSACUserStatEntry ::=
			SEQUENCE {				
				hwSACUserStatUserMac
					MacAddress,
				hwSACUserStatProtocolIndex
					Integer32,
				hwSACUserStatType
					INTEGER,
				hwSACUserStatProtocolName
					OCTET STRING,
				hwSACUserStatProtocolPktUpNum
					Counter64,
				hwSACUserStatProtocolByteUpNum
					Counter64,
				hwSACUserStatProtocolPktDnNum
					Counter64,
				hwSACUserStatProtocolByteDnNum
					Counter64,
				hwSACUserStatClear
					Integer32,
				hwSACUserStatRowstatus
					RowStatus 
			 }

		 --1.3.6.1.4.1.2011.6.139.20.1.5.1.1
		hwSACUserStatUserMac OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserStatEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.5.1.2
		hwSACUserStatProtocolIndex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserStatEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.20.1.5.1.3
		hwSACUserStatType OBJECT-TYPE
			SYNTAX INTEGER
				{
				total(1),
				period(2)
				}
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserStatEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.20.1.5.1.4
		hwSACUserStatProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserStatEntry 4 }

		 --1.3.6.1.4.1.2011.6.139.20.1.5.1.5
		hwSACUserStatProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserStatEntry 5 }

		 --1.3.6.1.4.1.2011.6.139.20.1.5.1.6
		hwSACUserStatProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserStatEntry 6 }

		 --1.3.6.1.4.1.2011.6.139.20.1.5.1.7
		hwSACUserStatProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserStatEntry 7 }

		 --1.3.6.1.4.1.2011.6.139.20.1.5.1.8
		hwSACUserStatProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserStatEntry 8 }

		 --1.3.6.1.4.1.2011.6.139.20.1.5.1.9
		hwSACUserStatClear OBJECT-TYPE
			SYNTAX Integer32 (1)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserStatEntry 9 }

		 --1.3.6.1.4.1.2011.6.139.20.1.5.1.10
		hwSACUserStatRowstatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserStatEntry 10 }

		--1.3.6.1.4.1.2011.6.139.20.1.6
		hwSACAppListTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwSACAppListEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSacObjects 6 }

		--1.3.6.1.4.1.2011.6.139.20.1.6.1
		hwSACAppListEntry OBJECT-TYPE
			SYNTAX HwSACAppListEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			INDEX { hwSACAppListAppIndex }
			::= { hwSACAppListTable 1 }


		HwSACAppListEntry ::=
			SEQUENCE {				
				hwSACAppListAppIndex
					Integer32,
				hwSACAppListAppID
					Integer32,
				hwSACAppListAppName
					OCTET STRING,
				hwSACAppListRowstatus
					RowStatus 
			 }

		 --1.3.6.1.4.1.2011.6.139.20.1.6.1.1
		hwSACAppListAppIndex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACAppListEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.6.1.2
		hwSACAppListAppID OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACAppListEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.20.1.6.1.3
		hwSACAppListAppName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACAppListEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.20.1.6.1.4
		hwSACAppListRowstatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACAppListEntry 4 }

		--1.3.6.1.4.1.2011.6.139.20.1.7
		hwSACInfo OBJECT IDENTIFIER ::= { hwSacObjects 7 }

		 --1.3.6.1.4.1.2011.6.139.20.1.7.1
		hwSACInfoSACEnable OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(1),
				enable(2)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACInfo 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.7.2
		hwSACInfoSignatureState OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(1),
				enable(2)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACInfo 2 }

		 --1.3.6.1.4.1.2011.6.139.20.1.7.3
		hwSACInfoSignatureName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (1..128))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACInfo 3 }

		 --1.3.6.1.4.1.2011.6.139.20.1.7.4
		hwSACInfoSignatureVersion OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (1..64))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACInfo 4 }

		 --1.3.6.1.4.1.2011.6.139.20.1.7.5
		hwSACInfoSignatureDate OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (1..64))
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACInfo 5 }

		 --1.3.6.1.4.1.2011.6.139.20.1.7.6
		hwSACInfoAppNum OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACInfo 6 }

		--1.3.6.1.4.1.2011.6.139.20.1.8
		hwSACVapTop10StatTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwSACVapTop10StatEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSacObjects 8 }

		--1.3.6.1.4.1.2011.6.139.20.1.8.1
		hwSACVapTop10StatEntry OBJECT-TYPE
			SYNTAX HwSACVapTop10StatEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			INDEX { hwSACVapTop10StatApName, hwSACVapTop10StatRadioId, hwSACVapTop10StatSsid, hwSACVapTop10StatType }
			::= { hwSACVapTop10StatTable 1 }


		HwSACVapTop10StatEntry ::=
			SEQUENCE {				
				hwSACVapTop10StatApName
					OCTET STRING,
				hwSACVapTop10StatRadioId
					Integer32,
				hwSACVapTop10StatSsid
					OCTET STRING,
				hwSACVapTop10StatType
					INTEGER,
				hwSACVapStatTotalPktUpNum
					Counter64,
				hwSACVapStatTotalByteUpNum
					Counter64,
				hwSACVapStatTotalPktDnNum
					Counter64,
				hwSACVapStatTotalByteDnNum
					Counter64,
				hwSACVapStat1stProtocolName
					OCTET STRING,
				hwSACVapStat1stProtocolPktUpNum
					Counter64,
				hwSACVapStat1stProtocolByteUpNum
					Counter64,
				hwSACVapStat1stProtocolPktDnNum
					Counter64,
				hwSACVapStat1stProtocolByteDnNum
					Counter64,
				hwSACVapStat2ndProtocolName
					OCTET STRING,
				hwSACVapStat2ndProtocolPktUpNum
					Counter64,
				hwSACVapStat2ndProtocolByteUpNum
					Counter64,
				hwSACVapStat2ndProtocolPktDnNum
					Counter64,
				hwSACVapStat2ndProtocolByteDnNum
					Counter64,
				hwSACVapStat3rdProtocolName
					OCTET STRING,
				hwSACVapStat3rdProtocolPktUpNum
					Counter64,
				hwSACVapStat3rdProtocolByteUpNum
					Counter64,
				hwSACVapStat3rdProtocolPktDnNum
					Counter64,
				hwSACVapStat3rdProtocolByteDnNum
					Counter64,
				hwSACVapStat4thProtocolName
					OCTET STRING,
				hwSACVapStat4thProtocolPktUpNum
					Counter64,
				hwSACVapStat4thProtocolByteUpNum
					Counter64,
				hwSACVapStat4thProtocolPktDnNum
					Counter64,
				hwSACVapStat4thProtocolByteDnNum
					Counter64,
				hwSACVapStat5thProtocolName
					OCTET STRING,
				hwSACVapStat5thProtocolPktUpNum
					Counter64,
				hwSACVapStat5thProtocolByteUpNum
					Counter64,
				hwSACVapStat5thProtocolPktDnNum
					Counter64,
				hwSACVapStat5thProtocolByteDnNum
					Counter64,
				hwSACVapStat6thProtocolName
					OCTET STRING,
				hwSACVapStat6thProtocolPktUpNum
					Counter64,
				hwSACVapStat6thProtocolByteUpNum
					Counter64,
				hwSACVapStat6thProtocolPktDnNum
					Counter64,
				hwSACVapStat6thProtocolByteDnNum
					Counter64,
				hwSACVapStat7thProtocolName
					OCTET STRING,
				hwSACVapStat7thProtocolPktUpNum
					Counter64,
				hwSACVapStat7thProtocolByteUpNum
					Counter64,
				hwSACVapStat7thProtocolPktDnNum
					Counter64,
				hwSACVapStat7thProtocolByteDnNum
					Counter64,
				hwSACVapStat8thProtocolName
					OCTET STRING,
				hwSACVapStat8thProtocolPktUpNum
					Counter64,
				hwSACVapStat8thProtocolByteUpNum
					Counter64,
				hwSACVapStat8thProtocolPktDnNum
					Counter64,
				hwSACVapStat8thProtocolByteDnNum
					Counter64,
				hwSACVapStat9thProtocolName
					OCTET STRING,
				hwSACVapStat9thProtocolPktUpNum
					Counter64,
				hwSACVapStat9thProtocolByteUpNum
					Counter64,
				hwSACVapStat9thProtocolPktDnNum
					Counter64,
				hwSACVapStat9thProtocolByteDnNum
					Counter64,
				hwSACVapStat10thProtocolName
					OCTET STRING,
				hwSACVapStat10thProtocolPktUpNum
					Counter64,
				hwSACVapStat10thProtocolByteUpNum
					Counter64,
				hwSACVapStat10thProtocolPktDnNum
					Counter64,
				hwSACVapStat10thProtocolByteDnNum
					Counter64,
				hwSACVapTop10StatClear
					Integer32,
				hwSACVapTop10StatRowstatus
					RowStatus 
			 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.1
		hwSACVapTop10StatApName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (1..32))
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.2
		hwSACVapTop10StatRadioId OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.3
		hwSACVapTop10StatSsid OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.4
		hwSACVapTop10StatType OBJECT-TYPE
			SYNTAX INTEGER
				{
				total(1),
				period(2)
				}
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 4 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.5
		hwSACVapStatTotalPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 5 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.6
		hwSACVapStatTotalByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 6 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.7
		hwSACVapStatTotalPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 7 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.8
		hwSACVapStatTotalByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 8 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.9
		hwSACVapStat1stProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 9 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.10
		hwSACVapStat1stProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 10 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.11
		hwSACVapStat1stProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 11 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.12
		hwSACVapStat1stProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 12 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.13
		hwSACVapStat1stProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 13 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.14
		hwSACVapStat2ndProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 14 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.15
		hwSACVapStat2ndProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 15 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.16
		hwSACVapStat2ndProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 16 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.17
		hwSACVapStat2ndProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 17 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.18
		hwSACVapStat2ndProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 18 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.19
		hwSACVapStat3rdProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 19 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.20
		hwSACVapStat3rdProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 20 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.21
		hwSACVapStat3rdProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 21 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.22
		hwSACVapStat3rdProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 22 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.23
		hwSACVapStat3rdProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 23 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.24
		hwSACVapStat4thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 24 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.25
		hwSACVapStat4thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 25 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.26
		hwSACVapStat4thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 26 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.27
		hwSACVapStat4thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 27 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.28
		hwSACVapStat4thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 28 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.29
		hwSACVapStat5thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 29 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.30
		hwSACVapStat5thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 30 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.31
		hwSACVapStat5thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 31 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.32
		hwSACVapStat5thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 32 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.33
		hwSACVapStat5thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 33 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.34
		hwSACVapStat6thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 34 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.35
		hwSACVapStat6thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 35 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.36
		hwSACVapStat6thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 36 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.37
		hwSACVapStat6thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 37 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.38
		hwSACVapStat6thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 38 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.39
		hwSACVapStat7thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 39 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.40
		hwSACVapStat7thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 40 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.41
		hwSACVapStat7thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 41 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.42
		hwSACVapStat7thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 42 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.43
		hwSACVapStat7thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 43 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.44
		hwSACVapStat8thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 44 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.45
		hwSACVapStat8thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 45 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.46
		hwSACVapStat8thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 46 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.47
		hwSACVapStat8thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 47 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.48
		hwSACVapStat8thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 48 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.49
		hwSACVapStat9thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 49 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.50
		hwSACVapStat9thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 50 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.51
		hwSACVapStat9thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 51 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.52
		hwSACVapStat9thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 52 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.53
		hwSACVapStat9thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 53 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.54
		hwSACVapStat10thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 54 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.55
		hwSACVapStat10thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 55 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.56
		hwSACVapStat10thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 56 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.57
		hwSACVapStat10thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 57 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.58
		hwSACVapStat10thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 58 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.59
		hwSACVapTop10StatClear OBJECT-TYPE
			SYNTAX Integer32 (1)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 59 }

		 --1.3.6.1.4.1.2011.6.139.20.1.8.1.60
		hwSACVapTop10StatRowstatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACVapTop10StatEntry 60 }

		--1.3.6.1.4.1.2011.6.139.20.1.9
		hwSACUserTop10StatTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwSACUserTop10StatEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSacObjects 9 }

		--1.3.6.1.4.1.2011.6.139.20.1.9.1
		hwSACUserTop10StatEntry OBJECT-TYPE
			SYNTAX HwSACUserTop10StatEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			INDEX { hwSACUserTop10StatUserMac, hwSACUserTop10StatType }
			::= { hwSACUserTop10StatTable 1 }


		HwSACUserTop10StatEntry ::=
			SEQUENCE {				
				hwSACUserTop10StatUserMac
					MacAddress,
				hwSACUserTop10StatType
					INTEGER,
				hwSACUserStatTotalPktUpNum
					Counter64,
				hwSACUserStatTotalByteUpNum
					Counter64,
				hwSACUserStatTotalPktDnNum
					Counter64,
				hwSACUserStatTotalByteDnNum
					Counter64,
				hwSACUserStat1stProtocolName
					OCTET STRING,
				hwSACUserStat1stProtocolPktUpNum
					Counter64,
				hwSACUserStat1stProtocolByteUpNum
					Counter64,
				hwSACUserStat1stProtocolPktDnNum
					Counter64,
				hwSACUserStat1stProtocolByteDnNum
					Counter64,
				hwSACUserStat2ndProtocolName
					OCTET STRING,
				hwSACUserStat2ndProtocolPktUpNum
					Counter64,
				hwSACUserStat2ndProtocolByteUpNum
					Counter64,
				hwSACUserStat2ndProtocolPktDnNum
					Counter64,
				hwSACUserStat2ndProtocolByteDnNum
					Counter64,
				hwSACUserStat3rdProtocolName
					OCTET STRING,
				hwSACUserStat3rdProtocolPktUpNum
					Counter64,
				hwSACUserStat3rdProtocolByteUpNum
					Counter64,
				hwSACUserStat3rdProtocolPktDnNum
					Counter64,
				hwSACUserStat3rdProtocolByteDnNum
					Counter64,
				hwSACUserStat4thProtocolName
					OCTET STRING,
				hwSACUserStat4thProtocolPktUpNum
					Counter64,
				hwSACUserStat4thProtocolByteUpNum
					Counter64,
				hwSACUserStat4thProtocolPktDnNum
					Counter64,
				hwSACUserStat4thProtocolByteDnNum
					Counter64,
				hwSACUserStat5thProtocolName
					OCTET STRING,
				hwSACUserStat5thProtocolPktUpNum
					Counter64,
				hwSACUserStat5thProtocolByteUpNum
					Counter64,
				hwSACUserStat5thProtocolPktDnNum
					Counter64,
				hwSACUserStat5thProtocolByteDnNum
					Counter64,
				hwSACUserStat6thProtocolName
					OCTET STRING,
				hwSACUserStat6thProtocolPktUpNum
					Counter64,
				hwSACUserStat6thProtocolByteUpNum
					Counter64,
				hwSACUserStat6thProtocolPktDnNum
					Counter64,
				hwSACUserStat6thProtocolByteDnNum
					Counter64,
				hwSACUserStat7thProtocolName
					OCTET STRING,
				hwSACUserStat7thProtocolPktUpNum
					Counter64,
				hwSACUserStat7thProtocolByteUpNum
					Counter64,
				hwSACUserStat7thProtocolPktDnNum
					Counter64,
				hwSACUserStat7thProtocolByteDnNum
					Counter64,
				hwSACUserStat8thProtocolName
					OCTET STRING,
				hwSACUserStat8thProtocolPktUpNum
					Counter64,
				hwSACUserStat8thProtocolByteUpNum
					Counter64,
				hwSACUserStat8thProtocolPktDnNum
					Counter64,
				hwSACUserStat8thProtocolByteDnNum
					Counter64,
				hwSACUserStat9thProtocolName
					OCTET STRING,
				hwSACUserStat9thProtocolPktUpNum
					Counter64,
				hwSACUserStat9thProtocolByteUpNum
					Counter64,
				hwSACUserStat9thProtocolPktDnNum
					Counter64,
				hwSACUserStat9thProtocolByteDnNum
					Counter64,
				hwSACUserStat10thProtocolName
					OCTET STRING,
				hwSACUserStat10thProtocolPktUpNum
					Counter64,
				hwSACUserStat10thProtocolByteUpNum
					Counter64,
				hwSACUserStat10thProtocolPktDnNum
					Counter64,
				hwSACUserStat10thProtocolByteDnNum
					Counter64,
				hwSACUserTop10StatClear
					Integer32,
				hwSACUserTop10StatRowstatus
					RowStatus 
			 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.1
		hwSACUserTop10StatUserMac OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.2
		hwSACUserTop10StatType OBJECT-TYPE
			SYNTAX INTEGER
				{
				total(1),
				period(2)
				}
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.3
		hwSACUserStatTotalPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.4
		hwSACUserStatTotalByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 4 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.5
		hwSACUserStatTotalPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 5 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.6
		hwSACUserStatTotalByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 6 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.7
		hwSACUserStat1stProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 7 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.8
		hwSACUserStat1stProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 8 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.9
		hwSACUserStat1stProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 9 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.10
		hwSACUserStat1stProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 10 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.11
		hwSACUserStat1stProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 11 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.12
		hwSACUserStat2ndProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 12 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.13
		hwSACUserStat2ndProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 13 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.14
		hwSACUserStat2ndProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 14 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.15
		hwSACUserStat2ndProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 15 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.16
		hwSACUserStat2ndProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 16 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.17
		hwSACUserStat3rdProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 17 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.18
		hwSACUserStat3rdProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 18 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.19
		hwSACUserStat3rdProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 19 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.20
		hwSACUserStat3rdProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 20 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.21
		hwSACUserStat3rdProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 21 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.22
		hwSACUserStat4thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 22 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.23
		hwSACUserStat4thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 23 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.24
		hwSACUserStat4thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 24 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.25
		hwSACUserStat4thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 25 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.26
		hwSACUserStat4thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 26 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.27
		hwSACUserStat5thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 27 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.28
		hwSACUserStat5thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 28 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.29
		hwSACUserStat5thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 29 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.30
		hwSACUserStat5thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 30 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.31
		hwSACUserStat5thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 31 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.32
		hwSACUserStat6thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 32 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.33
		hwSACUserStat6thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 33 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.34
		hwSACUserStat6thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 34 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.35
		hwSACUserStat6thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 35 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.36
		hwSACUserStat6thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 36 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.37
		hwSACUserStat7thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 37 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.38
		hwSACUserStat7thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 38 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.39
		hwSACUserStat7thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 39 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.40
		hwSACUserStat7thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 40 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.41
		hwSACUserStat7thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 41 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.42
		hwSACUserStat8thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 42 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.43
		hwSACUserStat8thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 43 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.44
		hwSACUserStat8thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 44 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.45
		hwSACUserStat8thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 45 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.46
		hwSACUserStat8thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 46 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.47
		hwSACUserStat9thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 47 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.48
		hwSACUserStat9thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 48 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.49
		hwSACUserStat9thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 49 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.50
		hwSACUserStat9thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 50 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.51
		hwSACUserStat9thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 51 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.52
		hwSACUserStat10thProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 52 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.53
		hwSACUserStat10thProtocolPktUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 53 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.54
		hwSACUserStat10thProtocolByteUpNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 54 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.55
		hwSACUserStat10thProtocolPktDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 55 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.56
		hwSACUserStat10thProtocolByteDnNum OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 56 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.57
		hwSACUserTop10StatClear OBJECT-TYPE
			SYNTAX Integer32 (1)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 57 }

		 --1.3.6.1.4.1.2011.6.139.20.1.9.1.58
		hwSACUserTop10StatRowstatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSACUserTop10StatEntry 58 }

		--1.3.6.1.4.1.2011.6.139.20.1.10
		hwMediaAwareConfig OBJECT IDENTIFIER ::= { hwSacObjects 10 }

		 --1.3.6.1.4.1.2011.6.139.20.1.10.1
		hwWlanVoiceAware OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(1),
				enable(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwMediaAwareConfig 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.10.2
		hwWlanVideoAware OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(1),
				enable(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwMediaAwareConfig 2 }

		--1.3.6.1.4.1.2011.6.139.20.1.11
		hwVoiceAwareProtocolTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwVoiceAwareProtocolEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSacObjects 11 }

		--1.3.6.1.4.1.2011.6.139.20.1.11.1
		hwVoiceAwareProtocolEntry OBJECT-TYPE
			SYNTAX HwVoiceAwareProtocolEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			INDEX { hwVoiceAwareProtocolName }
			::= { hwVoiceAwareProtocolTable 1 }


		HwVoiceAwareProtocolEntry ::=
			SEQUENCE {				
				hwVoiceAwareProtocolName
					OCTET STRING,
				hwVoiceAwarePortocolEnable
					INTEGER,
				hwVoiceAwarePortocolRowStatus
					RowStatus 
			 }

		 --1.3.6.1.4.1.2011.6.139.20.1.11.1.1
		hwVoiceAwareProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (1..255))
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwVoiceAwareProtocolEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.11.1.2
		hwVoiceAwarePortocolEnable OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(1),
				enable(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwVoiceAwareProtocolEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.20.1.11.1.3
		hwVoiceAwarePortocolRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwVoiceAwareProtocolEntry 3 }

		--1.3.6.1.4.1.2011.6.139.20.1.12
		hwVideoAwareProtocolTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwVideoAwareProtocolEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSacObjects 12 }

		--1.3.6.1.4.1.2011.6.139.20.1.12.1
		hwVideoAwareProtocolEntry OBJECT-TYPE
			SYNTAX HwVideoAwareProtocolEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			INDEX { hwVideoAwareProtocolName }
			::= { hwVideoAwareProtocolTable 1 }


		HwVideoAwareProtocolEntry ::=
			SEQUENCE {				
				hwVideoAwareProtocolName
					OCTET STRING,
				hwVideoAwarePortocolEnable
					INTEGER,
				hwVideoAwarePortocolRowStatus
					RowStatus 
			 }

		 --1.3.6.1.4.1.2011.6.139.20.1.12.1.1
		hwVideoAwareProtocolName OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (1..255))
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwVideoAwareProtocolEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.12.1.2
		hwVideoAwarePortocolEnable OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(1),
				enable(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwVideoAwareProtocolEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.20.1.12.1.3
		hwVideoAwarePortocolRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwVideoAwareProtocolEntry 3 }

		--1.3.6.1.4.1.2011.6.139.20.1.13
		hwLyncRecordTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwLyncRecordEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwSacObjects 13 }

		--1.3.6.1.4.1.2011.6.139.20.1.13.1
		hwLyncRecordEntry OBJECT-TYPE
			SYNTAX HwLyncRecordEntry 
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			INDEX { hwLyncRecordID }
			::= { hwLyncRecordTable 1 }


		HwLyncRecordEntry ::=
			SEQUENCE {				
				hwLyncRecordID
					Unsigned32,
				hwLyncRecordSrcApName
					OCTET STRING,
				hwLyncRecordSrcMAC
					MacAddress,
				hwLyncRecordSrcIP
					IpAddress,
				hwLyncRecordSrcPort
					Unsigned32,
				hwLyncRecordDstApName
					OCTET STRING,
				hwLyncRecordDstMAC
					MacAddress,
				hwLyncRecordDstIP
					IpAddress,
				hwLyncRecordDstPort
					Unsigned32,
				hwLyncRecordCallID
					OCTET STRING,
				hwLyncRecordStartTime
					OCTET STRING,
				hwLyncRecordEndTime
					OCTET STRING,
				hwLyncRecordProtocol
					Unsigned32,
				hwLyncRecordPacketUtilization
					Unsigned32,
				hwLyncRecordJitterInterArrival
					Unsigned32,
				hwLyncRecordJitterInterArrivalMax
					Unsigned32,
				hwLyncRecordRoundTrip
					Unsigned32,
				hwLyncRecordRoundTripMax
					Unsigned32,
				hwLyncRecordHealerPacketDropRatio
					OCTET STRING,
				hwLyncRecordDegradationAvg
					OCTET STRING,
				hwLyncRecordRatioConcealedSamplesAvg
					OCTET STRING,
				hwLyncRecordBurstGapDuration
					Unsigned32,
				hwLyncRecordDegradationMax
					OCTET STRING,
				hwLyncRecordRecvListenMOSMin
					OCTET STRING,
				hwLyncRecordRecvListenMOS
					OCTET STRING,
				hwLyncRecordOverallMinNetworkMOS
					OCTET STRING,
				hwLyncRecordOverallAvgNetworkMOS
					OCTET STRING,
				hwLyncRecordAppliedBandwidthLimit
					Unsigned32,
				hwLyncRecordRowstatus
					RowStatus 
			 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.1
		hwLyncRecordID OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 1 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.2
		hwLyncRecordSrcApName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 2 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.3
		hwLyncRecordSrcMAC OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 3 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.4
		hwLyncRecordSrcIP OBJECT-TYPE
			SYNTAX IpAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 4 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.5
		hwLyncRecordSrcPort OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 5 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.6
		hwLyncRecordDstApName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 6 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.7
		hwLyncRecordDstMAC OBJECT-TYPE
			SYNTAX MacAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 7 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.8
		hwLyncRecordDstIP OBJECT-TYPE
			SYNTAX IpAddress
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 8 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.9
		hwLyncRecordDstPort OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 9 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.10
		hwLyncRecordCallID OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 10 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.11
		hwLyncRecordStartTime OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 11 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.12
		hwLyncRecordEndTime OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 12 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.13
		hwLyncRecordProtocol OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 13 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.14
		hwLyncRecordPacketUtilization OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 14 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.15
		hwLyncRecordJitterInterArrival OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 15 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.16
		hwLyncRecordJitterInterArrivalMax OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 16 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.17
		hwLyncRecordRoundTrip OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 17 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.18
		hwLyncRecordRoundTripMax OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 18 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.19
		hwLyncRecordHealerPacketDropRatio OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 19 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.20
		hwLyncRecordDegradationAvg OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 20 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.21
		hwLyncRecordRatioConcealedSamplesAvg OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 21 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.22
		hwLyncRecordBurstGapDuration OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 22 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.23
		hwLyncRecordDegradationMax OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 23 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.24
		hwLyncRecordRecvListenMOSMin OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 24 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.25
		hwLyncRecordRecvListenMOS OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 25 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.26
		hwLyncRecordOverallMinNetworkMOS OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 26 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.27
		hwLyncRecordOverallAvgNetworkMOS OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 27 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.28
		hwLyncRecordAppliedBandwidthLimit OBJECT-TYPE
			SYNTAX Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 28 }

		 --1.3.6.1.4.1.2011.6.139.20.1.13.1.29
		hwLyncRecordRowstatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwLyncRecordEntry 29 }

		--1.3.6.1.4.1.2011.6.139.20.2
		hwWlanSacConformance OBJECT IDENTIFIER ::= { hwWlanSac 2 }

		--1.3.6.1.4.1.2011.6.139.20.2.1
		hwWlanSacCompliances OBJECT IDENTIFIER ::= { hwWlanSacConformance 1 }

		--1.3.6.1.4.1.2011.6.139.20.2.1.1
		hwWlanSacCompliance MODULE-COMPLIANCE
			STATUS current
			DESCRIPTION 
				"Description."
			MODULE
					MANDATORY-GROUPS { hwWlanSACGroup }
			::= { hwWlanSacCompliances 1 }

		--1.3.6.1.4.1.2011.6.139.20.2.2
		hwWlanSacObjectGroups OBJECT IDENTIFIER ::= { hwWlanSacConformance 2 }

		--1.3.6.1.4.1.2011.6.139.20.2.2.1
		hwWlanSACGroup OBJECT-GROUP
			OBJECTS { hwSACEnableOper, hwSACEnableRuleLibName, hwSACProtocolGroupRowstatus, hwSACProGroupProRowstatus, 
			hwSACVapStatProtocolName, hwSACVapStatProtocolPktUpNum, hwSACVapStatProtocolByteUpNum, hwSACVapStatProtocolPktDnNum, 
			hwSACVapStatProtocolByteDnNum, hwSACVapStatClear, hwSACVapStatRowstatus, 
			hwSACUserStatProtocolName, hwSACUserStatProtocolPktUpNum, hwSACUserStatProtocolByteUpNum, hwSACUserStatProtocolPktDnNum, 
			hwSACUserStatProtocolByteDnNum, hwSACUserStatClear, hwSACUserStatRowstatus, hwSACAppListAppID, 
			hwSACAppListAppName, hwSACAppListRowstatus, hwSACInfoSACEnable, hwSACInfoSignatureState, hwSACInfoSignatureName, 
			hwSACInfoSignatureVersion, hwSACInfoSignatureDate, hwSACInfoAppNum, 
			hwSACVapStatTotalPktUpNum, hwSACVapStatTotalByteUpNum, hwSACVapStatTotalPktDnNum, 
			hwSACVapStatTotalByteDnNum, hwSACVapStat1stProtocolName, hwSACVapStat1stProtocolPktUpNum, hwSACVapStat1stProtocolByteUpNum, hwSACVapStat1stProtocolPktDnNum, 
			hwSACVapStat1stProtocolByteDnNum, hwSACVapStat2ndProtocolName, hwSACVapStat2ndProtocolPktUpNum, hwSACVapStat2ndProtocolByteUpNum, hwSACVapStat2ndProtocolPktDnNum, 
			hwSACVapStat2ndProtocolByteDnNum, hwSACVapStat3rdProtocolName, hwSACVapStat3rdProtocolPktUpNum, hwSACVapStat3rdProtocolByteUpNum, hwSACVapStat3rdProtocolPktDnNum, 
			hwSACVapStat3rdProtocolByteDnNum, hwSACVapStat4thProtocolName, hwSACVapStat4thProtocolPktUpNum, hwSACVapStat4thProtocolByteUpNum, hwSACVapStat4thProtocolPktDnNum, 
			hwSACVapStat4thProtocolByteDnNum, hwSACVapStat5thProtocolName, hwSACVapStat5thProtocolPktUpNum, hwSACVapStat5thProtocolByteUpNum, hwSACVapStat5thProtocolPktDnNum, 
			hwSACVapStat5thProtocolByteDnNum, hwSACVapStat6thProtocolName, hwSACVapStat6thProtocolPktUpNum, hwSACVapStat6thProtocolByteUpNum, hwSACVapStat6thProtocolPktDnNum, 
			hwSACVapStat6thProtocolByteDnNum, hwSACVapStat7thProtocolName, hwSACVapStat7thProtocolPktUpNum, hwSACVapStat7thProtocolByteUpNum, hwSACVapStat7thProtocolPktDnNum, 
			hwSACVapStat7thProtocolByteDnNum, hwSACVapStat8thProtocolName, hwSACVapStat8thProtocolPktUpNum, hwSACVapStat8thProtocolByteUpNum, hwSACVapStat8thProtocolPktDnNum, 
			hwSACVapStat8thProtocolByteDnNum, hwSACVapStat9thProtocolName, hwSACVapStat9thProtocolPktUpNum, hwSACVapStat9thProtocolByteUpNum, hwSACVapStat9thProtocolPktDnNum, 
			hwSACVapStat9thProtocolByteDnNum, hwSACVapStat10thProtocolName, hwSACVapStat10thProtocolPktUpNum, hwSACVapStat10thProtocolByteUpNum, hwSACVapStat10thProtocolPktDnNum, 
			hwSACVapStat10thProtocolByteDnNum, hwSACVapTop10StatClear, hwSACVapTop10StatRowstatus, 
			hwSACUserStatTotalPktUpNum, hwSACUserStatTotalByteUpNum, hwSACUserStatTotalPktDnNum, hwSACUserStatTotalByteDnNum, hwSACUserStat1stProtocolName, 
			hwSACUserStat1stProtocolPktUpNum, hwSACUserStat1stProtocolByteUpNum, hwSACUserStat1stProtocolPktDnNum, hwSACUserStat1stProtocolByteDnNum, hwSACUserStat2ndProtocolName, 
			hwSACUserStat2ndProtocolPktUpNum, hwSACUserStat2ndProtocolByteUpNum, hwSACUserStat2ndProtocolPktDnNum, hwSACUserStat2ndProtocolByteDnNum, hwSACUserStat3rdProtocolName, 
			hwSACUserStat3rdProtocolPktUpNum, hwSACUserStat3rdProtocolByteUpNum, hwSACUserStat3rdProtocolPktDnNum, hwSACUserStat3rdProtocolByteDnNum, hwSACUserStat4thProtocolName, 
			hwSACUserStat4thProtocolPktUpNum, hwSACUserStat4thProtocolByteUpNum, hwSACUserStat4thProtocolPktDnNum, hwSACUserStat4thProtocolByteDnNum, hwSACUserStat5thProtocolName, 
			hwSACUserStat5thProtocolPktUpNum, hwSACUserStat5thProtocolByteUpNum, hwSACUserStat5thProtocolPktDnNum, hwSACUserStat5thProtocolByteDnNum, hwSACUserStat6thProtocolName, 
			hwSACUserStat6thProtocolPktUpNum, hwSACUserStat6thProtocolByteUpNum, hwSACUserStat6thProtocolPktDnNum, hwSACUserStat6thProtocolByteDnNum, hwSACUserStat7thProtocolName, 
			hwSACUserStat7thProtocolPktUpNum, hwSACUserStat7thProtocolByteUpNum, hwSACUserStat7thProtocolPktDnNum, hwSACUserStat7thProtocolByteDnNum, hwSACUserStat8thProtocolName, 
			hwSACUserStat8thProtocolPktUpNum, hwSACUserStat8thProtocolByteUpNum, hwSACUserStat8thProtocolPktDnNum, hwSACUserStat8thProtocolByteDnNum, hwSACUserStat9thProtocolName, 
			hwSACUserStat9thProtocolPktUpNum, hwSACUserStat9thProtocolByteUpNum, hwSACUserStat9thProtocolPktDnNum, hwSACUserStat9thProtocolByteDnNum, hwSACUserStat10thProtocolName, 
			hwSACUserStat10thProtocolPktUpNum, hwSACUserStat10thProtocolByteUpNum, hwSACUserStat10thProtocolPktDnNum, hwSACUserStat10thProtocolByteDnNum, hwSACUserTop10StatClear, 
			hwSACUserTop10StatRowstatus, hwWlanVoiceAware, hwWlanVideoAware, hwVoiceAwarePortocolEnable, 
			hwVoiceAwarePortocolRowStatus, hwVideoAwarePortocolEnable, hwVideoAwarePortocolRowStatus, 
			hwLyncRecordSrcApName, hwLyncRecordSrcMAC, hwLyncRecordSrcIP, hwLyncRecordSrcPort, hwLyncRecordDstApName, 
			hwLyncRecordDstMAC, hwLyncRecordDstIP, hwLyncRecordDstPort, hwLyncRecordCallID, hwLyncRecordStartTime, 
			hwLyncRecordEndTime, hwLyncRecordProtocol, hwLyncRecordPacketUtilization, hwLyncRecordJitterInterArrival, hwLyncRecordJitterInterArrivalMax, 
			hwLyncRecordRoundTrip, hwLyncRecordRoundTripMax, hwLyncRecordHealerPacketDropRatio, hwLyncRecordDegradationAvg, hwLyncRecordRatioConcealedSamplesAvg, 
			hwLyncRecordBurstGapDuration, hwLyncRecordDegradationMax, hwLyncRecordRecvListenMOSMin, hwLyncRecordRecvListenMOS, hwLyncRecordOverallMinNetworkMOS, 
			hwLyncRecordOverallAvgNetworkMOS, hwLyncRecordAppliedBandwidthLimit, hwLyncRecordRowstatus }
			STATUS current
			DESCRIPTION 
				"Description."
			::= { hwWlanSacObjectGroups 1 }


	END
--
-- HUAWEI-WLAN-SAC-MIB.mib
--
