--  ==================================================================
-- Copyright (C) 2016 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description: HUAWEI-EVC-MIB provides information about EVC
-- Reference:
-- Version: V1.01
-- History:
-- <author>,   <date>,  <contents>
--  HUAWEI   2014-09-011  EVC private MIB
-- ==================================================================
-- ==================================================================
-- 
-- Variables and types are imported
-- 
-- ==================================================================

	HUAWEI-EVC-MIB DEFINITIONS ::= BEGIN
 
		IMPORTS		
			hwDatacomm			
				FROM HUAWEI-MIB			
			OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP			
				FROM SNMPv2-CONF			
			Unsigned32, Counter64, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE			
				FROM SNMPv2-SMI;

-- September 11, 2014 at 16:55 GMT
		hwEVC MODULE-IDENTITY 
			LAST-UPDATED "201606170918Z"		-- September 11, 2014 at 16:55 GMT
			ORGANIZATION 
				"Huawei Technologies Co.,Ltd."
			CONTACT-INFO 
				"Huawei Industrial Base
				Bantian, Longgang
				 Shenzhen 518129
				 People's Republic of China
				 Website: http://www.huawei.com
				 Email: support@huawei.com
				"
			DESCRIPTION 
				"The EVC MIB module is defined to manage the EVC configuration under system or bride-domain view."
			REVISION "201606170918Z"		-- September 11, 2014 at 16:55 GMT
			DESCRIPTION
				"modify the range of Bridge-domain  ."
			REVISION "201409111655Z"		-- September 11, 2014 at 16:55 GMT
			DESCRIPTION
				"The initial revision of this MIB module."
			::= { hwDatacomm 336 }
		
--  Node definitions

		hwEVCMngObjects OBJECT IDENTIFIER ::= { hwEVC 1 }
		
		hwBDStatTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwBDStatEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"hwBDStatTable used to statistic total number of the inbound and outbound packets of bridge-domains."
			::= { hwEVCMngObjects 1 }
		
		hwBDStatEntry OBJECT-TYPE
			SYNTAX HwBDStatEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"The entry of hwBDStatTable."
			INDEX { hwBDStatBDID}
			::= { hwBDStatTable 1 }
		
		HwBDStatEntry ::=
			SEQUENCE { 
				hwBDStatBDID
					Unsigned32,
				hwBDStatInboundPackets
					Counter64,
				hwBDStatOutboundPackets
					Counter64,	
				hwBDStatInboundBytes
					Counter64,
				hwBDStatOutboundBytes
					Counter64	        
			 }

		hwBDStatBDID OBJECT-TYPE
			SYNTAX Unsigned32 (1..16777215)
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Bridge-domain id."
			::= { hwBDStatEntry 1 }		
		
		hwBDStatInboundPackets OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Inbound packets."
			::= { hwBDStatEntry 2 }

		hwBDStatOutboundPackets OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Outbound packets."
			::= { hwBDStatEntry 3 }

		hwBDStatInboundBytes OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Inbound bytes."
			::= { hwBDStatEntry 4 }

		hwBDStatOutboundBytes OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Outbound bytes."
			::= { hwBDStatEntry 5 }
			
		hwEVCConformance OBJECT IDENTIFIER ::= { hwEVC 2 }
		
		hwEVCCompliances OBJECT IDENTIFIER ::= { hwEVCConformance 1 }
		
		hwEVCCompliance MODULE-COMPLIANCE
        STATUS current
        DESCRIPTION
            "This is the EVC compliance."
        MODULE -- this module
            MANDATORY-GROUPS { hwBDStatGroup }
        ::= { hwEVCCompliances 1 }
		
		hwEVCGroups OBJECT IDENTIFIER ::= { hwEVCConformance 2 }
		
		hwBDStatGroup OBJECT-GROUP
			OBJECTS { hwBDStatInboundPackets, hwBDStatOutboundPackets, hwBDStatInboundBytes, hwBDStatOutboundBytes}
			STATUS current
			DESCRIPTION 
				"This is the bridge-domain statistics group."
			::= { hwEVCGroups 1 }	
					
	END