-- =================================================================
-- Copyright (C) 2003 by  HUAWEI TECHNOLOGIES. All rights reserved.
--
-- Description:HUAWEI-BRAS-VSM-MIB DEFINITIONS
-- Reference:
-- Version: V1.0
-- History:
--     
-- =================================================================

    HUAWEI-BRAS-VSM-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            hwBRASMib            
                FROM HUAWEI-MIB
            DisplayString, RowStatus, TruthValue, MacAddress, DateAndTime            
                FROM SNMPv2-TC
            EnabledStatus            
                FROM P-BRIDGE-MIB 
            OBJECT-TYPE, MODULE-IDENTITY            
                FROM SNMPv2-SMI;
            
        hwBRASVsm MODULE-IDENTITY 
            LAST-UPDATED "200504181334Z"        -- April 18, 2005 at 13:34 GMT
            ORGANIZATION 
                "Huawei Technologies Co., Ltd.
                "
            CONTACT-INFO 
                "
                NanJing Institute,Huawei Technologies Co.,Ltd.
                HuiHong Mansion,No.91 BaiXia Rd.
                NanJing, P.R. of China
                Zipcode:210001
                 
                Http://www.huawei.com                                       
                E-mail:support@huawei.com "
            DESCRIPTION 
                "The MIB contains objects of module VSM."
            ::= { hwBRASMib 9 }


--
-- Node definitions
--
    
--  ==================================================================
-- 
-- ======================= definition begin =========================
-- 
-- ================================================================== 

    hwVsmSetFlowQryTLenTable OBJECT IDENTIFIER ::= { hwBRASVsm 1 }
    --  ============== hwVsmSetFlowQryTLenTable  define beginning ==============
        
        hwVsmSetTimeLen OBJECT-TYPE
            SYNTAX Integer32  (2..10)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Flow query time length."
            DEFVAL { 2 }                 
            ::= { hwVsmSetFlowQryTLenTable 1 }        
    --  ============== hwVsmSetFlowQryTLenTable  define end ==============         

    --  ============== hwVsmServicePolicyTable  define beginning ==============
    hwVsmServicePolicyTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwVsmServicePolicyEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                " VSM service policy configuration."
            ::= { hwBRASVsm 2 }
        
        hwVsmServicePolicyEntry OBJECT-TYPE
            SYNTAX HwVsmServicePolicyEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                " Service policy entry,
                service policy name is identified as key word, direct a service policy when create, and don't allow to change.
                Index item is hwVsmServicePolicyName node. The table is used for configuration of service policy.
                Operation restriction description£º
                1. must input service policy name when created.
                2. if a service is being used for users, can't be deleted.
                3. if a service is being used by domain, can't be deleted."
            INDEX { hwVsmServicePolicyName }
            ::= { hwVsmServicePolicyTable 1 }
        
        HwVsmServicePolicyEntry ::=  SEQUENCE { 
                hwVsmServicePolicyName
                    DisplayString,
                hwVsmAcctSchemeName
                    DisplayString,
                hwVsmTrafficPolicyName
                    DisplayString,
                hwVsmSetIdleCutTime
                    Integer32,
                hwVsmSetIdleCutFlow
                    Integer32,
                hwVsmSevicePolicyRowStatus
                    RowStatus,
                hwVsmOutTrafficPolicyName
                    DisplayString,
                hwVsmDaaPolicyFlag
                    INTEGER,
                hwVsmSetTariffLevel1
                    DisplayString,
                hwVsmSetTariffLevel2
                    DisplayString,
                hwVsmSetTariffLevel3
                    DisplayString,
                hwVsmSetTariffLevel4
                    DisplayString,
                hwVsmSetTariffLevel5
                    DisplayString,
                hwVsmSetTariffLevel6
                    DisplayString,
                hwVsmSetTariffLevel7
                    DisplayString,
                hwVsmSetTariffLevel8
                    DisplayString,
                hwVsmTariffLevel1AcctSwitch
                    EnabledStatus,
                hwVsmTariffLevel2AcctSwitch
                    EnabledStatus,
                hwVsmTariffLevel3AcctSwitch
                    EnabledStatus,
                hwVsmTariffLevel4AcctSwitch
                    EnabledStatus,
                hwVsmTariffLevel5AcctSwitch
                    EnabledStatus,
                hwVsmTariffLevel6AcctSwitch
                    EnabledStatus,
                hwVsmTariffLevel7AcctSwitch
                    EnabledStatus,
                hwVsmTariffLevel8AcctSwitch
                    EnabledStatus            
                                                                               
             }

        hwVsmServicePolicyName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " The service policy name, is key word, must direct a service policy when create, and don't allow to change."
            ::= { hwVsmServicePolicyEntry 1 }
        
        hwVsmAcctSchemeName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The account scheme name, is key word, must direct a service policy when create, and don't allow to change."
            ::= { hwVsmServicePolicyEntry 2 }
        
        hwVsmTrafficPolicyName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " In traffic policy name£¬optional, if bind, must direct an acl policy name.
                  If the acl policy policy ACL has been bound by a service policy, it can't be bound by another service policy.
                "
            ::= { hwVsmServicePolicyEntry 3 }
        
        hwVsmSetIdleCutTime OBJECT-TYPE
            SYNTAX Integer32(0..120)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " The idle cut time, 0 means invalid, units: minute."
            DEFVAL { 0 }
            ::= { hwVsmServicePolicyEntry 4 }

        hwVsmSetIdleCutFlow OBJECT-TYPE
            SYNTAX Integer32 (0..768000)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " The idle cut data flow, units: KByte/min, range: 0~100*1024*60/8.
                "
            DEFVAL { 60 }
            ::= { hwVsmServicePolicyEntry 5 }

        hwVsmSevicePolicyRowStatus OBJECT-TYPE
            SYNTAX RowStatus     
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " The row administrator status, supporting add, delete, modify."
            ::= { hwVsmServicePolicyEntry 6 }         
            
       hwVsmOutTrafficPolicyName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " The out traffic policy name£¬optional, if bind, must direct an acl policy name.
                  If the acl policy policy ACL has been bound by a service policy, it can't be bound by another service policy.
                "
            ::= { hwVsmServicePolicyEntry 7 }
            
         hwVsmDaaPolicyFlag OBJECT-TYPE
            SYNTAX INTEGER
                    {
                    vas(0),
                    daa(1)
                    }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " The service policy type :                
                  vas(0): normal policy;
                  daa(1): destination add account policy.
                "
            DEFVAL { 0 }
            ::= { hwVsmServicePolicyEntry 8 }
            
        hwVsmSetTariffLevel1 OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The QOS profile of tariff level 1.
                "
            ::= { hwVsmServicePolicyEntry 9 }
        
        hwVsmSetTariffLevel2 OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                 The QOS profile of tariff level 2.
                "
            ::= { hwVsmServicePolicyEntry 10 }
            
        hwVsmSetTariffLevel3 OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The QOS profile of tariff level 3.
                "
            ::= { hwVsmServicePolicyEntry 11 }
        
        hwVsmSetTariffLevel4 OBJECT-TYPE
                SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The QOS profile of tariff level 4.
                "
            ::= { hwVsmServicePolicyEntry 12 }
        
        hwVsmSetTariffLevel5 OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The QOS profile of tariff level 5.
                "
            ::= { hwVsmServicePolicyEntry 13 }
        
        hwVsmSetTariffLevel6 OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The QOS profile of tariff level 6.
                "
            ::= { hwVsmServicePolicyEntry 14 }
        
        hwVsmSetTariffLevel7 OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The QOS profile of tariff level 7.
                "
            ::= { hwVsmServicePolicyEntry 15 }
        
        hwVsmSetTariffLevel8 OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The QOS profile of tariff level 8.
                "
            ::= { hwVsmServicePolicyEntry 16 }
        hwVsmTariffLevel1AcctSwitch OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The Account switch of tariff level 1.  
                acct-on  (1)     
                acct-off (2)
                "   
            DEFVAL { 1 }
            ::= { hwVsmServicePolicyEntry 17 }

        hwVsmTariffLevel2AcctSwitch OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The Account switch of tariff level 2.
                acct-on  (1)     
                acct-off (2)
                "   
             DEFVAL { 1 }
           ::= { hwVsmServicePolicyEntry 18 }

       hwVsmTariffLevel3AcctSwitch OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The Account switch of tariff level 3.
                acct-on  (1)     
                acct-off (2)
                "   
            DEFVAL { 1 }
            ::= { hwVsmServicePolicyEntry 19 }

         hwVsmTariffLevel4AcctSwitch OBJECT-TYPE
            SYNTAX  EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The Account switch of tariff level 4.
                acct-on  (1)     
                acct-off (2)
                "   
            DEFVAL { 1 }
            ::= { hwVsmServicePolicyEntry 20 }

         hwVsmTariffLevel5AcctSwitch OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The Account switch of tariff level 5.
                acct-on  (1)     
                acct-off (2)
                "   
            DEFVAL { 1 }
            ::= { hwVsmServicePolicyEntry 21 }

         hwVsmTariffLevel6AcctSwitch OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The Account switch of tariff level 6.
                acct-on  (1)     
                acct-off (2)
                "   
                DEFVAL { 1 }
            ::= { hwVsmServicePolicyEntry 22 }

        hwVsmTariffLevel7AcctSwitch OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The Account switch of tariff level 7.
                acct-on  (1)     
                acct-off (2)
                "   
                DEFVAL { 1 }
            ::= { hwVsmServicePolicyEntry 23 }

        hwVsmTariffLevel8AcctSwitch OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " 
                The Account switch of tariff level 8.
                acct-on  (1)     
                acct-off (2)
                "   
            DEFVAL { 1 }
            ::= { hwVsmServicePolicyEntry 24 }

    --  ============== hwVsmServicePolicyTable  define end ==============         
                
    --  ============== hwVsmValServiceTable  define beginning ==============
    hwVsmValServiceTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwVsmValServiceEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                " The VSM value-added-service detail. "
            ::= { hwBRASVsm 3 }
        
        hwVsmValServiceEntry OBJECT-TYPE
            SYNTAX HwVsmValServiceEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                  " Value-added-service detail entry,
                      VSM value-added-service detail, service ID is key word."
            INDEX { hwVsmServiceID, hwVsmServiceSlot}
            ::= { hwVsmValServiceTable 1 }
        
        HwVsmValServiceEntry ::=  SEQUENCE { 
                hwVsmServiceID
                    Integer32,
                hwVsmUserID
                    Integer32,
                hwVsmFlowNum
                    Integer32,
                hwVsmServiceSource
                    INTEGER,
                hwVsmServiceSlot
                    Integer32,
                hwVsmValServicePolicy
                    DisplayString,
                hwVsmAcctMethod
                    INTEGER,
                hwVsmAcctStartTime
                    DisplayString,
                hwVsmAcctServerName
                    DisplayString,
                hwVsmTwoLevelAcctServerName
                    DisplayString,
                hwVsmPhyInfoAcctServerName
                    DisplayString,
                hwVsmServiceIdleCutTime
                    Integer32,
                hwVsmServiceIdleCutFlow
                    Integer32,
                hwVsmUpPacketNum
                    Counter64,
                hwVsmUpByteNum
                    Counter64,
                hwVsmDownPacketNum
                    Counter64,
                hwVsmDownByteNum
                    Counter64,
                hwVsmDownloadServerName
                    DisplayString,    
                hwVsmAcctServerType
                    DisplayString                                                                                                                                                                                           
             }

        hwVsmServiceID OBJECT-TYPE
            SYNTAX Integer32(0..32767)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " 
                The value-added-service ID table index.
                "
            ::= { hwVsmValServiceEntry 1 }
        
        hwVsmUserID OBJECT-TYPE
            SYNTAX Integer32(0..65535)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " The user ID."
            DEFVAL { 4294967295 }
            ::= { hwVsmValServiceEntry 2 }    
                                
        hwVsmFlowNum OBJECT-TYPE
            SYNTAX Integer32(0..16)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " The service flow number, maximum 16 flows per service.
                "
            DEFVAL { 0 }
            ::= { hwVsmValServiceEntry 3 }    
            
        hwVsmServiceSource OBJECT-TYPE
            SYNTAX INTEGER
                {
                vsmSourceDefault(0),
                vsmSourceSig(1),
                vsmSourceIptn(2),
                vsmSourceRadius(3),
                vsmSourceBod(4),
                vsmSourceCopsNet(5),
                vsmSourceCopsNetPm(6),
                vsmSourceCopsUser(7),
                vsmSourceCopsPm(8),
                vsmSourceBmi(9),
                vsmSourceIpBod(10)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " The value-added-service source:
                  vsmSourceDefault(0):   local; 
                  vsmSourceSig(1):       from sig server;
                  vsmSourceIptn(2):      from IPTN server;
                  vsmSourceRadius(3):    from Radius server;
                  vsmSourceBod(4):       from BOD server;
                  vsmSourceCopsNet(5):   from COPS net policy content;
                  vsmSourceCopsNetPm(6): from cops user poicy name;
                  vsmSourceCopsUser(7):  from COPS net policy content;
                  vsmSourceCopsPm(8):    from COPS user policy name;
                  vsmSourceBmi(9):       from BMI server;
                  vsmSourceIpBod(10):    from Liangchuang BOD server."
            ::= { hwVsmValServiceEntry 4 }            
        
        hwVsmServiceSlot OBJECT-TYPE
            SYNTAX Integer32(1..16)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " 
                 The slot number corresponding slot of service, table index.
                "
            ::= { hwVsmValServiceEntry 5 }    
                                        
        hwVsmValServicePolicy OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The value-added-service policy name, optional, if not used , fill '--'.
                "
            ::= { hwVsmValServiceEntry 6 }
        
        hwVsmAcctMethod OBJECT-TYPE
            SYNTAX INTEGER
                {
                local(1),
                none(2),
                radius(3),
                cops(4)        
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The account method, it may be Local,None,Radius,Cops.
                "
            ::= { hwVsmValServiceEntry 7 }
        
        hwVsmAcctStartTime OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " 
                 The account start time, optional, if don't account, fill '--'.
                "
            ::= { hwVsmValServiceEntry 8 }
            
        hwVsmAcctServerName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The account server name show accounting server name. If don't account, show '--'.
                "
            ::= { hwVsmValServiceEntry 9 }
            
        hwVsmTwoLevelAcctServerName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The two level account server name, optional, if don't account, show  '--'.
                "
            ::= { hwVsmValServiceEntry 10 }
            
        hwVsmPhyInfoAcctServerName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The physical information account server name, optional, if don't exist, show  '--'.
                "
            ::= { hwVsmValServiceEntry 11 }    
        
        hwVsmServiceIdleCutTime OBJECT-TYPE
            SYNTAX Integer32(0..120)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The value-added-service idle cut time, 0 means invalid, units: minute.
                "
            DEFVAL { 0 }
            ::= { hwVsmValServiceEntry 12 }

        hwVsmServiceIdleCutFlow OBJECT-TYPE
            SYNTAX Integer32 (0..768000)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The value-added-service idle cut data flow, units: kbyte/min, range: 0~100*1024*60/8.
                "
            DEFVAL { 60 }
            ::= { hwVsmValServiceEntry 13 }
            
        hwVsmUpPacketNum OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The value-added-service up packet number(64 bit).
                "
            ::= { hwVsmValServiceEntry 14 }
        
        hwVsmUpByteNum OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The value-added-service up byte number(64 bit).
                "
            ::= { hwVsmValServiceEntry 15 }    
        
        hwVsmDownPacketNum OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The value-added-service down packet number(64 bit).
                "
            ::= { hwVsmValServiceEntry 16 }
            
        hwVsmDownByteNum OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The value-added-service down byte number(64 bit).
                "
            ::= { hwVsmValServiceEntry 17 }    
            
        hwVsmDownloadServerName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The download policy server name.
                "
            ::= { hwVsmValServiceEntry 18 }
            
        hwVsmAcctServerType OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..8))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                 The account server type.
                "
            ::= { hwVsmValServiceEntry 19 }    
    --  ============== hwVsmValServiceTable  define end ==============   

    --  ============== hwVsmAcctServicePolicyTable  define ==============
        hwVsmAcctServicePolicyEnableTable OBJECT IDENTIFIER ::= { hwBRASVsm 5 }

        hwVsmAcctServicePolicyEnable  OBJECT-TYPE
            SYNTAX DisplayString (SIZE (1..32))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " The Accounting service Enable. "
            ::= { hwVsmAcctServicePolicyEnableTable 1 }  
        hwVsmAcctServicePolicyDisable  OBJECT-TYPE
            SYNTAX Integer32 (1)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                " The Accounting service Disable. "
            ::= { hwVsmAcctServicePolicyEnableTable 2 }


    --  ============== hwVsmAcctServicePolicyTable  define end ==============
      

    --  ============== conformance information ==============
        hwVsmConformance OBJECT IDENTIFIER ::= { hwBRASVsm 4 }
        
        hwVsmCompliances OBJECT IDENTIFIER ::= { hwVsmConformance 1 }
        hwVsmCompliance MODULE-COMPLIANCE
               STATUS      current
               DESCRIPTION
                   "The compliance statement for systems supporting 
                the this module."

               MODULE      -- this module
               MANDATORY-GROUPS    {hwVsmSetFlowQryTLenObjectGroup, hwVsmServicePolicyObjectGroup,
                                    hwVsmValServiceObjectGroup }  
                                               
              ::= { hwVsmCompliances 1 }  
              
          
        --  ============== groups ==============  
        hwVsmObjectGroups OBJECT IDENTIFIER ::= { hwVsmConformance 2 } 
        
        hwVsmSetFlowQryTLenObjectGroup OBJECT-GROUP
            OBJECTS { hwVsmSetTimeLen }
            STATUS current
            DESCRIPTION 
                "Flow query time length group."
            ::= { hwVsmObjectGroups 1 }
            
        hwVsmServicePolicyObjectGroup OBJECT-GROUP
            OBJECTS { hwVsmServicePolicyName, hwVsmAcctSchemeName, hwVsmTrafficPolicyName,
                      hwVsmSetIdleCutTime, hwVsmSetIdleCutFlow, hwVsmSevicePolicyRowStatus,
                      hwVsmOutTrafficPolicyName, hwVsmDaaPolicyFlag, hwVsmSetTariffLevel1,
                      hwVsmSetTariffLevel2, hwVsmSetTariffLevel3, hwVsmSetTariffLevel4,
                      hwVsmSetTariffLevel5, hwVsmSetTariffLevel6, hwVsmSetTariffLevel7,
                      hwVsmSetTariffLevel8, hwVsmTariffLevel1AcctSwitch,    
                      hwVsmTariffLevel2AcctSwitch,hwVsmTariffLevel3AcctSwitch,  
                      hwVsmTariffLevel4AcctSwitch, hwVsmTariffLevel5AcctSwitch,
                      hwVsmTariffLevel6AcctSwitch, hwVsmTariffLevel7AcctSwitch,    
                      hwVsmTariffLevel8AcctSwitch }

            STATUS current
            DESCRIPTION 
                "The service policy group."
            ::= { hwVsmObjectGroups 2 }

            
        hwVsmValServiceObjectGroup OBJECT-GROUP
            OBJECTS {hwVsmServiceID, hwVsmUserID, hwVsmFlowNum,
                     hwVsmServiceSource, hwVsmServiceSlot, hwVsmValServicePolicy,
                     hwVsmAcctMethod, hwVsmAcctStartTime, hwVsmAcctServerName,
                     hwVsmTwoLevelAcctServerName, hwVsmPhyInfoAcctServerName,
                     hwVsmServiceIdleCutTime, hwVsmServiceIdleCutFlow, hwVsmUpPacketNum,
                     hwVsmUpByteNum, hwVsmDownPacketNum, hwVsmDownByteNum,
                     hwVsmDownloadServerName, hwVsmAcctServerType }
            STATUS current
            DESCRIPTION 
                "The VSM value service policy group."
            ::= { hwVsmObjectGroups 3 }



        --  ============== conformance information define end ==============                        
    
    END

